(kicad_pcb (version 4) (host pcbnew 4.0.4-stable)
  (general
    (links 71)
    (no_connects 4)
    (area 122.987999 71.806999 191.718001 125.297001)
    (thickness 1.6)
    (drawings 77)
    (tracks 224)
    (zones 0)
    (modules 28)
    (nets 52)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.5)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 4 4)
    (pad_drill 3)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 4)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 +5V)
  (net 3 +3V3)
  (net 4 /ESP_RST)
  (net 5 /SENSOR_RX)
  (net 6 /SENSOR_TX)
  (net 7 /SENSOR_IO2)
  (net 8 /SENSOR_IO1)
  (net 9 "Net-(SHIELD1-PadAD5)")
  (net 10 "Net-(SHIELD1-PadAD4)")
  (net 11 "Net-(SHIELD1-PadAD3)")
  (net 12 "Net-(SHIELD1-PadV_IN)")
  (net 13 "Net-(SHIELD1-Pad3V3)")
  (net 14 "Net-(SHIELD1-PadRST)")
  (net 15 /ESP_TX)
  (net 16 /MC_TX)
  (net 17 /MC_RST)
  (net 18 "Net-(SHIELD1-Pad3)")
  (net 19 /MC_CS)
  (net 20 "Net-(SHIELD1-Pad5)")
  (net 21 "Net-(SHIELD1-Pad6)")
  (net 22 "Net-(SHIELD1-Pad9)")
  (net 23 "Net-(SHIELD1-Pad10)")
  (net 24 "Net-(SHIELD1-Pad11)")
  (net 25 "Net-(SHIELD1-Pad12)")
  (net 26 "Net-(SHIELD1-Pad13)")
  (net 27 "Net-(SHIELD1-PadAREF)")
  (net 28 "Net-(U2-Pad5)")
  (net 29 "Net-(U2-Pad6)")
  (net 30 "Net-(U2-Pad7)")
  (net 31 "Net-(U2-Pad8)")
  (net 32 "Net-(U2-Pad9)")
  (net 33 "Net-(U2-Pad11)")
  (net 34 "Net-(U2-Pad12)")
  (net 35 "Net-(U2-Pad13)")
  (net 36 "Net-(U2-Pad14)")
  (net 37 "Net-(U2-Pad15)")
  (net 38 /ESP_RX)
  (net 39 /ESP_CS)
  (net 40 /ESP_IO_0)
  (net 41 "Net-(U4-Pad10)")
  (net 42 "Net-(U4-Pad13)")
  (net 43 "Net-(U4-Pad14)")
  (net 44 "Net-(U4-Pad2)")
  (net 45 "Net-(U4-Pad4)")
  (net 46 "Net-(U4-Pad5)")
  (net 47 "Net-(U4-Pad6)")
  (net 48 "Net-(U4-Pad7)")
  (net 49 /SW_GND)
  (net 50 /FILTER_OUT)
  (net 51 /SW_GND_G)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.5)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net +5V)
    (add_net /ESP_CS)
    (add_net /ESP_IO_0)
    (add_net /ESP_RST)
    (add_net /ESP_RX)
    (add_net /ESP_TX)
    (add_net /FILTER_OUT)
    (add_net /MC_CS)
    (add_net /MC_RST)
    (add_net /MC_TX)
    (add_net /SENSOR_IO1)
    (add_net /SENSOR_IO2)
    (add_net /SENSOR_RX)
    (add_net /SENSOR_TX)
    (add_net /SW_GND)
    (add_net /SW_GND_G)
    (add_net GND)
    (add_net "Net-(SHIELD1-Pad10)")
    (add_net "Net-(SHIELD1-Pad11)")
    (add_net "Net-(SHIELD1-Pad12)")
    (add_net "Net-(SHIELD1-Pad13)")
    (add_net "Net-(SHIELD1-Pad3)")
    (add_net "Net-(SHIELD1-Pad3V3)")
    (add_net "Net-(SHIELD1-Pad5)")
    (add_net "Net-(SHIELD1-Pad6)")
    (add_net "Net-(SHIELD1-Pad9)")
    (add_net "Net-(SHIELD1-PadAD3)")
    (add_net "Net-(SHIELD1-PadAD4)")
    (add_net "Net-(SHIELD1-PadAD5)")
    (add_net "Net-(SHIELD1-PadAREF)")
    (add_net "Net-(SHIELD1-PadRST)")
    (add_net "Net-(SHIELD1-PadV_IN)")
    (add_net "Net-(U2-Pad11)")
    (add_net "Net-(U2-Pad12)")
    (add_net "Net-(U2-Pad13)")
    (add_net "Net-(U2-Pad14)")
    (add_net "Net-(U2-Pad15)")
    (add_net "Net-(U2-Pad5)")
    (add_net "Net-(U2-Pad6)")
    (add_net "Net-(U2-Pad7)")
    (add_net "Net-(U2-Pad8)")
    (add_net "Net-(U2-Pad9)")
    (add_net "Net-(U4-Pad10)")
    (add_net "Net-(U4-Pad13)")
    (add_net "Net-(U4-Pad14)")
    (add_net "Net-(U4-Pad2)")
    (add_net "Net-(U4-Pad4)")
    (add_net "Net-(U4-Pad5)")
    (add_net "Net-(U4-Pad6)")
    (add_net "Net-(U4-Pad7)")
  )
  (module lib:logo (layer F.Cu) (tedit 5864F904)
    (at 144.526 91.186)
    (fp_text reference G*** (at 0.224 13.314) (layer F.SilkS) hide)
    (fp_text value LOGO (at -0.508 11.684) (layer F.SilkS) hide)
  )
  (module Pin_Headers:Pin_Header_Straight_1x01 (layer F.Cu) (tedit 577BA1C8)
    (at 189.103 89.662)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference HOLE (at 0 -5.1) (layer F.SilkS) hide)
    (fp_text value "" (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4 4) (drill 3) (layers *.Cu *.Mask F.SilkS))
  )
  (module Pin_Headers:Pin_Header_Straight_1x01 (layer F.Cu) (tedit 577BA1C8)
    (at 189.103 117.602)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference HOLE (at 0 -5.1) (layer F.SilkS) hide)
    (fp_text value "" (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4 4) (drill 3) (layers *.Cu *.Mask F.SilkS))
  )
  (module Pin_Headers:Pin_Header_Straight_1x01 (layer F.Cu) (tedit 577BA1C8)
    (at 137.033 122.682)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference HOLE (at 0 -5.1) (layer F.SilkS) hide)
    (fp_text value "" (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4 4) (drill 3) (layers *.Cu *.Mask F.SilkS))
  )
  (module Pin_Headers:Pin_Header_Straight_1x01 (layer F.Cu) (tedit 577BA1C8)
    (at 138.303 74.422)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference HOLE (at 4.826 0.127) (layer F.SilkS) hide)
    (fp_text value "" (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4 4) (drill 3) (layers *.Cu *.Mask F.SilkS))
  )
  (module arduino_shields:ARDUINO_SHIELD_2_040pins (layer F.Cu) (tedit 577BA176)
    (at 123.063 125.222)
    (fp_text reference SHIELD1 (at 26.035 -54.61) (layer F.SilkS) hide)
    (fp_text value ARDUINO_SHIELD (at 10.16 -54.61) (layer F.SilkS) hide)
    (pad AD5 thru_hole oval (at 63.5 -2.54 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(SHIELD1-PadAD5)"))
    (pad AD4 thru_hole oval (at 60.96 -2.54 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(SHIELD1-PadAD4)"))
    (pad AD3 thru_hole oval (at 58.42 -2.54 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(SHIELD1-PadAD3)"))
    (pad AD0 thru_hole oval (at 50.8 -2.54 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 /SENSOR_IO1))
    (pad AD1 thru_hole oval (at 53.34 -2.54 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 /SENSOR_IO2))
    (pad AD2 thru_hole oval (at 55.88 -2.54 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 51 /SW_GND_G))
    (pad V_IN thru_hole oval (at 45.72 -2.54 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(SHIELD1-PadV_IN)"))
    (pad GND2 thru_hole oval (at 43.18 -2.54 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad GND1 thru_hole oval (at 40.64 -2.54 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 3V3 thru_hole oval (at 35.56 -2.54 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(SHIELD1-Pad3V3)"))
    (pad RST thru_hole oval (at 33.02 -2.54 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(SHIELD1-PadRST)"))
    (pad 0 thru_hole oval (at 63.5 -50.8 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 /ESP_TX))
    (pad 1 thru_hole oval (at 60.96 -50.8 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 /MC_TX))
    (pad 2 thru_hole oval (at 58.42 -50.8 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 /MC_RST))
    (pad 3 thru_hole oval (at 55.88 -50.8 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 "Net-(SHIELD1-Pad3)"))
    (pad 4 thru_hole oval (at 53.34 -50.8 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 19 /MC_CS))
    (pad 5 thru_hole oval (at 50.8 -50.8 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 "Net-(SHIELD1-Pad5)"))
    (pad 6 thru_hole oval (at 48.26 -50.8 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(SHIELD1-Pad6)"))
    (pad 7 thru_hole oval (at 45.72 -50.8 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 /SENSOR_TX))
    (pad 8 thru_hole oval (at 41.656 -50.8 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 /SENSOR_RX))
    (pad 9 thru_hole oval (at 39.116 -50.8 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(SHIELD1-Pad9)"))
    (pad 10 thru_hole oval (at 36.576 -50.8 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(SHIELD1-Pad10)"))
    (pad 11 thru_hole oval (at 34.036 -50.8 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 24 "Net-(SHIELD1-Pad11)"))
    (pad 12 thru_hole oval (at 31.496 -50.8 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 25 "Net-(SHIELD1-Pad12)"))
    (pad 13 thru_hole oval (at 28.956 -50.8 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 26 "Net-(SHIELD1-Pad13)"))
    (pad GND3 thru_hole oval (at 26.416 -50.8 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad AREF thru_hole oval (at 23.876 -50.8 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 27 "Net-(SHIELD1-PadAREF)"))
    (pad 5V thru_hole oval (at 38.1 -2.54 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 +5V))
  )
  (module Housings_DIP:DIP-20_W7.62mm_LongPads (layer F.Cu) (tedit 54130A77)
    (at 152.019 89.662)
    (descr "20-lead dip package, row spacing 7.62 mm (300 mils), longer pads")
    (tags "dil dip 2.54 300")
    (fp_text reference U2 (at 3.481 26.088) (layer F.SilkS))
    (fp_text value SN74LVC245A (at 0 -3.72) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 3 +3V3))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 19 /MC_CS))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 17 /MC_RST))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 16 /MC_TX))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 28 "Net-(U2-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 29 "Net-(U2-Pad6)"))
    (pad 7 thru_hole oval (at 0 15.24) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 30 "Net-(U2-Pad7)"))
    (pad 8 thru_hole oval (at 0 17.78) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 31 "Net-(U2-Pad8)"))
    (pad 9 thru_hole oval (at 0 20.32) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 32 "Net-(U2-Pad9)"))
    (pad 10 thru_hole oval (at 0 22.86) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 11 thru_hole oval (at 7.62 22.86) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 33 "Net-(U2-Pad11)"))
    (pad 12 thru_hole oval (at 7.62 20.32) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 34 "Net-(U2-Pad12)"))
    (pad 13 thru_hole oval (at 7.62 17.78) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 35 "Net-(U2-Pad13)"))
    (pad 14 thru_hole oval (at 7.62 15.24) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 36 "Net-(U2-Pad14)"))
    (pad 15 thru_hole oval (at 7.62 12.7) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 37 "Net-(U2-Pad15)"))
    (pad 16 thru_hole oval (at 7.62 10.16) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 38 /ESP_RX))
    (pad 17 thru_hole oval (at 7.62 7.62) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 4 /ESP_RST))
    (pad 18 thru_hole oval (at 7.62 5.08) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 39 /ESP_CS))
    (pad 19 thru_hole oval (at 7.62 2.54) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 20 thru_hole oval (at 7.62 0) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 3 +3V3))
    (model Housings_DIP.3dshapes/DIP-20_W7.62mm_LongPads.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Radial_D6.3_L11.2_P2.5 (layer F.Cu) (tedit 0)
    (at 142.875 117.602)
    (descr "Radial Electrolytic Capacitor, Diameter 6.3mm x Length 11.2mm, Pitch 2.5mm")
    (tags "Electrolytic Capacitor")
    (fp_text reference C1 (at 1.25 -4.4) (layer F.SilkS))
    (fp_text value 220uF (at 1.25 4.4) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 +5V))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D6.3_L11.2_P2.5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Radial_D5_L11_P2.5 (layer F.Cu) (tedit 0)
    (at 172.9994 86.0552)
    (descr "Radial Electrolytic Capacitor Diameter 5mm x Length 11mm, Pitch 2.5mm")
    (tags "Electrolytic Capacitor")
    (fp_text reference C2 (at -1.2494 2.6948) (layer F.SilkS))
    (fp_text value 10uF (at 1.25 3.8) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 3 +3V3))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D5_L11_P2.5.wrl
      (at (xyz 0.049213 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Capacitors_ThroughHole:C_Radial_D5_L11_P2.5 (layer F.Cu) (tedit 0)
    (at 165.5 112.75 270)
    (descr "Radial Electrolytic Capacitor Diameter 5mm x Length 11mm, Pitch 2.5mm")
    (tags "Electrolytic Capacitor")
    (fp_text reference C5 (at 2.2968 3.9624 360) (layer F.SilkS))
    (fp_text value 10uF (at 1.25 3.8 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 3 +3V3))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D5_L11_P2.5.wrl
      (at (xyz 0.049213 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Connect:bornier3 (layer F.Cu) (tedit 0)
    (at 127.635 91.0336 270)
    (descr "Bornier d'alimentation 3 pins")
    (tags DEV)
    (fp_text reference P1 (at -7.0866 -4.699 360) (layer F.SilkS))
    (fp_text value CONN_PWR (at 0 5.08 270) (layer F.Fab))
    (pad 1 thru_hole rect (at -5.08 0 270) (size 2.54 2.54) (drill 1.524) (layers *.Cu *.Mask F.SilkS)
      (net 49 /SW_GND))
    (pad 2 thru_hole circle (at 0 0 270) (size 2.54 2.54) (drill 1.524) (layers *.Cu *.Mask F.SilkS)
      (net 2 +5V))
    (pad 3 thru_hole circle (at 5.08 0 270) (size 2.54 2.54) (drill 1.524) (layers *.Cu *.Mask F.SilkS)
      (net 3 +3V3))
    (model Connect.3dshapes/bornier3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connect:bornier2 (layer F.Cu) (tedit 0)
    (at 127.635 78.1304 270)
    (descr "Bornier d'alimentation 2 pins")
    (tags DEV)
    (fp_text reference P2 (at -4.5974 -4.826 360) (layer F.SilkS))
    (fp_text value CONN_SENSOR_SERIAL (at 0 5.08 270) (layer F.Fab))
    (pad 1 thru_hole rect (at -2.54 0 270) (size 2.54 2.54) (drill 1.524) (layers *.Cu *.Mask F.SilkS)
      (net 5 /SENSOR_RX))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 2.54 2.54) (drill 1.524) (layers *.Cu *.Mask F.SilkS)
      (net 6 /SENSOR_TX))
    (model Connect.3dshapes/bornier2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connect:bornier5 (layer F.Cu) (tedit 0)
    (at 127.635 111.506 270)
    (descr "Bornier d'alimentation 4 pins")
    (tags DEV)
    (fp_text reference P3 (at -12.192 -4.826 360) (layer F.SilkS))
    (fp_text value CONN_SENSOR (at 0 5.08 270) (layer F.Fab))
    (pad 2 thru_hole circle (at -5.08 0 270) (size 3.81 3.81) (drill 1.524) (layers *.Cu *.Mask F.SilkS)
      (net 7 /SENSOR_IO2))
    (pad 3 thru_hole circle (at 0 0 270) (size 3.81 3.81) (drill 1.524) (layers *.Cu *.Mask F.SilkS)
      (net 50 /FILTER_OUT))
    (pad 1 thru_hole rect (at -10.16 0 270) (size 3.81 3.81) (drill 1.524) (layers *.Cu *.Mask F.SilkS)
      (net 8 /SENSOR_IO1))
    (pad 4 thru_hole circle (at 5.08 0 270) (size 3.81 3.81) (drill 1.524) (layers *.Cu *.Mask F.SilkS)
      (net 2 +5V))
    (pad 5 thru_hole circle (at 10.16 0 270) (size 3.81 3.81) (drill 1.524) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model Connect.3dshapes/bornier5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 0)
    (at 135.8646 88.4428)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P4 (at -0.2286 -2.4638 180) (layer F.SilkS))
    (fp_text value CONN_PWR_H (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 49 /SW_GND))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 +5V))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 +3V3))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 54EA090C)
    (at 135.8646 78.6384)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P5 (at 2.5654 -0.6604 270) (layer F.SilkS))
    (fp_text value CONN_SENSOR_SERIAL_H (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 /SENSOR_RX))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 /SENSOR_TX))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 56648415)
    (at 138.811 107.442 270)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R1 (at 5.32892 -3.50012 270) (layer F.SilkS))
    (fp_text value 150 (at 5.08 3.81 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 50 /FILTER_OUT))
    (pad 2 thru_hole circle (at 10.16 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 2 +5V))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module ESP8266:ESP-01 (layer F.Cu) (tedit 553C10FF)
    (at 180.467 96.774)
    (descr "Module, ESP-8266, ESP-01, 8 pin")
    (tags "Module ESP-8266 ESP8266")
    (fp_text reference U3 (at 0.254 -4.572) (layer F.SilkS))
    (fp_text value ESP-01v090 (at 12.192 3.556) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 /ESP_TX))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 39 /ESP_CS))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 +3V3))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 /ESP_RST))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 40 /ESP_IO_0))
    (pad 7 thru_hole oval (at 0 7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 +3V3))
    (pad 8 thru_hole oval (at 2.54 7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 38 /ESP_RX))
  )
  (module Pin_Headers:Pin_Header_Straight_1x05 (layer F.Cu) (tedit 54EA0684)
    (at 135.509 102.362)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P6 (at 2.667 -1.143) (layer F.SilkS))
    (fp_text value CONN_SENSOR_H (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 /SENSOR_IO1))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 /SENSOR_IO2))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 50 /FILTER_OUT))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 +5V))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x05.wrl
      (at (xyz 0 -0.2 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module ESP8266:ESP-12 locked (layer F.Cu) (tedit 55BE5912)
    (at 178.751 93.218 270)
    (descr "Module, ESP-8266, ESP-12, 16 pad, SMD")
    (tags "Module ESP-8266 ESP8266")
    (fp_text reference U4 (at 1.5 16.6 270) (layer F.SilkS))
    (fp_text value ESP-12 (at 6.992 1 270) (layer F.Fab))
    (fp_text user "No Copper" (at 6.892 -5.4 270) (layer F.CrtYd))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.5 1.1) (drill 0.65 (offset -0.7 0)) (layers *.Cu *.Mask F.SilkS)
      (net 4 /ESP_RST))
    (pad 2 thru_hole oval (at 0 2 270) (size 2.5 1.1) (drill 0.65 (offset -0.7 0)) (layers *.Cu *.Mask F.SilkS)
      (net 44 "Net-(U4-Pad2)"))
    (pad 3 thru_hole oval (at 0 4 270) (size 2.5 1.1) (drill 0.65 (offset -0.7 0)) (layers *.Cu *.Mask F.SilkS)
      (net 39 /ESP_CS))
    (pad 4 thru_hole oval (at 0 6 270) (size 2.5 1.1) (drill 0.65 (offset -0.7 0)) (layers *.Cu *.Mask F.SilkS)
      (net 45 "Net-(U4-Pad4)"))
    (pad 5 thru_hole oval (at 0 8 270) (size 2.5 1.1) (drill 0.65 (offset -0.7 0)) (layers *.Cu *.Mask F.SilkS)
      (net 46 "Net-(U4-Pad5)"))
    (pad 6 thru_hole oval (at 0 10 270) (size 2.5 1.1) (drill 0.65 (offset -0.7 0)) (layers *.Cu *.Mask F.SilkS)
      (net 47 "Net-(U4-Pad6)"))
    (pad 7 thru_hole oval (at 0 12 270) (size 2.5 1.1) (drill 0.65 (offset -0.7 0)) (layers *.Cu *.Mask F.SilkS)
      (net 48 "Net-(U4-Pad7)"))
    (pad 8 thru_hole oval (at 0 14 270) (size 2.5 1.1) (drill 0.65 (offset -0.7 0)) (layers *.Cu *.Mask F.SilkS)
      (net 3 +3V3))
    (pad 9 thru_hole oval (at 14 14 270) (size 2.5 1.1) (drill 0.65 (offset 0.7 0)) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 10 thru_hole oval (at 14 12 270) (size 2.5 1.1) (drill 0.65 (offset 0.6 0)) (layers *.Cu *.Mask F.SilkS)
      (net 41 "Net-(U4-Pad10)"))
    (pad 11 thru_hole oval (at 14 10 270) (size 2.5 1.1) (drill 0.65 (offset 0.7 0)) (layers *.Cu *.Mask F.SilkS)
      (net 3 +3V3))
    (pad 12 thru_hole oval (at 14 8 270) (size 2.5 1.1) (drill 0.65 (offset 0.7 0)) (layers *.Cu *.Mask F.SilkS)
      (net 40 /ESP_IO_0))
    (pad 13 thru_hole oval (at 14 6 270) (size 2.5 1.1) (drill 0.65 (offset 0.7 0)) (layers *.Cu *.Mask F.SilkS)
      (net 42 "Net-(U4-Pad13)"))
    (pad 14 thru_hole oval (at 14 4 270) (size 2.5 1.1) (drill 0.65 (offset 0.7 0)) (layers *.Cu *.Mask F.SilkS)
      (net 43 "Net-(U4-Pad14)"))
    (pad 15 thru_hole oval (at 14 2 270) (size 2.5 1.1) (drill 0.65 (offset 0.7 0)) (layers *.Cu *.Mask F.SilkS)
      (net 38 /ESP_RX))
    (pad 16 thru_hole oval (at 14 0 270) (size 2.5 1.1) (drill 0.65 (offset 0.7 0)) (layers *.Cu *.Mask F.SilkS)
      (net 15 /ESP_TX))
    (model ${ESPLIB}/ESP8266.3dshapes/ESP-12.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 54EA090C)
    (at 189.103 112.522 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference JP1 (at -0.889 5.334 360) (layer F.SilkS))
    (fp_text value Jumper_NO_Small (at 0 -3.1 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 40 /ESP_IO_0))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 56648415)
    (at 189.103 107.442 90)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R2 (at 6.942 -2.103 90) (layer F.SilkS))
    (fp_text value 1K (at 5.08 3.81 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 40 /ESP_IO_0))
    (pad 2 thru_hole circle (at 10.16 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 3 +3V3))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-220_Neutral123_Vertical_LargePads (layer F.Cu) (tedit 0)
    (at 174.04 114.5)
    (descr "TO-220, Neutral, Vertical, Large Pads,")
    (tags "TO-220, Neutral, Vertical, Large Pads,")
    (fp_text reference U1 (at 4.71 2.5) (layer F.SilkS))
    (fp_text value LD1117S33CTR (at 0 3.81) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 0 90) (size 3.50012 1.69926) (drill 1.00076) (layers *.Cu *.Mask)
      (net 3 +3V3))
    (pad 1 thru_hole oval (at -2.54 0 90) (size 3.50012 1.69926) (drill 1.00076) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole oval (at 2.54 0 90) (size 3.50012 1.69926) (drill 1.00076) (layers *.Cu *.Mask)
      (net 2 +5V))
    (model TO_SOT_Packages_THT.3dshapes/TO-220_Neutral123_Vertical_LargePads.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-92_Inline_Wide (layer F.Cu) (tedit 58610935)
    (at 135.21 97.5)
    (descr "TO-92 leads in-line, wide, drill 0.8mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q1 (at 2.54 -3.556 180) (layer F.SilkS))
    (fp_text value ZVN4206A (at 2.54 2.794) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 51 /SW_GND_G))
    (pad 3 thru_hole circle (at 5.08 0 90) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 49 /SW_GND))
    (model TO_SOT_Packages_THT.3dshapes/TO-92_Inline_Wide.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D6_P5 (layer F.Cu) (tedit 0)
    (at 181.6 89.5 90)
    (descr "Capacitor 6mm Disc, Pitch 5mm")
    (tags Capacitor)
    (fp_text reference C3 (at 0.35 -3.1 90) (layer F.SilkS))
    (fp_text value 10nF (at 2.5 3.5 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 /ESP_RST))
    (pad 2 thru_hole circle (at 5 0 90) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D6_P5.wrl
      (at (xyz 0.0984252 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D6_P5 (layer F.Cu) (tedit 0)
    (at 182.25 114.25 270)
    (descr "Capacitor 6mm Disc, Pitch 5mm")
    (tags Capacitor)
    (fp_text reference C4 (at -1.5 1.75 360) (layer F.SilkS))
    (fp_text value 100nF (at 2.5 3.5 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 2 thru_hole circle (at 5 0 270) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D6_P5.wrl
      (at (xyz 0.0984252 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D6_P5 (layer F.Cu) (tedit 0)
    (at 164.5 87.25 45)
    (descr "Capacitor 6mm Disc, Pitch 5mm")
    (tags Capacitor)
    (fp_text reference C7 (at 6.717514 1.767767 45) (layer F.SilkS))
    (fp_text value 100nF (at 2.5 3.5 45) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 45) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 3 +3V3))
    (pad 2 thru_hole circle (at 5 0 45) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D6_P5.wrl
      (at (xyz 0.098425 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D6_P5 (layer F.Cu) (tedit 0)
    (at 154 85.25 45)
    (descr "Capacitor 6mm Disc, Pitch 5mm")
    (tags Capacitor)
    (fp_text reference C6 (at 0.176777 -3.005204 45) (layer F.SilkS))
    (fp_text value 10nF (at 2.5 3.5 45) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 45) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 3 +3V3))
    (pad 2 thru_hole circle (at 5 0 45) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D6_P5.wrl
      (at (xyz 0.098425 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04_Pitch2.54mm (layer F.Cu) (tedit 5862ED52)
    (at 148 99.21)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference P7 (at 0 -2.39) (layer F.SilkS))
    (fp_text value CONN_PROG (at 0 10.01) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 /MC_RST))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /MC_TX))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 /ESP_TX))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x04_Pitch2.54mm.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (gr_text RST (at 156.25 119 90) (layer F.SilkS))
  (gr_text 3V3 (at 158.75 119 90) (layer F.SilkS))
  (gr_text 5V (at 161.25 119.75 90) (layer F.SilkS))
  (gr_text GND (at 163.75 119 90) (layer F.SilkS))
  (gr_text GND (at 166.25 119 90) (layer F.SilkS))
  (gr_text Vin (at 169 119.5 90) (layer F.SilkS))
  (gr_text A0 (at 173.75 120 90) (layer F.SilkS))
  (gr_text A1 (at 176.5 120 90) (layer F.SilkS))
  (gr_text A2 (at 179 120 90) (layer F.SilkS))
  (gr_text A5 (at 186.5 119.75 90) (layer F.SilkS))
  (gr_text AREF (at 143.25 74.5 360) (layer F.SilkS))
  (gr_text GND (at 149.5 78.25 90) (layer F.SilkS))
  (gr_text D13 (at 152 78.25 90) (layer F.SilkS))
  (gr_text D12 (at 154.5 78.25 90) (layer F.SilkS))
  (gr_text D11 (at 157.25 78.25 90) (layer F.SilkS))
  (gr_text D10 (at 159.75 78.25 90) (layer F.SilkS))
  (gr_text D9 (at 162.25 77.5 90) (layer F.SilkS))
  (gr_text D8 (at 164.75 77.5 90) (layer F.SilkS))
  (gr_text D7 (at 169 77.5 90) (layer F.SilkS))
  (gr_text D6 (at 171.5 77.5 90) (layer F.SilkS))
  (gr_text D5 (at 174 77.5 90) (layer F.SilkS))
  (gr_text D4 (at 176.5 77.5 90) (layer F.SilkS))
  (gr_text D3 (at 179 77.5 90) (layer F.SilkS))
  (gr_text D2 (at 181.5 77.5 90) (layer F.SilkS))
  (gr_text D0 (at 186.75 77.5 90) (layer F.SilkS))
  (gr_text D1 (at 184 77.5 90) (layer F.SilkS))
  (dimension 68.5 (width 0.3) (layer Dwgs.User)
    (gr_text "68.500 mm" (at 157.25 127.4) (layer Dwgs.User))
    (feature1 (pts (xy 191.5 131.25) (xy 191.5 126.05)))
    (feature2 (pts (xy 123 131.25) (xy 123 126.05)))
    (crossbar (pts (xy 123 128.75) (xy 191.5 128.75)))
    (arrow1a (pts (xy 191.5 128.75) (xy 190.373496 129.336421)))
    (arrow1b (pts (xy 191.5 128.75) (xy 190.373496 128.163579)))
    (arrow2a (pts (xy 123 128.75) (xy 124.126504 129.336421)))
    (arrow2b (pts (xy 123 128.75) (xy 124.126504 128.163579)))
  )
  (dimension 21.523243 (width 0.3) (layer F.CrtYd)
    (gr_text "21.523 mm" (at 131.293726 82.815112 2.663000766) (layer F.CrtYd))
    (feature1 (pts (xy 144.25 129.75) (xy 141.981003 80.96657)))
    (feature2 (pts (xy 122.75 130.75) (xy 120.481003 81.96657)))
    (crossbar (pts (xy 120.606449 84.663654) (xy 142.106449 83.663654)))
    (arrow1a (pts (xy 142.106449 83.663654) (xy 141.008408 84.30178)))
    (arrow1b (pts (xy 142.106449 83.663654) (xy 140.953916 83.130205)))
    (arrow2a (pts (xy 120.606449 84.663654) (xy 121.758982 85.197103)))
    (arrow2b (pts (xy 120.606449 84.663654) (xy 121.70449 84.025528)))
  )
  (dimension 66.04 (width 0.3) (layer Dwgs.User)
    (gr_text "66.040 mm" (at 156.083 66.976) (layer Dwgs.User))
    (feature1 (pts (xy 189.103 71.247) (xy 189.103 65.626)))
    (feature2 (pts (xy 123.063 71.247) (xy 123.063 65.626)))
    (crossbar (pts (xy 123.063 68.326) (xy 189.103 68.326)))
    (arrow1a (pts (xy 189.103 68.326) (xy 187.976496 68.912421)))
    (arrow1b (pts (xy 189.103 68.326) (xy 187.976496 67.739579)))
    (arrow2a (pts (xy 123.063 68.326) (xy 124.189504 68.912421)))
    (arrow2b (pts (xy 123.063 68.326) (xy 124.189504 67.739579)))
  )
  (dimension 53.467 (width 0.3) (layer Dwgs.User)
    (gr_text "53.467 mm" (at 199.714202 98.472311 270) (layer Dwgs.User))
    (feature1 (pts (xy 190.617202 125.205811) (xy 201.064202 125.205811)))
    (feature2 (pts (xy 190.617202 71.738811) (xy 201.064202 71.738811)))
    (crossbar (pts (xy 198.364202 71.738811) (xy 198.364202 125.205811)))
    (arrow1a (pts (xy 198.364202 125.205811) (xy 197.777781 124.079307)))
    (arrow1b (pts (xy 198.364202 125.205811) (xy 198.950623 124.079307)))
    (arrow2a (pts (xy 198.364202 71.738811) (xy 197.777781 72.865315)))
    (arrow2b (pts (xy 198.364202 71.738811) (xy 198.950623 72.865315)))
  )
  (gr_text 2 (at 268.859 193.167) (layer Dwgs.User))
  (gr_text http://www.hackair.eu/ (at 271.018 185.674) (layer Dwgs.User))
  (gr_text http://research.ee.teiath.gr/ttss/ (at 265.303 183.134) (layer Dwgs.User))
  (gr_text "14 October 2016" (at 215.5 193.421) (layer Dwgs.User))
  (gr_text "hackAIR WiFi Air Quality Shield for Arduino" (at 210.566 189.484) (layer Dwgs.User))
  (gr_text 1/1 (at 187.325 183.134) (layer Dwgs.User))
  (gr_text "Arduino Shield footprint by Nicholas C Lewis, CC BY 3.0\nkicad-ESP8266 footprints & schematic by Jerry Dunmire, CC BY-SA 4.0\n\nAuthor: Thanasis Georgiou <contact@thgeorgiou.com>\nPart of the hackAIR project, available freely under the (CC BY 4.0) license." (at 178.308 173.736) (layer Dwgs.User))
  (gr_text hackair.eu (at 147.25 122.75) (layer F.SilkS))
  (gr_text hackAIR (at 144.018 89.916) (layer F.SilkS))
  (gr_text "HackAir WiFi Shield rev.3" (at 178.75 81.75) (layer F.SilkS))
  (gr_text GND (at 132.588 121.666 90) (layer F.SilkS))
  (gr_text 5V (at 132.715 116.586 90) (layer F.SilkS))
  (gr_text VF (at 132.715 111.633 90) (layer F.SilkS))
  (gr_text IO2 (at 132.588 106.426 90) (layer F.SilkS))
  (gr_text 3V3 (at 132.588 95.758 90) (layer F.SilkS))
  (gr_text IO1 (at 132.588 101.219 90) (layer F.SilkS))
  (gr_text 5V (at 132.588 91.059 90) (layer F.SilkS))
  (gr_text GND (at 132.715 86.741 90) (layer F.SilkS))
  (gr_text TX (at 132.588 80.899 90) (layer F.SilkS))
  (gr_text RX (at 132.588 75.819 90) (layer F.SilkS))
  (gr_line (start 123.063 125.222) (end 123.063 71.882) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 189.103 125.222) (end 123.063 125.222) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 189.103 122.682) (end 189.103 125.222) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 191.643 120.142) (end 189.103 122.682) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 191.643 87.122) (end 191.643 120.142) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 189.103 84.582) (end 191.643 87.122) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 189.103 73.406) (end 189.103 84.582) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 187.579 71.882) (end 189.103 73.406) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 123.063 71.882) (end 187.579 71.882) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 123.063 71.882) (xy 187.579 71.882) (xy 189.103 73.406) (xy 189.103 84.582) (xy 191.643 87.122)
        (xy 191.643 120.142) (xy 189.103 122.682) (xy 189.103 125.222) (xy 123.063 125.222)
      )
    )
  )
)
