(kicad_pcb (version 4) (host pcbnew 4.0.4-stable)
  (general
    (links 6)
    (no_connects 6)
    (area 148.1 88.161666 162.9214 115.584433)
    (thickness 1.6)
    (drawings 16)
    (tracks 19)
    (zones 0)
    (modules 3)
    (nets 4)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.35)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFEF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad3)")
  (net 2 "Net-(J1-Pad2)")
  (net 3 "Net-(J1-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.35)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
  )
  (module Jacks:Thonkiconn_3.5mm_Switching_Jack_Compact_With_Hole (layer F.Cu) (tedit 592CF918)
    (at 154.94 102.235)
    (fp_text reference J1 (at 0 -2.5) (layer F.Fab))
    (fp_text value JACK_2P (at 0 -7.62) (layer F.Fab))
    (pad 3 thru_hole circle (at 0 -4.92) (size 2.1 2.1) (drill 1.25) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(J1-Pad3)"))
    (pad 2 thru_hole circle (at 0 3.302) (size 2.1 2.1) (drill 1.25) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(J1-Pad2)"))
    (pad 1 thru_hole circle (at 0 5.715) (size 2.1 2.1) (drill 1.25) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(J1-Pad1)"))
    (pad 4 thru_hole circle (at 0 0) (size 3 3) (drill 3) (layers *.Cu *.Mask F.SilkS))
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 592CF913)
    (at 152.4 93.345 90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference P1 (at 0 -3.175 90) (layer F.Fab))
    (fp_text value CONN_01X03 (at 0 7.41 90) (layer F.Fab))
    (fp_text user %R (at 0 -2.33 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad3)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 592CF90B)
    (at 152.4 111.125 90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference P2 (at 0 -3.175 90) (layer F.Fab))
    (fp_text value CONN_01X03 (at 0.7239 9.2964 90) (layer F.Fab))
    (fp_text user %R (at 0 -2.33 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad3)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (gr_text G (at 158.242 107.95) (layer F.SilkS))
  (gr_text Tip (at 152.4 107.95) (layer F.SilkS))
  (gr_line (start 158.75 113.03) (end 151.13 113.03) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 159.385 92.075) (end 159.385 112.395) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 151.13 91.44) (end 158.75 91.44) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 150.495 112.395) (end 150.495 92.075) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 151.13 112.395) (end 151.13 113.03) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 158.75 112.395) (end 159.385 112.395) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 158.75 92.075) (end 158.75 91.44) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 151.13 92.075) (end 150.495 92.075) (angle 90) (layer Edge.Cuts) (width 0.15))
)
