(kicad_pcb (version 20171130) (host pcbnew "(5.1.2-1)-1")
  (general
    (thickness 1.6)
    (drawings 7964)
    (tracks 309)
    (zones 0)
    (modules 27)
    (nets 21)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.25)
    (user_trace_width 0.75)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 GND)
  (net 3 +3V3)
  (net 4 "Net-(J1-Pad1)")
  (net 5 "Net-(Q1-Pad3)")
  (net 6 /htron)
  (net 7 "Net-(R3-Pad1)")
  (net 8 "Net-(R4-Pad1)")
  (net 9 /mq135_adc)
  (net 10 +5V)
  (net 11 /RX)
  (net 12 /TX)
  (net 13 /~RST)
  (net 14 /GP0)
  (net 15 /SDA)
  (net 16 /SCL)
  (net 17 "Net-(R5-Pad2)")
  (net 18 "Net-(R9-Pad1)")
  (net 19 VBUS)
  (net 20 "Net-(Q1-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /GP0)
    (add_net /RX)
    (add_net /SCL)
    (add_net /SDA)
    (add_net /TX)
    (add_net /htron)
    (add_net /mq135_adc)
    (add_net /~RST)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(Q1-Pad1)")
    (add_net "Net-(R3-Pad1)")
    (add_net "Net-(R4-Pad1)")
    (add_net "Net-(R5-Pad2)")
    (add_net "Net-(R9-Pad1)")
  )
  (net_class Power ""
    (clearance 0.2)
    (trace_width 1.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net +5V)
    (add_net GND)
    (add_net "Net-(Q1-Pad3)")
    (add_net VBUS)
  )
  (module RF_Module:ESP-12E (layer F.Cu) (tedit 5CDDA182)
    (at 159.7 82.13 90)
    (descr "Wi-Fi Module, http://wiki.ai-thinker.com/_media/esp8266/docs/aithinker_esp_12f_datasheet_en.pdf")
    (tags "Wi-Fi Module")
    (attr smd)
    (fp_text reference U1 (at -9.81 -1.35 180) (layer F.SilkS))
    (fp_text value ESP-12F (at -0.06 -12.78 90) (layer F.Fab))
    (fp_text user %R (at 0.49 -0.8 90) (layer F.Fab))
    (fp_text user "KEEP-OUT ZONE" (at 0.03 -9.55 270) (layer Cmts.User))
    (fp_text user Antenna (at -0.06 -7 270) (layer Cmts.User))
    (pad 22 smd rect (at 7.6 -3.5 90) (size 2.5 1) (layers F.Cu F.Paste F.Mask)
      (net 12 /TX))
    (pad 21 smd rect (at 7.6 -1.5 90) (size 2.5 1) (layers F.Cu F.Paste F.Mask)
      (net 11 /RX))
    (pad 20 smd rect (at 7.6 0.5 90) (size 2.5 1) (layers F.Cu F.Paste F.Mask))
    (pad 19 smd rect (at 7.6 2.5 90) (size 2.5 1) (layers F.Cu F.Paste F.Mask)
      (net 6 /htron))
    (pad 18 smd rect (at 7.6 4.5 90) (size 2.5 1) (layers F.Cu F.Paste F.Mask)
      (net 14 /GP0))
    (pad 17 smd rect (at 7.6 6.5 90) (size 2.5 1) (layers F.Cu F.Paste F.Mask)
      (net 15 /SDA))
    (pad 16 smd rect (at 7.6 8.5 90) (size 2.5 1) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(R9-Pad1)"))
    (pad 15 smd rect (at 7.6 10.5 90) (size 2.5 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 14 smd rect (at 5 12 90) (size 1 1.8) (layers F.Cu F.Paste F.Mask))
    (pad 13 smd rect (at 3 12 90) (size 1 1.8) (layers F.Cu F.Paste F.Mask))
    (pad 12 smd rect (at 1 12 90) (size 1 1.8) (layers F.Cu F.Paste F.Mask))
    (pad 11 smd rect (at -1 12 90) (size 1 1.8) (layers F.Cu F.Paste F.Mask))
    (pad 10 smd rect (at -3 12 90) (size 1 1.8) (layers F.Cu F.Paste F.Mask))
    (pad 9 smd rect (at -5 12 90) (size 1 1.8) (layers F.Cu F.Paste F.Mask))
    (pad 8 smd rect (at -7.6 10.5 90) (size 2.5 1) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 7 smd rect (at -7.6 8.5 90) (size 2.5 1) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at -7.6 6.5 90) (size 2.5 1) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at -7.6 4.5 90) (size 2.5 1) (layers F.Cu F.Paste F.Mask)
      (net 16 /SCL))
    (pad 4 smd rect (at -7.6 2.5 90) (size 2.5 1) (layers F.Cu F.Paste F.Mask)
      (net 13 /~RST))
    (pad 3 smd rect (at -7.6 0.5 90) (size 2.5 1) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(R5-Pad2)"))
    (pad 2 smd rect (at -7.6 -1.5 90) (size 2.5 1) (layers F.Cu F.Paste F.Mask)
      (net 9 /mq135_adc))
    (pad 1 smd rect (at -7.6 -3.5 90) (size 2.5 1) (layers F.Cu F.Paste F.Mask)
      (net 13 /~RST))
    (model ${KIPRJMOD}/3dmodels/kicad-ESP8266/ESP8266.3dshapes/ESP-12-E-better.wrl
      (offset (xyz -7 3.5 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module logo:diamond (layer F.Cu) (tedit 0)
    (at 201.82 88.17 55)
    (fp_text reference G*** (at 0 0 55) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 55) (layer F.SilkS) hide)
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 190.775 62.675)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference REF** (at 4.85 2.85) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3 (at -0.525 -0.025) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 190.86 99.01)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference REF** (at 4.85 2.85) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3 (at -0.525 -0.025) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Sensor_Pressure:MQ_13X (layer F.Cu) (tedit 5CDCDB5B)
    (at 190.9 81.4)
    (fp_text reference U2 (at 1.89 -11.04) (layer F.SilkS))
    (fp_text value MQ-135 (at 0.44 6.79) (layer F.Fab))
    (pad 7 thru_hole oval (at -3.358757 -3.358757 45) (size 1.5 1.5) (drill 1.1) (layers *.Cu *.Mask)
      (net 9 /mq135_adc))
    (pad 6 thru_hole oval (at -4.75 0 45) (size 1.5 1.5) (drill 1.1) (layers *.Cu *.Mask)
      (net 5 "Net-(Q1-Pad3)"))
    (pad 5 thru_hole oval (at -3.358757 3.358757 45) (size 1.5 1.5) (drill 1.1) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 3.358757 3.358757 45) (size 1.5 1.5) (drill 1.1) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 4.75 0 45) (size 1.5 1.5) (drill 1.1) (layers *.Cu *.Mask)
      (net 10 +5V))
    (pad 1 thru_hole oval (at 3.358757 -3.358757 45) (size 1.5 1.5) (drill 1.1) (layers *.Cu *.Mask)
      (net 3 +3V3))
    (model ${KIPRJMOD}/3dmodels/mqxxx.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 90))
    )
  )
  (module Package_DFN_QFN:QFN-16-1EP_4x4mm_P0.65mm_EP2.15x2.15mm (layer F.Cu) (tedit 5C200589)
    (at 203.4 74 30)
    (descr "QFN, 16 Pin (https://www.analog.com/media/en/technical-documentation/data-sheets/4001f.pdf), generated with kicad-footprint-generator ipc_dfn_qfn_generator.py")
    (tags "QFN DFN_QFN")
    (attr smd)
    (fp_text reference U3 (at -3.498076 0.058846 300) (layer F.SilkS))
    (fp_text value LTC4055 (at 0 3.32 30) (layer F.Fab))
    (fp_text user %R (at 0 0 30) (layer F.Fab))
    (pad 16 smd roundrect (at -0.975 -1.8375 30) (size 0.3 1.075) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 15 smd roundrect (at -0.325 -1.8375 30) (size 0.3 1.075) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 14 smd roundrect (at 0.325 -1.8375 30) (size 0.3 1.075) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 13 smd roundrect (at 0.975 -1.8375 30) (size 0.3 1.075) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 12 smd roundrect (at 1.8375 -0.975 30) (size 1.075 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 "Net-(C1-Pad1)"))
    (pad 11 smd roundrect (at 1.8375 -0.325 30) (size 1.075 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 "Net-(R4-Pad1)"))
    (pad 10 smd roundrect (at 1.8375 0.325 30) (size 1.075 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 9 smd roundrect (at 1.8375 0.975 30) (size 1.075 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 "Net-(R3-Pad1)"))
    (pad 8 smd roundrect (at 0.975 1.8375 30) (size 0.3 1.075) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 +5V))
    (pad 7 smd roundrect (at 0.325 1.8375 30) (size 0.3 1.075) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 6 smd roundrect (at -0.325 1.8375 30) (size 0.3 1.075) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 5 smd roundrect (at -0.975 1.8375 30) (size 0.3 1.075) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 4 smd roundrect (at -1.8375 0.975 30) (size 1.075 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 VBUS))
    (pad 3 smd roundrect (at -1.8375 0.325 30) (size 1.075 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 +5V))
    (pad 2 smd roundrect (at -1.8375 -0.325 30) (size 1.075 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 "Net-(J1-Pad1)"))
    (pad 1 smd roundrect (at -1.8375 -0.975 30) (size 1.075 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 VBUS))
    (pad "" smd roundrect (at 0.54 0.54 30) (size 0.87 0.87) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.54 -0.54 30) (size 0.87 0.87) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.54 0.54 30) (size 0.87 0.87) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.54 -0.54 30) (size 0.87 0.87) (layers F.Paste) (roundrect_rratio 0.25))
    (pad 17 smd roundrect (at 0 0 30) (size 2.15 2.15) (layers F.Cu F.Mask) (roundrect_rratio 0.116279)
      (net 2 GND))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/QFN-16-1EP_4x4mm_P0.65mm_EP2.7x2.7mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 197.66 72.25 300)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1 (at -1.743801 1.360352 120) (layer F.SilkS))
    (fp_text value 0.1u (at -3.251666 -0.432051 120) (layer F.Fab))
    (fp_text user %R (at 0 0 120) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 300) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.7875 0 300) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:CP_Elec_3x5.3 (layer F.Cu) (tedit 5B303299)
    (at 179.9 90.5)
    (descr "SMT capacitor, aluminium electrolytic, 3x5.3, Cornell Dubilier Electronics ")
    (tags "Capacitor Electrolytic")
    (attr smd)
    (fp_text reference C2 (at 0.3 -2.7) (layer F.SilkS))
    (fp_text value 10u (at 0 2.7) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 1.5 0) (size 2.2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.5 0) (size 2.2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/CP_Elec_3x5.3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_JST:JST_EH_B02B-EH-A_1x02_P2.50mm_Vertical (layer F.Cu) (tedit 5B772AC7)
    (at 209.6 79.5 270)
    (descr "JST EH series connector, B02B-EH-A (http://www.jst-mfg.com/product/pdf/eng/eEH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST EH side entry")
    (fp_text reference J1 (at 6.2 1.4 270) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 3.7 3.4 270) (layer F.Fab) hide)
    (fp_text user %R (at 1.25 1.5 270) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.5 0 270) (size 1.7 2) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole roundrect (at 0 0 270) (size 1.7 2) (drill 1) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 4 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_EH_B02B-EH-A_1x02_P2.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 175.1 73.9)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at 2.5 -0.1) (layer F.SilkS))
    (fp_text value 1k (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 "Net-(Q1-Pad1)"))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 /htron))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 175 80.5)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R2 (at 2.5 -0.3) (layer F.SilkS))
    (fp_text value 10k (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 "Net-(Q1-Pad1)"))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 208.5 73.1 30)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R3 (at -0.229423 -1.402628 30) (layer F.SilkS))
    (fp_text value 97.6k (at 0.1 1.8 30) (layer F.Fab))
    (fp_text user %R (at 0 0 30) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 30) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.7875 0 30) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 "Net-(R3-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 206.7 70.4 30)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R4 (at 0 -1.43 30) (layer F.SilkS))
    (fp_text value 97.6k (at 1.908846 0.293782 120) (layer F.Fab))
    (fp_text user %R (at 0.294999 -0.095001 30) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 30) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.7875 0 30) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 "Net-(R4-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 175.1 88 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C3 (at -2.7 0.1) (layer F.SilkS))
    (fp_text value .1u (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:CP_Elec_3x5.3 (layer F.Cu) (tedit 5B303299)
    (at 203.7 81.3 270)
    (descr "SMT capacitor, aluminium electrolytic, 3x5.3, Cornell Dubilier Electronics ")
    (tags "Capacitor Electrolytic")
    (attr smd)
    (fp_text reference C4 (at 3.89 -0.73 90) (layer F.SilkS))
    (fp_text value 10u (at -2.4 2.1 90) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 1.5 0 270) (size 2.2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.5 0 270) (size 2.2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 10 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/CP_Elec_3x5.3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_1.27mm:PinHeader_1x06_P1.27mm_Vertical (layer F.Cu) (tedit 59FED6E3)
    (at 176.7 95.025 55)
    (descr "Through hole straight pin header, 1x06, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x06 1.27mm single row")
    (fp_text reference J2 (at 0.187517 8.200485 55) (layer F.SilkS))
    (fp_text value Conn_01x06_Male (at 4.255648 3.518445 145) (layer F.Fab) hide)
    (fp_text user %R (at 0 3.175 145) (layer F.Fab))
    (pad 6 thru_hole oval (at 0 6.35 55) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 5 thru_hole oval (at 0 5.08 55) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 3 +3V3))
    (pad 4 thru_hole oval (at 0 3.81 55) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 14 /GP0))
    (pad 3 thru_hole oval (at 0 2.54 55) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 13 /~RST))
    (pad 2 thru_hole oval (at 0 1.27 55) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 12 /TX))
    (pad 1 thru_hole rect (at 0 0 55) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 11 /RX))
    (model ${KISYS3DMOD}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x06_P1.27mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_JST:JST_PH_B4B-PH-K_1x04_P2.00mm_Vertical (layer F.Cu) (tedit 5B7745C2)
    (at 202.3 67.4 150)
    (descr "JST PH series connector, B4B-PH-K (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST PH side entry")
    (fp_text reference J3 (at 9.308588 1.322947 150) (layer F.SilkS))
    (fp_text value Conn_01x04_Male (at 3 4 150) (layer F.Fab) hide)
    (fp_text user %R (at 3 1.5 150) (layer F.Fab))
    (pad 4 thru_hole oval (at 6 0 150) (size 1.2 1.75) (drill 0.75) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole oval (at 4 0 150) (size 1.2 1.75) (drill 0.75) (layers *.Cu *.Mask)
      (net 3 +3V3))
    (pad 2 thru_hole oval (at 2 0 150) (size 1.2 1.75) (drill 0.75) (layers *.Cu *.Mask)
      (net 16 /SCL))
    (pad 1 thru_hole roundrect (at 0 0 150) (size 1.2 1.75) (drill 0.75) (layers *.Cu *.Mask) (roundrect_rratio 0.208333)
      (net 15 /SDA))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_PH_B4B-PH-K_1x04_P2.00mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 174.9 84.9 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R5 (at -1.5 2) (layer F.SilkS))
    (fp_text value 10k (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 "Net-(R5-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 175.1 91.8 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R6 (at 0.575 -1.75) (layer F.SilkS))
    (fp_text value 10k (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 /~RST))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 182.75 69.075 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R7 (at -2.41 1.025) (layer F.SilkS))
    (fp_text value 4.7k (at -0.14 0.385) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 /SDA))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 182.7 71.3 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R8 (at -2.6 0.61) (layer F.SilkS))
    (fp_text value 4.7k (at 0.27 0.36) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 16 /SCL))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 175.1 77.1)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R9 (at 2.4 -0.3) (layer F.SilkS))
    (fp_text value 10k (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 "Net-(R9-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:CP_Elec_3x5.3 (layer F.Cu) (tedit 5B303299)
    (at 205.9 91.4 300)
    (descr "SMT capacitor, aluminium electrolytic, 3x5.3, Cornell Dubilier Electronics ")
    (tags "Capacitor Electrolytic")
    (attr smd)
    (fp_text reference C5 (at 0 -2.7 120) (layer F.SilkS))
    (fp_text value 1u (at 1 2.6 120) (layer F.Fab))
    (fp_text user %R (at 0 0 120) (layer F.Fab))
    (pad 2 smd rect (at 1.5 0 300) (size 2.2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.5 0 300) (size 2.2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 19 VBUS))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/CP_Elec_3x5.3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_USB:USB_Micro-B_GCT_USB3076-30-A (layer F.Cu) (tedit 5A170D03)
    (at 198.905821 95.152006 30)
    (descr "GCT Micro USB https://gct.co/files/drawings/usb3076.pdf")
    (tags "Micro-USB SMD Typ-B GCT")
    (attr smd)
    (fp_text reference J4 (at 2.695218 -3.399897 30) (layer F.SilkS))
    (fp_text value USB_B_Micro (at 0 5.2 30) (layer F.Fab))
    (fp_text user %R (at 0 0.85 30) (layer F.Fab))
    (fp_text user "PCB Edge" (at 0 2.65 30) (layer Dwgs.User))
    (pad 6 smd rect (at -2.32 -1.03 30) (size 1.15 1.45) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 smd rect (at 2.32 -1.03 30) (size 1.15 1.45) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 thru_hole oval (at 3.575 1.2 30) (size 1.05 1.9) (drill oval 0.45 1.25) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 6 thru_hole oval (at -3.575 1.2 210) (size 1.05 1.9) (drill oval 0.45 1.25) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 6 smd rect (at -1.125 1.2 30) (size 1.75 1.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 0 -1.45 30) (size 0.4 1.4) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at 0.65 -1.45 30) (size 0.4 1.4) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 1.3 -1.45 30) (size 0.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.3 -1.45 30) (size 0.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 19 VBUS))
    (pad 2 smd rect (at -0.65 -1.45 30) (size 0.4 1.4) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at 1.125 1.2 30) (size 1.75 1.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Connector_USB.3dshapes/USB_Micro-B_Molex_47346-0001.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23-5 (layer F.Cu) (tedit 5A02FF57)
    (at 176.2 69.7 180)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U4 (at -0.3 3) (layer F.SilkS))
    (fp_text value MIC5504-3.3YM5 (at 0.3 -2.4) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 5 smd rect (at 1.1 -0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 4 smd rect (at 1.1 0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at -1.1 0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 10 +5V))
    (pad 2 smd rect (at -1.1 0 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.1 -0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 10 +5V))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer F.Cu) (tedit 5A02FF57)
    (at 179.3 84.7 15)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q1 (at 0 -2.500001 15) (layer F.SilkS))
    (fp_text value MMBT3904 (at 1.723509 0.213347 105) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 105) (layer F.Fab))
    (pad 3 smd rect (at 1 0 15) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(Q1-Pad3)"))
    (pad 2 smd rect (at -1 0.95 15) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1 -0.95 15) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(Q1-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Potentiometer_THT:Potentiometer_Bourns_3266X_Horizontal (layer F.Cu) (tedit 5A3D4994)
    (at 180.19 67.09 210)
    (descr "Potentiometer, horizontal, Bourns 3266X, https://www.bourns.com/docs/Product-Datasheets/3266.pdf")
    (tags "Potentiometer horizontal Bourns 3266X")
    (fp_text reference RV1 (at -9.536267 1.7573 30) (layer F.SilkS))
    (fp_text value 100k (at -2.501858 -0.266654 30) (layer F.Fab))
    (fp_text user %R (at -2.54 1.23 30) (layer F.Fab))
    (pad 3 thru_hole circle (at -5.08 0 210) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at -2.54 2.54 210) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at 0 0 210) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 /mq135_adc))
    (model ${KISYS3DMOD}/Potentiometer_THT.3dshapes/Potentiometer_Bourns_3266X_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "Bobby\nD" (at 201.87 88.16 48) (layer F.SilkS))
  (gr_arc (start 190.99249 80.896576) (end 172.7 93) (angle -300.8769352) (layer Edge.Cuts) (width 0.05))
  (gr_text "ESP Sensor\nNode" (at 190.55 93.825) (layer F.SilkS))
  (gr_text SDA (at 200.5 70.7 60) (layer F.SilkS))
  (gr_text SCL (at 198.7 69.6 60) (layer F.SilkS))
  (gr_text 3V3 (at 196.9 68.5 60) (layer F.SilkS))
  (gr_text GND (at 195.2 67.7 60) (layer F.SilkS))
  (gr_text GND (at 183.375 96.675 55) (layer F.SilkS))
  (gr_text 3V3 (at 182.375 96.025 55) (layer F.SilkS))
  (gr_text GP0 (at 181.275 95.25 55) (layer F.SilkS))
  (gr_text ~RST (at 180.2 94.6 55) (layer F.SilkS))
  (gr_text TxD (at 179.075 93.75 55) (layer F.SilkS))
  (gr_text RxD (at 177.8 92.875 55) (layer F.SilkS))
  (dimension 44.050003 (width 0.15) (layer Dwgs.User)
    (gr_text "44.050 mm" (at 215.827521 80.916505 -89.98048952) (layer Dwgs.User))
    (feature1 (pts (xy 190.875 58.9) (xy 215.106441 58.891749)))
    (feature2 (pts (xy 190.89 102.95) (xy 215.121441 102.941749)))
    (crossbar (pts (xy 214.535021 102.941948) (xy 214.520021 58.891948)))
    (arrow1a (pts (xy 214.520021 58.891948) (xy 215.106825 60.018252)))
    (arrow1b (pts (xy 214.520021 58.891948) (xy 213.933984 60.018651)))
    (arrow2a (pts (xy 214.535021 102.941948) (xy 215.121058 101.815245)))
    (arrow2b (pts (xy 214.535021 102.941948) (xy 213.948217 101.815644)))
  )
  (dimension 65.490003 (width 0.15) (layer Dwgs.User)
    (gr_text "65.490 mm" (at 180.334421 112.090513 0.01749756535) (layer Dwgs.User))
    (feature1 (pts (xy 147.58 81.25) (xy 147.589204 111.386933)))
    (feature2 (pts (xy 213.07 81.23) (xy 213.079204 111.366933)))
    (crossbar (pts (xy 213.079024 110.780513) (xy 147.589024 110.800513)))
    (arrow1a (pts (xy 147.589024 110.800513) (xy 148.715349 110.213748)))
    (arrow1b (pts (xy 147.589024 110.800513) (xy 148.715707 111.38659)))
    (arrow2a (pts (xy 213.079024 110.780513) (xy 211.952341 110.194436)))
    (arrow2b (pts (xy 213.079024 110.780513) (xy 211.952699 111.367278)))
  )
  (gr_line (start 155.3 93.04) (end 172.7 93) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 155.4 71.5) (end 155.3 93.04) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 171.216836 71.408078) (end 155.4 71.5) (layer Edge.Cuts) (width 0.05))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 155.4 58.9) (xy 212.9 59) (xy 212.9 102.9) (xy 155.5 102.9)
      )
    )
  )
)
