(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x00010fc_80000001)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "/Users/cwfink/Desktop/")
    )
  )
  (net 0 "")
  (net 1 "Net-(Jr1-B)")
  (net 2 "Net-(Cc1-Pad2)")
  (net 3 "Net-(Jr2-B)")
  (net 4 "Net-(Cc2-Pad2)")
  (net 5 "Net-(D1-Pad1)")
  (net 6 "Net-(Qr1-D)")
  (net 7 "Net-(Q1-D)")
  (net 8 "Net-(D1-Pad4)")
  (net 9 "unconnected-(D1-Pad5)")
  (net 10 "unconnected-(D1-Pad6)")
  (net 11 "unconnected-(D1-Pad7)")
  (net 12 "unconnected-(D1-Pad8)")
  (net 13 "Net-(D1-Pad9)")
  (net 14 "Net-(Q2-D)")
  (net 15 "Net-(Qr2-D)")
  (net 16 "Net-(D1-Pad12)")
  (net 17 "unconnected-(D1-Pad13)")
  (net 18 "Net-(D1-P14)")
  (net 19 "Net-(D1-P15)")
  (net 20 "Net-(D1-P16)")
  (net 21 "unconnected-(D1-P17-Pad17)")
  (net 22 "unconnected-(D1-P18-Pad18)")
  (net 23 "unconnected-(D1-P19-Pad19)")
  (net 24 "unconnected-(D1-P20-Pad20)")
  (net 25 "unconnected-(D1-P21-Pad21)")
  (net 26 "unconnected-(D1-P22-Pad22)")
  (net 27 "Net-(D1-P23)")
  (net 28 "Net-(D1-P24)")
  (net 29 "Net-(D1-P25)")
  (net 30 "Net-(Jr1-A)")
  (net 31 "Net-(Jr2-A)")
  (net 32 "thermal_gnd")
  (footprint "Capacitor_SMD:C_0402_1005Metric_Pad0.74x0.62mm_HandSolder" (layer "F.Cu")
    (at 62.713065 82.84949 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "base_temp_v2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "Cc2" (at -0.027687 -1.602572) (layer "F.SilkS"))
    (fp_text value "C=1" (at 0 1.16) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.5675 0 180) (size 0.735 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "Net-(Jr2-B)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.5675 0 180) (size 0.735 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "Net-(Cc2-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "charge_amp:detector" (layer "F.Cu")
    (at 67.86935 81.088519 90)
    (property "Sheetfile" "base_temp_v2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "Det1" (at -7.053163 0.268054 unlocked) (layer "F.SilkS"))
    (fp_text value "C=1" (at 0 1 90 unlocked) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at -5.08 0 90) (size 2 2) (drill 1.25) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at 5.08 0 90) (size 2 2) (drill 1.25) (layers "*.Cu" "*.Mask"))
    (pad "2" thru_hole circle (at 0 0 90) (size 1.5 1.5) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 2 "Net-(Cc1-Pad2)") (pintype "passive") (thermal_bridge_angle 90))
  )
  (footprint "MountingHole:MountingHole_2.2mm_M2_DIN965_Pad" (layer "F.Cu")
    (at 51.5 93)
    (descr "Mounting Hole 2.2mm, M2, DIN965")
    (tags "mounting hole 2.2mm m2 din965")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -2.9) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_2.2mm_M2_DIN965_Pad" (at 0 2.9) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 3.8 3.8) (drill 2.2) (layers "*.Cu" "*.Mask")
      (net 32 "thermal_gnd"))
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 55.39 88.09 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "base_temp_v2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "Rbs2" (at -0.064416 2.489279 90) (layer "F.SilkS"))
    (fp_text value "R=1" (at 0 1.82 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 16 "Net-(D1-Pad12)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 4 "Net-(Cc2-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.5mm" (layer "F.Cu")
    (at 44.5 55.5)
    (descr "Mounting Hole 2.5mm, no annular")
    (tags "mounting hole 2.5mm no annular")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -3.5) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_2.5mm" (at 0 3.5) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers "*.Cu" "*.Mask"))
  )
  (footprint "charge_amp:Q_NJFET_GDS" (layer "F.Cu")
    (at 56.327641 77.049239)
    (property "Sheetfile" "base_temp_v2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "N-JFET transistor, gate/drain/source")
    (property "ki_keywords" "transistor NJFET N-JFET")
    (attr smd)
    (fp_text reference "Qr2" (at -0.013868 -8.158948 unlocked) (layer "F.SilkS"))
    (fp_text value "1.8pF" (at 0 1 unlocked) (layer "F.Fab") hide)
    (fp_text user "G" (at -2.982 -3.095 180) (layer "F.SilkS"))
    (fp_text user "D" (at 0.373 5.615 180) (layer "F.SilkS"))
    (fp_text user "S" (at -2.982 -6.27 180) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 -5.08) (layer "F.Fab"))
    (pad "1" smd rect (at -0.95 -3.73 90) (size 1.65 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 28 "Net-(D1-P24)") (pinfunction "G") (pintype "input"))
    (pad "2" smd rect (at 0.95 -3.73 90) (size 1.65 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "Net-(Qr2-D)") (pinfunction "D") (pintype "passive"))
    (pad "3" smd rect (at 0 -6.44 90) (size 1.65 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 31 "Net-(Jr2-A)") (pinfunction "S") (pintype "passive"))
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 73.47 88.13 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "base_temp_v2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "Rbs1" (at 0 -1.82 90) (layer "F.SilkS"))
    (fp_text value "R=1" (at 0 1.82 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 5 "Net-(D1-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 2 "Net-(Cc1-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.2mm_M2_DIN965_Pad" (layer "F.Cu")
    (at 77.5 69)
    (descr "Mounting Hole 2.2mm, M2, DIN965")
    (tags "mounting hole 2.2mm m2 din965")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -2.9) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_2.2mm_M2_DIN965_Pad" (at 0 2.9) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 3.8 3.8) (drill 2.2) (layers "*.Cu" "*.Mask")
      (net 32 "thermal_gnd"))
  )
  (footprint "MountingHole:MountingHole_2.1mm" (layer "F.Cu")
    (at 78.84 81.07)
    (descr "Mounting Hole 2.1mm, no annular")
    (tags "mounting hole 2.1mm no annular")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -3.2) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_2.1mm" (at 0 3.2) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0) (size 2.1 2.1) (drill 2.1) (layers "*.Cu" "*.Mask"))
  )
  (footprint "charge_amp:Q_NJFET_GDS" (layer "F.Cu")
    (at 64.172934 79.91256)
    (property "Sheetfile" "base_temp_v2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "N-JFET transistor, gate/drain/source")
    (property "ki_keywords" "transistor NJFET N-JFET")
    (attr smd)
    (fp_text reference "Q2" (at -0.165637 -3.201645 unlocked) (layer "F.SilkS"))
    (fp_text value "1.8pF" (at 0 1 unlocked) (layer "F.Fab") hide)
    (fp_text user "S" (at -1.295493 -1.855722) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -0.95 1.35 90) (size 1.65 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "Net-(Jr2-B)") (pinfunction "G") (pintype "input"))
    (pad "2" smd rect (at 0.95 1.35 90) (size 1.65 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "Net-(Q2-D)") (pinfunction "D") (pintype "passive"))
    (pad "3" smd rect (at 0 -1.36 90) (size 1.65 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 27 "Net-(D1-P23)") (pinfunction "S") (pintype "passive"))
  )
  (footprint "charge_amp:MDM25SBSP" (layer "F.Cu")
    (at 64.5 43.34)
    (descr "MDM-25SBSP-4")
    (tags "Connector")
    (property "Sheetfile" "base_temp_v2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "25-pin female D-SUB connector")
    (property "ki_keywords" "female D-SUB connector")
    (attr through_hole)
    (fp_text reference "D1" (at 0 0.95) (layer "F.SilkS"))
    (fp_text value "MDM25_FEMALE" (at -15.24 0.95) (layer "F.SilkS") hide)
    (pad "1" thru_hole circle (at 15.24 0) (size 1.219 1.219) (drill 0.711) (layers "*.Cu" "*.Mask")
      (net 5 "Net-(D1-Pad1)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 12.7 0) (size 1.219 1.219) (drill 0.711) (layers "*.Cu" "*.Mask")
      (net 6 "Net-(Qr1-D)") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle (at 10.16 0) (size 1.219 1.219) (drill 0.711) (layers "*.Cu" "*.Mask")
      (net 7 "Net-(Q1-D)") (pinfunction "3") (pintype "passive"))
    (pad "4" thru_hole circle (at 7.62 0) (size 1.219 1.219) (drill 0.711) (layers "*.Cu" "*.Mask")
      (net 8 "Net-(D1-Pad4)") (pinfunction "4") (pintype "passive"))
    (pad "5" thru_hole circle (at 5.08 0) (size 1.219 1.219) (drill 0.711) (layers "*.Cu" "*.Mask")
      (net 9 "unconnected-(D1-Pad5)") (pinfunction "5") (pintype "passive"))
    (pad "6" thru_hole circle (at 2.54 0) (size 1.219 1.219) (drill 0.711) (layers "*.Cu" "*.Mask")
      (net 10 "unconnected-(D1-Pad6)") (pinfunction "6") (pintype "passive"))
    (pad "7" thru_hole circle (at 0 0) (size 1.219 1.219) (drill 0.711) (layers "*.Cu" "*.Mask")
      (net 11 "unconnected-(D1-Pad7)") (pinfunction "7") (pintype "passive"))
    (pad "8" thru_hole circle (at -2.54 0) (size 1.219 1.219) (drill 0.711) (layers "*.Cu" "*.Mask")
      (net 12 "unconnected-(D1-Pad8)") (pinfunction "8") (pintype "passive"))
    (pad "9" thru_hole circle (at -5.08 0) (size 1.219 1.219) (drill 0.711) (layers "*.Cu" "*.Mask")
      (net 13 "Net-(D1-Pad9)") (pinfunction "9") (pintype "passive"))
    (pad "10" thru_hole circle (at -7.62 0) (size 1.219 1.219) (drill 0.711) (layers "*.Cu" "*.Mask")
      (net 14 "Net-(Q2-D)") (pinfunction "10") (pintype "passive"))
    (pad "11" thru_hole circle (at -10.16 0) (size 1.219 1.219) (drill 0.711) (layers "*.Cu" "*.Mask")
      (net 15 "Net-(Qr2-D)") (pinfunction "11") (pintype "passive"))
    (pad "12" thru_hole circle (at -12.7 0) (size 1.219 1.219) (drill 0.711) (layers "*.Cu" "*.Mask")
      (net 16 "Net-(D1-Pad12)") (pinfunction "12") (pintype "passive"))
    (pad "13" thru_hole circle (at -15.24 0) (size 1.219 1.219) (drill 0.711) (layers "*.Cu" "*.Mask")
      (net 17 "unconnected-(D1-Pad13)") (pinfunction "13") (pintype "passive"))
    (pad "14" thru_hole circle (at 13.97 2.54) (size 1.219 1.219) (drill 0.711) (layers "*.Cu" "*.Mask")
      (net 18 "Net-(D1-P14)") (pinfunction "P14") (pintype "passive"))
    (pad "15" thru_hole circle (at 11.43 2.54) (size 1.219 1.219) (drill 0.711) (layers "*.Cu" "*.Mask")
      (net 19 "Net-(D1-P15)") (pinfunction "P15") (pintype "passive"))
    (pad "16" thru_hole circle (at 8.89 2.54) (size 1.219 1.219) (drill 0.711) (layers "*.Cu" "*.Mask")
      (net 20 "Net-(D1-P16)") (pinfunction "P16") (pintype "passive"))
    (pad "17" thru_hole circle (at 6.35 2.54) (size 1.219 1.219) (drill 0.711) (layers "*.Cu" "*.Mask")
      (net 21 "unconnected-(D1-P17-Pad17)") (pinfunction "P17") (pintype "passive"))
    (pad "18" thru_hole circle (at 3.81 2.54) (size 1.219 1.219) (drill 0.711) (layers "*.Cu" "*.Mask")
      (net 22 "unconnected-(D1-P18-Pad18)") (pinfunction "P18") (pintype "passive"))
    (pad "19" thru_hole circle (at 1.27 2.54) (size 1.219 1.219) (drill 0.711) (layers "*.Cu" "*.Mask")
      (net 23 "unconnected-(D1-P19-Pad19)") (pinfunction "P19") (pintype "passive"))
    (pad "20" thru_hole circle (at -1.27 2.54) (size 1.219 1.219) (drill 0.711) (layers "*.Cu" "*.Mask")
      (net 24 "unconnected-(D1-P20-Pad20)") (pinfunction "P20") (pintype "passive"))
    (pad "21" thru_hole circle (at -3.81 2.54) (size 1.219 1.219) (drill 0.711) (layers "*.Cu" "*.Mask")
      (net 25 "unconnected-(D1-P21-Pad21)") (pinfunction "P21") (pintype "passive"))
    (pad "22" thru_hole circle (at -6.35 2.54) (size 1.219 1.219) (drill 0.711) (layers "*.Cu" "*.Mask")
      (net 26 "unconnected-(D1-P22-Pad22)") (pinfunction "P22") (pintype "passive"))
    (pad "23" thru_hole circle (at -8.89 2.54) (size 1.219 1.219) (drill 0.711) (layers "*.Cu" "*.Mask")
      (net 27 "Net-(D1-P23)") (pinfunction "P23") (pintype "passive"))
    (pad "24" thru_hole circle (at -11.43 2.54) (size 1.219 1.219) (drill 0.711) (layers "*.Cu" "*.Mask")
      (net 28 "Net-(D1-P24)") (pinfunction "P24") (pintype "passive"))
    (pad "25" thru_hole circle (at -13.97 2.54) (size 1.219 1.219) (drill 0.711) (layers "*.Cu" "*.Mask")
      (net 29 "Net-(D1-P25)") (pinfunction "P25") (pintype "passive"))
    (pad "MH1" thru_hole circle (at 19.05 1.27) (size 4.155 4.155) (drill 2.77) (layers "*.Cu" "*.Mask")
      (net 32 "thermal_gnd"))
    (pad "MH2" thru_hole circle (at -19.05 1.27) (size 4.155 4.155) (drill 2.77) (layers "*.Cu" "*.Mask")
      (net 32 "thermal_gnd"))
    (model "MDM-25SBSP.stp"
      (offset (xyz -15.23999954 -1.299999933 6.760000127))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Wire:SolderWirePad_1x01_SMD_1x2mm" (layer "F.Cu")
    (at 73.5 86.52)
    (descr "Wire Pad, Square, SMD Pad,  1mm x 2mm,")
    (tags "MesurementPoint Square SMDPad 1mmx2mm ")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "ch1_rtn" (at 0.34 -2.64) (layer "B.SilkS"))
    (fp_text value "SolderWirePad_1x01_SMD_1x2mm" (at 0 2.54) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at 0 0) (size 1 2) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 18 "Net-(D1-P14)"))
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric_Pad0.74x0.62mm_HandSolder" (layer "F.Cu")
    (at 68.89 82.9 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "base_temp_v2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "Cc1" (at -0.125312 -1.573299) (layer "F.SilkS"))
    (fp_text value "C=1" (at 0 1.16) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.5675 0 180) (size 0.735 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "Net-(Jr1-B)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.5675 0 180) (size 0.735 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "Net-(Cc1-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "charge_amp:Q_NJFET_GDS" (layer "F.Cu")
    (at 71.46 78.44)
    (property "Sheetfile" "base_temp_v2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "N-JFET transistor, gate/drain/source")
    (property "ki_keywords" "transistor NJFET N-JFET")
    (attr smd)
    (fp_text reference "Qr1" (at 0.137249 -8.476483 unlocked) (layer "F.SilkS"))
    (fp_text value "1.8pF" (at 0 1 unlocked) (layer "F.Fab") hide)
    (fp_text user "S" (at -2.982 -6.27 180) (layer "F.SilkS"))
    (fp_text user "D" (at 2.733 -3.095 180) (layer "F.SilkS"))
    (fp_text user "G" (at -2.42 -3.83 180) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 -5.08) (layer "F.Fab"))
    (pad "1" smd rect (at -0.95 -3.73 90) (size 1.65 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 19 "Net-(D1-P15)") (pinfunction "G") (pintype "input"))
    (pad "2" smd rect (at 0.95 -3.73 90) (size 1.65 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "Net-(Qr1-D)") (pinfunction "D") (pintype "passive"))
    (pad "3" smd rect (at 0 -6.44 90) (size 1.65 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 30 "Net-(Jr1-A)") (pinfunction "S") (pintype "passive"))
  )
  (footprint "MountingHole:MountingHole_2.2mm_M2_DIN965_Pad" (layer "F.Cu")
    (at 51.5 69)
    (descr "Mounting Hole 2.2mm, M2, DIN965")
    (tags "mounting hole 2.2mm m2 din965")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -2.9) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_2.2mm_M2_DIN965_Pad" (at 0 2.9) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 3.8 3.8) (drill 2.2) (layers "*.Cu" "*.Mask")
      (net 32 "thermal_gnd"))
  )
  (footprint "MountingHole:MountingHole_2.5mm" (layer "F.Cu")
    (at 84.5 55.5)
    (descr "Mounting Hole 2.5mm, no annular")
    (tags "mounting hole 2.5mm no annular")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -3.5) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_2.5mm" (at 0 3.5) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Connector_Wire:SolderWirePad_1x01_SMD_1x2mm" (layer "F.Cu")
    (at 55.5 86.46)
    (descr "Wire Pad, Square, SMD Pad,  1mm x 2mm,")
    (tags "MesurementPoint Square SMDPad 1mmx2mm ")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "ch2_rtn" (at -0.29 -2.59) (layer "B.SilkS"))
    (fp_text value "SolderWirePad_1x01_SMD_1x2mm" (at 0 2.54) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at 0 0) (size 1 2) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 29 "Net-(D1-P25)"))
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 64.458344 72.100311 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "base_temp_v2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "Rfb1" (at -3.229213 -0.08787) (layer "F.SilkS"))
    (fp_text value "R=1" (at 0 1.82 -90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 8 "Net-(D1-Pad4)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 1 "Net-(Jr1-B)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "charge_amp:detector" (layer "F.Cu")
    (at 61.130647 81.072006 90)
    (property "Sheetfile" "base_temp_v2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "Det2" (at -6.990013 -0.004027 unlocked) (layer "F.SilkS"))
    (fp_text value "C=1" (at 0 1 90 unlocked) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at -5.08 0 90) (size 2 2) (drill 1.25) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at 5.08 0 90) (size 2 2) (drill 1.25) (layers "*.Cu" "*.Mask"))
    (pad "2" thru_hole circle (at 0 0 90) (size 1.5 1.5) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 4 "Net-(Cc2-Pad2)") (pintype "passive") (thermal_bridge_angle 90))
  )
  (footprint "charge_amp:Q_NJFET_GDS" (layer "F.Cu")
    (at 70.625438 79.806386)
    (property "Sheetfile" "base_temp_v2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "N-JFET transistor, gate/drain/source")
    (property "ki_keywords" "transistor NJFET N-JFET")
    (attr smd)
    (fp_text reference "Q1" (at 0.016343 -3.275674 unlocked) (layer "F.SilkS"))
    (fp_text value "1.8pF" (at 0 1 unlocked) (layer "F.Fab") hide)
    (fp_text user "D" (at 2.733 1.985 180) (layer "F.SilkS"))
    (fp_text user "G" (at -2.070452 -0.267385 180) (layer "F.SilkS"))
    (fp_text user "S" (at 1.120224 -1.491556 180) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -0.95 1.35 90) (size 1.65 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "Net-(Jr1-B)") (pinfunction "G") (pintype "input"))
    (pad "2" smd rect (at 0.95 1.35 90) (size 1.65 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "Net-(Q1-D)") (pinfunction "D") (pintype "passive"))
    (pad "3" smd rect (at 0 -1.36 90) (size 1.65 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 20 "Net-(D1-P16)") (pinfunction "S") (pintype "passive"))
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 60.96 72.150595 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "base_temp_v2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "Rfb2" (at -3.257529 0.829241) (layer "F.SilkS"))
    (fp_text value "R=1" (at 0 1.82 -90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 13 "Net-(D1-Pad9)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 3 "Net-(Jr2-B)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0402_1005Metric_Pad0.72x0.64mm_HandSolder" (layer "F.Cu")
    (at 56.916629 76.619209)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "base_temp_v2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Jumper, 2-pole, closed/bridged")
    (property "ki_keywords" "Jumper SPST")
    (attr smd)
    (fp_text reference "Jr2" (at -0.63383 1.40839) (layer "F.SilkS"))
    (fp_text value "R=0" (at 0 1.17) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at -2.471429 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.5975 0) (size 0.715 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 31 "Net-(Jr2-A)") (pinfunction "A") (pintype "passive"))
    (pad "2" smd roundrect (at 0.5975 0) (size 0.715 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "Net-(Jr2-B)") (pinfunction "B") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0402_1005Metric_Pad0.72x0.64mm_HandSolder" (layer "F.Cu")
    (at 66.347008 73.0625 -90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "base_temp_v2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Jumper, 2-pole, closed/bridged")
    (property "ki_keywords" "Jumper SPST")
    (attr smd)
    (fp_text reference "Jr1" (at -0.118806 -1.156608 -270) (layer "F.SilkS"))
    (fp_text value "R=0" (at 0 1.17 -270) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 -270) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.5975 0 270) (size 0.715 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 30 "Net-(Jr1-A)") (pinfunction "A") (pintype "passive"))
    (pad "2" smd roundrect (at 0.5975 0 270) (size 0.715 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "Net-(Jr1-B)") (pinfunction "B") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.1mm" (layer "F.Cu")
    (at 50.16 81.07)
    (descr "Mounting Hole 2.1mm, no annular")
    (tags "mounting hole 2.1mm no annular")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -3.2) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_2.1mm" (at 0 3.2) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0) (size 2.1 2.1) (drill 2.1) (layers "*.Cu" "*.Mask"))
  )
  (footprint "MountingHole:MountingHole_2.2mm_M2_DIN965_Pad" (layer "F.Cu")
    (at 77.5 93)
    (descr "Mounting Hole 2.2mm, M2, DIN965")
    (tags "mounting hole 2.2mm m2 din965")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -2.9) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_2.2mm_M2_DIN965_Pad" (at 0 2.9) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 3.8 3.8) (drill 2.2) (layers "*.Cu" "*.Mask")
      (net 32 "thermal_gnd"))
  )
  (gr_line (start 48.5 66) (end 62.3 66)
    (layer "Edge.Cuts"))
  (gr_line (start 48.5 66) (end 48.5 96)
    (layer "Edge.Cuts"))
  (gr_line (start 41 59) (end 62.3 59)
    (layer "Edge.Cuts"))
  (gr_line (start 66.7 59) (end 66.7 66)
    (layer "Edge.Cuts"))
  (gr_line (start 41 39) (end 88 39)
    (layer "Edge.Cuts"))
  (gr_line (start 88 59) (end 88 39)
    (layer "Edge.Cuts"))
  (gr_line (start 66.7 59) (end 88 59)
    (layer "Edge.Cuts"))
  (gr_line (start 41 59) (end 41 39)
    (layer "Edge.Cuts"))
  (gr_line (start 80.5 66) (end 80.5 96)
    (layer "Edge.Cuts"))
  (gr_line (start 48.5 96) (end 80.5 96)
    (layer "Edge.Cuts"))
  (gr_line (start 62.3 59) (end 62.3 66)
    (layer "Edge.Cuts"))
  (gr_line (start 80.5 66) (end 66.7 66)
    (layer "Edge.Cuts"))
  (gr_text "G" (at 62.12 80.47) (layer "F.SilkS"))
  (zone (net 32) (net_name "thermal_gnd") (layers "F&B.Cu") (hatch edge 0.5)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 40.64 37.993981)
        (xy 40.541805 59.491126)
        (xy 88.521945 59.515657)
        (xy 88.4472 37.992023)
      )
    )
  )
  (zone (net 32) (net_name "thermal_gnd") (layers "F&B.Cu") (hatch edge 0.5)
    (priority 1)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 47.625 65.405)
        (xy 47.625 96.52)
        (xy 81.915 96.52)
        (xy 81.915 65.405)
      )
    )
  )
  (zone (net 0) (net_name "") (layers "F&B.Cu") (name "no copper") (hatch edge 0.5)
    (connect_pads (clearance 0))
    (min_thickness 0.25) (filled_areas_thickness no)
    (keepout (tracks allowed) (vias allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 78.105 67.945)
        (xy 78.105 93.345)
        (xy 50.8 93.345)
        (xy 50.8 67.945)
      )
    )
  )
  (zone (net 32) (net_name "thermal_gnd") (layers "F&B.Cu") (hatch edge 0.5)
    (priority 2)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 61.59 49.57)
        (xy 61.55 66.42)
        (xy 67.19 66.42)
        (xy 67.19 49.57)
      )
    )
  )
)
