(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 47)
    (no_connects 0)
    (area 92.522381 57.236666 113.72762 83.505)
    (thickness 1.6)
    (drawings 27)
    (tracks 162)
    (zones 0)
    (modules 33)
    (nets 23)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.18)
    (zone_clearance 0.2)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2.5 2.5)
    (pad_drill 0)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFEFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 VDD)
  (net 2 GND)
  (net 3 "Net-(D1-Pad2)")
  (net 4 "Net-(J5-Pad1)")
  (net 5 "Net-(J10-Pad1)")
  (net 6 "Net-(J5-Pad3)")
  (net 7 "Net-(J5-Pad6)")
  (net 8 "Net-(J6-Pad1)")
  (net 9 "Net-(J8-Pad1)")
  (net 10 "Net-(J11-Pad1)")
  (net 11 "Net-(J12-Pad1)")
  (net 12 "Net-(J13-Pad1)")
  (net 13 "Net-(J15-Pad1)")
  (net 14 "Net-(J16-Pad1)")
  (net 15 "Net-(J17-Pad1)")
  (net 16 "Net-(J18-Pad1)")
  (net 17 "Net-(J19-Pad1)")
  (net 18 "Net-(J20-Pad1)")
  (net 19 "Net-(J21-Pad1)")
  (net 20 "Net-(J22-Pad1)")
  (net 21 "Net-(J23-Pad1)")
  (net 22 "Net-(J24-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.18)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(J10-Pad1)")
    (add_net "Net-(J11-Pad1)")
    (add_net "Net-(J12-Pad1)")
    (add_net "Net-(J13-Pad1)")
    (add_net "Net-(J15-Pad1)")
    (add_net "Net-(J16-Pad1)")
    (add_net "Net-(J17-Pad1)")
    (add_net "Net-(J18-Pad1)")
    (add_net "Net-(J19-Pad1)")
    (add_net "Net-(J20-Pad1)")
    (add_net "Net-(J21-Pad1)")
    (add_net "Net-(J22-Pad1)")
    (add_net "Net-(J23-Pad1)")
    (add_net "Net-(J24-Pad1)")
    (add_net "Net-(J5-Pad1)")
    (add_net "Net-(J5-Pad3)")
    (add_net "Net-(J5-Pad6)")
    (add_net "Net-(J6-Pad1)")
    (add_net "Net-(J8-Pad1)")
    (add_net VDD)
  )
  (module PIC:C_0603 (layer F.Cu) (tedit 59F21761)
    (at 103.75 71 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at 0 -1.5 180) (layer F.SilkS) hide)
    (fp_text value C (at 0 1.5 180) (layer F.Fab))
    (pad 2 smd oval (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 1 smd oval (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module PIC:LED_0603 (layer F.Cu) (tedit 59F21753)
    (at 105.25 66 270)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D1 (at 0 -1.25 270) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.35 270) (layer F.Fab))
    (pad 2 smd rect (at 0.8 0 90) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at -0.8 0 90) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module PIC:Test_Pad (layer F.Cu) (tedit 59F21758)
    (at 103.75 81)
    (fp_text reference J1 (at 0 -1.75) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 1.45) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
  )
  (module PIC:Test_Pad (layer F.Cu) (tedit 59F2175B)
    (at 110.5 66.75)
    (fp_text reference J2 (at 0 -1.75) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 1.45) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
  )
  (module PIC:Test_Pad (layer F.Cu) (tedit 59F21768)
    (at 110.5 68.25)
    (fp_text reference J3 (at 0 -1.75) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 1.45) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module PIC:Test_Pad (layer F.Cu) (tedit 59F21763)
    (at 102.25 81)
    (fp_text reference J4 (at 0 -1.75) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 1.45) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module PIC:Pin_Header_Straight_1x06_Pitch2.54mm (layer F.Cu) (tedit 59F21721)
    (at 109.5 62.25 270)
    (descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x06 2.54mm single row")
    (fp_text reference J5 (at 0 -2.33 270) (layer F.SilkS) hide)
    (fp_text value CONN_01X06 (at 0 15.03 270) (layer F.Fab))
    (fp_text user %R (at 0 6.35 360) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J5-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J10-Pad1)"))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(J5-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 VDD))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(J5-Pad6)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x06_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module PIC:Test_Pad (layer F.Cu) (tedit 59F21766)
    (at 95.75 66.75)
    (fp_text reference J6 (at 0 -1.75) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 1.45) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(J6-Pad1)"))
  )
  (module PIC:Test_Pad (layer F.Cu) (tedit 59F2175E)
    (at 110.5 69.75)
    (fp_text reference J7 (at 0 -1.75) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 1.45) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(J5-Pad3)"))
  )
  (module PIC:Test_Pad (layer F.Cu) (tedit 59F2179D)
    (at 95.75 68.25)
    (fp_text reference J8 (at 0 -1.75) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 1.45) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(J8-Pad1)"))
  )
  (module PIC:Test_Pad (layer F.Cu) (tedit 59F2179A)
    (at 95.75 69.75)
    (fp_text reference J9 (at 0 -1.75) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 1.45) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(J5-Pad6)"))
  )
  (module PIC:Test_Pad (layer F.Cu) (tedit 59F21798)
    (at 110.5 71.25)
    (fp_text reference J10 (at 0 -1.75) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 1.45) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(J10-Pad1)"))
  )
  (module PIC:Test_Pad (layer F.Cu) (tedit 59F21795)
    (at 95.75 72.75)
    (fp_text reference J12 (at 0 -1.75) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 1.45) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(J12-Pad1)"))
  )
  (module PIC:Test_Pad (layer F.Cu) (tedit 59F21793)
    (at 95.75 71.25)
    (fp_text reference J13 (at 0 -1.75) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 1.45) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(J13-Pad1)"))
  )
  (module PIC:Test_Pad (layer F.Cu) (tedit 59F21790)
    (at 110.5 72.75)
    (fp_text reference J14 (at 0 -1.75) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 1.45) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(J11-Pad1)"))
  )
  (module PIC:Test_Pad (layer F.Cu) (tedit 59F2178A)
    (at 110.5 74.25)
    (fp_text reference J15 (at 0 -1.75) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 1.45) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(J15-Pad1)"))
  )
  (module PIC:Test_Pad (layer F.Cu) (tedit 59F2178D)
    (at 95.75 74.25)
    (fp_text reference J16 (at 0 -1.75) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 1.45) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(J16-Pad1)"))
  )
  (module PIC:Test_Pad (layer F.Cu) (tedit 59F217C0)
    (at 95.75 75.75)
    (fp_text reference J17 (at 0 -1.75) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 1.45) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(J17-Pad1)"))
  )
  (module PIC:Test_Pad (layer F.Cu) (tedit 59F217C3)
    (at 110.5 77.25)
    (fp_text reference J18 (at 0 -1.75) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 1.45) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(J18-Pad1)"))
  )
  (module PIC:Test_Pad (layer F.Cu) (tedit 59F217C5)
    (at 110.5 75.75)
    (fp_text reference J19 (at 0 -1.75) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 1.45) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(J19-Pad1)"))
  )
  (module PIC:Test_Pad (layer F.Cu) (tedit 59F217BE)
    (at 95.75 77.25)
    (fp_text reference J20 (at 0 -1.75) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 1.45) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(J20-Pad1)"))
  )
  (module PIC:Test_Pad (layer F.Cu) (tedit 59F217BB)
    (at 108.25 81)
    (fp_text reference J21 (at 0 -1.75) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 1.45) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(J21-Pad1)"))
  )
  (module PIC:Test_Pad (layer F.Cu) (tedit 59F217B9)
    (at 97.75 81)
    (fp_text reference J22 (at 0 -1.75) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 1.45) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(J22-Pad1)"))
  )
  (module PIC:Test_Pad (layer F.Cu) (tedit 59F217CB)
    (at 99.25 81)
    (fp_text reference J23 (at 0 -1.75) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 1.45) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(J23-Pad1)"))
  )
  (module PIC:Test_Pad (layer F.Cu) (tedit 59F217CD)
    (at 106.75 81)
    (fp_text reference J24 (at 0 -1.75) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 1.45) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(J24-Pad1)"))
  )
  (module PIC:R_0603 (layer F.Cu) (tedit 59F21755)
    (at 103.75 68.75 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at 0 -1.45 270) (layer F.SilkS) hide)
    (fp_text value R (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(J11-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module PIC:R_0603 (layer F.Cu) (tedit 59F2176B)
    (at 105.25 68.75 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at 0 -1.45 90) (layer F.SilkS) hide)
    (fp_text value R (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(J13-Pad1)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module PIC:UQFN-20-1EP_4x4mm_Pitch0.5mm (layer F.Cu) (tedit 59F26E58)
    (at 103 74.75)
    (descr "20-Lead Ultra Thin Plastic Quad Flat, No Lead Package (GZ) - 4x4x0.5 mm Body [UQFN]; (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFN 0.5")
    (attr smd)
    (fp_text reference U1 (at 0 -3.4) (layer F.SilkS) hide)
    (fp_text value PIC16F1829 (at 0 3.4) (layer F.Fab))
    (pad 1 smd oval (at -2 -1) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(J5-Pad6)"))
    (pad 2 smd oval (at -2 -0.5) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(J13-Pad1)"))
    (pad 3 smd oval (at -2 0) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(J12-Pad1)"))
    (pad 4 smd oval (at -2 0.5) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(J16-Pad1)"))
    (pad 5 smd oval (at -2 1) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(J17-Pad1)"))
    (pad 6 smd oval (at -1 2 90) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(J20-Pad1)"))
    (pad 7 smd oval (at -0.5 2 90) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(J22-Pad1)"))
    (pad 8 smd oval (at 0 2 90) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(J24-Pad1)"))
    (pad 9 smd oval (at 0.5 2 90) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(J23-Pad1)"))
    (pad 10 smd oval (at 1 2 90) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(J21-Pad1)"))
    (pad 11 smd oval (at 2 1) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(J18-Pad1)"))
    (pad 12 smd oval (at 2 0.5) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(J19-Pad1)"))
    (pad 13 smd oval (at 2 0) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(J15-Pad1)"))
    (pad 14 smd oval (at 2 -0.5) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(J11-Pad1)"))
    (pad 15 smd oval (at 2 -1) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(J10-Pad1)"))
    (pad 16 smd oval (at 1 -2 90) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(J5-Pad3)"))
    (pad 17 smd oval (at 0.5 -2 90) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 18 smd oval (at 0 -2 90) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 19 smd oval (at -0.5 -2 90) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(J6-Pad1)"))
    (pad 20 smd oval (at -1 -2 90) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(J8-Pad1)"))
    (pad 21 smd rect (at 0 0) (size 2.5 2.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Housings_DFN_QFN.3dshapes/UQFN-20-1EP_4x4mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module PIC:KMR621NG (layer F.Cu) (tedit 59F26F5B)
    (at 101.5 67 90)
    (fp_text reference J11 (at 0 2.55 90) (layer F.SilkS) hide)
    (fp_text value TEST_2P (at 0 -2.3 90) (layer F.Fab))
    (pad 1 smd rect (at 2.05 0.8 90) (size 0.9 1) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(J11-Pad1)"))
    (pad 2 smd rect (at 2.05 -0.8 90) (size 0.9 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -2.05 -0.8 90) (size 0.9 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -2.05 0.8 90) (size 0.9 1) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(J11-Pad1)"))
  )
  (module PIC:R_0603 (layer B.Cu) (tedit 59F267D6)
    (at 99.5 77 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at 0 1.45 270) (layer B.SilkS) hide)
    (fp_text value R (at 0 -1.5 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 20 "Net-(J22-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module PIC:R_0603 (layer B.Cu) (tedit 59F267D4)
    (at 101.5 77 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at 0 1.45 270) (layer B.SilkS) hide)
    (fp_text value R (at 0 -1.5 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 22 "Net-(J24-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module PIC:R_0603 (layer B.Cu) (tedit 59F267D1)
    (at 106.5 77 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at 0 1.45 90) (layer B.SilkS) hide)
    (fp_text value R (at 0 -1.5 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 19 "Net-(J21-Pad1)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module PIC:R_0603 (layer B.Cu) (tedit 59F267D2)
    (at 104.5 77 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R6 (at 0 1.45 90) (layer B.SilkS) hide)
    (fp_text value R (at 0 -1.5 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 21 "Net-(J23-Pad1)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 1 VDD))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text PIC16F1829 (at 96.25 76 90) (layer B.SilkS))
  (gr_text RC7 (at 97.5 77.25) (layer F.SilkS))
  (gr_text VDD (at 108.75 66.75) (layer F.SilkS))
  (gr_text GND (at 108.75 68.25) (layer F.SilkS))
  (gr_text RA0 (at 108.75 69.75) (layer F.SilkS))
  (gr_text RA1 (at 108.75 71.25) (layer F.SilkS))
  (gr_text RA2 (at 108.75 72.75) (layer F.SilkS))
  (gr_text RC0 (at 108.75 74.25) (layer F.SilkS))
  (gr_text RC1 (at 108.75 75.75) (layer F.SilkS))
  (gr_text RA5 (at 97.5 66.75) (layer F.SilkS))
  (gr_text RA4 (at 97.5 68.25) (layer F.SilkS))
  (gr_text RA3 (at 97.5 69.75) (layer F.SilkS))
  (gr_text RC5 (at 97.5 71.25) (layer F.SilkS))
  (gr_text RC4 (at 97.5 72.75) (layer F.SilkS))
  (gr_text RC3 (at 97.5 74.25) (layer F.SilkS))
  (gr_text RC6 (at 97.5 75.75) (layer F.SilkS))
  (gr_text RC2 (at 108.75 77.25) (layer F.SilkS))
  (gr_text VDD (at 103.75 79.25 270) (layer F.SilkS))
  (gr_text GND (at 102.25 79.25 270) (layer F.SilkS))
  (gr_text SCL2 (at 97.75 79 270) (layer F.SilkS))
  (gr_text SDA2 (at 99.25 79 270) (layer F.SilkS))
  (gr_text SCL1 (at 106.75 79 270) (layer F.SilkS))
  (gr_line (start 95 81.75) (end 95 60.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 111.25 81.75) (end 95 81.75) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 111.25 60.5) (end 111.25 81.75) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 95 60.5) (end 111.25 60.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text SDA1 (at 108.25 79 270) (layer F.SilkS))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.2) (thermal_bridge_width 0.22))
    (polygon
      (pts
        (xy 111.25 81.75) (xy 95 81.75) (xy 95 60.5) (xy 111.25 60.5)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.2) (thermal_bridge_width 0.22))
    (polygon
      (pts
        (xy 111.25 81.75) (xy 95 81.75) (xy 95 60.5) (xy 111.25 60.5)
      )
    )
  )
)
