<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="26.34" y2="0" width="0" layer="20"/>
<wire x1="26.34" y1="0" x2="26.34" y2="49.52" width="0" layer="20"/>
<wire x1="26.34" y1="49.52" x2="0" y2="49.52" width="0" layer="20"/>
<wire x1="0" y1="49.52" x2="0" y2="0" width="0" layer="20"/>
<text>Piezo</text>
<text>Attiny45</text>
<text>0.33</text>
<text>0.01</text>
<text>0.1</text>
<text>0.1</text>
<text>0.01</text>
<text>0.01</text>
<text>JackYack</text>
<text>Rev A</text>
<hole x="3.81" y="45.72" drill="3.9624"/>
<hole x="22.86" y="3.81" drill="3.9624"/>
</plain>
<libraries>
<library name="adafruit">
<packages>
<package name="TO92">
<description>&lt;b&gt;TO-92&lt;/b&gt;</description>
</package>
<package name="TO92-EBC-OVAL">
<description>&lt;b&gt;TO-92&lt;/b&gt;&lt;p&gt;
grid 5.08 mm</description>
</package>
</packages>
</library>
<library name="SparkFun">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CAP-PTH-SMALL-KIT">
<description>&lt;h3&gt;CAP-PTH-SMALL-KIT&lt;/h3&gt;
Commonly used for small ceramic capacitors. Like our 0.1uF (http://www.sparkfun.com/products/8375) or 22pF caps (http://www.sparkfun.com/products/8571).&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Warning:&lt;/b&gt; This is the KIT version of this package. This package has a smaller diameter top stop mask, which doesn't cover the diameter of the pad. This means only the bottom side of the pads' copper will be exposed. You'll only be able to solder to the bottom side.</description>
</package>
<package name="DIP08">
<description>&lt;b&gt;Dual In Line&lt;/b&gt;</description>
</package>
<package name="AXIAL-0.4">
<description>1/4W Resistor, 0.4" wide&lt;p&gt;

Yageo CFR series &lt;a href="http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf"&gt;http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf&lt;/a&gt;</description>
</package>
</packages>
</library>
<library name="solpad">
<description>&lt;b&gt;Solder Pads/Test Points&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="LSP10">
<description>&lt;b&gt;SOLDER PAD&lt;/b&gt;&lt;p&gt;
drill 1.0 mm</description>
</package>
</packages>
</library>
<library name="diode">
<description>&lt;b&gt;Diodes&lt;/b&gt;&lt;p&gt;
Based on the following sources:
&lt;ul&gt;
&lt;li&gt;Motorola : www.onsemi.com
&lt;li&gt;Fairchild : www.fairchildsemi.com
&lt;li&gt;Philips : www.semiconductors.com
&lt;li&gt;Vishay : www.vishay.de
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DO41-7.6">
<description>&lt;b&gt;DO41&lt;/b&gt; 7.6mm x 2mm&lt;p&gt;
Source: http://www.diodes.com/datasheets/ds23001.pdf</description>
</package>
</packages>
</library>
<library name="test2">
<packages>
<package name="PS12">
<description>mouser PN 254-pb140-rox 5V piezo speaker</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC1" library="adafruit" package="TO92" value="78L05Z">
<attribute name="NAME"/>
</element>
<element name="C3" library="SparkFun" package="CAP-PTH-SMALL-KIT" value="0.1uF"/>
<element name="U$1" library="SparkFun" package="DIP08" value="ATTINY45DIP8"/>
<element name="C4" library="SparkFun" package="CAP-PTH-SMALL-KIT" value="0.1uF"/>
<element name="R2" library="SparkFun" package="AXIAL-0.4" value="4k7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="SparkFun" package="CAP-PTH-SMALL-KIT" value="0.01uF"/>
<element name="C5" library="SparkFun" package="CAP-PTH-SMALL-KIT" value="0.01uF"/>
<element name="R1" library="SparkFun" package="AXIAL-0.4" value="4k7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="T1" library="adafruit" package="TO92-EBC-OVAL" value="2N2222">
<attribute name="VALUE"/>
</element>
<element name="C1" library="SparkFun" package="CAP-PTH-SMALL-KIT" value="0.01uF"/>
<element name="KEY+" library="solpad" package="LSP10" value="LSP10">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="KG" library="solpad" package="LSP10" value="LSP10">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="BTN" library="solpad" package="LSP10" value="LSP10">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="BG" library="solpad" package="LSP10" value="LSP10">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="PWR+" library="solpad" package="LSP10" value="LSP10">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="PG" library="solpad" package="LSP10" value="LSP10">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="SparkFun" package="CAP-PTH-SMALL-KIT" value="0.33uF"/>
<element name="D1" library="diode" package="DO41-7.6" value="1N5817-T"/>
<element name="DIT" library="solpad" package="LSP10" value="LSP10">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="DAH" library="solpad" package="LSP10" value="LSP10">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="DG" library="solpad" package="LSP10" value="LSP10">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SP1" library="test2" package="PS12" value="SPEAKERPB140"/>
</elements>
<signals>
<signal name="GND">
<contactref element="IC1" pad="2"/>
<contactref element="C3" pad="1"/>
<contactref element="C2" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="U$1" pad="4"/>
<contactref element="C6" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="T1" pad="E"/>
<contactref element="C1" pad="2"/>
<contactref element="KG" pad="MP"/>
<contactref element="BG" pad="MP"/>
<contactref element="DG" pad="MP"/>
<contactref element="SP1" pad="P$2"/>
<contactref element="PG" pad="MP"/>
</signal>
<signal name="N$34">
<contactref element="PWR+" pad="MP"/>
<contactref element="D1" pad="A"/>
</signal>
<signal name="N$35">
<contactref element="IC1" pad="3"/>
<contactref element="C2" pad="1"/>
<contactref element="D1" pad="C"/>
</signal>
<signal name="RST">
<contactref element="R2" pad="P$2"/>
<contactref element="U$1" pad="1"/>
</signal>
<signal name="N$38">
<contactref element="U$1" pad="3"/>
<contactref element="C6" pad="1"/>
<contactref element="DAH" pad="MP"/>
</signal>
<signal name="N$39">
<contactref element="U$1" pad="2"/>
<contactref element="C5" pad="1"/>
<contactref element="DIT" pad="MP"/>
</signal>
<signal name="BUTTON">
<contactref element="U$1" pad="7"/>
<contactref element="BTN" pad="MP"/>
</signal>
<signal name="N$42">
<contactref element="U$1" pad="5"/>
<contactref element="R1" pad="P$1"/>
</signal>
<signal name="N$43">
<contactref element="R1" pad="P$2"/>
<contactref element="T1" pad="B"/>
</signal>
<signal name="KEY">
<contactref element="T1" pad="C"/>
<contactref element="C1" pad="1"/>
<contactref element="KEY+" pad="MP"/>
</signal>
<signal name="N$3">
<contactref element="C3" pad="2"/>
<contactref element="IC1" pad="1"/>
<contactref element="U$1" pad="8"/>
<contactref element="C4" pad="1"/>
<contactref element="R2" pad="P$1"/>
</signal>
<signal name="N$1">
<contactref element="U$1" pad="6"/>
<contactref element="SP1" pad="P$1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
