(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 66)
    (no_connects 0)
    (area 128.724999 91.974999 150.875001 111.825001)
    (thickness 0.8)
    (drawings 55)
    (tracks 327)
    (zones 0)
    (modules 31)
    (nets 24)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.2)
    (user_trace_width 0.3)
    (trace_clearance 0.1524)
    (zone_clearance 0.2)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.3)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.2 1.2)
    (pad_drill 0.7)
    (pad_to_mask_clearance 0.06)
    (aux_axis_origin 128.8 92.05)
    (grid_origin 128.8 92.05)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x00000_00000001)
      (usegerberextensions false)
      (excludeedgelayer false)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask true)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference false)
      (plotvalue false)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 4)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory C:/src/Temp/git/TinyDivercityRX5808/KiCad/))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 /PROG_PWR)
  (net 3 VCC)
  (net 4 "Net-(D1-Pad1)")
  (net 5 "Net-(D2-Pad1)")
  (net 6 "Net-(J1-Pad1)")
  (net 7 "Net-(J1-Pad2)")
  (net 8 "Net-(J1-Pad3)")
  (net 9 /RSSI_A)
  (net 10 /AUD_IN)
  (net 11 /VideoOut)
  (net 12 "Net-(J2-Pad1)")
  (net 13 "Net-(J2-Pad2)")
  (net 14 "Net-(J2-Pad3)")
  (net 15 /AUD_OUT)
  (net 16 /VideoA)
  (net 17 /RSSI_B)
  (net 18 "Net-(J3-Pad7)")
  (net 19 /VideoB)
  (net 20 /MISO)
  (net 21 /SCK)
  (net 22 /MOSI)
  (net 23 /RST)
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.2)
    (via_dia 0.6)
    (via_drill 0.3)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /AUD_IN)
    (add_net /AUD_OUT)
    (add_net /MISO)
    (add_net /MOSI)
    (add_net /RSSI_A)
    (add_net /RSSI_B)
    (add_net /RST)
    (add_net /SCK)
    (add_net /VideoA)
    (add_net /VideoB)
    (add_net /VideoOut)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J3-Pad7)")
  )
  (net_class GND ""
    (clearance 0.2)
    (trace_width 0.3)
    (via_dia 1)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
  )
  (net_class VCC ""
    (clearance 0.1524)
    (trace_width 0.3)
    (via_dia 1)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /PROG_PWR)
    (add_net VCC)
  )
  (module Connectors:Pin_d0.7mm_L6.5mm_W1.8mm_FlatFork (layer F.Cu) (tedit 5AAFB37B)
    (at 148.15 92.075)
    (descr "solder Pin_ with flat fork, hole diameter 0.7mm, length 6.5mm, width 1.8mm")
    (tags "solder Pin_ with flat fork")
    (fp_text reference REF** (at 0 1.8) (layer F.SilkS) hide)
    (fp_text value Pin_d0.7mm_L6.5mm_W1.8mm_FlatFork (at 0 -1.8) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 3 VCC))
    (model ${KISYS3DMOD}/Connectors.3dshapes/Pin_d0.7mm_L6.5mm_W1.8mm_FlatFork.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors:Pin_d0.7mm_L6.5mm_W1.8mm_FlatFork (layer F.Cu) (tedit 5AAFB38D)
    (at 145.9 92.075)
    (descr "solder Pin_ with flat fork, hole diameter 0.7mm, length 6.5mm, width 1.8mm")
    (tags "solder Pin_ with flat fork")
    (fp_text reference REF** (at 0 1.8) (layer F.SilkS) hide)
    (fp_text value Pin_d0.7mm_L6.5mm_W1.8mm_FlatFork (at 0 -1.8) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 5 "Net-(D2-Pad1)"))
    (model ${KISYS3DMOD}/Connectors.3dshapes/Pin_d0.7mm_L6.5mm_W1.8mm_FlatFork.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors:Pin_d0.7mm_L6.5mm_W1.8mm_FlatFork (layer F.Cu) (tedit 5AAFB39C)
    (at 133.7 92.075)
    (descr "solder Pin_ with flat fork, hole diameter 0.7mm, length 6.5mm, width 1.8mm")
    (tags "solder Pin_ with flat fork")
    (fp_text reference REF** (at 0 1.8) (layer F.SilkS) hide)
    (fp_text value Pin_d0.7mm_L6.5mm_W1.8mm_FlatFork (at 0 -1.8) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 4 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Connectors.3dshapes/Pin_d0.7mm_L6.5mm_W1.8mm_FlatFork.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors:Pin_d0.7mm_L6.5mm_W1.8mm_FlatFork (layer F.Cu) (tedit 5AAFB370)
    (at 131.425 92.075)
    (descr "solder Pin_ with flat fork, hole diameter 0.7mm, length 6.5mm, width 1.8mm")
    (tags "solder Pin_ with flat fork")
    (fp_text reference REF** (at 0 1.8) (layer F.SilkS) hide)
    (fp_text value Pin_d0.7mm_L6.5mm_W1.8mm_FlatFork (at 0 -1.8) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 3 VCC))
    (model ${KISYS3DMOD}/Connectors.3dshapes/Pin_d0.7mm_L6.5mm_W1.8mm_FlatFork.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_2.5mm (layer F.Cu) (tedit 5A3B72BF)
    (at 148.3 106.05)
    (descr "Mounting Hole 2.5mm, no annular")
    (tags "mounting hole 2.5mm no annular")
    (clearance 0.7)
    (attr virtual)
    (fp_text reference REF** (at 0 -3.5) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.5mm (at 0 3.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at -0.7 0) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_2.5mm (layer F.Cu) (tedit 5A3A848B)
    (at 132 106.05)
    (descr "Mounting Hole 2.5mm, no annular")
    (tags "mounting hole 2.5mm no annular")
    (clearance 0.7)
    (attr virtual)
    (fp_text reference REF** (at 0 -3.5) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.5mm (at 0 3.5) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask))
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 5A3A5749)
    (at 147.03 92.85)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D2 (at 0 -1.45) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.55) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.25) (layer F.Fab) hide)
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D2-Pad1)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 5A3A57BB)
    (at 132.56 92.85 180)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D1 (at 0 -1.45 180) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.55 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.25 180) (layer F.Fab) hide)
    (pad 2 smd rect (at 1.1 0) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 1 smd rect (at -1.1 0) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Connectors_Molex:Molex_PicoBlade_53047-0910_09x1.25mm_Straight (layer F.Cu) (tedit 5A3A354A)
    (at 144.8 109 180)
    (descr "Molex PicoBlade, single row, top entry type, through hole, PN:53047-0910")
    (tags "connector molex picoblade")
    (fp_text reference J1 (at 5 2.5 180) (layer F.SilkS) hide)
    (fp_text value Googles (at 4.95 -4.325 180) (layer F.Fab))
    (fp_text user %R (at 5 -1.25 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad1)"))
    (pad 2 thru_hole circle (at 1.25 0 180) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-Pad2)"))
    (pad 3 thru_hole circle (at 2.5 0 180) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 8 "Net-(J1-Pad3)"))
    (pad 4 thru_hole circle (at 3.75 0 180) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 5 thru_hole circle (at 5 0 180) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 6 thru_hole circle (at 6.25 0 180) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 9 /RSSI_A))
    (pad 7 thru_hole circle (at 7.5 0 180) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 10 /AUD_IN))
    (pad 8 thru_hole circle (at 8.75 0 180) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 11 /VideoOut))
    (pad 9 thru_hole circle (at 10 0 180) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND))
    (model Connectors_Molex.3dshapes/Molex_PicoBlade_53047-0910.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5A393691)
    (at 135.61 101.67 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at 0 -1.5 180) (layer F.SilkS) hide)
    (fp_text value 100n (at 0 1.5 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 /PROG_PWR))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5A393695)
    (at 135.61 100.29 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at 0 -1.5 180) (layer F.SilkS) hide)
    (fp_text value 10n (at 0 1.5 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 /PROG_PWR))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5A393669)
    (at 135.62 97.07)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C3 (at 0 -1.5) (layer F.SilkS) hide)
    (fp_text value 100n (at 0 1.5) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 /PROG_PWR))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5A393663)
    (at 135.62 98.45)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C4 (at 0 -1.5) (layer F.SilkS) hide)
    (fp_text value 10uf (at 0 1.5) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 /PROG_PWR))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiCadCustomLibs:Pads_prog_6pin1.25mm (layer F.Cu) (tedit 5A393015)
    (at 140.42 94.16 180)
    (fp_text reference J4 (at 0.5 2 180) (layer F.SilkS) hide)
    (fp_text value Conn_01x06 (at 0 -2.25 180) (layer F.Fab) hide)
    (pad 6 smd oval (at 3.125 0 180) (size 0.8 2) (layers F.Cu F.Paste F.Mask)
      (net 23 /RST))
    (pad 1 smd oval (at -3.125 0 180) (size 0.8 2) (layers F.Cu F.Paste F.Mask)
      (net 2 /PROG_PWR))
    (pad 5 smd oval (at 1.875 0 180) (size 0.8 2) (layers F.Cu F.Paste F.Mask)
      (net 21 /SCK))
    (pad 2 smd oval (at -1.875 0 180) (size 0.8 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd oval (at -0.625 0 180) (size 0.8 2) (layers F.Cu F.Paste F.Mask)
      (net 22 /MOSI))
    (pad 4 smd oval (at 0.625 0 180) (size 0.8 2) (layers F.Cu F.Paste F.Mask)
      (net 20 /MISO))
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 5A3A3385)
    (at 141.925 110.575 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at 0 1.45 270) (layer B.SilkS) hide)
    (fp_text value 1K (at 0 -1.5 270) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(J1-Pad3)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 14 "Net-(J2-Pad3)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 5A3A3367)
    (at 143.55 110.575 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at 0 1.45 270) (layer B.SilkS) hide)
    (fp_text value 1K (at 0 -1.5 270) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(J1-Pad2)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(J2-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 5A3A3306)
    (at 145.175 110.575 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at 0 1.45 270) (layer B.SilkS) hide)
    (fp_text value 1K (at 0 -1.5 270) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(J1-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(J2-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 5A393602)
    (at 140.28 101.79 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at 0 1.45 270) (layer B.SilkS) hide)
    (fp_text value 100K (at 0 -1.5 270) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 9 /RSSI_A))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 5A3935E4)
    (at 142.07 101.79 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at 0 1.45 270) (layer B.SilkS) hide)
    (fp_text value 100K (at 0 -1.5 270) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 17 /RSSI_B))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 5A3930FB)
    (at 138.63 98.8 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R6 (at 0 1.45 180) (layer B.SilkS) hide)
    (fp_text value 1K (at 0 -1.5 180) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 21 /SCK))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 5A3930ED)
    (at 141.93 98.8)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R7 (at 0 1.45) (layer B.SilkS) hide)
    (fp_text value 1K (at 0 -1.5) (layer B.Fab) hide)
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 20 /MISO))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(D2-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 5A3A38C8)
    (at 132.1 95.55 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R8 (at 0 1.45 180) (layer B.SilkS) hide)
    (fp_text value 30 (at 0 -1.5 180) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 10 /AUD_IN))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 15 /AUD_OUT))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 5A3A3ED7)
    (at 138.53 101.78 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R9 (at 0 1.45 90) (layer B.SilkS) hide)
    (fp_text value 10K (at 0 -1.5 90) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 23 /RST))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 2 /PROG_PWR))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23-6 (layer F.Cu) (tedit 5A392FC3)
    (at 135.64 104.61 270)
    (descr "6-pin SOT-23 package")
    (tags SOT-23-6)
    (attr smd)
    (fp_text reference U1 (at 0 -2.9 270) (layer F.SilkS) hide)
    (fp_text value MAX4624 (at 0 2.9 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 360) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 22 /MOSI))
    (pad 2 smd rect (at -1.1 0 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 /PROG_PWR))
    (pad 3 smd rect (at -1.1 0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 1.1 0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 16 /VideoA))
    (pad 6 smd rect (at 1.1 -0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 19 /VideoB))
    (pad 5 smd rect (at 1.1 0 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 11 /VideoOut))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiCadCustomLibs:Button_TS-018 (layer B.Cu) (tedit 5A3931E7)
    (at 139.775 92.8 180)
    (fp_text reference SW1 (at 0 -1.6 180) (layer B.SilkS))
    (fp_text value SW_Push (at 0 1.75 180) (layer B.Fab))
    (pad "" np_thru_hole circle (at -0.85 0 180) (size 0.7 0.7) (drill 0.7) (layers *.Cu *.Mask))
    (pad 2 smd rect (at 1.675 -1.55 180) (size 1.15 1.3) (layers B.Cu B.Paste B.Mask)
      (net 23 /RST))
    (pad 1 smd rect (at -1.675 -1.55 180) (size 1.15 1.3) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad "" smd rect (at -2.3 0 180) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask))
    (pad "" smd rect (at 2.3 0 180) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask))
    (pad "" np_thru_hole circle (at 0.85 0 180) (size 0.7 0.7) (drill 0.7) (layers *.Cu *.Mask))
  )
  (module KiCadCustomLibs:Pads_9pin_chess (layer F.Cu) (tedit 5A3A8529)
    (at 147.125 99.725 270)
    (fp_text reference J3 (at 0.5 4.25 270) (layer F.SilkS) hide)
    (fp_text value RX_B (at 0.25 -2.25 270) (layer F.Fab))
    (pad 8 smd oval (at 2.25 2 270) (size 1 1.8) (layers F.Cu F.Paste F.Mask)
      (net 19 /VideoB))
    (pad 6 smd oval (at 0.75 2 270) (size 1 1.8) (layers F.Cu F.Paste F.Mask)
      (net 17 /RSSI_B))
    (pad 2 smd oval (at -2.25 2 270) (size 1 1.8) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(J2-Pad2)"))
    (pad 4 smd oval (at -0.75 2 270) (size 1 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 9 smd oval (at 3 0 270) (size 1 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd oval (at -3 0 270) (size 1 1.8) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(J2-Pad1)"))
    (pad 3 smd oval (at -1.5 0 270) (size 1 1.8) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(J2-Pad3)"))
    (pad 7 smd oval (at 1.5 0 270) (size 1 1.8) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(J3-Pad7)") (solder_mask_margin -1))
    (pad 5 smd oval (at 0 0 270) (size 1 1.8) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
  )
  (module KiCadCustomLibs:Pads_9pin_chess (layer F.Cu) (tedit 5A392FC7)
    (at 130.325 99.7 90)
    (fp_text reference J2 (at 0.5 4.25 90) (layer F.SilkS) hide)
    (fp_text value RX_A (at 0.25 -2.25 90) (layer F.Fab))
    (pad 8 smd oval (at 2.25 2 90) (size 1 1.8) (layers F.Cu F.Paste F.Mask)
      (net 16 /VideoA))
    (pad 6 smd oval (at 0.75 2 90) (size 1 1.8) (layers F.Cu F.Paste F.Mask)
      (net 9 /RSSI_A))
    (pad 2 smd oval (at -2.25 2 90) (size 1 1.8) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(J2-Pad2)"))
    (pad 4 smd oval (at -0.75 2 90) (size 1 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 9 smd oval (at 3 0 90) (size 1 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd oval (at -3 0 90) (size 1 1.8) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(J2-Pad1)"))
    (pad 3 smd oval (at -1.5 0 90) (size 1 1.8) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(J2-Pad3)"))
    (pad 7 smd oval (at 1.5 0 90) (size 1 1.8) (layers F.Cu F.Paste F.Mask)
      (net 15 /AUD_OUT))
    (pad 5 smd oval (at 0 0 90) (size 1 1.8) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
  )
  (module Housings_SOIC:SOIJ-8_5.3x5.3mm_Pitch1.27mm (layer F.Cu) (tedit 5A3A55F6)
    (at 140.31 100.18 90)
    (descr "8-Lead Plastic Small Outline (SM) - Medium, 5.28 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U2 (at 0 -3.68 90) (layer F.SilkS) hide)
    (fp_text value ATTINY85-20SU (at 0 3.68 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -3.65 -1.905 90) (size 1.7 0.65) (layers F.Cu F.Paste F.Mask)
      (net 23 /RST))
    (pad 2 smd rect (at -3.65 -0.635 90) (size 1.7 0.65) (layers F.Cu F.Paste F.Mask)
      (net 9 /RSSI_A))
    (pad 3 smd rect (at -3.65 0.635 90) (size 1.7 0.65) (layers F.Cu F.Paste F.Mask)
      (net 17 /RSSI_B))
    (pad 4 smd rect (at -3.65 1.905 90) (size 1.7 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 3.65 1.905 90) (size 1.7 0.65) (layers F.Cu F.Paste F.Mask)
      (net 22 /MOSI))
    (pad 6 smd rect (at 3.65 0.635 90) (size 1.7 0.65) (layers F.Cu F.Paste F.Mask)
      (net 20 /MISO))
    (pad 7 smd rect (at 3.65 -0.635 90) (size 1.7 0.65) (layers F.Cu F.Paste F.Mask)
      (net 21 /SCK))
    (pad 8 smd rect (at 3.65 -1.905 90) (size 1.7 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 /PROG_PWR))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIJ-8_5.3x5.3mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer B.Cu) (tedit 5A3A5749)
    (at 147.03 92.85)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D2 (at 0 1.45) (layer B.SilkS) hide)
    (fp_text value LED (at 0 -1.55) (layer B.Fab) hide)
    (fp_text user %R (at 0 1.25) (layer B.Fab) hide)
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 1.2) (layers B.Cu B.Paste B.Mask)
      (net 3 VCC))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 1.2) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(D2-Pad1)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer B.Cu) (tedit 5A3A72BA)
    (at 132.56 92.85 180)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D1 (at 0 1.45 180) (layer B.SilkS) hide)
    (fp_text value LED (at 0 -1.55 180) (layer B.Fab) hide)
    (fp_text user %R (at 0 1.25 180) (layer B.Fab) hide)
    (pad 2 smd rect (at 1.1 0) (size 1.2 1.2) (layers B.Cu B.Paste B.Mask)
      (net 3 VCC))
    (pad 1 smd rect (at -1.1 0) (size 1.2 1.2) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Diodes_SMD:D_SOD-323 (layer F.Cu) (tedit 5AB21793)
    (at 148.93 94.93)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D3 (at 1.07 -1.43) (layer F.SilkS) hide)
    (fp_text value D_Schottky (at 0.1 1.9) (layer F.Fab) hide)
    (fp_text user %R (at 3.14 -0.26) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.05 0) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 2 /PROG_PWR))
    (pad 2 smd rect (at 1.05 0) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text tVRX (at 142.63 106.65) (layer F.SilkS))
  (gr_text 1K (at 141.8 97.55) (layer B.SilkS))
  (gr_text 1K (at 138.6 97.55) (layer B.SilkS))
  (gr_text 100K (at 142.3 104.55 90) (layer B.SilkS))
  (gr_text 100K (at 140.2 104.55 90) (layer B.SilkS))
  (gr_text 10K (at 136.7 102.05) (layer B.SilkS))
  (gr_text 30 (at 134.16 95.51) (layer B.SilkS))
  (gr_text 1Kx3 (at 147.7 110.25) (layer B.SilkS))
  (gr_line (start 132.8 111.05) (end 134.3 111.05) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 132.8 111.75) (end 132.8 111.05) (angle 90) (layer Edge.Cuts) (width 0.15))
  (dimension 22 (width 0.3) (layer Dwgs.User)
    (gr_text "22,000 mm" (at 139.8 87.2) (layer Dwgs.User))
    (feature1 (pts (xy 150.8 92.05) (xy 150.8 85.85)))
    (feature2 (pts (xy 128.8 92.05) (xy 128.8 85.85)))
    (crossbar (pts (xy 128.8 88.55) (xy 150.8 88.55)))
    (arrow1a (pts (xy 150.8 88.55) (xy 149.673496 89.136421)))
    (arrow1b (pts (xy 150.8 88.55) (xy 149.673496 87.963579)))
    (arrow2a (pts (xy 128.8 88.55) (xy 129.926504 89.136421)))
    (arrow2b (pts (xy 128.8 88.55) (xy 129.926504 87.963579)))
  )
  (gr_line (start 128.8 107.75) (end 128.8 92.05) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 132.8 107.75) (end 132.8 111.75) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 146.8 111.75) (end 139.9 111.75) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 150.8 107.75) (end 150.8 100.55) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 146.8 107.75) (end 150.8 107.75) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 139.9 111.05) (end 137.3 111.05) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 139.9 111.75) (end 139.9 111.05) (angle 90) (layer Edge.Cuts) (width 0.15))
  (dimension 15.6 (width 0.3) (layer Dwgs.User)
    (gr_text "15,600 mm" (at 139.8 118.9) (layer Dwgs.User))
    (feature1 (pts (xy 147.6 106.05) (xy 147.6 120.25)))
    (feature2 (pts (xy 132 106.05) (xy 132 120.25)))
    (crossbar (pts (xy 132 117.55) (xy 147.6 117.55)))
    (arrow1a (pts (xy 147.6 117.55) (xy 146.473496 118.136421)))
    (arrow1b (pts (xy 147.6 117.55) (xy 146.473496 116.963579)))
    (arrow2a (pts (xy 132 117.55) (xy 133.126504 118.136421)))
    (arrow2b (pts (xy 132 117.55) (xy 133.126504 116.963579)))
  )
  (gr_text A (at 148.67 101.29 90) (layer F.SilkS))
  (gr_text 2 (at 133.79 101.95 270) (layer F.SilkS))
  (gr_text 1 (at 130.31 103.65 270) (layer F.SilkS))
  (gr_text G (at 133.77 100.44 270) (layer F.SilkS))
  (gr_text R (at 133.78 99 270) (layer F.SilkS))
  (gr_text V (at 133.79 97.34 270) (layer F.SilkS))
  (gr_text G (at 130.32 95.7 270) (layer F.SilkS))
  (gr_text 2 (at 143.72 97.48 90) (layer F.SilkS))
  (gr_text G (at 143.71 98.95 90) (layer F.SilkS))
  (gr_text R (at 143.67 100.47 90) (layer F.SilkS))
  (gr_text V (at 143.66 101.94 90) (layer F.SilkS))
  (gr_text G (at 148.67 102.83 90) (layer F.SilkS))
  (gr_text + (at 148.62 99.7 90) (layer F.SilkS))
  (gr_text 3 (at 148.59 98.21 90) (layer F.SilkS))
  (gr_text 1 (at 148.6 96.76 90) (layer F.SilkS))
  (gr_text G (at 134.79 107.73) (layer B.SilkS))
  (gr_text V (at 136.06 107.71) (layer B.SilkS))
  (gr_text A (at 137.31 107.71) (layer B.SilkS))
  (gr_text R (at 138.55 107.71) (layer B.SilkS))
  (gr_text + (at 139.88 107.72) (layer B.SilkS))
  (gr_text G (at 141.07 107.7) (layer B.SilkS))
  (gr_text 3 (at 142.31 107.7) (layer B.SilkS))
  (gr_text 2 (at 143.57 107.71) (layer B.SilkS))
  (gr_text 1 (at 144.83 107.71) (layer B.SilkS))
  (gr_text GND (at 142.32 92.64) (layer F.SilkS))
  (gr_text 5V (at 143.52 95.78) (layer F.SilkS))
  (gr_text RST (at 137.03 95.83) (layer F.SilkS))
  (dimension 20 (width 0.3) (layer Dwgs.User)
    (gr_text "20,000 mm" (at 122.95 102.05 270) (layer Dwgs.User))
    (feature1 (pts (xy 128.8 112.05) (xy 121.6 112.05)))
    (feature2 (pts (xy 128.8 92.05) (xy 121.6 92.05)))
    (crossbar (pts (xy 124.3 92.05) (xy 124.3 112.05)))
    (arrow1a (pts (xy 124.3 112.05) (xy 123.713579 110.923496)))
    (arrow1b (pts (xy 124.3 112.05) (xy 124.886421 110.923496)))
    (arrow2a (pts (xy 124.3 92.05) (xy 123.713579 93.176504)))
    (arrow2b (pts (xy 124.3 92.05) (xy 124.886421 93.176504)))
  )
  (gr_text B (at 145.66 94.44) (layer F.SilkS))
  (gr_text A (at 133.98 94.57) (layer F.SilkS))
  (gr_line (start 150.8 97.55) (end 150.8 92.05) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 149.3 97.55) (end 150.8 97.55) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 149.3 100.55) (end 149.3 97.55) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 150.8 100.55) (end 149.3 100.55) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 134.3 111.05) (end 137.3 111.05) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 128.8 92.05) (end 150.8 92.05) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.25)
    (fill yes (arc_segments 16) (thermal_gap 0.2) (thermal_bridge_width 1))
    (polygon
      (pts
        (xy 128.525 91.825) (xy 150.975 91.8) (xy 151.05 112.525) (xy 128.325 112.875)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.25)
    (fill yes (arc_segments 16) (thermal_gap 0.2) (thermal_bridge_width 1))
    (polygon
      (pts
        (xy 151.025 91.7) (xy 128.2 91.725) (xy 128.225 112.675) (xy 151.425 112.3)
      )
    )
  )
)
