(kicad_pcb (version 20171130) (host pcbnew 5.1.5)
  (general
    (thickness 1.6)
    (drawings 24)
    (tracks 248)
    (zones 0)
    (modules 64)
    (nets 9)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.2)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.254)
    (via_min_size 0.4)
    (via_min_drill 0.254)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.0508)
    (solder_mask_min_width 0.127)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010f0_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerbers"))
  )
  (net 0 "")
  (net 1 /A0B0)
  (net 2 /A1B1)
  (net 3 /A2B2)
  (net 4 /A3B3)
  (net 5 /A4B4)
  (net 6 /A5B5)
  (net 7 /A6B6)
  (net 8 /A7B7)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.2)
    (via_dia 0.8)
    (via_drill 0.254)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (diff_pair_width 0.25)
    (diff_pair_gap 0.25)
    (add_net /A0B0)
    (add_net /A1B1)
    (add_net /A2B2)
    (add_net /A3B3)
    (add_net /A4B4)
    (add_net /A5B5)
    (add_net /A6B6)
    (add_net /A7B7)
  )
  (module hc245t-bypass:PAD (layer F.Cu) (tedit 5ECF580E)
    (at 20.73 20.8 180)
    (fp_text reference TP12 (at 0 4.445) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 3.175) (layer F.Fab) hide)
    (pad 1 thru_hole oval (at 0 0 180) (size 0.4 1) (drill 0.254 (offset 0 0.254)) (layers *.Cu *.Mask)
      (net 6 /A5B5))
  )
  (module hc245t-bypass:PAD (layer F.Cu) (tedit 5ECF580E)
    (at 20.08 20.8 180)
    (fp_text reference TP14 (at 0 4.445) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 3.175) (layer F.Fab) hide)
    (pad 1 thru_hole oval (at 0 0 180) (size 0.4 1) (drill 0.254 (offset 0 0.254)) (layers *.Cu *.Mask)
      (net 7 /A6B6))
  )
  (module hc245t-bypass:PAD (layer F.Cu) (tedit 5ECF580E)
    (at 20.73 25.2)
    (fp_text reference TP9 (at 0 4.445) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 3.175) (layer F.Fab) hide)
    (pad 1 thru_hole oval (at 0 0) (size 0.4 1) (drill 0.254 (offset 0 0.254)) (layers *.Cu *.Mask)
      (net 5 /A4B4))
  )
  (module hc245t-bypass:PAD (layer F.Cu) (tedit 5ECF580E)
    (at 23.33 25.2)
    (fp_text reference TP1 (at 0 4.445) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 3.175) (layer F.Fab) hide)
    (pad 1 thru_hole oval (at 0 0) (size 0.4 1) (drill 0.254 (offset 0 0.254)) (layers *.Cu *.Mask)
      (net 1 /A0B0))
  )
  (module hc245t-bypass:PAD (layer F.Cu) (tedit 5ECF580E)
    (at 23.98 20.8 180)
    (fp_text reference TP2 (at 0 4.445) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 3.175) (layer F.Fab) hide)
    (pad 1 thru_hole oval (at 0 0 180) (size 0.4 1) (drill 0.254 (offset 0 0.254)) (layers *.Cu *.Mask)
      (net 1 /A0B0))
  )
  (module hc245t-bypass:PAD (layer F.Cu) (tedit 5ECF580E)
    (at 22.68 25.2)
    (fp_text reference TP3 (at 0 4.445) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 3.175) (layer F.Fab) hide)
    (pad 1 thru_hole oval (at 0 0) (size 0.4 1) (drill 0.254 (offset 0 0.254)) (layers *.Cu *.Mask)
      (net 2 /A1B1))
  )
  (module hc245t-bypass:PAD (layer F.Cu) (tedit 5ECF580E)
    (at 22.68 20.8 180)
    (fp_text reference TP6 (at 0 4.445) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 3.175) (layer F.Fab) hide)
    (pad 1 thru_hole oval (at 0 0 180) (size 0.4 1) (drill 0.254 (offset 0 0.254)) (layers *.Cu *.Mask)
      (net 3 /A2B2))
  )
  (module hc245t-bypass:PAD (layer F.Cu) (tedit 5ECF580E)
    (at 19.43 20.8 180)
    (fp_text reference TP16 (at 0 4.445) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 3.175) (layer F.Fab) hide)
    (pad 1 thru_hole oval (at 0 0 180) (size 0.4 1) (drill 0.254 (offset 0 0.254)) (layers *.Cu *.Mask)
      (net 8 /A7B7))
  )
  (module hc245t-bypass:PAD (layer F.Cu) (tedit 5ECF580E)
    (at 18.78 25.2)
    (fp_text reference TP15 (at 0 4.445) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 3.175) (layer F.Fab) hide)
    (pad 1 thru_hole oval (at 0 0) (size 0.4 1) (drill 0.254 (offset 0 0.254)) (layers *.Cu *.Mask)
      (net 8 /A7B7))
  )
  (module hc245t-bypass:PAD (layer F.Cu) (tedit 5ECF580E)
    (at 21.38 25.2)
    (fp_text reference TP7 (at 0 4.445) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 3.175) (layer F.Fab) hide)
    (pad 1 thru_hole oval (at 0 0) (size 0.4 1) (drill 0.254 (offset 0 0.254)) (layers *.Cu *.Mask)
      (net 4 /A3B3))
  )
  (module hc245t-bypass:PAD (layer F.Cu) (tedit 5ECF580E)
    (at 23.33 20.8 180)
    (fp_text reference TP4 (at 0 4.445) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 3.175) (layer F.Fab) hide)
    (pad 1 thru_hole oval (at 0 0 180) (size 0.4 1) (drill 0.254 (offset 0 0.254)) (layers *.Cu *.Mask)
      (net 2 /A1B1))
  )
  (module hc245t-bypass:PAD (layer F.Cu) (tedit 5ECF580E)
    (at 21.38 20.8 180)
    (fp_text reference TP10 (at 0 4.445) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 3.175) (layer F.Fab) hide)
    (pad 1 thru_hole oval (at 0 0 180) (size 0.4 1) (drill 0.254 (offset 0 0.254)) (layers *.Cu *.Mask)
      (net 5 /A4B4))
  )
  (module hc245t-bypass:PAD (layer F.Cu) (tedit 5ECF580E)
    (at 22.03 20.8 180)
    (fp_text reference TP8 (at 0 4.445) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 3.175) (layer F.Fab) hide)
    (pad 1 thru_hole oval (at 0 0 180) (size 0.4 1) (drill 0.254 (offset 0 0.254)) (layers *.Cu *.Mask)
      (net 4 /A3B3))
  )
  (module hc245t-bypass:PAD (layer F.Cu) (tedit 5ECF580E)
    (at 19.43 25.2)
    (fp_text reference TP13 (at 0 4.445) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 3.175) (layer F.Fab) hide)
    (pad 1 thru_hole oval (at 0 0) (size 0.4 1) (drill 0.254 (offset 0 0.254)) (layers *.Cu *.Mask)
      (net 7 /A6B6))
  )
  (module hc245t-bypass:PAD (layer F.Cu) (tedit 5ECF580E)
    (at 22.03 25.2)
    (fp_text reference TP5 (at 0 4.445) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 3.175) (layer F.Fab) hide)
    (pad 1 thru_hole oval (at 0 0) (size 0.4 1) (drill 0.254 (offset 0 0.254)) (layers *.Cu *.Mask)
      (net 3 /A2B2))
  )
  (module hc245t-bypass:PAD (layer F.Cu) (tedit 5ECF580E)
    (at 20.08 25.2)
    (fp_text reference TP11 (at 0 4.445) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 3.175) (layer F.Fab) hide)
    (pad 1 thru_hole oval (at 0 0) (size 0.4 1) (drill 0.254 (offset 0 0.254)) (layers *.Cu *.Mask)
      (net 6 /A5B5))
  )
  (module hc245t-bypass:PAD (layer F.Cu) (tedit 5ECF580E)
    (at 21.38 32.2)
    (fp_text reference TP7 (at 0 4.445) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 3.175) (layer F.Fab) hide)
    (pad 1 thru_hole oval (at 0 0) (size 0.4 1) (drill 0.254 (offset 0 0.254)) (layers *.Cu *.Mask)
      (net 4 /A3B3))
  )
  (module hc245t-bypass:PAD (layer F.Cu) (tedit 5ECF580E)
    (at 23.33 32.2)
    (fp_text reference TP1 (at 0 4.445) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 3.175) (layer F.Fab) hide)
    (pad 1 thru_hole oval (at 0 0) (size 0.4 1) (drill 0.254 (offset 0 0.254)) (layers *.Cu *.Mask)
      (net 1 /A0B0))
  )
  (module hc245t-bypass:PAD (layer F.Cu) (tedit 5ECF580E)
    (at 19.43 32.2)
    (fp_text reference TP13 (at 0 4.445) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 3.175) (layer F.Fab) hide)
    (pad 1 thru_hole oval (at 0 0) (size 0.4 1) (drill 0.254 (offset 0 0.254)) (layers *.Cu *.Mask)
      (net 7 /A6B6))
  )
  (module hc245t-bypass:PAD (layer F.Cu) (tedit 5ECF580E)
    (at 20.08 32.2)
    (fp_text reference TP11 (at 0 4.445) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 3.175) (layer F.Fab) hide)
    (pad 1 thru_hole oval (at 0 0) (size 0.4 1) (drill 0.254 (offset 0 0.254)) (layers *.Cu *.Mask)
      (net 6 /A5B5))
  )
  (module hc245t-bypass:PAD (layer F.Cu) (tedit 5ECF580E)
    (at 23.98 27.8 180)
    (fp_text reference TP2 (at 0 4.445) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 3.175) (layer F.Fab) hide)
    (pad 1 thru_hole oval (at 0 0 180) (size 0.4 1) (drill 0.254 (offset 0 0.254)) (layers *.Cu *.Mask)
      (net 1 /A0B0))
  )
  (module hc245t-bypass:PAD (layer F.Cu) (tedit 5ECF580E)
    (at 22.68 32.2)
    (fp_text reference TP3 (at 0 4.445) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 3.175) (layer F.Fab) hide)
    (pad 1 thru_hole oval (at 0 0) (size 0.4 1) (drill 0.254 (offset 0 0.254)) (layers *.Cu *.Mask)
      (net 2 /A1B1))
  )
  (module hc245t-bypass:PAD (layer F.Cu) (tedit 5ECF580E)
    (at 20.73 32.2)
    (fp_text reference TP9 (at 0 4.445) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 3.175) (layer F.Fab) hide)
    (pad 1 thru_hole oval (at 0 0) (size 0.4 1) (drill 0.254 (offset 0 0.254)) (layers *.Cu *.Mask)
      (net 5 /A4B4))
  )
  (module hc245t-bypass:PAD (layer F.Cu) (tedit 5ECF580E)
    (at 20.08 27.8 180)
    (fp_text reference TP14 (at 0 4.445) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 3.175) (layer F.Fab) hide)
    (pad 1 thru_hole oval (at 0 0 180) (size 0.4 1) (drill 0.254 (offset 0 0.254)) (layers *.Cu *.Mask)
      (net 7 /A6B6))
  )
  (module hc245t-bypass:PAD (layer F.Cu) (tedit 5ECF580E)
    (at 23.33 27.8 180)
    (fp_text reference TP4 (at 0 4.445) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 3.175) (layer F.Fab) hide)
    (pad 1 thru_hole oval (at 0 0 180) (size 0.4 1) (drill 0.254 (offset 0 0.254)) (layers *.Cu *.Mask)
      (net 2 /A1B1))
  )
  (module hc245t-bypass:PAD (layer F.Cu) (tedit 5ECF580E)
    (at 18.78 32.2)
    (fp_text reference TP15 (at 0 4.445) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 3.175) (layer F.Fab) hide)
    (pad 1 thru_hole oval (at 0 0) (size 0.4 1) (drill 0.254 (offset 0 0.254)) (layers *.Cu *.Mask)
      (net 8 /A7B7))
  )
  (module hc245t-bypass:PAD (layer F.Cu) (tedit 5ECF580E)
    (at 20.73 27.8 180)
    (fp_text reference TP12 (at 0 4.445) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 3.175) (layer F.Fab) hide)
    (pad 1 thru_hole oval (at 0 0 180) (size 0.4 1) (drill 0.254 (offset 0 0.254)) (layers *.Cu *.Mask)
      (net 6 /A5B5))
  )
  (module hc245t-bypass:PAD (layer F.Cu) (tedit 5ECF580E)
    (at 19.43 27.8 180)
    (fp_text reference TP16 (at 0 4.445) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 3.175) (layer F.Fab) hide)
    (pad 1 thru_hole oval (at 0 0 180) (size 0.4 1) (drill 0.254 (offset 0 0.254)) (layers *.Cu *.Mask)
      (net 8 /A7B7))
  )
  (module hc245t-bypass:PAD (layer F.Cu) (tedit 5ECF580E)
    (at 21.38 27.8 180)
    (fp_text reference TP10 (at 0 4.445) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 3.175) (layer F.Fab) hide)
    (pad 1 thru_hole oval (at 0 0 180) (size 0.4 1) (drill 0.254 (offset 0 0.254)) (layers *.Cu *.Mask)
      (net 5 /A4B4))
  )
  (module hc245t-bypass:PAD (layer F.Cu) (tedit 5ECF580E)
    (at 22.68 27.8 180)
    (fp_text reference TP6 (at 0 4.445) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 3.175) (layer F.Fab) hide)
    (pad 1 thru_hole oval (at 0 0 180) (size 0.4 1) (drill 0.254 (offset 0 0.254)) (layers *.Cu *.Mask)
      (net 3 /A2B2))
  )
  (module hc245t-bypass:PAD (layer F.Cu) (tedit 5ECF580E)
    (at 22.03 27.8 180)
    (fp_text reference TP8 (at 0 4.445) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 3.175) (layer F.Fab) hide)
    (pad 1 thru_hole oval (at 0 0 180) (size 0.4 1) (drill 0.254 (offset 0 0.254)) (layers *.Cu *.Mask)
      (net 4 /A3B3))
  )
  (module hc245t-bypass:PAD (layer F.Cu) (tedit 5ECF580E)
    (at 22.03 32.2)
    (fp_text reference TP5 (at 0 4.445) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 3.175) (layer F.Fab) hide)
    (pad 1 thru_hole oval (at 0 0) (size 0.4 1) (drill 0.254 (offset 0 0.254)) (layers *.Cu *.Mask)
      (net 3 /A2B2))
  )
  (module hc245t-bypass:PAD (layer F.Cu) (tedit 5ECF580E)
    (at 28.97 27.8 180)
    (fp_text reference TP5 (at 0 4.445) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 3.175) (layer F.Fab) hide)
    (pad 1 thru_hole oval (at 0 0 180) (size 0.4 1) (drill 0.254 (offset 0 0.254)) (layers *.Cu *.Mask)
      (net 3 /A2B2))
  )
  (module hc245t-bypass:PAD (layer F.Cu) (tedit 5ECF580E)
    (at 28.97 32.2)
    (fp_text reference TP8 (at 0 4.445) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 3.175) (layer F.Fab) hide)
    (pad 1 thru_hole oval (at 0 0) (size 0.4 1) (drill 0.254 (offset 0 0.254)) (layers *.Cu *.Mask)
      (net 4 /A3B3))
  )
  (module hc245t-bypass:PAD (layer F.Cu) (tedit 5ECF580E)
    (at 27.02 32.2)
    (fp_text reference TP2 (at 0 4.445) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 3.175) (layer F.Fab) hide)
    (pad 1 thru_hole oval (at 0 0) (size 0.4 1) (drill 0.254 (offset 0 0.254)) (layers *.Cu *.Mask)
      (net 1 /A0B0))
  )
  (module hc245t-bypass:PAD (layer F.Cu) (tedit 5ECF580E)
    (at 31.57 27.8 180)
    (fp_text reference TP13 (at 0 4.445) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 3.175) (layer F.Fab) hide)
    (pad 1 thru_hole oval (at 0 0 180) (size 0.4 1) (drill 0.254 (offset 0 0.254)) (layers *.Cu *.Mask)
      (net 7 /A6B6))
  )
  (module hc245t-bypass:PAD (layer F.Cu) (tedit 5ECF580E)
    (at 30.92 32.2)
    (fp_text reference TP14 (at 0 4.445) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 3.175) (layer F.Fab) hide)
    (pad 1 thru_hole oval (at 0 0) (size 0.4 1) (drill 0.254 (offset 0 0.254)) (layers *.Cu *.Mask)
      (net 7 /A6B6))
  )
  (module hc245t-bypass:PAD (layer F.Cu) (tedit 5ECF580E)
    (at 30.92 27.8 180)
    (fp_text reference TP11 (at 0 4.445) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 3.175) (layer F.Fab) hide)
    (pad 1 thru_hole oval (at 0 0 180) (size 0.4 1) (drill 0.254 (offset 0 0.254)) (layers *.Cu *.Mask)
      (net 6 /A5B5))
  )
  (module hc245t-bypass:PAD (layer F.Cu) (tedit 5ECF580E)
    (at 32.22 27.8 180)
    (fp_text reference TP15 (at 0 4.445) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 3.175) (layer F.Fab) hide)
    (pad 1 thru_hole oval (at 0 0 180) (size 0.4 1) (drill 0.254 (offset 0 0.254)) (layers *.Cu *.Mask)
      (net 8 /A7B7))
  )
  (module hc245t-bypass:PAD (layer F.Cu) (tedit 5ECF580E)
    (at 31.57 32.2)
    (fp_text reference TP16 (at 0 4.445) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 3.175) (layer F.Fab) hide)
    (pad 1 thru_hole oval (at 0 0) (size 0.4 1) (drill 0.254 (offset 0 0.254)) (layers *.Cu *.Mask)
      (net 8 /A7B7))
  )
  (module hc245t-bypass:PAD (layer F.Cu) (tedit 5ECF580E)
    (at 28.32 32.2)
    (fp_text reference TP6 (at 0 4.445) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 3.175) (layer F.Fab) hide)
    (pad 1 thru_hole oval (at 0 0) (size 0.4 1) (drill 0.254 (offset 0 0.254)) (layers *.Cu *.Mask)
      (net 3 /A2B2))
  )
  (module hc245t-bypass:PAD (layer F.Cu) (tedit 5ECF580E)
    (at 29.62 27.8 180)
    (fp_text reference TP7 (at 0 4.445) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 3.175) (layer F.Fab) hide)
    (pad 1 thru_hole oval (at 0 0 180) (size 0.4 1) (drill 0.254 (offset 0 0.254)) (layers *.Cu *.Mask)
      (net 4 /A3B3))
  )
  (module hc245t-bypass:PAD (layer F.Cu) (tedit 5ECF580E)
    (at 30.27 27.8 180)
    (fp_text reference TP9 (at 0 4.445) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 3.175) (layer F.Fab) hide)
    (pad 1 thru_hole oval (at 0 0 180) (size 0.4 1) (drill 0.254 (offset 0 0.254)) (layers *.Cu *.Mask)
      (net 5 /A4B4))
  )
  (module hc245t-bypass:PAD (layer F.Cu) (tedit 5ECF580E)
    (at 27.67 27.8 180)
    (fp_text reference TP1 (at 0 4.445) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 3.175) (layer F.Fab) hide)
    (pad 1 thru_hole oval (at 0 0 180) (size 0.4 1) (drill 0.254 (offset 0 0.254)) (layers *.Cu *.Mask)
      (net 1 /A0B0))
  )
  (module hc245t-bypass:PAD (layer F.Cu) (tedit 5ECF580E)
    (at 27.67 32.2)
    (fp_text reference TP4 (at 0 4.445) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 3.175) (layer F.Fab) hide)
    (pad 1 thru_hole oval (at 0 0) (size 0.4 1) (drill 0.254 (offset 0 0.254)) (layers *.Cu *.Mask)
      (net 2 /A1B1))
  )
  (module hc245t-bypass:PAD (layer F.Cu) (tedit 5ECF580E)
    (at 30.27 32.2)
    (fp_text reference TP12 (at 0 4.445) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 3.175) (layer F.Fab) hide)
    (pad 1 thru_hole oval (at 0 0) (size 0.4 1) (drill 0.254 (offset 0 0.254)) (layers *.Cu *.Mask)
      (net 6 /A5B5))
  )
  (module hc245t-bypass:PAD (layer F.Cu) (tedit 5ECF580E)
    (at 29.62 32.2)
    (fp_text reference TP10 (at 0 4.445) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 3.175) (layer F.Fab) hide)
    (pad 1 thru_hole oval (at 0 0) (size 0.4 1) (drill 0.254 (offset 0 0.254)) (layers *.Cu *.Mask)
      (net 5 /A4B4))
  )
  (module hc245t-bypass:PAD (layer F.Cu) (tedit 5ECF580E)
    (at 28.32 27.8 180)
    (fp_text reference TP3 (at 0 4.445) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 3.175) (layer F.Fab) hide)
    (pad 1 thru_hole oval (at 0 0 180) (size 0.4 1) (drill 0.254 (offset 0 0.254)) (layers *.Cu *.Mask)
      (net 2 /A1B1))
  )
  (module hc245t-bypass:PAD (layer F.Cu) (tedit 5ECF580E)
    (at 31.57 25.2)
    (fp_text reference TP16 (at 0 4.445) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 3.175) (layer F.Fab) hide)
    (pad 1 thru_hole oval (at 0 0) (size 0.4 1) (drill 0.254 (offset 0 0.254)) (layers *.Cu *.Mask)
      (net 8 /A7B7))
  )
  (module hc245t-bypass:PAD (layer F.Cu) (tedit 5ECF580E)
    (at 32.22 20.8 180)
    (fp_text reference TP15 (at 0 4.445) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 3.175) (layer F.Fab) hide)
    (pad 1 thru_hole oval (at 0 0 180) (size 0.4 1) (drill 0.254 (offset 0 0.254)) (layers *.Cu *.Mask)
      (net 8 /A7B7))
  )
  (module hc245t-bypass:PAD (layer F.Cu) (tedit 5ECF580E)
    (at 30.92 25.2)
    (fp_text reference TP14 (at 0 4.445) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 3.175) (layer F.Fab) hide)
    (pad 1 thru_hole oval (at 0 0) (size 0.4 1) (drill 0.254 (offset 0 0.254)) (layers *.Cu *.Mask)
      (net 7 /A6B6))
  )
  (module hc245t-bypass:PAD (layer F.Cu) (tedit 5ECF580E)
    (at 31.57 20.8 180)
    (fp_text reference TP13 (at 0 4.445) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 3.175) (layer F.Fab) hide)
    (pad 1 thru_hole oval (at 0 0 180) (size 0.4 1) (drill 0.254 (offset 0 0.254)) (layers *.Cu *.Mask)
      (net 7 /A6B6))
  )
  (module hc245t-bypass:PAD (layer F.Cu) (tedit 5ECF580E)
    (at 30.27 25.2)
    (fp_text reference TP12 (at 0 4.445) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 3.175) (layer F.Fab) hide)
    (pad 1 thru_hole oval (at 0 0) (size 0.4 1) (drill 0.254 (offset 0 0.254)) (layers *.Cu *.Mask)
      (net 6 /A5B5))
  )
  (module hc245t-bypass:PAD (layer F.Cu) (tedit 5ECF580E)
    (at 30.92 20.8 180)
    (fp_text reference TP11 (at 0 4.445) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 3.175) (layer F.Fab) hide)
    (pad 1 thru_hole oval (at 0 0 180) (size 0.4 1) (drill 0.254 (offset 0 0.254)) (layers *.Cu *.Mask)
      (net 6 /A5B5))
  )
  (module hc245t-bypass:PAD (layer F.Cu) (tedit 5ECF580E)
    (at 29.62 25.2)
    (fp_text reference TP10 (at 0 4.445) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 3.175) (layer F.Fab) hide)
    (pad 1 thru_hole oval (at 0 0) (size 0.4 1) (drill 0.254 (offset 0 0.254)) (layers *.Cu *.Mask)
      (net 5 /A4B4))
  )
  (module hc245t-bypass:PAD (layer F.Cu) (tedit 5ECF580E)
    (at 30.27 20.8 180)
    (fp_text reference TP9 (at 0 4.445) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 3.175) (layer F.Fab) hide)
    (pad 1 thru_hole oval (at 0 0 180) (size 0.4 1) (drill 0.254 (offset 0 0.254)) (layers *.Cu *.Mask)
      (net 5 /A4B4))
  )
  (module hc245t-bypass:PAD (layer F.Cu) (tedit 5ECF580E)
    (at 28.97 25.2)
    (fp_text reference TP8 (at 0 4.445) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 3.175) (layer F.Fab) hide)
    (pad 1 thru_hole oval (at 0 0) (size 0.4 1) (drill 0.254 (offset 0 0.254)) (layers *.Cu *.Mask)
      (net 4 /A3B3))
  )
  (module hc245t-bypass:PAD (layer F.Cu) (tedit 5ECF580E)
    (at 29.62 20.8 180)
    (fp_text reference TP7 (at 0 4.445) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 3.175) (layer F.Fab) hide)
    (pad 1 thru_hole oval (at 0 0 180) (size 0.4 1) (drill 0.254 (offset 0 0.254)) (layers *.Cu *.Mask)
      (net 4 /A3B3))
  )
  (module hc245t-bypass:PAD (layer F.Cu) (tedit 5ECF580E)
    (at 28.32 25.2)
    (fp_text reference TP6 (at 0 4.445) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 3.175) (layer F.Fab) hide)
    (pad 1 thru_hole oval (at 0 0) (size 0.4 1) (drill 0.254 (offset 0 0.254)) (layers *.Cu *.Mask)
      (net 3 /A2B2))
  )
  (module hc245t-bypass:PAD (layer F.Cu) (tedit 5ECF580E)
    (at 28.97 20.8 180)
    (fp_text reference TP5 (at 0 4.445) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 3.175) (layer F.Fab) hide)
    (pad 1 thru_hole oval (at 0 0 180) (size 0.4 1) (drill 0.254 (offset 0 0.254)) (layers *.Cu *.Mask)
      (net 3 /A2B2))
  )
  (module hc245t-bypass:PAD (layer F.Cu) (tedit 5ECF580E)
    (at 27.67 25.2)
    (fp_text reference TP4 (at 0 4.445) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 3.175) (layer F.Fab) hide)
    (pad 1 thru_hole oval (at 0 0) (size 0.4 1) (drill 0.254 (offset 0 0.254)) (layers *.Cu *.Mask)
      (net 2 /A1B1))
  )
  (module hc245t-bypass:PAD (layer F.Cu) (tedit 5ECF580E)
    (at 28.32 20.8 180)
    (fp_text reference TP3 (at 0 4.445) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 3.175) (layer F.Fab) hide)
    (pad 1 thru_hole oval (at 0 0 180) (size 0.4 1) (drill 0.254 (offset 0 0.254)) (layers *.Cu *.Mask)
      (net 2 /A1B1))
  )
  (module hc245t-bypass:PAD (layer F.Cu) (tedit 5ECF580E)
    (at 27.02 25.2)
    (fp_text reference TP2 (at 0 4.445) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 3.175) (layer F.Fab) hide)
    (pad 1 thru_hole oval (at 0 0) (size 0.4 1) (drill 0.254 (offset 0 0.254)) (layers *.Cu *.Mask)
      (net 1 /A0B0))
  )
  (module hc245t-bypass:PAD (layer F.Cu) (tedit 5ECF580E)
    (at 27.67 20.8 180)
    (fp_text reference TP1 (at 0 4.445) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 3.175) (layer F.Fab) hide)
    (pad 1 thru_hole oval (at 0 0 180) (size 0.4 1) (drill 0.254 (offset 0 0.254)) (layers *.Cu *.Mask)
      (net 1 /A0B0))
  )
  (gr_line (start 26 33) (end 25 33) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 26 26) (end 26 27) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 25 26) (end 25 27) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 25 20) (end 26 20) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 25 26) (end 18.4 26) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 18.4 20) (end 25 20) (layer Edge.Cuts) (width 0.05))
  (gr_text "HC245\nbypass" (at 21.5 23 180) (layer F.SilkS))
  (gr_line (start 18.4 26) (end 18.4 20) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 18.4 27) (end 25 27) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 25 33) (end 18.4 33) (layer Edge.Cuts) (width 0.05))
  (gr_text "HC245\nbypass" (at 21.5 30 180) (layer F.SilkS))
  (gr_line (start 18.4 33) (end 18.4 27) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 32.6 33) (end 26 33) (layer Edge.Cuts) (width 0.05))
  (gr_text "HC245\nbypass" (at 29.5 30) (layer F.SilkS))
  (gr_line (start 32.6 27) (end 32.6 33) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 26 27) (end 32.6 27) (layer Edge.Cuts) (width 0.05))
  (gr_text "HC245\nbypass" (at 29.5 23) (layer F.SilkS))
  (gr_line (start 32.6 26) (end 26 26) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 32.6 20) (end 32.6 26) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 26 20) (end 32.6 20) (layer Edge.Cuts) (width 0.05))
)
