<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="36" y2="0" width="0" layer="20"/>
<wire x1="36" y1="0" x2="36" y2="43" width="0" layer="20"/>
<wire x1="36" y1="43" x2="0" y2="43" width="0" layer="20"/>
<wire x1="0" y1="43" x2="0" y2="0" width="0" layer="20"/>
<text>VCC</text>
<text>VCC</text>
<text>G</text>
<text>G</text>
<text>SO</text>
<text>SI</text>
<text>PS</text>
<text>PS</text>
<text>CLK</text>
<text>CLK</text>
<text>OUT</text>
<text>IN</text>
<text>PD</text>
<text>VCC</text>
<text>VCC</text>
<text>1-16</text>
<text>17-32</text>
<text>v0.6</text>
<text>74HC165</text>
<text>74HC165</text>
<text>74HC165</text>
<text>74HC165</text>
<text>10K</text>
<text>10K</text>
<text>10K</text>
<text>10K</text>
</plain>
<libraries>
<library name="holes">
<description>&lt;b&gt;Mounting Holes and Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="2,8">
<description>&lt;b&gt;MOUNTING HOLE&lt;/b&gt; 2.8 mm with drill center</description>
</package>
</packages>
</library>
<library name="resistor-bourns">
<description>&lt;b&gt;Bourns Resistor Networks&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="4816P">
<description>&lt;b&gt;BOURNS RESISTOR NETWORK&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="con-molex">
<description>&lt;b&gt;Molex Connectors&lt;/b&gt; -  v1.03 (09/07/05)&lt;p&gt;

&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;br&gt;&lt;br&gt;
&lt;author&gt;additions and modifications by Bob Starr (rtzaudio@mindspring.com) &lt;/author&gt;</description>
<packages>
<package name="7395-05">
<description>&lt;b&gt;MOLEX 2.54mm KK RA CONNECTOR&lt;/b&gt;
&lt;br&gt;Fixed Orientation</description>
</package>
</packages>
</library>
<library name="74xx-eu">
<description>&lt;b&gt;TTL Devices, 74xx Series with European Symbols&lt;/b&gt;&lt;p&gt;
Based on the following sources:
&lt;ul&gt;
&lt;li&gt;Texas Instruments &lt;i&gt;TTL Data Book&lt;/i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;Volume 1, 1996.
&lt;li&gt;TTL Data Book, Volume 2 , 1993
&lt;li&gt;National Seminconductor Databook 1990, ALS/LS Logic
&lt;li&gt;ttl 74er digital data dictionary, ECA Electronic + Acustic GmbH, ISBN 3-88109-032-0
&lt;li&gt;http://icmaster.com/ViewCompare.asp
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SO16">
<description>&lt;b&gt;SMALL OUTLINE INTEGRATED CIRCUIT&lt;/b&gt;&lt;p&gt;
body 3.9 mm/JEDEC MS-012AC</description>
</package>
</packages>
</library>
<library name="rc-master">
<description>&lt;b&gt;R/C MASTER! - v1.19 (10/25/2011)&lt;/b&gt;&lt;p&gt;
&lt;p&gt;This library is a collection of SMD and through hole resistors and capacitors by various manufacturers. Some of these include types from Panasonic, Kemet, BC Components and others. Many of the packages were adapted from &lt;b&gt;rcl.lbr&lt;/b&gt; and &lt;b&gt;cap-pan40.lbr&lt;/b&gt; and have been renamed and grouped in a more logical form.&lt;/p&gt;&lt;p&gt;Silkscreen elements are a minimum of 8 mils in width with larger components using 10 mil widths. Most of the SMD components have text sizes of 0 .04" and thru-hole components are 0.05" in size.  A text ratio of 14 is used in both cases. Where practical, the elements are aligned on a 12.5 mil or 6.25 mil grid depending on the pad size and spacing.&lt;/p&gt;
&lt;p&gt;&lt;h4&gt;All capacitors are grouped by the following naming conventions:&lt;/h4&gt;&lt;/p&gt;
&lt;table width="380" border="1" bordercolor="#000000"&gt;
  &lt;tr&gt; 
    &lt;td width="81" bgcolor="#33CCFF"&gt;&lt;div align="center"&gt;&lt;strong&gt;Prefix&lt;/strong&gt;&lt;/div&gt;&lt;/td&gt;
    &lt;td width="289" bgcolor="#33CCFF"&gt;&lt;div align="center"&gt;&lt;strong&gt;Description&lt;/strong&gt;&lt;/div&gt;&lt;/td&gt;
  &lt;/tr&gt;
  &lt;tr&gt; 
    &lt;td&gt;&lt;div align="center"&gt;CBP_&lt;/div&gt;&lt;/td&gt;
    &lt;td&gt;&lt;div align="center"&gt;Bipolar Electrolytic Types&lt;/div&gt;&lt;/td&gt;
  &lt;/tr&gt;
  &lt;tr&gt; 
    &lt;td&gt;&lt;div align="center"&gt;CCA_&lt;/div&gt;&lt;/td&gt;
    &lt;td&gt;&lt;div align="center"&gt;Chip Cap Array Types&lt;/div&gt;&lt;/td&gt;
  &lt;/tr&gt;
  &lt;tr&gt; 
    &lt;td&gt;&lt;div align="center"&gt;CP_&lt;/div&gt;&lt;/td&gt;
    &lt;td&gt;&lt;div align="center"&gt;Polarized Electrolytic/Tantalum Types&lt;/div&gt;&lt;/td&gt;
  &lt;/tr&gt;
  &lt;tr&gt; 
    &lt;td&gt;&lt;div align="center"&gt;C_&lt;/div&gt;&lt;/td&gt;
    &lt;td&gt;&lt;div align="center"&gt;Non-Polarized Film / Chip Types&lt;/div&gt;&lt;/td&gt;
  &lt;/tr&gt;
  &lt;tr&gt; 
    &lt;td&gt;&lt;div align="center"&gt;FB_&lt;/div&gt;&lt;/td&gt;
    &lt;td&gt;&lt;div align="center"&gt;Simple Ferrite Bead Types&lt;/div&gt;&lt;/td&gt;
  &lt;/tr&gt;
  &lt;tr&gt; 
    &lt;td&gt;&lt;div align="center"&gt;L_&lt;/div&gt;&lt;/td&gt;
    &lt;td&gt;&lt;div align="center"&gt;Simple Chip Inductors&lt;/div&gt;&lt;/td&gt;
  &lt;/tr&gt;
  &lt;tr&gt; 
    &lt;td&gt;&lt;div align="center"&gt;R_&lt;/div&gt;&lt;/td&gt;
    &lt;td&gt;&lt;div align="center"&gt;Resistor Types&lt;/div&gt;&lt;/td&gt;
  &lt;/tr&gt;
&lt;/table&gt;
&lt;p&gt;
As a general guideline, SMD resistors are typically rated as follows:&lt;p&gt;
0402 = 1/16 watt&lt;br&gt;
0603 = 1/10 watt&lt;br&gt;
0805 = 1/8  watt&lt;br&gt;
1206 = 1/4  watt&lt;br&gt;
2010 = 1/2  watt&lt;br&gt;
2512 = 1    watt&lt;br&gt;&lt;p&gt;
&lt;author&gt;THIS LIBRARY IS PROVIDED AS IS AND WITHOUT WARRANTY OF ANY KIND, EXPRESSED OR IMPLIED.&lt;br&gt;Copyright (C) 2007-2008, Bob Starr&lt;br&gt; 
&lt;a href="http://www.bobstarr.net"&gt;http://www.bobstarr.net&lt;/a&gt;
&lt;/author&gt;</description>
<packages>
<package name="C0805MP">
<description>&lt;b&gt;SMD CHIP CAP&lt;/b&gt; - MicroPitch&lt;p&gt;
0805, grid 5 mil</description>
</package>
</packages>
</library>
<library name="jdc">
<packages>
<package name="2X09">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt; - 0.1"</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="HOLE1" library="holes" package="2,8" value="MOUNT-HOLE-2.8">
<attribute name="BOM" value="EXCLUDE"/>
</element>
<element name="HOLE2" library="holes" package="2,8" value="MOUNT-HOLE-2.8">
<attribute name="BOM" value="EXCLUDE"/>
</element>
<element name="HOLE3" library="holes" package="2,8" value="MOUNT-HOLE-2.8">
<attribute name="BOM" value="EXCLUDE"/>
</element>
<element name="HOLE4" library="holes" package="2,8" value="MOUNT-HOLE-2.8">
<attribute name="BOM" value="EXCLUDE"/>
</element>
<element name="JP1" library="jdc" package="2X09" value="">
<attribute name="VALUE"/>
</element>
<element name="JP2" library="jdc" package="2X09" value="">
<attribute name="VALUE"/>
</element>
<element name="R1" library="resistor-bourns" package="4816P" value="10K">
<attribute name="VALUE"/>
</element>
<element name="R2" library="resistor-bourns" package="4816P" value="10K">
<attribute name="VALUE"/>
</element>
<element name="R3" library="resistor-bourns" package="4816P" value="10K">
<attribute name="VALUE"/>
</element>
<element name="R4" library="resistor-bourns" package="4816P" value="10K">
<attribute name="VALUE"/>
</element>
<element name="J1" library="con-molex" package="7395-05" value="OUTPUT">
<attribute name="VALUE"/>
</element>
<element name="J2" library="con-molex" package="7395-05" value="INPUT">
<attribute name="VALUE"/>
</element>
<element name="U1" library="74xx-eu" package="SO16" value="74HC165D">
<attribute name="VALUE"/>
</element>
<element name="U2" library="74xx-eu" package="SO16" value="74HC165D">
<attribute name="VALUE"/>
</element>
<element name="C2" library="rc-master" package="C0805MP" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U4" library="74xx-eu" package="SO16" value="74HC165D">
<attribute name="VALUE"/>
</element>
<element name="U3" library="74xx-eu" package="SO16" value="74HC165D">
<attribute name="VALUE"/>
</element>
<element name="C4" library="rc-master" package="C0805MP" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="S2">
<contactref element="JP1" pad="2"/>
<contactref element="U1" pad="12"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="GND">
<contactref element="J1" pad="5"/>
<contactref element="J2" pad="5"/>
<contactref element="U1" pad="8"/>
<contactref element="U1" pad="15"/>
<contactref element="U2" pad="8"/>
<contactref element="C2" pad="1"/>
<contactref element="U2" pad="15"/>
<contactref element="U4" pad="8"/>
<contactref element="U3" pad="8"/>
<contactref element="C4" pad="1"/>
<contactref element="U3" pad="15"/>
<contactref element="R1" pad="9"/>
<contactref element="R1" pad="10"/>
<contactref element="R1" pad="11"/>
<contactref element="R1" pad="12"/>
<contactref element="R1" pad="13"/>
<contactref element="R1" pad="14"/>
<contactref element="R1" pad="15"/>
<contactref element="R1" pad="16"/>
<contactref element="R2" pad="9"/>
<contactref element="R2" pad="10"/>
<contactref element="R2" pad="11"/>
<contactref element="R2" pad="12"/>
<contactref element="R2" pad="13"/>
<contactref element="R2" pad="14"/>
<contactref element="R2" pad="15"/>
<contactref element="R2" pad="16"/>
<contactref element="R4" pad="9"/>
<contactref element="R4" pad="10"/>
<contactref element="R4" pad="11"/>
<contactref element="R4" pad="12"/>
<contactref element="R4" pad="13"/>
<contactref element="R4" pad="14"/>
<contactref element="R4" pad="15"/>
<contactref element="R4" pad="16"/>
<contactref element="R3" pad="13"/>
<contactref element="R3" pad="9"/>
<contactref element="R3" pad="10"/>
<contactref element="R3" pad="11"/>
<contactref element="R3" pad="12"/>
<contactref element="R3" pad="14"/>
<contactref element="R3" pad="15"/>
<contactref element="R3" pad="16"/>
<contactref element="U4" pad="15"/>
</signal>
<signal name="VCC">
<contactref element="J2" pad="1"/>
<contactref element="U1" pad="16"/>
<contactref element="C2" pad="2"/>
<contactref element="U2" pad="16"/>
<contactref element="C4" pad="2"/>
<contactref element="U3" pad="16"/>
<contactref element="U4" pad="16"/>
<contactref element="JP2" pad="18"/>
<contactref element="JP2" pad="17"/>
<contactref element="JP1" pad="18"/>
<contactref element="JP1" pad="17"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="S7">
<contactref element="JP1" pad="7"/>
<contactref element="U1" pad="5"/>
<contactref element="R1" pad="7"/>
</signal>
<signal name="S1">
<contactref element="JP1" pad="1"/>
<contactref element="U1" pad="11"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="S6">
<contactref element="JP1" pad="6"/>
<contactref element="U1" pad="4"/>
<contactref element="R1" pad="6"/>
</signal>
<signal name="S5">
<contactref element="JP1" pad="5"/>
<contactref element="U1" pad="3"/>
<contactref element="R1" pad="5"/>
</signal>
<signal name="S8">
<contactref element="JP1" pad="8"/>
<contactref element="U1" pad="6"/>
<contactref element="R1" pad="8"/>
</signal>
<signal name="LOAD">
<contactref element="J1" pad="3"/>
<contactref element="J2" pad="3"/>
<contactref element="U1" pad="1"/>
<contactref element="U2" pad="1"/>
<contactref element="U3" pad="1"/>
<contactref element="U4" pad="1"/>
</signal>
<signal name="S10">
<contactref element="JP1" pad="10"/>
<contactref element="U2" pad="12"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="S15">
<contactref element="JP1" pad="15"/>
<contactref element="U2" pad="5"/>
<contactref element="R2" pad="7"/>
</signal>
<signal name="S9">
<contactref element="JP1" pad="9"/>
<contactref element="U2" pad="11"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="S14">
<contactref element="JP1" pad="14"/>
<contactref element="U2" pad="4"/>
<contactref element="R2" pad="6"/>
</signal>
<signal name="S13">
<contactref element="JP1" pad="13"/>
<contactref element="U2" pad="3"/>
<contactref element="R2" pad="5"/>
</signal>
<signal name="S16">
<contactref element="JP1" pad="16"/>
<contactref element="U2" pad="6"/>
<contactref element="R2" pad="8"/>
</signal>
<signal name="S18">
<contactref element="JP2" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="U3" pad="12"/>
</signal>
<signal name="S23">
<contactref element="JP2" pad="7"/>
<contactref element="R3" pad="7"/>
<contactref element="U3" pad="5"/>
</signal>
<signal name="S17">
<contactref element="JP2" pad="1"/>
<contactref element="R3" pad="1"/>
<contactref element="U3" pad="11"/>
</signal>
<signal name="S22">
<contactref element="JP2" pad="6"/>
<contactref element="R3" pad="6"/>
<contactref element="U3" pad="4"/>
</signal>
<signal name="S21">
<contactref element="JP2" pad="5"/>
<contactref element="R3" pad="5"/>
<contactref element="U3" pad="3"/>
</signal>
<signal name="S24">
<contactref element="JP2" pad="8"/>
<contactref element="R3" pad="8"/>
<contactref element="U3" pad="6"/>
</signal>
<signal name="S26">
<contactref element="JP2" pad="10"/>
<contactref element="U4" pad="12"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="S31">
<contactref element="JP2" pad="15"/>
<contactref element="U4" pad="5"/>
<contactref element="R4" pad="7"/>
</signal>
<signal name="S25">
<contactref element="JP2" pad="9"/>
<contactref element="U4" pad="11"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="S30">
<contactref element="JP2" pad="14"/>
<contactref element="U4" pad="4"/>
<contactref element="R4" pad="6"/>
</signal>
<signal name="S29">
<contactref element="JP2" pad="13"/>
<contactref element="U4" pad="3"/>
<contactref element="R4" pad="5"/>
</signal>
<signal name="S32">
<contactref element="JP2" pad="16"/>
<contactref element="U4" pad="6"/>
<contactref element="R4" pad="8"/>
</signal>
<signal name="S4">
<contactref element="JP1" pad="4"/>
<contactref element="U1" pad="14"/>
<contactref element="R1" pad="4"/>
</signal>
<signal name="S3">
<contactref element="JP1" pad="3"/>
<contactref element="U1" pad="13"/>
<contactref element="R1" pad="3"/>
</signal>
<signal name="S12">
<contactref element="JP1" pad="12"/>
<contactref element="U2" pad="14"/>
<contactref element="R2" pad="4"/>
</signal>
<signal name="S11">
<contactref element="JP1" pad="11"/>
<contactref element="U2" pad="13"/>
<contactref element="R2" pad="3"/>
</signal>
<signal name="S20">
<contactref element="JP2" pad="4"/>
<contactref element="R3" pad="4"/>
<contactref element="U3" pad="14"/>
</signal>
<signal name="S19">
<contactref element="JP2" pad="3"/>
<contactref element="R3" pad="3"/>
<contactref element="U3" pad="13"/>
</signal>
<signal name="S28">
<contactref element="JP2" pad="12"/>
<contactref element="U4" pad="14"/>
<contactref element="R4" pad="4"/>
</signal>
<signal name="S27">
<contactref element="JP2" pad="11"/>
<contactref element="U4" pad="13"/>
<contactref element="R4" pad="3"/>
</signal>
<signal name="MISO_IN">
<contactref element="J2" pad="2"/>
<contactref element="U4" pad="10"/>
</signal>
<signal name="SCK">
<contactref element="U1" pad="2"/>
<contactref element="J1" pad="4"/>
<contactref element="J2" pad="4"/>
<contactref element="U2" pad="2"/>
<contactref element="U3" pad="2"/>
<contactref element="U4" pad="2"/>
</signal>
<signal name="MISO">
<contactref element="J1" pad="2"/>
<contactref element="U1" pad="9"/>
</signal>
<signal name="N$3">
<contactref element="U2" pad="10"/>
<contactref element="U3" pad="9"/>
</signal>
<signal name="N$1">
<contactref element="U2" pad="9"/>
<contactref element="U1" pad="10"/>
</signal>
<signal name="XX">
<contactref element="U4" pad="9"/>
<contactref element="U3" pad="10"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
