(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 153)
    (no_connects 0)
    (area 53.949999 53.949999 134.050001 114.050001)
    (thickness 1.6)
    (drawings 23)
    (tracks 599)
    (zones 0)
    (modules 78)
    (nets 55)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 0.6 0.6)
    (pad_drill 0.3)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFEF77F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 +3V3)
  (net 3 "Net-(C10-Pad1)")
  (net 4 "Net-(C11-Pad1)")
  (net 5 +24V)
  (net 6 "Net-(D2-Pad1)")
  (net 7 "Net-(D2-Pad2)")
  (net 8 "Net-(J1-Pad1)")
  (net 9 "Net-(J1-Pad2)")
  (net 10 "Net-(J1-Pad3)")
  (net 11 "Net-(J1-Pad4)")
  (net 12 "Net-(J1-Pad5)")
  (net 13 "Net-(J1-Pad6)")
  (net 14 "Net-(J1-Pad7)")
  (net 15 "Net-(J1-Pad8)")
  (net 16 /ETH0_TX+)
  (net 17 /ETH0_TX-)
  (net 18 /ETH0_RX+)
  (net 19 /ETH0_RX-)
  (net 20 /ETH_PWR+)
  (net 21 /ETH_PWR-)
  (net 22 "Net-(J8-Pad9)")
  (net 23 /ETH0_LED)
  (net 24 "Net-(J8-Pad11)")
  (net 25 /WLAN_LED)
  (net 26 /Omega_RX)
  (net 27 /Omega_TX)
  (net 28 "Net-(R7-Pad2)")
  (net 29 /USB+)
  (net 30 /USB-)
  (net 31 "Net-(C16-Pad1)")
  (net 32 /PPoE+)
  (net 33 /USBPWR)
  (net 34 +5V)
  (net 35 /LNA_EN_A)
  (net 36 "Net-(J3-Pad12)")
  (net 37 "Net-(J3-Pad7)")
  (net 38 "Net-(J3-Pad8)")
  (net 39 "Net-(J3-Pad9)")
  (net 40 "Net-(J3-Pad10)")
  (net 41 "Net-(J3-Pad11)")
  (net 42 "Net-(J3-Pad13)")
  (net 43 /SPI_CS1_RAK)
  (net 44 /SPI_MOSI)
  (net 45 /SPI_MISO)
  (net 46 /SPI_CLK)
  (net 47 /RAK_RESET)
  (net 48 /RADIO_EN_A)
  (net 49 /PA_G8)
  (net 50 /RADIO_EN_B)
  (net 51 /PA_G16)
  (net 52 /PA_EN_A)
  (net 53 /RADIO_RST)
  (net 54 /5VPWR)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /5VPWR)
    (add_net /ETH0_LED)
    (add_net /ETH0_RX+)
    (add_net /ETH0_RX-)
    (add_net /ETH0_TX+)
    (add_net /ETH0_TX-)
    (add_net /LNA_EN_A)
    (add_net /Omega_RX)
    (add_net /Omega_TX)
    (add_net /PA_EN_A)
    (add_net /PA_G16)
    (add_net /PA_G8)
    (add_net /RADIO_EN_A)
    (add_net /RADIO_EN_B)
    (add_net /RADIO_RST)
    (add_net /RAK_RESET)
    (add_net /SPI_CLK)
    (add_net /SPI_CS1_RAK)
    (add_net /SPI_MISO)
    (add_net /SPI_MOSI)
    (add_net /USB+)
    (add_net /USB-)
    (add_net /WLAN_LED)
    (add_net "Net-(C10-Pad1)")
    (add_net "Net-(C11-Pad1)")
    (add_net "Net-(C16-Pad1)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J1-Pad7)")
    (add_net "Net-(J1-Pad8)")
    (add_net "Net-(J3-Pad10)")
    (add_net "Net-(J3-Pad11)")
    (add_net "Net-(J3-Pad12)")
    (add_net "Net-(J3-Pad13)")
    (add_net "Net-(J3-Pad7)")
    (add_net "Net-(J3-Pad8)")
    (add_net "Net-(J3-Pad9)")
    (add_net "Net-(J8-Pad11)")
    (add_net "Net-(J8-Pad9)")
    (add_net "Net-(R7-Pad2)")
  )
  (net_class Power ""
    (clearance 0.2)
    (trace_width 1)
    (via_dia 1)
    (via_drill 0.6)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +24V)
    (add_net +3V3)
    (add_net +5V)
    (add_net /ETH_PWR+)
    (add_net /ETH_PWR-)
    (add_net /PPoE+)
    (add_net GND)
  )
  (net_class PowerSmall ""
    (clearance 0.1)
    (trace_width 0.4)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /USBPWR)
  )
  (module plan44:Stitching-VIA-0.6mm (layer F.Cu) (tedit 59FF1D37)
    (at 69.25 95)
    (fp_text reference VIA (at 0 1.905) (layer F.SilkS) hide)
    (fp_text value Stitching-VIA-0.6mm (at 0 -1.905) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module plan44:Stitching-VIA-0.6mm (layer F.Cu) (tedit 59FF1D37)
    (at 116.25 100.5)
    (fp_text reference VIA (at 0 1.905) (layer F.SilkS) hide)
    (fp_text value Stitching-VIA-0.6mm (at 0 -1.905) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module plan44:Stitching-VIA-0.6mm (layer F.Cu) (tedit 59FF1D37)
    (at 102.75 95.5)
    (fp_text reference VIA (at 0 1.905) (layer F.SilkS) hide)
    (fp_text value Stitching-VIA-0.6mm (at 0 -1.905) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module plan44:Stitching-VIA-0.6mm (layer F.Cu) (tedit 59FF1D37)
    (at 89.75 83.5)
    (fp_text reference VIA (at 0 1.905) (layer F.SilkS) hide)
    (fp_text value Stitching-VIA-0.6mm (at 0 -1.905) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module plan44:Stitching-VIA-0.6mm (layer F.Cu) (tedit 59FF1D37)
    (at 98.75 75.25)
    (fp_text reference VIA (at 0 1.905) (layer F.SilkS) hide)
    (fp_text value Stitching-VIA-0.6mm (at 0 -1.905) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module plan44:Stitching-VIA-0.6mm (layer F.Cu) (tedit 59FF1D37)
    (at 97.25 71)
    (fp_text reference VIA (at 0 1.905) (layer F.SilkS) hide)
    (fp_text value Stitching-VIA-0.6mm (at 0 -1.905) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module plan44:Stitching-VIA-0.6mm (layer F.Cu) (tedit 59FF1D37)
    (at 97.25 65.75)
    (fp_text reference VIA (at 0 1.905) (layer F.SilkS) hide)
    (fp_text value Stitching-VIA-0.6mm (at 0 -1.905) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module plan44:Stitching-VIA-0.6mm (layer F.Cu) (tedit 59FF1D37)
    (at 122.25 78.25)
    (fp_text reference VIA (at 0 1.905) (layer F.SilkS) hide)
    (fp_text value Stitching-VIA-0.6mm (at 0 -1.905) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module plan44:Stitching-VIA-0.6mm (layer F.Cu) (tedit 59FF1D37)
    (at 122 72)
    (fp_text reference VIA (at 0 1.905) (layer F.SilkS) hide)
    (fp_text value Stitching-VIA-0.6mm (at 0 -1.905) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module plan44:Stitching-VIA-0.6mm (layer F.Cu) (tedit 59FF1D37)
    (at 118 72)
    (fp_text reference VIA (at 0 1.905) (layer F.SilkS) hide)
    (fp_text value Stitching-VIA-0.6mm (at 0 -1.905) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module plan44:Stitching-VIA-0.6mm (layer F.Cu) (tedit 59FF1D37)
    (at 118 64.75)
    (fp_text reference VIA (at 0 1.905) (layer F.SilkS) hide)
    (fp_text value Stitching-VIA-0.6mm (at 0 -1.905) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module plan44:Stitching-VIA-0.6mm (layer F.Cu) (tedit 59FF1D37)
    (at 105 65.75)
    (fp_text reference VIA (at 0 1.905) (layer F.SilkS) hide)
    (fp_text value Stitching-VIA-0.6mm (at 0 -1.905) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module plan44:Stitching-VIA-0.6mm (layer F.Cu) (tedit 59FF1D37)
    (at 114.5 86.5)
    (fp_text reference VIA (at 0 1.905) (layer F.SilkS) hide)
    (fp_text value Stitching-VIA-0.6mm (at 0 -1.905) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module plan44:Stitching-VIA-0.6mm (layer F.Cu) (tedit 59FF1D37)
    (at 109.5 86.5)
    (fp_text reference VIA (at 0 1.905) (layer F.SilkS) hide)
    (fp_text value Stitching-VIA-0.6mm (at 0 -1.905) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module plan44:Stitching-VIA-0.6mm (layer F.Cu) (tedit 59FF1D37)
    (at 104.5 86.5)
    (fp_text reference VIA (at 0 1.905) (layer F.SilkS) hide)
    (fp_text value Stitching-VIA-0.6mm (at 0 -1.905) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module plan44:Stitching-VIA-0.6mm (layer F.Cu) (tedit 59FF1D37)
    (at 132 84)
    (fp_text reference VIA (at 0 1.905) (layer F.SilkS) hide)
    (fp_text value Stitching-VIA-0.6mm (at 0 -1.905) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module plan44:Stitching-VIA-0.6mm (layer F.Cu) (tedit 59FF1D37)
    (at 127 84)
    (fp_text reference VIA (at 0 1.905) (layer F.SilkS) hide)
    (fp_text value Stitching-VIA-0.6mm (at 0 -1.905) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module plan44:Stitching-VIA-0.6mm (layer F.Cu) (tedit 59FF1D37)
    (at 132 89)
    (fp_text reference VIA (at 0 1.905) (layer F.SilkS) hide)
    (fp_text value Stitching-VIA-0.6mm (at 0 -1.905) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module plan44:Stitching-VIA-0.6mm (layer F.Cu) (tedit 59FF1D37)
    (at 127 89)
    (fp_text reference VIA (at 0 1.905) (layer F.SilkS) hide)
    (fp_text value Stitching-VIA-0.6mm (at 0 -1.905) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module plan44:Stitching-VIA-0.6mm (layer F.Cu) (tedit 59FF1D37)
    (at 132 94)
    (fp_text reference VIA (at 0 1.905) (layer F.SilkS) hide)
    (fp_text value Stitching-VIA-0.6mm (at 0 -1.905) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module plan44:Stitching-VIA-0.6mm (layer F.Cu) (tedit 59FF1D37)
    (at 127 94)
    (fp_text reference VIA (at 0 1.905) (layer F.SilkS) hide)
    (fp_text value Stitching-VIA-0.6mm (at 0 -1.905) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module plan44:Stitching-VIA-0.6mm (layer F.Cu) (tedit 59FF1D37)
    (at 132 99)
    (fp_text reference VIA (at 0 1.905) (layer F.SilkS) hide)
    (fp_text value Stitching-VIA-0.6mm (at 0 -1.905) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module plan44:Stitching-VIA-0.6mm (layer F.Cu) (tedit 59FF1D37)
    (at 127 99)
    (fp_text reference VIA (at 0 1.905) (layer F.SilkS) hide)
    (fp_text value Stitching-VIA-0.6mm (at 0 -1.905) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module plan44:Stitching-VIA-0.6mm (layer F.Cu) (tedit 59FF1D37)
    (at 116.75 107.5)
    (fp_text reference VIA (at 0 1.905) (layer F.SilkS) hide)
    (fp_text value Stitching-VIA-0.6mm (at 0 -1.905) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module plan44:Stitching-VIA-0.6mm (layer F.Cu) (tedit 59FF1D37)
    (at 109.25 107.5)
    (fp_text reference VIA (at 0 1.905) (layer F.SilkS) hide)
    (fp_text value Stitching-VIA-0.6mm (at 0 -1.905) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module plan44:Stitching-VIA-0.6mm (layer F.Cu) (tedit 59FF1D37)
    (at 101.75 107.5)
    (fp_text reference VIA (at 0 1.905) (layer F.SilkS) hide)
    (fp_text value Stitching-VIA-0.6mm (at 0 -1.905) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module plan44:Stitching-VIA-0.6mm (layer F.Cu) (tedit 59FF1D37)
    (at 68.25 88.75)
    (fp_text reference VIA (at 0 1.905) (layer F.SilkS) hide)
    (fp_text value Stitching-VIA-0.6mm (at 0 -1.905) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer B.Cu) (tedit 58AA84D1)
    (at 61.976 71.12 90)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C3 (at 0 1.75 90) (layer B.SilkS))
    (fp_text value 100nF (at 0 -2 90) (layer B.Fab))
    (fp_text user %R (at 0 1.75 90) (layer B.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 34 +5V))
    (pad 2 smd rect (at 2 0 90) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer B.Cu) (tedit 59FF17F1)
    (at 91.44 91.948 270)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C4 (at 3.937 0 360) (layer B.SilkS))
    (fp_text value 100nF (at 0 -2 270) (layer B.Fab))
    (fp_text user %R (at 0 1.75 270) (layer B.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 54 /5VPWR))
    (pad 2 smd rect (at 2 0 270) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:CP_Radial_D7.5mm_P2.50mm (layer F.Cu) (tedit 59FF192A)
    (at 94.488 89.789 270)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=7.5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 7.5mm Electrolytic Capacitor")
    (fp_text reference C5 (at -2.159 3.302 360) (layer F.SilkS))
    (fp_text value "22uF 25V" (at 1.25 5.06 270) (layer F.Fab))
    (fp_text user %R (at 1.25 0 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 54 /5VPWR))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D7.5mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer B.Cu) (tedit 58AA84D1)
    (at 75.057 95.631 180)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C9 (at 0 1.75 180) (layer B.SilkS))
    (fp_text value 100nF (at 0 -2 180) (layer B.Fab))
    (fp_text user %R (at 0 1.75 180) (layer B.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 2 +3V3))
    (pad 2 smd rect (at 2 0 180) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer B.Cu) (tedit 59FF183D)
    (at 106.172 102.235 270)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C10 (at 4.191 0.508 360) (layer B.SilkS))
    (fp_text value 100nF (at 0 -2 270) (layer B.Fab))
    (fp_text user %R (at 0 1.75 270) (layer B.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(C10-Pad1)"))
    (pad 2 smd rect (at 2 0 270) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer B.Cu) (tedit 59FF1845)
    (at 108.839 102.235 270)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C11 (at 4.191 -0.381 360) (layer B.SilkS))
    (fp_text value 100nF (at 0 -2 270) (layer B.Fab))
    (fp_text user %R (at 0 1.75 270) (layer B.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(C11-Pad1)"))
    (pad 2 smd rect (at 2 0 270) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 59FF18EB)
    (at 121.158 83.82 270)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C12 (at -4.064 -0.254 360) (layer F.SilkS))
    (fp_text value 100nF (at 0 2 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 5 +24V))
    (pad 2 smd rect (at 2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:CP_Radial_D7.5mm_P2.50mm (layer F.Cu) (tedit 597BC7C2)
    (at 94.361 70.739 90)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=7.5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 7.5mm Electrolytic Capacitor")
    (fp_text reference C13 (at 1.25 -5.06 90) (layer F.SilkS))
    (fp_text value "10uF 50VDC" (at 1.25 5.06 90) (layer F.Fab))
    (fp_text user %R (at 1.25 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 +24V))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D7.5mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer B.Cu) (tedit 59FF179E)
    (at 70.104 72.771 90)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C14 (at 1.651 1.651 90) (layer B.SilkS))
    (fp_text value 100nF (at 0 -2 90) (layer B.Fab))
    (fp_text user %R (at 0 1.75 90) (layer B.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 2 +3V3))
    (pad 2 smd rect (at 2 0 90) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:CP_Radial_D7.5mm_P2.50mm (layer F.Cu) (tedit 59FF1939)
    (at 105.537 83.185 90)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=7.5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 7.5mm Electrolytic Capacitor")
    (fp_text reference C15 (at 5.461 -2.667 180) (layer F.SilkS))
    (fp_text value "22uF 25V" (at 1.25 5.06 90) (layer F.Fab))
    (fp_text user %R (at 1.25 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 +3V3))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D7.5mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 59FF19A8)
    (at 118.999 97.536 270)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C16 (at 4.318 -0.381 360) (layer F.SilkS))
    (fp_text value 1uF (at 0 2 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(C16-Pad1)"))
    (pad 2 smd rect (at 2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer B.Cu) (tedit 59FF17FB)
    (at 100.203 89.535 90)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C17 (at 1.905 2.032 270) (layer B.SilkS))
    (fp_text value 100nF (at 0 -2 90) (layer B.Fab))
    (fp_text user %R (at 0 1.75 90) (layer B.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 34 +5V))
    (pad 2 smd rect (at 2 0 90) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer B.Cu) (tedit 59FF1821)
    (at 108.585 81.915 90)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C18 (at 4.191 0.127 180) (layer B.SilkS))
    (fp_text value 100nF (at 0 -2 90) (layer B.Fab))
    (fp_text user %R (at 0 1.75 90) (layer B.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 2 +3V3))
    (pad 2 smd rect (at 2 0 90) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SMB_Handsoldering (layer B.Cu) (tedit 590B3D55)
    (at 111.633 61.341)
    (descr "Diode SMB (DO-214AA) Handsoldering")
    (tags "Diode SMB (DO-214AA) Handsoldering")
    (attr smd)
    (fp_text reference D2 (at 0 3) (layer B.SilkS))
    (fp_text value DO-214AA (at 0 -3) (layer B.Fab))
    (fp_text user %R (at 0 3) (layer B.Fab))
    (pad 1 smd rect (at -2.7 0) (size 3.5 2.3) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(D2-Pad1)"))
    (pad 2 smd rect (at 2.7 0) (size 3.5 2.3) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(D2-Pad2)"))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SMB.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SMB_Handsoldering (layer B.Cu) (tedit 590B3D55)
    (at 111.633 65.278)
    (descr "Diode SMB (DO-214AA) Handsoldering")
    (tags "Diode SMB (DO-214AA) Handsoldering")
    (attr smd)
    (fp_text reference D3 (at 0 3) (layer B.SilkS))
    (fp_text value DO-214AA (at 0 -3) (layer B.Fab))
    (fp_text user %R (at 0 3) (layer B.Fab))
    (pad 1 smd rect (at -2.7 0) (size 3.5 2.3) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(D2-Pad2)"))
    (pad 2 smd rect (at 2.7 0) (size 3.5 2.3) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SMB.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SMB_Handsoldering (layer B.Cu) (tedit 590B3D55)
    (at 101.473 62.611)
    (descr "Diode SMB (DO-214AA) Handsoldering")
    (tags "Diode SMB (DO-214AA) Handsoldering")
    (attr smd)
    (fp_text reference D4 (at 0 3) (layer B.SilkS))
    (fp_text value DO-214AA (at 0 -3) (layer B.Fab))
    (fp_text user %R (at 0 3) (layer B.Fab))
    (pad 1 smd rect (at -2.7 0) (size 3.5 2.3) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(D2-Pad1)"))
    (pad 2 smd rect (at 2.7 0) (size 3.5 2.3) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SMB.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SMA_Handsoldering (layer B.Cu) (tedit 59FF17DB)
    (at 96.52 80.137 270)
    (descr "Diode SMA (DO-214AC) Handsoldering")
    (tags "Diode SMA (DO-214AC) Handsoldering")
    (attr smd)
    (fp_text reference D5 (at -5.207 0 360) (layer B.SilkS))
    (fp_text value STPS1L30A (at 0 -2.6 270) (layer B.Fab))
    (fp_text user %R (at 0 2.5 270) (layer B.Fab))
    (pad 1 smd rect (at -2.5 0 270) (size 3.5 1.8) (layers B.Cu B.Paste B.Mask)
      (net 5 +24V))
    (pad 2 smd rect (at 2.5 0 270) (size 3.5 1.8) (layers B.Cu B.Paste B.Mask)
      (net 33 /USBPWR))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SMA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SMA_Handsoldering (layer B.Cu) (tedit 59FF1818)
    (at 116.459 80.518 90)
    (descr "Diode SMA (DO-214AC) Handsoldering")
    (tags "Diode SMA (DO-214AC) Handsoldering")
    (attr smd)
    (fp_text reference D6 (at 5.334 0.127 180) (layer B.SilkS))
    (fp_text value STPS1L30A (at 0 -2.6 90) (layer B.Fab))
    (fp_text user %R (at 0 2.5 90) (layer B.Fab))
    (pad 1 smd rect (at -2.5 0 90) (size 3.5 1.8) (layers B.Cu B.Paste B.Mask)
      (net 5 +24V))
    (pad 2 smd rect (at 2.5 0 90) (size 3.5 1.8) (layers B.Cu B.Paste B.Mask)
      (net 32 /PPoE+))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SMA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SMA_Handsoldering (layer B.Cu) (tedit 59FF17D4)
    (at 100.711 80.137 90)
    (descr "Diode SMA (DO-214AC) Handsoldering")
    (tags "Diode SMA (DO-214AC) Handsoldering")
    (attr smd)
    (fp_text reference D7 (at 5.207 0.254 180) (layer B.SilkS))
    (fp_text value STPS1L30A (at 0 -2.6 90) (layer B.Fab))
    (fp_text user %R (at 0 2.5 90) (layer B.Fab))
    (pad 1 smd rect (at -2.5 0 90) (size 3.5 1.8) (layers B.Cu B.Paste B.Mask)
      (net 34 +5V))
    (pad 2 smd rect (at 2.5 0 90) (size 3.5 1.8) (layers B.Cu B.Paste B.Mask)
      (net 33 /USBPWR))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SMA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SMA_Handsoldering (layer B.Cu) (tedit 59FF17E4)
    (at 94.107 86.614 180)
    (descr "Diode SMA (DO-214AC) Handsoldering")
    (tags "Diode SMA (DO-214AC) Handsoldering")
    (attr smd)
    (fp_text reference D8 (at 5.207 0.254 270) (layer B.SilkS))
    (fp_text value STPS1L30A (at 0 -2.6 180) (layer B.Fab))
    (fp_text user %R (at 0 2.5 180) (layer B.Fab))
    (pad 1 smd rect (at -2.5 0 180) (size 3.5 1.8) (layers B.Cu B.Paste B.Mask)
      (net 34 +5V))
    (pad 2 smd rect (at 2.5 0 180) (size 3.5 1.8) (layers B.Cu B.Paste B.Mask)
      (net 54 /5VPWR))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SMA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x04_Pitch2.54mm (layer F.Cu) (tedit 59FF1982)
    (at 80.645 61.595 270)
    (descr "Through hole straight pin header, 2x04, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x04 2.54mm double row")
    (fp_text reference J1 (at -0.889 10.541 360) (layer F.SilkS))
    (fp_text value CONN_02X04 (at 1.27 9.95 270) (layer F.Fab))
    (fp_text user %R (at 1.27 3.81 360) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(J1-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(J1-Pad2)"))
    (pad 3 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(J1-Pad3)"))
    (pad 4 thru_hole oval (at 2.54 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(J1-Pad4)"))
    (pad 5 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(J1-Pad5)"))
    (pad 6 thru_hole oval (at 2.54 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(J1-Pad6)"))
    (pad 7 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(J1-Pad7)"))
    (pad 8 thru_hole oval (at 2.54 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(J1-Pad8)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x04_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module plan44:RAK831 locked (layer B.Cu) (tedit 59FE1D36)
    (at 58.674 63.5)
    (descr "Through hole straight pin header, 2x12, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x12 2.54mm double row")
    (fp_text reference J3 (at -1.55 4.07 180) (layer B.SilkS))
    (fp_text value RAK831 (at -1.55 36.67) (layer B.Fab))
    (pad 1 thru_hole rect (at -0.28 6.4 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 +5V))
    (pad 2 thru_hole oval (at -2.82 6.4 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 +5V))
    (pad 3 thru_hole oval (at -0.28 8.94 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4 thru_hole oval (at -2.82 8.94 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 /LNA_EN_A))
    (pad 5 thru_hole oval (at -0.28 11.48 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6 thru_hole oval (at -2.82 11.48 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 "Net-(J3-Pad12)"))
    (pad 7 thru_hole oval (at -0.28 14.02 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 "Net-(J3-Pad7)"))
    (pad 8 thru_hole oval (at -2.82 14.02 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 "Net-(J3-Pad8)"))
    (pad 9 thru_hole oval (at -0.28 16.56 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 "Net-(J3-Pad9)"))
    (pad 10 thru_hole oval (at -2.82 16.56 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 "Net-(J3-Pad10)"))
    (pad 11 thru_hole oval (at -0.28 19.1 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 "Net-(J3-Pad11)"))
    (pad 12 thru_hole oval (at -2.82 19.1 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 "Net-(J3-Pad12)"))
    (pad 13 thru_hole oval (at -0.28 21.64 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 "Net-(J3-Pad13)"))
    (pad 14 thru_hole oval (at -2.82 21.64 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 "Net-(J3-Pad12)"))
    (pad 15 thru_hole oval (at -0.28 24.18 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 /SPI_CS1_RAK))
    (pad 16 thru_hole oval (at -2.82 24.18 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 /SPI_MOSI))
    (pad 17 thru_hole oval (at -0.28 26.72 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 45 /SPI_MISO))
    (pad 18 thru_hole oval (at -2.82 26.72 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 46 /SPI_CLK))
    (pad 19 thru_hole oval (at -0.28 29.26 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 47 /RAK_RESET))
    (pad 20 thru_hole oval (at -2.82 29.26 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 21 thru_hole oval (at -0.28 31.8 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 22 thru_hole oval (at -2.82 31.8 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 23 thru_hole oval (at -0.28 34.34 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 24 thru_hole oval (at -2.82 34.34 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 70.8 41.11) (size 5.6 5.6) (drill 3.2) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 70.82 0.41) (size 5.6 5.6) (drill 3.2) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at -0.03 0.42) (size 5.6 5.6) (drill 3.2) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at -0.04 41.13) (size 5.6 5.6) (drill 3.2) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x12_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connect:USB_A (layer F.Cu) (tedit 59FF18F9)
    (at 111.252 72.136 180)
    (descr "USB A connector")
    (tags "USB USB_A")
    (fp_text reference J4 (at 12.446 12.192 180) (layer F.SilkS))
    (fp_text value USB_A (at 3.84 7.44 180) (layer F.Fab))
    (pad 4 thru_hole circle (at 7.11 0 90) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole circle (at 4.57 0 90) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(D2-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(D2-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 34 +5V))
    (pad 5 thru_hole circle (at 10.16 2.67 90) (size 3 3) (drill 2.3) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 5 thru_hole circle (at -3.56 2.67 90) (size 3 3) (drill 2.3) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connectors.3dshapes/USB_A.wrl
      (at (xyz 0.14 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module plan44:USB_Micro-B-SMD (layer F.Cu) (tedit 59FF190A)
    (at 89.916 104.902)
    (descr "Micro USB Type B Receptacle")
    (tags "USB USB_B USB_micro USB_OTG")
    (clearance 0.18)
    (attr smd)
    (fp_text reference J6 (at 5.842 3.556) (layer F.SilkS))
    (fp_text value USB_Micro_AB (at 0 5.3) (layer F.Fab))
    (pad 6 thru_hole circle (at -2.25 -1.65) (size 1.1 1.1) (drill 0.65) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.3 -1.35 90) (size 1.35 0.4) (layers F.Cu F.Paste F.Mask)
      (net 33 /USBPWR))
    (pad 2 smd rect (at -0.65 -1.35 90) (size 1.35 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at 0 -1.35 90) (size 1.35 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at 0.65 -1.35 90) (size 1.35 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 1.3 -1.35 90) (size 1.35 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 thru_hole circle (at -4.15 1.4 90) (size 1.55 1.55) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6 thru_hole circle (at 4.25 1.4 90) (size 1.55 1.55) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6 thru_hole circle (at 2.25 -1.65) (size 1.1 1.1) (drill 0.65) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module plan44:HLJ-6115ANL (layer F.Cu) (tedit 59FF1901)
    (at 106.172 98.044 180)
    (descr "ETHERNET CONNECTOR (MAGJACK) FOR POE")
    (tags "ETHERNET CONNECTOR (MAGJACK) FOR POE")
    (attr virtual)
    (fp_text reference J8 (at -11.176 -10.414 360) (layer F.SilkS))
    (fp_text value HLJ-6115ANL (at -1.4 -8.75 180) (layer F.Fab))
    (pad "" np_thru_hole circle (at 4.45 -0.5 180) (size 3.25 3.25) (drill 3.25) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 3.15468 5.8801 180) (size 1.4986 1.4986) (drill 0.89916) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 16 /ETH0_TX+))
    (pad 2 thru_hole circle (at 1.88468 8.4201 180) (size 1.4986 1.4986) (drill 0.89916) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 17 /ETH0_TX-))
    (pad 3 thru_hole circle (at 0.61468 5.8801 180) (size 1.4986 1.4986) (drill 0.89916) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 18 /ETH0_RX+))
    (pad 4 thru_hole circle (at -0.65278 8.4201 180) (size 1.4986 1.4986) (drill 0.89916) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 31 "Net-(C16-Pad1)"))
    (pad 5 thru_hole circle (at -1.92278 5.8801 180) (size 1.4986 1.4986) (drill 0.89916) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 31 "Net-(C16-Pad1)"))
    (pad 6 thru_hole circle (at -3.19278 8.4201 180) (size 1.4986 1.4986) (drill 0.89916) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 19 /ETH0_RX-))
    (pad 7 thru_hole circle (at -4.46278 5.8801 180) (size 1.4986 1.4986) (drill 0.89916) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 20 /ETH_PWR+))
    (pad 8 thru_hole circle (at -5.73278 8.4201 180) (size 1.4986 1.4986) (drill 0.89916) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 21 /ETH_PWR-))
    (pad 9 thru_hole circle (at 5.36956 -5.36956 180) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 22 "Net-(J8-Pad9)"))
    (pad 10 thru_hole circle (at 2.82956 -5.36956 180) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 23 /ETH0_LED))
    (pad 11 thru_hole circle (at -5.32892 -5.36956 180) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 24 "Net-(J8-Pad11)"))
    (pad 12 thru_hole circle (at -7.86892 -5.36956 180) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 25 /WLAN_LED))
    (pad S1 thru_hole circle (at 6.477 2.54 180) (size 3.048 3.048) (drill 1.59766) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 1 GND))
    (pad S2 thru_hole circle (at -9.017 2.54 180) (size 3.048 3.048) (drill 1.59766) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 1 GND))
    (pad "" np_thru_hole circle (at -6.95 -0.5 180) (size 3.25 3.25) (drill 3.25) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_DIN965_Pad locked (layer F.Cu) (tedit 59FF18AA)
    (at 65 62.25)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (attr virtual)
    (fp_text reference MH1 (at 0 -3.8) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 3.8) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.6 5.6) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_DIN965_Pad locked (layer F.Cu) (tedit 59FF18B0)
    (at 123 62.25)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (attr virtual)
    (fp_text reference MH2 (at 0 -3.8) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 3.8) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.6 5.6) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_DIN965_Pad locked (layer F.Cu) (tedit 59FF18BB)
    (at 65 105.75)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (attr virtual)
    (fp_text reference MH3 (at 0 -3.8) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 3.8) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.6 5.6) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_DIN965_Pad locked (layer F.Cu) (tedit 59FF18C2)
    (at 123 105.75)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (attr virtual)
    (fp_text reference MH4 (at 0 -3.8) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 3.8) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.6 5.6) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Pin_Headers:Pin_Header_Straight_1x06_Pitch2.54mm (layer F.Cu) (tedit 59FF1995)
    (at 69.85 105.918 90)
    (descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x06 2.54mm single row")
    (fp_text reference P1 (at -2.794 -0.254 180) (layer F.SilkS))
    (fp_text value FDI_Cable (at 0 15.03 90) (layer F.Fab))
    (fp_text user %R (at 0 6.35 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 /Omega_RX))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 /Omega_TX))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x06_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x02_Pitch2.54mm (layer F.Cu) (tedit 59FF19B2)
    (at 120.65 91.821 180)
    (descr "Through hole straight pin header, 2x02, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x02 2.54mm double row")
    (fp_text reference P3 (at -2.794 -0.127 180) (layer F.SilkS))
    (fp_text value CONN_02X02 (at 1.27 4.87 180) (layer F.Fab))
    (fp_text user %R (at 1.27 1.27 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 /PPoE+))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 /ETH_PWR+))
    (pad 3 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4 thru_hole oval (at 2.54 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 /ETH_PWR-))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x02_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 59FF1966)
    (at 121.285 67.437)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R7 (at -2.413 2.159 180) (layer F.SilkS))
    (fp_text value 10k (at 0 1.9) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(R7-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 59FF1978)
    (at 89.662 64.008)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R9 (at -4.318 0.254 90) (layer F.SilkS))
    (fp_text value 47R (at 0 1.9) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 29 /USB+))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D2-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 59FF1971)
    (at 89.662 61.087)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R10 (at -4.318 -0.381 90) (layer F.SilkS))
    (fp_text value 47R (at 0 1.9) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 30 /USB-))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D2-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 59FF185C)
    (at 105.156 96.139 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R11 (at 0.889 -1.778 90) (layer B.SilkS))
    (fp_text value 49.9_1% (at 0 -1.75 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(C10-Pad1)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 16 /ETH0_TX+))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 59FF1876)
    (at 107.569 96.139 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R12 (at 8.255 0.127 180) (layer B.SilkS))
    (fp_text value 49.9_1% (at 0 -1.75 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(C10-Pad1)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 17 /ETH0_TX-))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 59FF182A)
    (at 114.427 90.678 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R13 (at 3.302 0.127 180) (layer B.SilkS))
    (fp_text value 49.9_1% (at 0 -1.75 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(C11-Pad1)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 18 /ETH0_RX+))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 59FF1856)
    (at 109.982 96.139 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R14 (at 1.143 1.778 90) (layer B.SilkS))
    (fp_text value 49.9_1% (at 0 -1.75 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(C11-Pad1)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 19 /ETH0_RX-))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer B.Cu) (tedit 59FF1791)
    (at 64.262 76.2)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R15 (at 1.778 -1.905) (layer B.SilkS))
    (fp_text value 0R (at 0 -1.9) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers B.Cu B.Paste B.Mask)
      (net 37 "Net-(J3-Pad7)"))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers B.Cu B.Paste B.Mask)
      (net 48 /RADIO_EN_A))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 59FF191F)
    (at 93.853 100.457 180)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R16 (at 4.191 -0.127 270) (layer F.SilkS))
    (fp_text value 1k (at 0 1.9 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(J8-Pad9)"))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 59FF191A)
    (at 93.853 97.536 180)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R17 (at 4.191 0.254 270) (layer F.SilkS))
    (fp_text value 1k (at 0 1.9 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(J8-Pad11)"))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer B.Cu) (tedit 59FF17B4)
    (at 64.262 88.265 180)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R18 (at -4.318 0 270) (layer B.SilkS))
    (fp_text value 0R (at 0 -1.9 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers B.Cu B.Paste B.Mask)
      (net 49 /PA_G8))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers B.Cu B.Paste B.Mask)
      (net 38 "Net-(J3-Pad8)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer B.Cu) (tedit 59FF17A7)
    (at 64.262 80.01)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R19 (at 4.318 0 90) (layer B.SilkS))
    (fp_text value 0R (at 0 -1.9) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers B.Cu B.Paste B.Mask)
      (net 39 "Net-(J3-Pad9)"))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers B.Cu B.Paste B.Mask)
      (net 50 /RADIO_EN_B))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer B.Cu) (tedit 59FF17AE)
    (at 64.262 83.82 180)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R20 (at -4.318 0 270) (layer B.SilkS))
    (fp_text value 0R (at 0 -1.9 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers B.Cu B.Paste B.Mask)
      (net 51 /PA_G16))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers B.Cu B.Paste B.Mask)
      (net 40 "Net-(J3-Pad10)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer B.Cu) (tedit 59FF17C2)
    (at 64.262 96.901)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R21 (at 4.318 0.254 90) (layer B.SilkS))
    (fp_text value 0R (at 0 -1.9) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers B.Cu B.Paste B.Mask)
      (net 41 "Net-(J3-Pad11)"))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers B.Cu B.Paste B.Mask)
      (net 52 /PA_EN_A))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer B.Cu) (tedit 59FF17BC)
    (at 64.262 92.583)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R22 (at 4.318 0.127 90) (layer B.SilkS))
    (fp_text value 0R (at 0 -1.9) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers B.Cu B.Paste B.Mask)
      (net 42 "Net-(J3-Pad13)"))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers B.Cu B.Paste B.Mask)
      (net 53 /RADIO_RST))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_ThroughHole:SW_PUSH_6mm_h4.3mm (layer F.Cu) (tedit 59FF195C)
    (at 130.429 71.501 270)
    (descr "tactile push button, 6x6mm e.g. PHAP33xx series, height=4.3mm")
    (tags "tact sw push 6mm")
    (fp_text reference SW1 (at 9.017 2.159 360) (layer F.SilkS))
    (fp_text value "Omron PB" (at 3.75 6.7 270) (layer F.Fab))
    (fp_text user %R (at 3.25 2.25 270) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 4.5) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 28 "Net-(R7-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 +3V3))
    (pad 2 thru_hole circle (at 6.5 4.5) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 28 "Net-(R7-Pad2)"))
    (pad 1 thru_hole circle (at 6.5 0) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 +3V3))
    (model ${KISYS3DMOD}/Buttons_Switches_THT.3dshapes/SW_PUSH_6mm_h4.3mm.wrl
      (at (xyz 0.005 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module plan44:ONION-OMEGA2S (layer F.Cu) (tedit 5971C332)
    (at 74.168 80.518 180)
    (clearance 0.25)
    (fp_text reference U1 (at 8.55 -20.5 180) (layer F.SilkS))
    (fp_text value ONION-OMEGA2S (at 4.4 -3.9 270) (layer F.Fab))
    (pad A13 smd rect (at -9.8155 -20.5055 270) (size 2.375 1) (layers F.Cu F.Paste F.Mask))
    (pad A12 smd rect (at -8.5455 -20.5055 270) (size 2.375 1) (layers F.Cu F.Paste F.Mask))
    (pad A11 smd rect (at -7.2755 -20.5055 270) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 44 /SPI_MOSI))
    (pad A10 smd rect (at -6.0055 -20.5055 270) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 45 /SPI_MISO))
    (pad A9 smd rect (at -4.7355 -20.5055 270) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 46 /SPI_CLK))
    (pad A8 smd rect (at -3.4655 -20.5055 270) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 43 /SPI_CS1_RAK))
    (pad A7 smd rect (at -2.1955 -20.5055 270) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad A6 smd rect (at -0.9255 -20.5055 270) (size 2.375 1) (layers F.Cu F.Paste F.Mask))
    (pad A5 smd rect (at 0.3445 -20.5055 270) (size 2.375 1) (layers F.Cu F.Paste F.Mask))
    (pad A4 smd rect (at 1.6145 -20.5055 270) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 52 /PA_EN_A))
    (pad A3 smd rect (at 2.8845 -20.5055 270) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 53 /RADIO_RST))
    (pad A2 smd rect (at 4.1545 -20.5055 270) (size 2.375 1) (layers F.Cu F.Paste F.Mask))
    (pad B1 smd rect (at -13.0125 -17.78 180) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 27 /Omega_TX))
    (pad B2 smd rect (at -13.0125 -16.51 180) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 26 /Omega_RX))
    (pad B3 smd rect (at -13.0125 -15.24 180) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 18 /ETH0_RX+))
    (pad B4 smd rect (at -13.0125 -13.97 180) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 19 /ETH0_RX-))
    (pad B5 smd rect (at -13.0125 -12.7 180) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 16 /ETH0_TX+))
    (pad B6 smd rect (at -13.0125 -11.43 180) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 17 /ETH0_TX-))
    (pad B7 smd rect (at -13.0125 -10.16 180) (size 2.375 1) (layers F.Cu F.Paste F.Mask))
    (pad B8 smd rect (at -13.0125 -8.89 180) (size 2.375 1) (layers F.Cu F.Paste F.Mask))
    (pad B9 smd rect (at -13.0125 -7.62 180) (size 2.375 1) (layers F.Cu F.Paste F.Mask))
    (pad B10 smd rect (at -13.0125 -6.35 180) (size 2.375 1) (layers F.Cu F.Paste F.Mask))
    (pad B11 smd rect (at -13.0125 -5.08 180) (size 2.375 1) (layers F.Cu F.Paste F.Mask))
    (pad B12 smd rect (at -13.0125 -3.81 180) (size 2.375 1) (layers F.Cu F.Paste F.Mask))
    (pad B13 smd rect (at -13.0125 -2.54 180) (size 2.375 1) (layers F.Cu F.Paste F.Mask))
    (pad B14 smd rect (at -13.0125 -1.27 180) (size 2.375 1) (layers F.Cu F.Paste F.Mask))
    (pad B15 smd rect (at -13.0125 0 180) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(J1-Pad2)"))
    (pad B16 smd rect (at -13.0125 1.27 180) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(J1-Pad4)"))
    (pad B17 smd rect (at -13.0125 2.54 180) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(J1-Pad6)"))
    (pad B18 smd rect (at -13.0125 3.81 180) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(J1-Pad8)"))
    (pad B19 smd rect (at -13.0125 5.08 180) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(J1-Pad7)"))
    (pad B20 smd rect (at -13.0125 6.35 180) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(J1-Pad5)"))
    (pad B21 smd rect (at -13.0125 7.62 180) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(J1-Pad3)"))
    (pad B22 smd rect (at -13.0125 8.89 180) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(J1-Pad1)"))
    (pad B23 smd rect (at -13.0125 10.16 180) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 29 /USB+))
    (pad B24 smd rect (at -13.0125 11.43 180) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 30 /USB-))
    (pad B25 smd rect (at -13.0125 12.7 180) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad C1 smd rect (at 8.5675 -17.78 180) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad C2 smd rect (at 8.5675 -16.51 180) (size 2.375 1) (layers F.Cu F.Paste F.Mask))
    (pad C3 smd rect (at 8.5675 -15.24 180) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad C4 smd rect (at 8.5675 -13.97 180) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad C5 smd rect (at 8.5675 -12.7 180) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 51 /PA_G16))
    (pad C6 smd rect (at 8.5675 -11.43 180) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 49 /PA_G8))
    (pad C7 smd rect (at 8.5675 -10.16 180) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 25 /WLAN_LED))
    (pad C8 smd rect (at 8.5675 -8.89 180) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 23 /ETH0_LED))
    (pad C9 smd rect (at 8.5675 -7.62 180) (size 2.375 1) (layers F.Cu F.Paste F.Mask))
    (pad C10 smd rect (at 8.5675 -6.35 180) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 35 /LNA_EN_A))
    (pad C11 smd rect (at 8.5675 -5.08 180) (size 2.375 1) (layers F.Cu F.Paste F.Mask))
    (pad C12 smd rect (at 8.5675 -3.81 180) (size 2.375 1) (layers F.Cu F.Paste F.Mask))
    (pad C13 smd rect (at 8.5675 -2.54 180) (size 2.375 1) (layers F.Cu F.Paste F.Mask))
    (pad C14 smd rect (at 8.5675 -1.27 180) (size 2.375 1) (layers F.Cu F.Paste F.Mask))
    (pad C15 smd rect (at 8.5675 0 180) (size 2.375 1) (layers F.Cu F.Paste F.Mask))
    (pad C16 smd rect (at 8.5675 1.27 180) (size 2.375 1) (layers F.Cu F.Paste F.Mask))
    (pad C17 smd rect (at 8.5675 2.54 180) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad C18 smd rect (at 8.5675 3.81 180) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad C19 smd rect (at 8.5675 5.08 180) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 50 /RADIO_EN_B))
    (pad C20 smd rect (at 8.5675 6.35 180) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 48 /RADIO_EN_A))
    (pad C21 smd rect (at 8.5675 7.62 180) (size 2.375 1) (layers F.Cu F.Paste F.Mask))
    (pad C22 smd rect (at 8.5675 8.89 180) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(R7-Pad2)"))
    (pad C23 smd rect (at 8.5675 10.16 180) (size 2.375 1) (layers F.Cu F.Paste F.Mask))
    (pad C24 smd rect (at 8.5675 11.43 180) (size 2.375 1) (layers F.Cu F.Paste F.Mask))
    (pad C25 smd rect (at 8.5675 12.7 180) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad A1 smd rect (at 5.4245 -20.5055 270) (size 2.375 1) (layers F.Cu F.Paste F.Mask)
      (net 47 /RAK_RESET))
    (pad "" thru_hole rect (at -5.65 -6.9 180) (size 1.1 1.1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 0))
    (pad 3 smd rect (at -3.15 -3.55 180) (size 10 15) (layers B.Cu B.Paste B.Mask)
      (zone_connect 0))
    (pad "" thru_hole rect (at -4.65 -6.9 180) (size 1.1 1.1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 0))
    (pad "" thru_hole rect (at -3.65 -6.9 180) (size 1.1 1.1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 0))
    (pad "" thru_hole rect (at -2.65 -6.9 180) (size 1.1 1.1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 0))
    (pad "" thru_hole rect (at -1.65 -6.9 180) (size 1.1 1.1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 0))
    (pad "" thru_hole rect (at -0.65 -6.9 180) (size 1.1 1.1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 0))
    (pad "" thru_hole rect (at -5.65 -5.9 180) (size 1.1 1.1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 0))
    (pad "" thru_hole rect (at -4.65 -5.9 180) (size 1.1 1.1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 0))
    (pad "" thru_hole rect (at -3.65 -5.9 180) (size 1.1 1.1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 0))
    (pad "" thru_hole rect (at -2.65 -5.9 180) (size 1.1 1.1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 0))
    (pad "" thru_hole rect (at -1.65 -5.9 180) (size 1.1 1.1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 0))
    (pad "" thru_hole rect (at -0.65 -5.9 180) (size 1.1 1.1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 0))
    (pad "" thru_hole rect (at -5.65 -4.9 180) (size 1.1 1.1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 0))
    (pad "" thru_hole rect (at -4.65 -4.9 180) (size 1.1 1.1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 0))
    (pad "" thru_hole rect (at -1.65 -4.9 180) (size 1.1 1.1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 0))
    (pad "" thru_hole rect (at -0.65 -4.9 180) (size 1.1 1.1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 0))
    (pad "" thru_hole rect (at -5.65 -3.9 180) (size 1.1 1.1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 0))
    (pad "" thru_hole rect (at -4.65 -3.9 180) (size 1.1 1.1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 0))
    (pad "" thru_hole rect (at -1.65 -3.9 180) (size 1.1 1.1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 0))
    (pad "" thru_hole rect (at -0.65 -3.9 180) (size 1.1 1.1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 0))
    (pad "" thru_hole rect (at -5.65 -2.9 180) (size 1.1 1.1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 0))
    (pad "" thru_hole rect (at -4.65 -2.9 180) (size 1.1 1.1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 0))
    (pad "" thru_hole rect (at -3.65 -2.9 180) (size 1.1 1.1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 0))
    (pad "" thru_hole rect (at -2.65 -2.9 180) (size 1.1 1.1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 0))
    (pad "" thru_hole rect (at -1.65 -2.9 180) (size 1.1 1.1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 0))
    (pad "" thru_hole rect (at -0.65 -2.9 180) (size 1.1 1.1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 0))
    (pad "" thru_hole rect (at -5.65 -1.9 180) (size 1.1 1.1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 0))
    (pad "" thru_hole rect (at -4.65 -1.9 180) (size 1.1 1.1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 0))
    (pad "" thru_hole rect (at -3.65 -1.9 180) (size 1.1 1.1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 0))
    (pad "" thru_hole rect (at -2.65 -1.9 180) (size 1.1 1.1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 0))
    (pad "" thru_hole rect (at -1.65 -1.9 180) (size 1.1 1.1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 0))
    (pad "" thru_hole rect (at -0.65 -1.9 180) (size 1.1 1.1) (drill 0.5) (layers *.Cu *.Mask)
      (zone_connect 0))
  )
  (module plan44:Recom-R78Cxx (layer F.Cu) (tedit 59FF1945)
    (at 92.456 82.804 90)
    (descr "Recom R-78HBxx.0.5")
    (tags "Recom DCDC R-78")
    (fp_text reference U2 (at 7.874 7.874 180) (layer F.SilkS))
    (fp_text value R-78C5.0-1.0 (at 2.4 -3.2 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 2.032 2.54) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 1 thru_hole oval (at 5.08 0 90) (size 2.032 2.54) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 5 +24V))
    (pad 3 thru_hole oval (at 0 0 90) (size 2.032 2.54) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 54 /5VPWR))
  )
  (module plan44:Recom-R78Cxx (layer F.Cu) (tedit 59FF194C)
    (at 112.522 83.058 90)
    (descr "Recom R-78HBxx.0.5")
    (tags "Recom DCDC R-78")
    (fp_text reference U3 (at 7.874 8.128 180) (layer F.SilkS))
    (fp_text value R_783.3-0.5 (at 2.4 -3.2 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 2.032 2.54) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 1 thru_hole oval (at 5.08 0 90) (size 2.032 2.54) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 5 +24V))
    (pad 3 thru_hole oval (at 0 0 90) (size 2.032 2.54) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 2 +3V3))
  )
  (module plan44:Stitching-VIA-0.6mm (layer F.Cu) (tedit 59FF1D37)
    (at 62.5 66)
    (fp_text reference VIA (at 0 1.905) (layer F.SilkS) hide)
    (fp_text value Stitching-VIA-0.6mm (at 0 -1.905) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (dimension 80.01 (width 0.3) (layer Dwgs.User)
    (gr_text "80.010 mm" (at 93.98 148.035) (layer Dwgs.User))
    (feature1 (pts (xy 133.985 109.855) (xy 133.985 149.385)))
    (feature2 (pts (xy 53.975 109.855) (xy 53.975 149.385)))
    (crossbar (pts (xy 53.975 146.685) (xy 133.985 146.685)))
    (arrow1a (pts (xy 133.985 146.685) (xy 132.858496 147.271421)))
    (arrow1b (pts (xy 133.985 146.685) (xy 132.858496 146.098579)))
    (arrow2a (pts (xy 53.975 146.685) (xy 55.101504 147.271421)))
    (arrow2b (pts (xy 53.975 146.685) (xy 55.101504 146.098579)))
  )
  (dimension 51.435 (width 0.3) (layer Dwgs.User)
    (gr_text "51.435 mm" (at 148.67 84.1375 270) (layer Dwgs.User))
    (feature1 (pts (xy 133.985 109.855) (xy 150.02 109.855)))
    (feature2 (pts (xy 133.985 58.42) (xy 150.02 58.42)))
    (crossbar (pts (xy 147.32 58.42) (xy 147.32 109.855)))
    (arrow1a (pts (xy 147.32 109.855) (xy 146.733579 108.728496)))
    (arrow1b (pts (xy 147.32 109.855) (xy 147.906421 108.728496)))
    (arrow2a (pts (xy 147.32 58.42) (xy 146.733579 59.546504)))
    (arrow2b (pts (xy 147.32 58.42) (xy 147.906421 59.546504)))
  )
  (gr_line (start 53.975 109.855) (end 53.975 58.42) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 133.985 58.42) (end 133.985 109.855) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 53.975 109.855) (end 133.985 109.855) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 53.975 58.42) (end 133.985 58.42) (angle 90) (layer Edge.Cuts) (width 0.1))
  (dimension 43.5 (width 0.3) (layer Dwgs.User)
    (gr_text "43.500 mm" (at 28.9 84 270) (layer Dwgs.User))
    (feature1 (pts (xy 127 105.75) (xy 27.55 105.75)))
    (feature2 (pts (xy 127 62.25) (xy 27.55 62.25)))
    (crossbar (pts (xy 30.25 62.25) (xy 30.25 105.75)))
    (arrow1a (pts (xy 30.25 105.75) (xy 29.663579 104.623496)))
    (arrow1b (pts (xy 30.25 105.75) (xy 30.836421 104.623496)))
    (arrow2a (pts (xy 30.25 62.25) (xy 29.663579 63.376504)))
    (arrow2b (pts (xy 30.25 62.25) (xy 30.836421 63.376504)))
  )
  (dimension 58 (width 0.3) (layer Dwgs.User)
    (gr_text "58.000 mm" (at 94 139.85) (layer Dwgs.User))
    (feature1 (pts (xy 123 62) (xy 123 141.2)))
    (feature2 (pts (xy 65 62) (xy 65 141.2)))
    (crossbar (pts (xy 65 138.5) (xy 123 138.5)))
    (arrow1a (pts (xy 123 138.5) (xy 121.873496 139.086421)))
    (arrow1b (pts (xy 123 138.5) (xy 121.873496 137.913579)))
    (arrow2a (pts (xy 65 138.5) (xy 66.126504 139.086421)))
    (arrow2b (pts (xy 65 138.5) (xy 66.126504 137.913579)))
  )
  (dimension 84 (width 0.3) (layer Dwgs.User)
    (gr_text "84.000 mm" (at 38.15 84 270) (layer Dwgs.User))
    (feature1 (pts (xy 52 126) (xy 36.8 126)))
    (feature2 (pts (xy 52 42) (xy 36.8 42)))
    (crossbar (pts (xy 39.5 42) (xy 39.5 126)))
    (arrow1a (pts (xy 39.5 126) (xy 38.913579 124.873496)))
    (arrow1b (pts (xy 39.5 126) (xy 40.086421 124.873496)))
    (arrow2a (pts (xy 39.5 42) (xy 38.913579 43.126504)))
    (arrow2b (pts (xy 39.5 42) (xy 40.086421 43.126504)))
  )
  (dimension 65 (width 0.3) (layer Dwgs.User)
    (gr_text "65.000 mm" (at 44.65 84 270) (layer Dwgs.User))
    (feature1 (pts (xy 52 116.5) (xy 43.3 116.5)))
    (feature2 (pts (xy 52 51.5) (xy 43.3 51.5)))
    (crossbar (pts (xy 46 51.5) (xy 46 116.5)))
    (arrow1a (pts (xy 46 116.5) (xy 45.413579 115.373496)))
    (arrow1b (pts (xy 46 116.5) (xy 46.586421 115.373496)))
    (arrow2a (pts (xy 46 51.5) (xy 45.413579 52.626504)))
    (arrow2b (pts (xy 46 51.5) (xy 46.586421 52.626504)))
  )
  (dimension 84 (width 0.3) (layer Dwgs.User)
    (gr_text "84.000 mm" (at 94 36.15) (layer Dwgs.User))
    (feature1 (pts (xy 136 42) (xy 136 34.8)))
    (feature2 (pts (xy 52 42) (xy 52 34.8)))
    (crossbar (pts (xy 52 37.5) (xy 136 37.5)))
    (arrow1a (pts (xy 136 37.5) (xy 134.873496 38.086421)))
    (arrow1b (pts (xy 136 37.5) (xy 134.873496 36.913579)))
    (arrow2a (pts (xy 52 37.5) (xy 53.126504 38.086421)))
    (arrow2b (pts (xy 52 37.5) (xy 53.126504 36.913579)))
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 133.75 109.5) (xy 54.25 109.5) (xy 54.25 58.75) (xy 133.75 58.75)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 54.25 58.75) (xy 133.75 58.75) (xy 133.75 109.5) (xy 54.25 109.5)
      )
    )
  )
)
