(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 0)
    (no_connects 0)
    (area 143.434999 107.239999 191.845001 144.855001)
    (thickness 1.6)
    (drawings 13)
    (tracks 89)
    (zones 0)
    (modules 17)
    (nets 8)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
  )
  (setup
    (last_trace_width 0.1524)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.6858)
    (uvia_drill 0.3302)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 4.064 4.064)
    (pad_drill 3.048)
    (pad_to_mask_clearance 0.0508)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 VCC)
  (net 2 GND)
  (net 3 VEE)
  (net 4 +12V)
  (net 5 -12VA)
  (net 6 "Net-(R1-Pad2)")
  (net 7 "Net-(R3-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (add_net "Net-(R1-Pad2)")
    (add_net "Net-(R3-Pad2)")
  )
  (net_class Wide ""
    (clearance 0.25)
    (trace_width 1.27)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (add_net +12V)
    (add_net -12VA)
    (add_net GND)
    (add_net VCC)
    (add_net VEE)
  )
  (module Capacitors_Tantalum_SMD:CP_Tantalum_Case-B_EIA-3528-21_Hand (layer F.Cu) (tedit 5A48785F)
    (at 182.626 125.857 270)
    (descr "Tantalum capacitor, Case B, EIA 3528-21, 3.5x2.8x1.9mm, Hand soldering footprint")
    (tags "capacitor tantalum smd")
    (attr smd)
    (fp_text reference C4 (at -3.175 -2.54 270) (layer F.SilkS))
    (fp_text value 10u (at 0 -2.54 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -2.15 0 270) (size 3.2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 2.15 0 270) (size 3.2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 5 -12VA))
    (model Capacitors_Tantalum_SMD.3dshapes/CP_Tantalum_Case-B_EIA-3528-21.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_Tantalum_SMD:CP_Tantalum_Case-B_EIA-3528-21_Hand (layer F.Cu) (tedit 5A487872)
    (at 152.7175 125.984 90)
    (descr "Tantalum capacitor, Case B, EIA 3528-21, 3.5x2.8x1.9mm, Hand soldering footprint")
    (tags "capacitor tantalum smd")
    (attr smd)
    (fp_text reference C1 (at -3.175 -2.54 90) (layer F.SilkS))
    (fp_text value 10u (at 0 -2.54 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -2.15 0 90) (size 3.2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at 2.15 0 90) (size 3.2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_Tantalum_SMD.3dshapes/CP_Tantalum_Case-B_EIA-3528-21.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_Tantalum_SMD:CP_Tantalum_Case-B_EIA-3528-21_Hand (layer F.Cu) (tedit 5A48785B)
    (at 182.626 115.8875 90)
    (descr "Tantalum capacitor, Case B, EIA 3528-21, 3.5x2.8x1.9mm, Hand soldering footprint")
    (tags "capacitor tantalum smd")
    (attr smd)
    (fp_text reference C2 (at 3.175 2.54 90) (layer F.SilkS))
    (fp_text value 10u (at 0 2.54 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -2.15 0 90) (size 3.2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 2.15 0 90) (size 3.2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 3 VEE))
    (model Capacitors_Tantalum_SMD.3dshapes/CP_Tantalum_Case-B_EIA-3528-21.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_Tantalum_SMD:CP_Tantalum_Case-B_EIA-3528-21_Hand (layer F.Cu) (tedit 5A487875)
    (at 152.7175 115.8875 270)
    (descr "Tantalum capacitor, Case B, EIA 3528-21, 3.5x2.8x1.9mm, Hand soldering footprint")
    (tags "capacitor tantalum smd")
    (attr smd)
    (fp_text reference C3 (at 3.175 2.54 270) (layer F.SilkS))
    (fp_text value 10u (at 0 2.54 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -2.15 0 270) (size 3.2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 4 +12V))
    (pad 2 smd rect (at 2.15 0 270) (size 3.2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_Tantalum_SMD.3dshapes/CP_Tantalum_Case-B_EIA-3528-21.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Terminal_Blocks:TerminalBlock_bornier-6_P5.08mm (layer F.Cu) (tedit 5A4878A2)
    (at 154.94 138.43)
    (descr "simple 6pin terminal block, pitch 5.08mm, revamped version of bornier6")
    (tags "terminal block bornier6")
    (fp_text reference J1 (at 12.65 -4.55) (layer F.SilkS))
    (fp_text value Screw_Terminal_1x06 (at 12.7 4.75) (layer F.Fab) hide)
    (fp_text user %R (at 12.7 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 5.08 0) (size 3 3) (drill 1.52) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole circle (at 10.16 0) (size 3 3) (drill 1.52) (layers *.Cu *.Mask)
      (net 4 +12V))
    (pad 1 thru_hole rect (at 0 0) (size 3 3) (drill 1.52) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 4 thru_hole circle (at 15.24 0) (size 3 3) (drill 1.52) (layers *.Cu *.Mask)
      (net 3 VEE))
    (pad 5 thru_hole circle (at 20.32 0) (size 3 3) (drill 1.52) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 6 thru_hole circle (at 25.4 0) (size 3 3) (drill 1.52) (layers *.Cu *.Mask)
      (net 5 -12VA))
    (model ${KISYS3DMOD}/Terminal_Blocks.3dshapes/TerminalBlock_bornier-6_P5.08mm.wrl
      (at (xyz 0.5 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5A487867)
    (at 174.3075 127.3175 180)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R1 (at -4.445 0 180) (layer F.SilkS))
    (fp_text value 4K02 (at 0 1.9 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(R1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5A487863)
    (at 174.3075 131.1275 180)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R2 (at -4.445 0 180) (layer F.SilkS))
    (fp_text value 36K5 (at 0 1.9 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 5 -12VA))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(R1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5A48786E)
    (at 163.5125 131.1275)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R3 (at -4.445 0) (layer F.SilkS))
    (fp_text value 4K02 (at 0 1.9) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(R3-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5A48786A)
    (at 164.7825 127.3175 180)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R4 (at 4.445 0 180) (layer F.SilkS))
    (fp_text value 36K5 (at 0 1.9 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(R3-Pad2)"))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 +12V))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module DDPAK:DDPAK-5_Q (layer F.Cu) (tedit 5A4878E7)
    (at 174.9425 114.6175)
    (attr smd)
    (fp_text reference U1 (at -4.7625 -6.2865) (layer F.SilkS))
    (fp_text value LM2991SX (at 4.0005 -6.2865) (layer F.SilkS))
    (pad 1 smd rect (at -3.4036 8.6106) (size 1.016 2.286) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(R1-Pad2)"))
    (pad 2 smd rect (at -1.7018 8.6106) (size 1.016 2.286) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 0 8.6106) (size 1.016 2.286) (layers F.Cu F.Paste F.Mask)
      (net 3 VEE))
    (pad 4 smd rect (at 1.7018 8.6106) (size 1.016 2.286) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd rect (at 3.4036 8.6106) (size 1.016 2.286) (layers F.Cu F.Paste F.Mask)
      (net 5 -12VA))
    (pad 6 smd rect (at 0 0) (size 10.5918 11.6332) (layers F.Cu F.Paste F.Mask)
      (net 3 VEE))
  )
  (module DDPAK:DDPAK-5_Q (layer F.Cu) (tedit 5A4878EB)
    (at 160.9725 114.6175)
    (attr smd)
    (fp_text reference U2 (at -4.8895 -6.2865) (layer F.SilkS))
    (fp_text value LT1963AEQPBF (at 3.7465 -6.2865) (layer F.SilkS))
    (pad 1 smd rect (at -3.4036 8.6106) (size 1.016 2.286) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at -1.7018 8.6106) (size 1.016 2.286) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 3 smd rect (at 0 8.6106) (size 1.016 2.286) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 1.7018 8.6106) (size 1.016 2.286) (layers F.Cu F.Paste F.Mask)
      (net 4 +12V))
    (pad 5 smd rect (at 3.4036 8.6106) (size 1.016 2.286) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(R3-Pad2)"))
    (pad 6 smd rect (at 0 0) (size 10.5918 11.6332) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module Connectors:1pin (layer F.Cu) (tedit 5A4878B6)
    (at 188.595 111.125)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 3) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask))
  )
  (module Connectors:1pin (layer F.Cu) (tedit 5A4878BD)
    (at 146.685 111.125)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 3) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask))
  )
  (module Connectors:1pin (layer F.Cu) (tedit 5A4878C1)
    (at 146.685 141.478)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 3) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask))
  )
  (module Connectors:1pin (layer F.Cu) (tedit 5A4878B9)
    (at 188.595 141.478)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 3) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask))
  )
  (module DDPAK:wohali-logo (layer F.Cu) (tedit 0)
    (at 179.07 135.128)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module DDPAK:wohali-logo (layer F.Cu) (tedit 0)
    (at 188.722 117.094 90)
    (fp_text reference G*** (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 90) (layer F.SilkS) hide)
  )
  (gr_text "¯\\_(ʘ‿ʘ)_/¯" (at 167.894 124.46 360) (layer B.SilkS))
  (gr_text "Back in action!" (at 146.812 126.492 270) (layer F.SilkS))
  (gr_text "© Wohali 2017" (at 188.722 128.778 90) (layer F.SilkS))
  (gr_text -12 (at 179.832 143.51) (layer F.SilkS))
  (gr_text GND (at 175.26 143.51) (layer F.SilkS))
  (gr_text -15 (at 169.926 143.51) (layer F.SilkS))
  (gr_text +12 (at 165.1 143.51) (layer F.SilkS))
  (gr_text GND (at 160.02 143.51) (layer F.SilkS))
  (gr_text +15 (at 154.432 143.51) (layer F.SilkS))
  (gr_line (start 143.51 144.78) (end 191.77 144.78) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 143.51 107.315) (end 143.51 144.78) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 191.77 107.315) (end 143.51 107.315) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 191.77 144.78) (end 191.77 107.315) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 149.86 107.696) (xy 185.928 107.696) (xy 185.674 142.494) (xy 149.86 142.494)
      )
    )
  )
)
