(kicad_pcb (version 4) (host pcbnew 4.0.6-e0-6349~53~ubuntu16.04.1)
  (general
    (links 0)
    (no_connects 0)
    (area 94.949999 67.949999 191.050001 132.050001)
    (thickness 1.6)
    (drawings 25)
    (tracks 2)
    (zones 0)
    (modules 8)
    (nets 3)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 1)
    (trace_clearance 0.2)
    (zone_clearance 0)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 3.2 3.2)
    (pad_drill 3.2)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 190 100)
    (grid_origin 190 100)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 HF)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 1)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net HF)
  )
  (module Mounting_Holes:MountingHole_2.7mm (layer F.Cu) (tedit 59960DA9)
    (at 183 103)
    (descr "Mounting Hole 2.7mm, no annular")
    (tags "mounting hole 2.7mm no annular")
    (fp_text reference REF** (at 0 -3.7) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.7mm (at 0 3.7) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (module Measurement_Points:Measurement_Point_Square-SMD-Pad_Small (layer B.Cu) (tedit 59983141)
    (at 100.8 100)
    (descr "Mesurement Point, Square, SMD Pad,  1.5mm x 1.5mm,")
    (tags "Mesurement Point Square SMD Pad 1.5x1.5mm")
    (attr virtual)
    (fp_text reference TP1 (at 0 2) (layer B.SilkS) hide)
    (fp_text value TEST (at 0 -2) (layer B.Fab) hide)
    (pad 1 smd rect (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 1 GND))
  )
  (module Measurement_Points:Measurement_Point_Square-SMD-Pad_Small (layer F.Cu) (tedit 59960DC9)
    (at 100.8 100)
    (descr "Mesurement Point, Square, SMD Pad,  1.5mm x 1.5mm,")
    (tags "Mesurement Point Square SMD Pad 1.5x1.5mm")
    (attr virtual)
    (fp_text reference TP2 (at 0 -2) (layer F.SilkS) hide)
    (fp_text value TEST (at 0 2) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 1.5 1.5) (layers F.Cu F.Mask)
      (net 2 HF))
  )
  (module Mounting_Holes:MountingHole_2.7mm (layer F.Cu) (tedit 59960DCD)
    (at 98.7 100)
    (descr "Mounting Hole 2.7mm, no annular")
    (tags "mounting hole 2.7mm no annular")
    (fp_text reference REF** (at 0 -3.7) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.7mm (at 0 3.7) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_ISO7380 (layer F.Cu) (tedit 59960DB8)
    (at 187 128)
    (descr "Mounting Hole 3.2mm, no annular, M3, ISO7380")
    (tags "mounting hole 3.2mm no annular m3 iso7380")
    (fp_text reference REF** (at 0 -3.85) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3_ISO7380 (at 0 3.85) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_ISO7380 (layer F.Cu) (tedit 59960DC0)
    (at 187 72)
    (descr "Mounting Hole 3.2mm, no annular, M3, ISO7380")
    (tags "mounting hole 3.2mm no annular m3 iso7380")
    (fp_text reference REF** (at 0 -3.85) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3_ISO7380 (at 0 3.85) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_2.7mm (layer F.Cu) (tedit 59960DA0)
    (at 183 97)
    (descr "Mounting Hole 2.7mm, no annular")
    (tags "mounting hole 2.7mm no annular")
    (fp_text reference REF** (at 0 -3.7) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.7mm (at 0 3.7) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (module OPENHARDWARE:OSHWLOGO0.3IN (layer F.Cu) (tedit 0)
    (at 183 89 90)
    (descr "OSHW LOGO")
    (tags "Open Source Hardware Logo")
    (fp_text reference G*** (at 0 7.27964 90) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0 -7.27964 90) (layer F.SilkS) hide)
  )
  (dimension 56 (width 0.3) (layer Cmts.User)
    (gr_text "56.000 mm" (at 197.35 100 90) (layer Cmts.User))
    (feature1 (pts (xy 187 72) (xy 198.7 72)))
    (feature2 (pts (xy 187 128) (xy 198.7 128)))
    (crossbar (pts (xy 196 128) (xy 196 72)))
    (arrow1a (pts (xy 196 72) (xy 196.586421 73.126504)))
    (arrow1b (pts (xy 196 72) (xy 195.413579 73.126504)))
    (arrow2a (pts (xy 196 128) (xy 196.586421 126.873496)))
    (arrow2b (pts (xy 196 128) (xy 195.413579 126.873496)))
  )
  (dimension 64 (width 0.3) (layer Cmts.User)
    (gr_text "64.000 mm" (at 204.35 100 90) (layer Cmts.User))
    (feature1 (pts (xy 191 68) (xy 205.7 68)))
    (feature2 (pts (xy 191 132) (xy 205.7 132)))
    (crossbar (pts (xy 203 132) (xy 203 68)))
    (arrow1a (pts (xy 203 68) (xy 203.586421 69.126504)))
    (arrow1b (pts (xy 203 68) (xy 202.413579 69.126504)))
    (arrow2a (pts (xy 203 132) (xy 203.586421 130.873496)))
    (arrow2b (pts (xy 203 132) (xy 202.413579 130.873496)))
  )
  (dimension 96 (width 0.3) (layer Cmts.User)
    (gr_text "96.000 mm" (at 143 62.65) (layer Cmts.User))
    (feature1 (pts (xy 191 92) (xy 191 61.3)))
    (feature2 (pts (xy 95 92) (xy 95 61.3)))
    (crossbar (pts (xy 95 64) (xy 191 64)))
    (arrow1a (pts (xy 191 64) (xy 189.873496 64.586421)))
    (arrow1b (pts (xy 191 64) (xy 189.873496 63.413579)))
    (arrow2a (pts (xy 95 64) (xy 96.126504 64.586421)))
    (arrow2b (pts (xy 95 64) (xy 96.126504 63.413579)))
  )
  (gr_text "3.2 dBi - 6.7 dBi" (at 184 116 90) (layer B.SilkS))
  (gr_text git.dk0tu.de/db4um/LPDA (at 188 100 90) (layer B.SilkS))
  (gr_text "DB4UM 2017 CC-BY-SA " (at 188 103.5 90) (layer F.SilkS))
  (gr_text "LPDA Antenna   2 GHz - 6 GHz" (at 138 81 17) (layer F.SilkS))
  (gr_line (start 191 132) (end 191 68) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 191 68) (end 174 68) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 174 132) (end 191 132) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 95 108) (end 174 132) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 95 92) (end 95 108) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 174 68) (end 95 92) (layer Edge.Cuts) (width 0.1))
  (zone (net 2) (net_name HF) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254)
    (fill yes (arc_segments 16) (thermal_gap 0) (thermal_bridge_width 0))
    (polygon
      (pts
        (xy 100 102.1) (xy 100 97.9) (xy 105.6 97.9) (xy 105.6 94.25) (xy 106.4 94.25)
        (xy 106.4 97.9) (xy 109.62 97.9) (xy 109.62 93.06) (xy 110.59 93.06) (xy 110.59 97.9)
        (xy 114.47 97.9) (xy 114.47 91.62) (xy 115.65 91.62) (xy 115.65 97.9) (xy 120.33 97.9)
        (xy 120.33 89.88) (xy 121.75 89.88) (xy 121.75 97.9) (xy 127.41 97.9) (xy 127.41 87.77)
        (xy 129.12 87.77) (xy 129.12 97.9) (xy 135.96 97.9) (xy 135.96 85.24) (xy 138.03 85.24)
        (xy 138.03 97.9) (xy 146.28 97.9) (xy 146.28 82.17) (xy 148.78 82.17) (xy 148.78 97.9)
        (xy 158.74 97.9) (xy 158.74 78.47) (xy 161.76 78.47) (xy 161.76 97.9) (xy 173.8 97.9)
        (xy 173.8 74) (xy 177.44 74) (xy 177.44 102.1) (xy 169.23 102.1) (xy 169.23 123.66)
        (xy 165.91 123.66) (xy 165.91 102.1) (xy 154.96 102.1) (xy 154.96 119.59) (xy 152.22 119.59)
        (xy 152.22 102.1) (xy 143.15 102.1) (xy 143.15 116.22) (xy 140.88 116.22) (xy 140.88 102.1)
        (xy 133.36 102.1) (xy 133.36 113.44) (xy 131.48 113.44) (xy 131.48 102.1) (xy 125.26 102.1)
        (xy 125.26 111.13) (xy 123.7 111.13) (xy 123.7 102.1) (xy 118.55 102.1) (xy 118.55 109.21)
        (xy 117.26 109.21) (xy 117.26 102.1) (xy 113 102.1) (xy 113 107.63) (xy 111.93 107.63)
        (xy 111.93 102.1) (xy 108.4 102.1) (xy 108.4 106.32) (xy 107.51 106.32) (xy 107.51 102.1)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 100 97.9) (xy 100 102.1) (xy 105.6 102.1) (xy 105.6 105.75) (xy 106.4 105.75)
        (xy 106.4 102.1) (xy 109.62 102.1) (xy 109.62 106.94) (xy 110.59 106.94) (xy 110.59 102.1)
        (xy 114.47 102.1) (xy 114.47 108.38) (xy 115.65 108.38) (xy 115.65 102.1) (xy 120.33 102.1)
        (xy 120.33 110.12) (xy 121.75 110.12) (xy 121.75 102.1) (xy 127.41 102.1) (xy 127.41 112.23)
        (xy 129.12 112.23) (xy 129.12 102.1) (xy 135.96 102.1) (xy 135.96 114.76) (xy 138.03 114.76)
        (xy 138.03 102.1) (xy 146.28 102.1) (xy 146.28 117.83) (xy 148.78 117.83) (xy 148.78 102.1)
        (xy 158.74 102.1) (xy 158.74 121.53) (xy 161.76 121.53) (xy 161.76 102.1) (xy 173.8 102.1)
        (xy 173.8 126) (xy 177.44 126) (xy 177.44 97.9) (xy 169.23 97.9) (xy 169.23 76.34)
        (xy 165.91 76.34) (xy 165.91 97.9) (xy 154.96 97.9) (xy 154.96 80.41) (xy 152.22 80.41)
        (xy 152.22 97.9) (xy 143.15 97.9) (xy 143.15 83.78) (xy 140.88 83.78) (xy 140.88 97.9)
        (xy 133.36 97.9) (xy 133.36 86.56) (xy 131.48 86.56) (xy 131.48 97.9) (xy 125.26 97.9)
        (xy 125.26 88.87) (xy 123.7 88.87) (xy 123.7 97.9) (xy 118.55 97.9) (xy 118.55 90.79)
        (xy 117.26 90.79) (xy 117.26 97.9) (xy 113 97.9) (xy 113 92.37) (xy 111.93 92.37)
        (xy 111.93 97.9) (xy 108.4 97.9) (xy 108.4 93.68) (xy 107.51 93.68) (xy 107.51 97.9)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254)
    (fill yes (arc_segments 16) (thermal_gap 0) (thermal_bridge_width 0))
    (polygon
      (pts
        (xy 97 96) (xy 179 71) (xy 179 129) (xy 97 104)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Mask) (hatch edge 0.508)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254)
    (fill yes (arc_segments 16) (thermal_gap 0) (thermal_bridge_width 0))
    (polygon
      (pts
        (xy 97 96) (xy 179 71) (xy 179 129) (xy 97 104)
      )
    )
  )
)
