<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.5.2">
<drawing>
<board>
<plain>
<wire x1="3.5" y1="2.5" x2="61.5" y2="2.5" width="0" layer="20"/>
<wire x1="61.5" y1="2.5" x2="65" y2="6" width="0" layer="20" curve="90"/>
<wire x1="65" y1="6" x2="65" y2="29" width="0" layer="20"/>
<wire x1="65" y1="29" x2="61.5" y2="32.5" width="0" layer="20" curve="90"/>
<wire x1="61.5" y1="32.5" x2="3.5" y2="32.5" width="0" layer="20"/>
<wire x1="3.5" y1="32.5" x2="0" y2="29" width="0" layer="20" curve="90"/>
<wire x1="0" y1="29" x2="0" y2="6" width="0" layer="20"/>
<wire x1="0" y1="6" x2="3.5" y2="2.5" width="0" layer="20" curve="90"/>
<hole x="3.5" y="6" drill="2.75"/>
<hole x="3.5" y="29" drill="2.75"/>
<hole x="61.5" y="29" drill="2.75"/>
<hole x="61.5" y="6" drill="2.75"/>
<text>PiGarage</text>
<text>mk1.revB</text>
<text>PiGarage</text>
<text>Stephen Papierski/2020
PinonValleyProjects</text>
<text>CLOSED</text>
<text>BETWEEN</text>
<text>OPEN</text>
<text>DOOR_CTRL</text>
<text>DOOR_CLOSED</text>
<text>DOOR_OPEN</text>
<text>DOOR_CTRL</text>
<text>POWER</text>
</plain>
<libraries>
<library name="eagle_stephen_v1.1">
<packages>
<package name="RPI-GPIO-20X2">
<description>&lt;h3&gt;Plated Through Hole - 2x20&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:40&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_20x2&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="G5LE">
<description>&lt;b&gt;RELAY&lt;/b&gt;&lt;p&gt;
1 x switch, 10 A/120 V AC, 8 A/30 V ADC, Omron</description>
</package>
<package name="SOT23">
<description>&lt;b&gt;SOT-23&lt;/b&gt;</description>
</package>
<package name="JST_2PIN_RIGHT_HEADER">
<description>2-pin JST PH Shrouded Header &lt;br&gt;
2.0mm pitch &lt;br&gt;
https://www.sparkfun.com/products/9749 &lt;br&gt;</description>
</package>
<package name="DUMMY">
<description>&lt;h3&gt;Dummy Footprint&lt;/h3&gt;
&lt;p&gt;NOTHING HERE!!! For when you want a symbol with no package as an option against symbols with a package.&lt;/p&gt;

&lt;p&gt;Devices using:
&lt;ul&gt;&lt;li&gt;BADGERHACK_LOGO&lt;/li&gt;
&lt;li&gt;FRAME-LETTER&lt;/li&gt;&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Resistors&lt;/h3&gt;
This library contains resistors. Reference designator:R. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
<description>&lt;p&gt;&lt;b&gt;Generic 2012 (0805) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="led">
<description>&lt;b&gt;LEDs&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;br&gt;
Extended by Federico Battaglin &lt;author&gt;&amp;lt;federico.rd@fdpinternational.com&amp;gt;&lt;/author&gt; with DUOLED</description>
<packages>
<package name="CHIPLED_1206">
<description>&lt;b&gt;CHIPLED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LG_LY N971.pdf</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J4" library="eagle_stephen_v1.1" package="RPI-GPIO-20X2" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="K1" library="eagle_stephen_v1.1" package="G5LE" value="G5LE">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="SparkFun-Resistors" package="0805" value="10k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value=" "/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="SparkFun-Resistors" package="0805" value="10k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value=" "/>
<attribute name="VALUE"/>
</element>
<element name="LED3" library="led" package="CHIPLED_1206" value="HSMS-C150">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED2" library="led" package="CHIPLED_1206" value="HSMY-C150">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED1" library="led" package="CHIPLED_1206" value="HSMG-C150">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED4" library="led" package="CHIPLED_1206" value="HSMN-C150">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="SparkFun-Resistors" package="0805" value="150">
<attribute name="NAME"/>
<attribute name="PROD_ID" value=" "/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="0805" value="120">
<attribute name="NAME"/>
<attribute name="PROD_ID" value=" "/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="0805" value="200">
<attribute name="NAME"/>
<attribute name="PROD_ID" value=" "/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="SparkFun-Resistors" package="0805" value="680">
<attribute name="NAME"/>
<attribute name="PROD_ID" value=" "/>
<attribute name="VALUE"/>
</element>
<element name="T1" library="eagle_stephen_v1.1" package="SOT23" value="NUD3105">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="eagle_stephen_v1.1" package="JST_2PIN_RIGHT_HEADER" value="JST_2PIN_HEADER">
<attribute name="NAME"/>
</element>
<element name="J2" library="eagle_stephen_v1.1" package="JST_2PIN_RIGHT_HEADER" value="JST_2PIN_HEADER">
<attribute name="NAME"/>
</element>
<element name="J3" library="eagle_stephen_v1.1" package="JST_2PIN_RIGHT_HEADER" value="JST_2PIN_HEADER">
<attribute name="NAME"/>
</element>
<element name="LED5" library="led" package="CHIPLED_1206" value="DNP">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="SparkFun-Resistors" package="0805" value="DNP">
<attribute name="NAME"/>
<attribute name="PROD_ID" value=" "/>
<attribute name="VALUE"/>
</element>
<element name="FRAME1" library="eagle_stephen_v1.1" package="DUMMY" value="FRAME-LETTERNO_PACKAGE">
<attribute name="DESIGNER" value="Stephen Papierski"/>
<attribute name="REV" value="mk1.revB"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="R4" pad="1"/>
<contactref element="R5" pad="1"/>
<contactref element="J4" pad="GND_1"/>
<contactref element="J4" pad="GND"/>
<contactref element="J4" pad="GND_2"/>
<contactref element="J4" pad="GND_3"/>
<contactref element="J4" pad="GND_5"/>
<contactref element="J4" pad="GND_6"/>
<contactref element="J4" pad="GND_7"/>
<contactref element="J4" pad="GND_4"/>
<contactref element="R1" pad="1"/>
<contactref element="R2" pad="1"/>
<contactref element="R3" pad="1"/>
<contactref element="T1" pad="2"/>
<contactref element="R6" pad="1"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="K1" pad="2"/>
<contactref element="T1" pad="3"/>
</signal>
<signal name="N$4">
<contactref element="K1" pad="NO"/>
<contactref element="J3" pad="P1"/>
</signal>
<signal name="N$5">
<contactref element="K1" pad="P"/>
<contactref element="J3" pad="P2"/>
</signal>
<signal name="DOOR_CLOSED">
<contactref element="J4" pad="29"/>
<contactref element="R4" pad="2"/>
<contactref element="J1" pad="P1"/>
</signal>
<signal name="DOOR_OPEN">
<contactref element="R5" pad="2"/>
<contactref element="J4" pad="31"/>
<contactref element="J2" pad="P1"/>
</signal>
<signal name="+5V">
<contactref element="K1" pad="1"/>
<contactref element="J4" pad="+5V"/>
<contactref element="J4" pad="+5V_1"/>
<contactref element="LED4" pad="A"/>
</signal>
<signal name="DOOR_CTRL">
<contactref element="T1" pad="1"/>
<contactref element="J4" pad="33"/>
<contactref element="LED5" pad="A"/>
</signal>
<signal name="+3V3">
<contactref element="J4" pad="+3.3V_OUT"/>
<contactref element="J4" pad="+3.3V_OUT_1"/>
<contactref element="J1" pad="P2"/>
<contactref element="J2" pad="P2"/>
</signal>
<signal name="N$6">
<contactref element="R6" pad="2"/>
<contactref element="LED4" pad="C"/>
</signal>
<signal name="N$7">
<contactref element="LED1" pad="A"/>
<contactref element="J4" pad="11"/>
</signal>
<signal name="N$8">
<contactref element="LED2" pad="A"/>
<contactref element="J4" pad="13"/>
</signal>
<signal name="N$9">
<contactref element="LED3" pad="A"/>
<contactref element="J4" pad="15"/>
</signal>
<signal name="N$11">
<contactref element="LED1" pad="C"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="N$12">
<contactref element="LED2" pad="C"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="N$13">
<contactref element="LED3" pad="C"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="R7" pad="2"/>
<contactref element="LED5" pad="C"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
