(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 62)
    (no_connects 0)
    (area 117.98 69.015 187.43 130.495)
    (thickness 1.6)
    (drawings 14)
    (tracks 94)
    (zones 0)
    (modules 15)
    (nets 69)
  )
  (page USLetter)
  (title_block
    (title "NeoPixel and potentiometer adapter for micro:bit")
    (date 2018-09-03)
    (rev 1.0)
    (company "Patrick Pelletier")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.508)
    (user_trace_width 1.016)
    (trace_clearance 0.2)
    (zone_clearance 0.3048)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 0.6 0.6)
    (pad_drill 0.3)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFEF77F)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerber))
  )
  (net 0 "")
  (net 1 +5V)
  (net 2 GND)
  (net 3 "Net-(C4-Pad1)")
  (net 4 +3V3)
  (net 5 /P0)
  (net 6 /P1)
  (net 7 /P2)
  (net 8 "Net-(J5-Pad80)")
  (net 9 "Net-(J5-Pad78)")
  (net 10 "Net-(J5-Pad76)")
  (net 11 "Net-(J5-Pad74)")
  (net 12 "Net-(J5-Pad72)")
  (net 13 "Net-(J5-Pad70)")
  (net 14 "Net-(J5-Pad68)")
  (net 15 "Net-(J5-Pad66)")
  (net 16 "Net-(J5-Pad64)")
  (net 17 "Net-(J5-Pad62)")
  (net 18 "Net-(J5-Pad60)")
  (net 19 "Net-(J5-Pad58)")
  (net 20 "Net-(J5-Pad56)")
  (net 21 "Net-(J5-Pad54)")
  (net 22 "Net-(J5-Pad52)")
  (net 23 "Net-(J5-Pad50)")
  (net 24 "Net-(J5-Pad48)")
  (net 25 "Net-(J5-Pad46)")
  (net 26 "Net-(J5-Pad44)")
  (net 27 "Net-(J5-Pad4)")
  (net 28 "Net-(J5-Pad2)")
  (net 29 "Net-(J5-Pad6)")
  (net 30 "Net-(J5-Pad8)")
  (net 31 "Net-(J5-Pad10)")
  (net 32 "Net-(J5-Pad12)")
  (net 33 "Net-(J5-Pad14)")
  (net 34 "Net-(J5-Pad16)")
  (net 35 "Net-(J5-Pad18)")
  (net 36 "Net-(J5-Pad20)")
  (net 37 "Net-(J5-Pad22)")
  (net 38 "Net-(J5-Pad24)")
  (net 39 "Net-(J5-Pad26)")
  (net 40 "Net-(J5-Pad28)")
  (net 41 "Net-(J5-Pad30)")
  (net 42 "Net-(J5-Pad32)")
  (net 43 "Net-(J5-Pad34)")
  (net 44 "Net-(J5-Pad36)")
  (net 45 "Net-(J5-Pad38)")
  (net 46 "Net-(J5-Pad40)")
  (net 47 "Net-(J5-Pad42)")
  (net 48 "Net-(R2-Pad1)")
  (net 49 "Net-(U1-Pad8)")
  (net 50 "Net-(U1-Pad11)")
  (net 51 "Net-(U1-Pad6)")
  (net 52 "Net-(J4-Pad1)")
  (net 53 "Net-(J5-Pad13)")
  (net 54 "Net-(J5-Pad15)")
  (net 55 "Net-(J5-Pad29)")
  (net 56 "Net-(J5-Pad31)")
  (net 57 "Net-(J5-Pad33)")
  (net 58 "Net-(J5-Pad35)")
  (net 59 "Net-(J5-Pad45)")
  (net 60 "Net-(J5-Pad47)")
  (net 61 "Net-(J5-Pad49)")
  (net 62 "Net-(J5-Pad51)")
  (net 63 "Net-(J5-Pad53)")
  (net 64 "Net-(J5-Pad63)")
  (net 65 "Net-(J5-Pad65)")
  (net 66 "Net-(J5-Pad67)")
  (net 67 "Net-(J5-Pad69)")
  (net 68 "Net-(J5-Pad79)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net +5V)
    (add_net /P0)
    (add_net /P1)
    (add_net /P2)
    (add_net GND)
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(J4-Pad1)")
    (add_net "Net-(J5-Pad10)")
    (add_net "Net-(J5-Pad12)")
    (add_net "Net-(J5-Pad13)")
    (add_net "Net-(J5-Pad14)")
    (add_net "Net-(J5-Pad15)")
    (add_net "Net-(J5-Pad16)")
    (add_net "Net-(J5-Pad18)")
    (add_net "Net-(J5-Pad2)")
    (add_net "Net-(J5-Pad20)")
    (add_net "Net-(J5-Pad22)")
    (add_net "Net-(J5-Pad24)")
    (add_net "Net-(J5-Pad26)")
    (add_net "Net-(J5-Pad28)")
    (add_net "Net-(J5-Pad29)")
    (add_net "Net-(J5-Pad30)")
    (add_net "Net-(J5-Pad31)")
    (add_net "Net-(J5-Pad32)")
    (add_net "Net-(J5-Pad33)")
    (add_net "Net-(J5-Pad34)")
    (add_net "Net-(J5-Pad35)")
    (add_net "Net-(J5-Pad36)")
    (add_net "Net-(J5-Pad38)")
    (add_net "Net-(J5-Pad4)")
    (add_net "Net-(J5-Pad40)")
    (add_net "Net-(J5-Pad42)")
    (add_net "Net-(J5-Pad44)")
    (add_net "Net-(J5-Pad45)")
    (add_net "Net-(J5-Pad46)")
    (add_net "Net-(J5-Pad47)")
    (add_net "Net-(J5-Pad48)")
    (add_net "Net-(J5-Pad49)")
    (add_net "Net-(J5-Pad50)")
    (add_net "Net-(J5-Pad51)")
    (add_net "Net-(J5-Pad52)")
    (add_net "Net-(J5-Pad53)")
    (add_net "Net-(J5-Pad54)")
    (add_net "Net-(J5-Pad56)")
    (add_net "Net-(J5-Pad58)")
    (add_net "Net-(J5-Pad6)")
    (add_net "Net-(J5-Pad60)")
    (add_net "Net-(J5-Pad62)")
    (add_net "Net-(J5-Pad63)")
    (add_net "Net-(J5-Pad64)")
    (add_net "Net-(J5-Pad65)")
    (add_net "Net-(J5-Pad66)")
    (add_net "Net-(J5-Pad67)")
    (add_net "Net-(J5-Pad68)")
    (add_net "Net-(J5-Pad69)")
    (add_net "Net-(J5-Pad70)")
    (add_net "Net-(J5-Pad72)")
    (add_net "Net-(J5-Pad74)")
    (add_net "Net-(J5-Pad76)")
    (add_net "Net-(J5-Pad78)")
    (add_net "Net-(J5-Pad79)")
    (add_net "Net-(J5-Pad8)")
    (add_net "Net-(J5-Pad80)")
    (add_net "Net-(R2-Pad1)")
    (add_net "Net-(U1-Pad11)")
    (add_net "Net-(U1-Pad6)")
    (add_net "Net-(U1-Pad8)")
  )
  (module Capacitors_THT:CP_Radial_D10.0mm_P5.00mm (layer F.Cu) (tedit 597BC7C2)
    (at 166.37 111.76 180)
    (descr "CP, Radial series, Radial, pin pitch=5.00mm, , diameter=10mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 5.00mm  diameter 10mm Electrolytic Capacitor")
    (fp_text reference C1 (at 2.5 -6.31 180) (layer F.SilkS))
    (fp_text value 1000µF (at 2.5 6.31 180) (layer F.Fab))
    (fp_text user %R (at 2.5 0 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 2 thru_hole circle (at 5 0 180) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D10.0mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Rect_L7.0mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 5B88BF4C)
    (at 140.335 114.3 90)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7*2.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7mm width 2.5mm Capacitor")
    (fp_text reference C2 (at 7.62 0 90) (layer F.SilkS))
    (fp_text value 0.1µF (at 2.5 2.56 90) (layer F.Fab))
    (fp_text user %R (at 2.5 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 2 thru_hole circle (at 5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Rect_L7.0mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Rect_L7.0mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 5B8B1B9F)
    (at 154.94 111.125 270)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7*2.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7mm width 2.5mm Capacitor")
    (fp_text reference C3 (at 2.54 -2.54 270) (layer F.SilkS))
    (fp_text value 1µF (at 2.5 2.56 270) (layer F.Fab))
    (fp_text user %R (at 2.5 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 2 thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Rect_L7.0mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Rect_L7.0mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 5B8B1BB7)
    (at 144.78 111.125 270)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7*2.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7mm width 2.5mm Capacitor")
    (fp_text reference C4 (at -0.635 -2.54 270) (layer F.SilkS))
    (fp_text value 1µF (at 2.5 2.56 270) (layer F.Fab))
    (fp_text user %R (at 2.5 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C4-Pad1)"))
    (pad 2 thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Rect_L7.0mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_THT:D_DO-15_P10.16mm_Horizontal (layer F.Cu) (tedit 5921392E)
    (at 154.94 107.315 180)
    (descr "D, DO-15 series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=7.6*3.6mm^2, , http://www.diodes.com/_files/packages/DO-15.pdf")
    (tags "D DO-15 series Axial Horizontal pin pitch 10.16mm  length 7.6mm diameter 3.6mm")
    (fp_text reference D1 (at 5.08 -2.86 180) (layer F.SilkS))
    (fp_text value D_Schottky (at 5.08 2.86 180) (layer F.Fab))
    (fp_text user %R (at 5.08 0 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 4 +3V3))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 3 "Net-(C4-Pad1)"))
    (model ${KISYS3DMOD}/Diodes_THT.3dshapes/D_DO-15_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:BarrelJack_CUI_PJ-063AH_Horizontal_CircularHoles (layer F.Cu) (tedit 5B0886B5)
    (at 173.355 111.76 90)
    (descr "Barrel Jack, 2.0mm ID, 5.5mm OD, 24V, 8A, no switch, https://www.cui.com/product/resource/pj-063ah.pdf")
    (tags "barrel jack cui dc power")
    (fp_text reference J2 (at 0 -3.3 90) (layer F.SilkS))
    (fp_text value Barrel_Jack_MountingPin (at 0 13 90) (layer F.Fab))
    (fp_text user %R (at 0 5.5 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 4 4) (drill 3) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 2 thru_hole circle (at 0 6 90) (size 3.3 3.3) (drill 2.3) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad MP thru_hole circle (at -4.5 7 90) (size 3.5 3.5) (drill 2.5) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad MP thru_hole circle (at 4.5 7 90) (size 3.5 3.5) (drill 2.5) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad "" np_thru_hole circle (at 0 9 90) (size 1.6 1.6) (drill 1.6) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_BarrelJack.3dshapes/BarrelJack_CUI_PJ-063AH_Horizontal_CircularHoles.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_JST:JST_PH_S3B-PH-K_03x2.00mm_Angled (layer F.Cu) (tedit 5B8B1B72)
    (at 179.07 91.44 90)
    (descr "JST PH series connector, S3B-PH-K, side entry type, through hole, Datasheet: http://www.jst-mfg.com/product/pdf/eng/ePH.pdf")
    (tags "connector jst ph")
    (fp_text reference J4 (at -3.175 5.715 90) (layer F.SilkS))
    (fp_text value NeoPixels (at 2 7.25 90) (layer F.Fab))
    (fp_text user %R (at 2 2.5 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 52 "Net-(J4-Pad1)"))
    (pad 2 thru_hole oval (at 2 0 90) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole oval (at 4 0 90) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 1 +5V))
    (model ${KISYS3DMOD}/Connectors_JST.3dshapes/JST_PH_S3B-PH-K_03x2.00mm_Angled.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5B8B1B88)
    (at 182.88 103.505 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R2 (at -0.635 1.905 90) (layer F.SilkS))
    (fp_text value 470 (at 3.81 2.31 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 48 "Net-(R2-Pad1)"))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 52 "Net-(J4-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-14_W7.62mm (layer F.Cu) (tedit 5B8B1B46)
    (at 136.525 107.95 270)
    (descr "14-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U1 (at 8.89 -1.905 270) (layer F.SilkS))
    (fp_text value 74AHCT125 (at 3.81 17.57 270) (layer F.Fab))
    (fp_text user %R (at 3.81 7.62 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 8 thru_hole oval (at 7.62 15.24 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 49 "Net-(U1-Pad8)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 /P0))
    (pad 9 thru_hole oval (at 7.62 12.7 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 48 "Net-(R2-Pad1)"))
    (pad 10 thru_hole oval (at 7.62 10.16 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 11 thru_hole oval (at 7.62 7.62 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 50 "Net-(U1-Pad11)"))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 12 thru_hole oval (at 7.62 5.08 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 51 "Net-(U1-Pad6)"))
    (pad 13 thru_hole oval (at 7.62 2.54 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 7 thru_hole oval (at 0 15.24 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 14 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 +5V))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-14_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-92_Inline_Narrow_Oval (layer F.Cu) (tedit 5B8B1BC2)
    (at 151.13 113.03 180)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.6mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference U2 (at 3.175 -3.175 180) (layer F.SilkS))
    (fp_text value MCP1702-3302E_TO92 (at 1.27 2.79 180) (layer F.Fab))
    (fp_text user %R (at 1.27 -3.56 180) (layer F.Fab))
    (pad 2 thru_hole oval (at 1.27 0) (size 0.9 1.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 3 thru_hole oval (at 2.54 0) (size 0.9 1.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 3 "Net-(C4-Pad1)"))
    (pad 1 thru_hole rect (at 0 0) (size 0.9 1.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-92_Inline_Narrow_Oval.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module footprints:4UCON_10156_90deg (layer F.Cu) (tedit 5B8B1B5F)
    (at 172.72 91.44 180)
    (descr "BBC micro:bit right-angle edge connector")
    (tags "bbc microbit edge connector right-angle")
    (fp_text reference J5 (at 22.86 -2.54 180) (layer F.SilkS))
    (fp_text value microbit_edge_connector (at 24.765 21.45 180) (layer F.Fab))
    (fp_text user %R (at 24.765 9.515 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 0 3.8 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 28 "Net-(J5-Pad2)"))
    (pad 3 thru_hole circle (at 1.27 1.9 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole circle (at 1.27 5.7 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 27 "Net-(J5-Pad4)"))
    (pad 5 thru_hole circle (at 2.54 0 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 6 thru_hole circle (at 2.54 3.8 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 29 "Net-(J5-Pad6)"))
    (pad 7 thru_hole circle (at 3.81 1.9 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 8 thru_hole circle (at 3.81 5.7 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 30 "Net-(J5-Pad8)"))
    (pad 9 thru_hole circle (at 5.08 0 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 10 thru_hole circle (at 5.08 3.8 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 31 "Net-(J5-Pad10)"))
    (pad 11 thru_hole circle (at 6.35 1.9 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 12 thru_hole circle (at 6.35 5.7 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 32 "Net-(J5-Pad12)"))
    (pad 13 thru_hole circle (at 7.62 0 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 53 "Net-(J5-Pad13)"))
    (pad 14 thru_hole circle (at 7.62 3.8 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 33 "Net-(J5-Pad14)"))
    (pad 15 thru_hole circle (at 8.89 1.9 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 54 "Net-(J5-Pad15)"))
    (pad 16 thru_hole circle (at 8.89 5.7 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 34 "Net-(J5-Pad16)"))
    (pad 17 thru_hole circle (at 10.16 0 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 4 +3V3))
    (pad 18 thru_hole circle (at 10.16 3.8 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 35 "Net-(J5-Pad18)"))
    (pad 19 thru_hole circle (at 11.43 1.9 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 4 +3V3))
    (pad 20 thru_hole circle (at 11.43 5.7 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 36 "Net-(J5-Pad20)"))
    (pad 21 thru_hole circle (at 12.7 0 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 4 +3V3))
    (pad 22 thru_hole circle (at 12.7 3.8 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 37 "Net-(J5-Pad22)"))
    (pad 23 thru_hole circle (at 13.97 1.9 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 4 +3V3))
    (pad 24 thru_hole circle (at 13.97 5.7 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 38 "Net-(J5-Pad24)"))
    (pad 25 thru_hole circle (at 15.24 0 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 4 +3V3))
    (pad 26 thru_hole circle (at 15.24 3.8 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 39 "Net-(J5-Pad26)"))
    (pad 27 thru_hole circle (at 16.51 1.9 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 4 +3V3))
    (pad 28 thru_hole circle (at 16.51 5.7 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 40 "Net-(J5-Pad28)"))
    (pad 29 thru_hole circle (at 17.78 0 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 55 "Net-(J5-Pad29)"))
    (pad 30 thru_hole circle (at 17.78 3.8 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 41 "Net-(J5-Pad30)"))
    (pad 31 thru_hole circle (at 19.05 1.9 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 56 "Net-(J5-Pad31)"))
    (pad 32 thru_hole circle (at 19.05 5.7 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 42 "Net-(J5-Pad32)"))
    (pad 33 thru_hole circle (at 20.32 0 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 57 "Net-(J5-Pad33)"))
    (pad 34 thru_hole circle (at 20.32 3.8 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 43 "Net-(J5-Pad34)"))
    (pad 35 thru_hole circle (at 21.59 1.9 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 58 "Net-(J5-Pad35)"))
    (pad 36 thru_hole circle (at 21.59 5.7 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 44 "Net-(J5-Pad36)"))
    (pad 37 thru_hole circle (at 22.86 0 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 7 /P2))
    (pad 38 thru_hole circle (at 22.86 3.8 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 45 "Net-(J5-Pad38)"))
    (pad 39 thru_hole circle (at 24.13 1.9 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 7 /P2))
    (pad 40 thru_hole circle (at 24.13 5.7 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 46 "Net-(J5-Pad40)"))
    (pad 41 thru_hole circle (at 25.4 0 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 7 /P2))
    (pad 42 thru_hole circle (at 25.4 3.8 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 47 "Net-(J5-Pad42)"))
    (pad 43 thru_hole circle (at 26.67 1.9 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 7 /P2))
    (pad 44 thru_hole circle (at 26.67 5.7 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 26 "Net-(J5-Pad44)"))
    (pad 45 thru_hole circle (at 27.94 0 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 59 "Net-(J5-Pad45)"))
    (pad 46 thru_hole circle (at 27.94 3.8 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 25 "Net-(J5-Pad46)"))
    (pad 47 thru_hole circle (at 29.21 1.9 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 60 "Net-(J5-Pad47)"))
    (pad 48 thru_hole circle (at 29.21 5.7 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(J5-Pad48)"))
    (pad 49 thru_hole circle (at 30.48 0 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 61 "Net-(J5-Pad49)"))
    (pad 50 thru_hole circle (at 30.48 3.8 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(J5-Pad50)"))
    (pad 51 thru_hole circle (at 31.75 1.9 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 62 "Net-(J5-Pad51)"))
    (pad 52 thru_hole circle (at 31.75 5.7 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(J5-Pad52)"))
    (pad 53 thru_hole circle (at 33.02 0 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 63 "Net-(J5-Pad53)"))
    (pad 54 thru_hole circle (at 33.02 3.8 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(J5-Pad54)"))
    (pad 55 thru_hole circle (at 34.29 1.9 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 6 /P1))
    (pad 56 thru_hole circle (at 34.29 5.7 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(J5-Pad56)"))
    (pad 57 thru_hole circle (at 35.56 0 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 6 /P1))
    (pad 58 thru_hole circle (at 35.56 3.8 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(J5-Pad58)"))
    (pad 59 thru_hole circle (at 36.83 1.9 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 6 /P1))
    (pad 60 thru_hole circle (at 36.83 5.7 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(J5-Pad60)"))
    (pad 61 thru_hole circle (at 38.1 0 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 6 /P1))
    (pad 62 thru_hole circle (at 38.1 3.8 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(J5-Pad62)"))
    (pad 63 thru_hole circle (at 39.37 1.9 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 64 "Net-(J5-Pad63)"))
    (pad 64 thru_hole circle (at 39.37 5.7 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(J5-Pad64)"))
    (pad 65 thru_hole circle (at 40.64 0 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 65 "Net-(J5-Pad65)"))
    (pad 66 thru_hole circle (at 40.64 3.8 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(J5-Pad66)"))
    (pad 67 thru_hole circle (at 41.91 1.9 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 66 "Net-(J5-Pad67)"))
    (pad 68 thru_hole circle (at 41.91 5.7 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(J5-Pad68)"))
    (pad 69 thru_hole circle (at 43.18 0 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 67 "Net-(J5-Pad69)"))
    (pad 70 thru_hole circle (at 43.18 3.8 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(J5-Pad70)"))
    (pad 71 thru_hole circle (at 44.45 1.9 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 5 /P0))
    (pad 72 thru_hole circle (at 44.45 5.7 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(J5-Pad72)"))
    (pad 73 thru_hole circle (at 45.72 0 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 5 /P0))
    (pad 74 thru_hole circle (at 45.72 3.8 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(J5-Pad74)"))
    (pad 75 thru_hole circle (at 46.99 1.9 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 5 /P0))
    (pad 76 thru_hole circle (at 46.99 5.7 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(J5-Pad76)"))
    (pad 77 thru_hole circle (at 48.26 0 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 5 /P0))
    (pad 78 thru_hole circle (at 48.26 3.8 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(J5-Pad78)"))
    (pad 79 thru_hole circle (at 49.53 1.9 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 68 "Net-(J5-Pad79)"))
    (pad 80 thru_hole circle (at 49.53 5.7 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(J5-Pad80)"))
    (model ${KISYS3DMOD}/Connectors_4UCON.3dshapes/4UCON_10156_90deg.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:Bourns_PTA4543 (layer F.Cu) (tedit 5B8B1B53)
    (at 120.65 97.79)
    (descr "Bourns single-gang slide potentiometer, 45mm travel")
    (tags "Bourns single-gang slide potentiometer 45mm")
    (fp_text reference RV1 (at 16.51 7.62) (layer F.SilkS))
    (fp_text value 10K (at 29.25 7.5) (layer F.Fab))
    (fp_text user %R (at 29.25 1.75) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.2 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 0 3.5) (size 2.2 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 6 /P1))
    (pad 3 thru_hole circle (at 58.5 0) (size 2.2 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 4 +3V3))
    (pad MP thru_hole circle (at 5.35 -2.45) (size 2.7 2.7) (drill 1.7) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad MP thru_hole circle (at 53.15 -2.45) (size 2.7 2.7) (drill 1.7) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad MP thru_hole circle (at 4.15 5.95) (size 2.7 2.7) (drill 1.7) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad MP thru_hole circle (at 54.35 5.95) (size 2.7 2.7) (drill 1.7) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Potentiometers_THT.3dshapes/Bourns_PTA4543.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:Bourns_PTA4543 (layer F.Cu) (tedit 5B8B0252)
    (at 120.65 121.92)
    (descr "Bourns single-gang slide potentiometer, 45mm travel")
    (tags "Bourns single-gang slide potentiometer 45mm")
    (fp_text reference RV2 (at 29.25 -4) (layer F.SilkS))
    (fp_text value 10K (at 29.25 7.5) (layer F.Fab))
    (fp_text user %R (at 29.25 1.75) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.2 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 0 3.5) (size 2.2 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 7 /P2))
    (pad 3 thru_hole circle (at 58.5 0) (size 2.2 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 4 +3V3))
    (pad MP thru_hole circle (at 5.35 -2.45) (size 2.7 2.7) (drill 1.7) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad MP thru_hole circle (at 53.15 -2.45) (size 2.7 2.7) (drill 1.7) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad MP thru_hole circle (at 4.15 5.95) (size 2.7 2.7) (drill 1.7) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad MP thru_hole circle (at 54.35 5.95) (size 2.7 2.7) (drill 1.7) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Potentiometers_THT.3dshapes/Bourns_PTA4543.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:Fingerprint (layer B.Cu) (tedit 0)
    (at 165.1 121.92 180)
    (fp_text reference G*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (module Symbols:OSHW-Symbol_6.7x6mm_SilkScreen (layer B.Cu) (tedit 0)
    (at 139.7 121.92 180)
    (descr "Open Source Hardware Symbol")
    (tags "Logo Symbol OSHW")
    (attr virtual)
    (fp_text reference REF*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value OSHW-Symbol_6.7x6mm_SilkScreen (at 0.75 0 180) (layer B.Fab) hide)
  )
  (gr_text NeoPixels (at 185 89.5 90) (layer B.SilkS))
  (gr_text "5VDC IN" (at 184.785 111.76 90) (layer B.SilkS))
  (gr_text DATA (at 180.5 91.5) (layer B.SilkS))
  (gr_text GND (at 180.5 89.5) (layer B.SilkS))
  (gr_text 5V (at 180.5 87.5) (layer B.SilkS))
  (gr_text "2018-09-03\nhttps://github.com/ppelleti/NeoBit\ndesigned by Patrick Pelletier" (at 154.94 99.06) (layer B.SilkS))
  (gr_line (start 183.515 83.82) (end 121.285 83.82) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 186.055 127) (end 186.055 86.36) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 121.285 129.54) (end 183.515 129.54) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 118.745 86.36) (end 118.745 127) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 183.515 127) (end 186.055 127) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 183.515 86.36) (end 183.515 83.82) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 121.285 127) (end 121.285 129.54) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 121.285 86.36) (end 118.745 86.36) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name +5V) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 181.61 85.725) (xy 181.61 115.57) (xy 163.83 115.57) (xy 163.83 95.25) (xy 173.99 85.725)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 186.055 129.54) (xy 118.745 129.54) (xy 118.745 83.82) (xy 186.055 83.82)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 186.055 129.54) (xy 118.745 129.54) (xy 118.745 83.82) (xy 186.055 83.82)
      )
    )
  )
)
