(kicad_pcb (version 4) (host pcbnew 4.0.4+e1-6308~48~ubuntu16.04.1-stable)
  (general
    (links 24)
    (no_connects 0)
    (area 148.885 94.073809 172.927334 114.627)
    (thickness 1.6)
    (drawings 8)
    (tracks 122)
    (zones 0)
    (modules 11)
    (nets 12)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.7)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 149.9 113)
    (grid_origin 149.9 113)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin true)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerber/))
  )
  (net 0 "")
  (net 1 VCC)
  (net 2 GND)
  (net 3 "Net-(D1-Pad1)")
  (net 4 "Net-(D1-Pad2)")
  (net 5 "Net-(D2-Pad2)")
  (net 6 "Net-(D2-Pad1)")
  (net 7 "Net-(D3-Pad2)")
  (net 8 "Net-(D3-Pad1)")
  (net 9 "Net-(P1-Pad3)")
  (net 10 "Net-(P1-Pad2)")
  (net 11 +3V3)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.7)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net GND)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D3-Pad1)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(P1-Pad2)")
    (add_net "Net-(P1-Pad3)")
    (add_net VCC)
  )
  (module LEDs:LED_1206 (layer F.Cu) (tedit 5857E855)
    (at 168.8 99.65 180)
    (descr "LED 1206 smd package")
    (tags "LED1206 SMD")
    (attr smd)
    (fp_text reference D2 (at 0 -2 180) (layer F.SilkS) hide)
    (fp_text value "LED green" (at 0 2 180) (layer F.Fab) hide)
    (pad 2 smd rect (at 1.41986 0) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D2-Pad2)"))
    (pad 1 smd rect (at -1.41986 0) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D2-Pad1)"))
    (model LEDs.3dshapes/LED_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Housings_SSOP:SSOP-28_5.3x10.2mm_Pitch0.65mm (layer F.Cu) (tedit 5857E840)
    (at 161.03 106.97 180)
    (descr "28-Lead Plastic Shrink Small Outline (SS)-5.30 mm Body [SSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U1 (at 0 -6.25 180) (layer F.SilkS) hide)
    (fp_text value FT232RL (at 0 6.25 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -3.6 -4.225 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D3-Pad2)"))
    (pad 2 smd rect (at -3.6 -3.575 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at -3.6 -2.925 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at -3.6 -2.275 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 11 +3V3))
    (pad 5 smd rect (at -3.6 -1.625 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D3-Pad1)"))
    (pad 6 smd rect (at -3.6 -0.975 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask))
    (pad 7 smd rect (at -3.6 -0.325 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 8 smd rect (at -3.6 0.325 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask))
    (pad 9 smd rect (at -3.6 0.975 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask))
    (pad 10 smd rect (at -3.6 1.625 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask))
    (pad 11 smd rect (at -3.6 2.275 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask))
    (pad 12 smd rect (at -3.6 2.925 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask))
    (pad 13 smd rect (at -3.6 3.575 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask))
    (pad 14 smd rect (at -3.6 4.225 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask))
    (pad 15 smd rect (at 3.6 4.225 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(P1-Pad3)"))
    (pad 16 smd rect (at 3.6 3.575 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(P1-Pad2)"))
    (pad 17 smd rect (at 3.6 2.925 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 11 +3V3))
    (pad 18 smd rect (at 3.6 2.275 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 19 smd rect (at 3.6 1.625 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask))
    (pad 20 smd rect (at 3.6 0.975 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 21 smd rect (at 3.6 0.325 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 22 smd rect (at 3.6 -0.325 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D2-Pad1)"))
    (pad 23 smd rect (at 3.6 -0.975 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(D1-Pad1)"))
    (pad 24 smd rect (at 3.6 -1.625 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask))
    (pad 25 smd rect (at 3.6 -2.275 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 26 smd rect (at 3.6 -2.925 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask))
    (pad 27 smd rect (at 3.6 -3.575 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask))
    (pad 28 smd rect (at 3.6 -4.225 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask))
    (model Housings_SSOP.3dshapes/SSOP-28_5.3x10.2mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 5857E816)
    (at 158.84 99.69)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C3 (at 0.01 0.06) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 2.3) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.5 0) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 11 +3V3))
    (pad 2 smd rect (at 1.5 0) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 5857E81E)
    (at 163.74 99.68)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C1 (at 0.01 0.02) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 2.3) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.5 0) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at 1.5 0) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_Tantalum_SMD:Tantalum_Case-C_EIA-6032-28_Hand (layer B.Cu) (tedit 585834F5)
    (at 161.036 106.934 90)
    (descr "Tantalum capacitor, Case C, EIA 6032-28, 6.0x3.2x2.5mm, Hand soldering footprint")
    (tags "capacitor tantalum smd")
    (attr smd)
    (fp_text reference C2 (at 0 3.35 90) (layer B.SilkS) hide)
    (fp_text value 10µF (at 0 -3.35 90) (layer B.Fab))
    (pad 1 smd rect (at -3.125 0 90) (size 3.75 2.5) (layers B.Cu B.Paste B.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at 3.125 0 90) (size 3.75 2.5) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_Tantalum_SMD.3dshapes/Tantalum_Case-C_EIA-6032-28.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer B.Cu) (tedit 5857E84D)
    (at 168.91 111.252 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R1 (at 0 2.3 180) (layer B.SilkS) hide)
    (fp_text value 330 (at 0 -2.3 180) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 11 +3V3))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(D1-Pad2)"))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer B.Cu) (tedit 5857E85B)
    (at 168.8 99.65 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R2 (at 0 2.3 180) (layer B.SilkS) hide)
    (fp_text value 330 (at 0 -2.3 180) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 11 +3V3))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(D2-Pad2)"))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_1206 (layer F.Cu) (tedit 5857E845)
    (at 168.91 111.252 180)
    (descr "LED 1206 smd package")
    (tags "LED1206 SMD")
    (attr smd)
    (fp_text reference D1 (at 0 -2 180) (layer F.SilkS) hide)
    (fp_text value "LED red" (at 0 2 180) (layer F.Fab) hide)
    (pad 2 smd rect (at 1.41986 0) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at -1.41986 0) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(D1-Pad1)"))
    (model LEDs.3dshapes/LED_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module SMD_Packages:SMD-1206_Pol (layer B.Cu) (tedit 585834F0)
    (at 165.1 105.41 270)
    (attr smd)
    (fp_text reference D3 (at 0 0 270) (layer B.SilkS) hide)
    (fp_text value "TS 4148" (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -1.651 0 270) (size 1.524 2.032) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(D3-Pad1)"))
    (pad 2 smd rect (at 1.651 0 270) (size 1.524 2.032) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(D3-Pad2)"))
    (model SMD_Packages.3dshapes/SMD-1206_Pol.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.17 0.16 0.16))
      (rotate (xyz 0 0 0))
    )
  )
  (module LUM2410-08:LUM2410-08 (layer F.Cu) (tedit 5857EB5F)
    (at 152.4 105.41 270)
    (fp_text reference P1 (at -10.16 2.54 270) (layer F.SilkS) hide)
    (fp_text value USB_A (at -8.6 -5.7 270) (layer F.Fab) hide)
    (pad "" thru_hole oval (at 5.7 0 270) (size 1.6 4) (drill oval 1 2.5) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at -5.7 0 270) (size 1.6 4) (drill oval 1 2.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 2.25 0 270) (size 1.8 1.8) (drill 1.1) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at -2.25 0 270) (size 1.8 1.8) (drill 1.1) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 1 -2.1 270) (size 1.6 1.6) (drill 0.92) (layers *.Cu *.Mask)
      (net 10 "Net-(P1-Pad2)"))
    (pad 3 thru_hole circle (at -1 -2.1 270) (size 1.6 1.6) (drill 0.92) (layers *.Cu *.Mask)
      (net 9 "Net-(P1-Pad3)"))
    (pad 1 thru_hole circle (at 3.5 -2.1 270) (size 1.6 1.6) (drill 0.92) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 4 thru_hole circle (at -3.5 -2.1 270) (size 1.6 1.6) (drill 0.92) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 58583F44)
    (at 167.894 102.87)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P2 (at 0 -5.1) (layer F.SilkS) hide)
    (fp_text value CONN_01X03 (at 0 -3.1) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 8 "Net-(D3-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (gr_text G (at 170.434 107.95) (layer B.SilkS))
  (gr_text S (at 170.434 102.87) (layer B.SilkS))
  (gr_text "Rev 1.0" (at 162.052 99.568) (layer B.SilkS))
  (gr_text USBtele (at 157.226 105.664 90) (layer B.SilkS))
  (gr_line (start 171.704 113.03) (end 171.704 97.79) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 171.704 113.03) (end 149.86 113.03) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 149.86 97.79) (end 171.704 97.79) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 149.86 113.03) (end 149.86 97.79) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 171.958 113.284) (xy 149.606 113.284) (xy 149.606 97.536) (xy 171.958 97.536)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 171.958 113.284) (xy 149.606 113.284) (xy 149.606 97.536) (xy 171.958 97.536)
      )
    )
  )
)
