(kicad_pcb (version 4) (host pcbnew 4.0.5)
  (general
    (links 27)
    (no_connects 0)
    (area 132.761667 57.709999 168.863334 133.425001)
    (thickness 1.6)
    (drawings 4)
    (tracks 24)
    (zones 0)
    (modules 10)
    (nets 4)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 3.175)
    (trace_clearance 0.2)
    (zone_clearance 0.2032)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 +12V)
  (net 2 GND)
  (net 3 +5V)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +12V)
    (add_net +5V)
    (add_net GND)
  )
  (module Connectors:molex-77-156-4 (layer F.Cu) (tedit 5CF50EB3)
    (at 144.78 63.5)
    (fp_text reference P1 (at 0.127 3.048) (layer F.SilkS))
    (fp_text value CONN_01X04 (at 5.715 2.54) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 3.175 3.175) (drill 1.524) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 2 thru_hole circle (at 3.9624 0) (size 3.175 3.175) (drill 1.524) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole circle (at 7.9248 0) (size 3.175 3.175) (drill 1.524) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole circle (at 11.8872 0) (size 3.175 3.175) (drill 1.524) (layers *.Cu *.Mask)
      (net 3 +5V))
  )
  (module Connectors:molex-77-156-4 (layer F.Cu) (tedit 5CF50EB7)
    (at 144.78 76.2)
    (fp_text reference P2 (at 0.127 3.556) (layer F.SilkS))
    (fp_text value CONN_01X04 (at 5.715 2.54) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 3.175 3.175) (drill 1.524) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 2 thru_hole circle (at 3.9624 0) (size 3.175 3.175) (drill 1.524) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole circle (at 7.9248 0) (size 3.175 3.175) (drill 1.524) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole circle (at 11.8872 0) (size 3.175 3.175) (drill 1.524) (layers *.Cu *.Mask)
      (net 3 +5V))
  )
  (module Connectors:molex-77-156-4 (layer F.Cu) (tedit 5CF50EC4)
    (at 144.78 101.6)
    (fp_text reference P3 (at 0 3.302) (layer F.SilkS))
    (fp_text value CONN_01X04 (at 5.715 2.54) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 3.175 3.175) (drill 1.524) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 2 thru_hole circle (at 3.9624 0) (size 3.175 3.175) (drill 1.524) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole circle (at 7.9248 0) (size 3.175 3.175) (drill 1.524) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole circle (at 11.8872 0) (size 3.175 3.175) (drill 1.524) (layers *.Cu *.Mask)
      (net 3 +5V))
  )
  (module Connectors:molex-77-156-4 (layer F.Cu) (tedit 5CF50EC9)
    (at 144.78 114.3)
    (fp_text reference P4 (at -0.254 3.302) (layer F.SilkS))
    (fp_text value CONN_01X04 (at 5.715 2.54) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 3.175 3.175) (drill 1.524) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 2 thru_hole circle (at 3.9624 0) (size 3.175 3.175) (drill 1.524) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole circle (at 7.9248 0) (size 3.175 3.175) (drill 1.524) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole circle (at 11.8872 0) (size 3.175 3.175) (drill 1.524) (layers *.Cu *.Mask)
      (net 3 +5V))
  )
  (module Connectors:molex-77-156-4 (layer F.Cu) (tedit 5CF50ECC)
    (at 144.78 127)
    (fp_text reference P5 (at 0 -3.048) (layer F.SilkS))
    (fp_text value CONN_01X04 (at 5.715 2.54) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 3.175 3.175) (drill 1.524) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 2 thru_hole circle (at 3.9624 0) (size 3.175 3.175) (drill 1.524) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole circle (at 7.9248 0) (size 3.175 3.175) (drill 1.524) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole circle (at 11.8872 0) (size 3.175 3.175) (drill 1.524) (layers *.Cu *.Mask)
      (net 3 +5V))
  )
  (module Connectors:molex-77-156-6 (layer F.Cu) (tedit 5CF50EBD)
    (at 140.97 88.9)
    (fp_text reference P6 (at 0 3.175) (layer F.SilkS))
    (fp_text value CONN_01X06 (at 15.24 -3.81) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 3.175 3.175) (drill 1.524) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 2 thru_hole circle (at 3.9624 0) (size 3.175 3.175) (drill 1.524) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 3 thru_hole circle (at 7.9248 0) (size 3.175 3.175) (drill 1.524) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole circle (at 11.8872 0) (size 3.175 3.175) (drill 1.524) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 5 thru_hole circle (at 15.8496 0) (size 3.175 3.175) (drill 1.524) (layers *.Cu *.Mask)
      (net 3 +5V))
    (pad 6 thru_hole circle (at 19.812 0) (size 3.175 3.175) (drill 1.524) (layers *.Cu *.Mask)
      (net 3 +5V))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_Pad (layer F.Cu) (tedit 5CF50EEC)
    (at 137.795 120.65)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (attr virtual)
    (fp_text reference P7 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 4.2) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_Pad (layer F.Cu) (tedit 5CF50EE7)
    (at 163.83 120.65)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (attr virtual)
    (fp_text reference P8 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 4.2) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_Pad (layer F.Cu) (tedit 5CF50EE1)
    (at 163.83 69.85)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (attr virtual)
    (fp_text reference P9 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 4.2) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_Pad (layer F.Cu) (tedit 5CF50EDC)
    (at 137.795 69.85)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (attr virtual)
    (fp_text reference P10 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 4.2) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (gr_line (start 133.985 133.35) (end 167.64 133.35) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 133.985 57.785) (end 133.985 133.35) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 167.64 57.785) (end 133.985 57.785) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 167.64 133.35) (end 167.64 57.785) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2032))
    (min_thickness 0.1778)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 167.005 132.715) (xy 134.62 132.715) (xy 134.62 58.42) (xy 167.005 58.42)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2032))
    (min_thickness 0.1778)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 167.005 132.715) (xy 134.62 132.715) (xy 134.62 58.42) (xy 167.005 58.42)
      )
    )
  )
)
