(kicad_pcb (version 20171130) (host pcbnew 5.1.6-c6e7f7d~87~ubuntu20.04.1)
  (general
    (thickness 1.6)
    (drawings 19)
    (tracks 55)
    (zones 0)
    (modules 3)
    (nets 9)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.1778)
    (user_trace_width 0.2032)
    (user_trace_width 0.254)
    (user_trace_width 0.4064)
    (trace_clearance 0.1778)
    (zone_clearance 0.1524)
    (zone_45_only no)
    (trace_min 0.1778)
    (via_size 0.4064)
    (via_drill 0.254)
    (via_min_size 0.4064)
    (via_min_drill 0.254)
    (user_via 0.4064 0.254)
    (uvia_size 0.4064)
    (uvia_drill 0.254)
    (uvias_allowed no)
    (uvia_min_size 0.4064)
    (uvia_min_drill 0.254)
    (edge_width 0.0254)
    (segment_width 0.1778)
    (pcb_text_width 0.2032)
    (pcb_text_size 1.2192 1.2192)
    (mod_edge_width 0.127)
    (mod_text_size 0.7112 0.7112)
    (mod_text_width 0.1016)
    (pad_size 1.7 1.7)
    (pad_drill 1)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (grid_origin 147.32 96.52)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 /DTR)
  (net 2 /DCD)
  (net 3 GND)
  (net 4 /CTS)
  (net 5 /RTS)
  (net 6 /RX)
  (net 7 /TX)
  (net 8 /DSR)
  (net_class Default "This is the default net class."
    (clearance 0.1778)
    (trace_width 0.1778)
    (via_dia 0.4064)
    (via_drill 0.254)
    (uvia_dia 0.4064)
    (uvia_drill 0.254)
    (diff_pair_width 0.1778)
    (diff_pair_gap 0.1778)
    (add_net /CTS)
    (add_net /DCD)
    (add_net /DSR)
    (add_net /DTR)
    (add_net /RTS)
    (add_net /RX)
    (add_net /TX)
    (add_net GND)
  )
  (module 0_LOCAL:DSUB-25_Female_Vertical_P2.77x2.84mm (layer B.Cu) (tedit 5F5851B1)
    (at 131.1572 88.2904 180)
    (descr "25-pin D-Sub connector, straight/vertical, THT-mount, female, pitch 2.77x2.84mm, distance of mounting holes 47.1mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf")
    (tags "25-pin D-Sub connector straight vertical THT female pitch 2.77x2.84mm mounting holes distance 47.1mm")
    (fp_text reference J2 (at 0 -1.4478 180) (layer B.SilkS))
    (fp_text value "DB25 Female" (at 5.54 -8.73 180) (layer B.Fab))
    (fp_text user %R (at 5.54 -1.42 180) (layer B.Fab))
    (pad 25 thru_hole circle (at -31.855 -2.84 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask))
    (pad 24 thru_hole circle (at -29.085 -2.84 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask))
    (pad 23 thru_hole circle (at -26.315 -2.84 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask))
    (pad 22 thru_hole circle (at -23.545 -2.84 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask))
    (pad 21 thru_hole circle (at -20.775 -2.84 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask))
    (pad 20 thru_hole circle (at -18.005 -2.84 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask)
      (net 1 /DTR))
    (pad 19 thru_hole circle (at -15.235 -2.84 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask))
    (pad 18 thru_hole circle (at -12.465 -2.84 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask))
    (pad 17 thru_hole circle (at -9.695 -2.84 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask))
    (pad 16 thru_hole circle (at -6.925 -2.84 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask))
    (pad 15 thru_hole circle (at -4.155 -2.84 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask))
    (pad 14 thru_hole circle (at -1.385 -2.84 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask))
    (pad 13 thru_hole circle (at -33.24 0 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask))
    (pad 12 thru_hole circle (at -30.47 0 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask))
    (pad 11 thru_hole circle (at -27.7 0 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask))
    (pad 10 thru_hole circle (at -24.93 0 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask))
    (pad 9 thru_hole circle (at -22.16 0 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask))
    (pad 8 thru_hole circle (at -19.39 0 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask)
      (net 2 /DCD))
    (pad 7 thru_hole circle (at -16.62 0 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 6 thru_hole circle (at -13.85 0 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask)
      (net 8 /DSR))
    (pad 5 thru_hole circle (at -11.08 0 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask)
      (net 4 /CTS))
    (pad 4 thru_hole circle (at -8.31 0 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask)
      (net 5 /RTS))
    (pad 3 thru_hole circle (at -5.54 0 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask)
      (net 6 /RX))
    (pad 2 thru_hole circle (at -2.77 0 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask)
      (net 7 /TX))
    (pad 1 thru_hole roundrect (at 0 0 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask) (roundrect_rratio 0.1)
      (net 3 GND))
    (model ${KIPRJMOD}/0_LOCAL.3dshapes/DSUB25_Female_v_t_cut.step
      (offset (xyz -16.62 -1.42 6.2992))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 0_LOCAL:DSUB-9_Male_Vertical_P2.77x2.84mm (layer F.Cu) (tedit 5F57BF9C)
    (at 142.24 95.758)
    (descr "9-pin D-Sub connector, straight/vertical, THT-mount, male, pitch 2.77x2.84mm, distance of mounting holes 25mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf")
    (tags "9-pin D-Sub connector straight vertical THT male pitch 2.77x2.84mm mounting holes distance 25mm")
    (fp_text reference J1 (at 0 -1.524) (layer F.SilkS))
    (fp_text value DE9_Male (at 5.54 8.73) (layer F.Fab))
    (fp_text user %R (at 5.54 1.42) (layer F.Fab))
    (pad 9 thru_hole circle (at 9.695 2.84) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask)
      (net 1 /DTR))
    (pad 8 thru_hole circle (at 6.925 2.84) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask)
      (net 2 /DCD))
    (pad 7 thru_hole circle (at 4.155 2.84) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 6 thru_hole circle (at 1.385 2.84) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask))
    (pad 5 thru_hole circle (at 11.08 0) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask)
      (net 4 /CTS))
    (pad 4 thru_hole circle (at 8.31 0) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask)
      (net 5 /RTS))
    (pad 3 thru_hole circle (at 5.54 0) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask)
      (net 6 /RX))
    (pad 2 thru_hole circle (at 2.77 0) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask)
      (net 7 /TX))
    (pad 1 thru_hole roundrect (at 0 0) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask) (roundrect_rratio 0.1))
    (model ${KIPRJMOD}/0_LOCAL.3dshapes/A_DS_9_PP_Z_cut.step
      (offset (xyz 5.54 -1.42 6.3))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 0_LOCAL:NetTie-2_SMD_10 (layer B.Cu) (tedit 5F3D08F8)
    (at 147.7772 89.7382 180)
    (descr "Net tie, 2 pin, 0.5mm square SMD pads")
    (tags "net tie")
    (attr virtual)
    (fp_text reference NT1 (at 0 1.2) (layer B.SilkS) hide)
    (fp_text value Net-Tie_2 (at 0 -1.2) (layer B.Fab) hide)
    (pad 2 smd circle (at 0.254 0 180) (size 0.254 0.254) (layers B.Cu)
      (net 8 /DSR))
    (pad 1 smd circle (at -0.254 0 180) (size 0.254 0.254) (layers B.Cu)
      (net 2 /DCD))
  )
  (gr_arc (start 156.6926 94.5134) (end 156.6926 91.9734) (angle -90) (layer Edge.Cuts) (width 0.0254))
  (gr_arc (start 138.8618 94.5134) (end 141.4018 94.5134) (angle -90) (layer Edge.Cuts) (width 0.0254))
  (gr_text "Z88 to \"Model T\" RS-232 github.com/bkw777/Z88_RS232" (at 147.7772 89.7382) (layer F.SilkS))
  (gr_text "DB25F THIS SIDE" (at 147.7772 89.7382) (layer B.SilkS))
  (gr_text "DE9M THIS SIDE" (at 147.7772 97.2312) (layer F.SilkS))
  (gr_line (start 165.227 88.2904) (end 165.227 90.1954) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 156.6926 91.9734) (end 163.449 91.9734) (layer Edge.Cuts) (width 0.0254))
  (gr_arc (start 163.449 90.1954) (end 163.449 91.9734) (angle -90) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 131.1656 87.4522) (end 164.3888 87.4522) (layer Edge.Cuts) (width 0.0254))
  (gr_arc (start 164.3888 88.2904) (end 165.227 88.2904) (angle -90) (layer Edge.Cuts) (width 0.0254))
  (gr_arc (start 131.1656 88.2904) (end 131.1656 87.4522) (angle -90) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 138.8618 91.9734) (end 132.1054 91.9734) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 141.4018 97.663) (end 141.4018 94.5134) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 152.3746 99.441) (end 143.1798 99.441) (layer Edge.Cuts) (width 0.0254))
  (gr_arc (start 143.1798 97.663) (end 141.4018 97.663) (angle -90) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 154.1526 97.663) (end 154.1526 94.5134) (layer Edge.Cuts) (width 0.0254))
  (gr_arc (start 132.1054 90.1954) (end 130.3274 90.1954) (angle -90) (layer Edge.Cuts) (width 0.0254))
  (gr_arc (start 152.3746 97.663) (end 152.3746 99.441) (angle -90) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 130.3274 90.1954) (end 130.3274 88.2904) (layer Edge.Cuts) (width 0.0254))
  (zone (net 3) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.0762))
    (polygon
      (pts
        (xy 166.878 101.854) (xy 128.524 101.854) (xy 128.524 85.598) (xy 166.878 85.598)
      )
    )
  )
  (zone (net 3) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.0762))
    (polygon
      (pts
        (xy 166.878 101.854) (xy 128.524 101.854) (xy 128.524 85.598) (xy 166.878 85.598)
      )
    )
  )
)
