(kicad_pcb (version 20171130) (host pcbnew 5.0.2-1.fc29)
  (general
    (thickness 1.6)
    (drawings 33)
    (tracks 51)
    (zones 0)
    (modules 6)
    (nets 16)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.1524)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.6858)
    (uvia_drill 0.3302)
    (uvias_allowed no)
    (uvia_min_size 0.6858)
    (uvia_min_drill 0.3302)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.2 0.9)
    (pad_drill 0)
    (pad_to_mask_clearance 0.2)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(A1-Pad1)")
  (net 3 +3V3)
  (net 4 "Net-(J1-Pad2)")
  (net 5 "Net-(J1-Pad3)")
  (net 6 "Net-(J1-Pad4)")
  (net 7 "Net-(J1-Pad5)")
  (net 8 "Net-(J1-Pad6)")
  (net 9 "Net-(J1-Pad7)")
  (net 10 "Net-(J2-Pad1)")
  (net 11 "Net-(J2-Pad3)")
  (net 12 "Net-(J2-Pad4)")
  (net 13 "Net-(J2-Pad6)")
  (net 14 "Net-(J2-Pad7)")
  (net 15 "Net-(J2-Pad8)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (add_net +3V3)
    (add_net GND)
    (add_net "Net-(A1-Pad1)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J1-Pad7)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J2-Pad4)")
    (add_net "Net-(J2-Pad6)")
    (add_net "Net-(J2-Pad7)")
    (add_net "Net-(J2-Pad8)")
  )
  (module "My Footprints:Aerial_SMA_Regular" (layer F.Cu) (tedit 5A6F91B6)
    (at 148.629115 97.750331)
    (fp_text reference A1 (at -14.644115 3.849669) (layer F.SilkS) hide)
    (fp_text value Antenna_Shield (at 0 -5.120331) (layer F.Fab) hide)
    (pad 2 thru_hole circle (at -2.499115 -2.500331 90) (size 1.8 1.8) (drill 1.3) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at -2.499115 2.499669 90) (size 1.8 1.8) (drill 1.3) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.500885 2.499669 90) (size 1.8 1.8) (drill 1.3) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.500885 -2.500331 90) (size 1.8 1.8) (drill 1.3) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0.000885 -0.000331 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 "Net-(A1-Pad1)"))
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 5A6F91F8)
    (at 145.73 112.141)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at -13.65 0.889) (layer B.SilkS) hide)
    (fp_text value 10uF (at -12.38 -8.89) (layer B.Fab) hide)
    (fp_text user %R (at -13.65 -0.635) (layer B.Fab) hide)
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 5A6F91FA)
    (at 145.73 110.8456)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at -13.7008 -2.0828) (layer B.SilkS) hide)
    (fp_text value 0.1uF (at -12.38 -5.715) (layer B.Fab) hide)
    (fp_text user %R (at -13.65 -0.635) (layer B.Fab) hide)
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x08_Pitch2.54mm (layer F.Cu) (tedit 5A6F88BE)
    (at 160.02 116.84 180)
    (descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x08 2.54mm single row")
    (fp_text reference J1 (at -2.54 0 180) (layer F.SilkS) hide)
    (fp_text value CONN_01X08 (at -2.54 8.89 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 8.89 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(J1-Pad6)"))
    (pad 7 thru_hole oval (at 0 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(J1-Pad7)"))
    (pad 8 thru_hole oval (at 0 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x08_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x08_Pitch2.54mm (layer F.Cu) (tedit 5A6F88BB)
    (at 137.16 99.06)
    (descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x08 2.54mm single row")
    (fp_text reference J2 (at -1.905 17.78) (layer F.SilkS) hide)
    (fp_text value CONN_01X08 (at -2.54 8.89 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 8.89 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(J2-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(J2-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(J2-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +3V3))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(J2-Pad6)"))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(J2-Pad7)"))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(J2-Pad8)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x08_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "My Footprints:RFM95W" (layer F.Cu) (tedit 5A6F88B8)
    (at 148.5011 109.84 180)
    (fp_text reference U1 (at -14.0589 8.875 180) (layer F.SilkS) hide)
    (fp_text value RFM95W (at 18.5039 -5.065 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -7.7 -7 180) (size 3 1.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -7.7 -5 180) (size 3 1.4) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J1-Pad2)"))
    (pad 3 smd rect (at -7.7 -3 180) (size 3 1.4) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(J1-Pad3)"))
    (pad 4 smd rect (at -7.7 -1 180) (size 3 1.4) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(J1-Pad4)"))
    (pad 5 smd rect (at -7.7 1 180) (size 3 1.4) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(J1-Pad5)"))
    (pad 6 smd rect (at -7.7 3 180) (size 3 1.4) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(J1-Pad6)"))
    (pad 7 smd rect (at -7.7 5 180) (size 3 1.4) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(J1-Pad7)"))
    (pad 8 smd rect (at -7.7 7 180) (size 3 1.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 9 smd rect (at 7.7 7 180) (size 3 1.4) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(J2-Pad1)"))
    (pad 10 smd rect (at 7.7 5 180) (size 3 1.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 11 smd rect (at 7.7 3 180) (size 3 1.4) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(J2-Pad3)"))
    (pad 12 smd rect (at 7.7 1 180) (size 3 1.4) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(J2-Pad4)"))
    (pad 13 smd rect (at 7.7 -1 180) (size 3 1.4) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 14 smd rect (at 7.7 -3 180) (size 3 1.4) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(J2-Pad6)"))
    (pad 15 smd rect (at 7.7 -5 180) (size 3 1.4) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(J2-Pad7)"))
    (pad 16 smd rect (at 7.7 -7 180) (size 3 1.4) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(J2-Pad8)"))
  )
  (gr_text NC (at 140.055458 99.042182 180) (layer B.SilkS))
  (gr_text C2 (at 148.59 110.7948 180) (layer B.SilkS))
  (gr_text C1 (at 148.59 112.0902 180) (layer B.SilkS))
  (gr_text A1 (at 148.59 99.695 180) (layer F.SilkS))
  (gr_text GND (at 158.623 116.84 180) (layer B.SilkS))
  (gr_text DIO5 (at 158.623 101.6 180) (layer B.SilkS))
  (gr_text ~RESET (at 158.496 104.14 180) (layer B.SilkS))
  (gr_text NSS (at 158.623 106.68 180) (layer B.SilkS))
  (gr_text SCK (at 158.623 109.22 180) (layer B.SilkS))
  (gr_text MOSI (at 158.623 111.76 180) (layer B.SilkS))
  (gr_text MISO (at 158.623 114.3 180) (layer B.SilkS))
  (gr_text DIO2 (at 138.531458 116.822182 180) (layer B.SilkS))
  (gr_text DIO1 (at 138.531458 114.282182 180) (layer B.SilkS))
  (gr_text DIO0 (at 138.531458 111.742182 180) (layer B.SilkS))
  (gr_text 3.3V (at 138.594958 109.265682 180) (layer B.SilkS))
  (gr_text DIO4 (at 138.531458 106.662182 180) (layer B.SilkS))
  (gr_text DIO3 (at 138.531458 104.185682 180) (layer B.SilkS))
  (gr_text GND (at 138.594958 101.582182 180) (layer B.SilkS))
  (gr_text GND (at 158.623 99.06 180) (layer B.SilkS))
  (gr_text 9 (at 137.16 96.901 180) (layer B.SilkS))
  (gr_text 8 (at 160.02 96.901) (layer B.SilkS))
  (gr_text "Breakout\nv0.1" (at 155.575 95.25 180) (layer B.SilkS))
  (gr_text RFM95W (at 140.97 95.25 180) (layer B.SilkS))
  (gr_text 8 (at 160.02 96.901) (layer F.SilkS))
  (gr_text 9 (at 137.16 96.901 180) (layer F.SilkS))
  (gr_text "(c) packom.net\n2018" (at 148.59 115.443 180) (layer B.SilkS))
  (gr_text "Breakout\nv0.1" (at 141.605 95.25 180) (layer F.SilkS))
  (gr_text RFM95W (at 156.21 95.25 180) (layer F.SilkS))
  (gr_text RFM95W (at 148.59 106.045 180) (layer F.SilkS))
  (gr_line (start 161.29 93.345) (end 135.89 93.345) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 161.29 118.11) (end 161.29 93.345) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 135.89 118.11) (end 135.89 93.345) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 161.29 118.11) (end 135.89 118.11) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 161.29 118.11) (xy 161.29 93.345) (xy 135.89 93.345) (xy 135.89 118.11)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.SilkS) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 153.67 102.235) (xy 153.67 109.22) (xy 143.51 109.22) (xy 143.51 102.235)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 161.29 93.345) (xy 135.89 93.345) (xy 135.89 118.11) (xy 161.29 118.11)
      )
    )
  )
)
