(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 166)
    (no_connects 0)
    (area 134.290999 107.874999 159.841001 133.425001)
    (thickness 1.6)
    (drawings 5)
    (tracks 218)
    (zones 0)
    (modules 133)
    (nets 30)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.254)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 0.5 0.5)
    (mod_text_width 0.1)
    (pad_size 2.032 1.7)
    (pad_drill 1)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (grid_origin 134.366 107.95)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer false)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 4)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 /IF_I)
  (net 3 "Net-(C2-Pad1)")
  (net 4 GND)
  (net 5 "Net-(C3-Pad1)")
  (net 6 +3.3V)
  (net 7 "Net-(C5-Pad1)")
  (net 8 "Net-(C5-Pad2)")
  (net 9 "Net-(C6-Pad1)")
  (net 10 /OUT_I)
  (net 11 "Net-(C7-Pad2)")
  (net 12 "Net-(C8-Pad1)")
  (net 13 /IF_Q)
  (net 14 "Net-(C9-Pad1)")
  (net 15 "Net-(C10-Pad1)")
  (net 16 "Net-(C12-Pad1)")
  (net 17 "Net-(C12-Pad2)")
  (net 18 "Net-(C13-Pad1)")
  (net 19 /OUT_Q)
  (net 20 "Net-(C14-Pad2)")
  (net 21 "Net-(R4-Pad1)")
  (net 22 "Net-(R7-Pad1)")
  (net 23 "Net-(R13-Pad1)")
  (net 24 "Net-(R16-Pad1)")
  (net 25 "Net-(RV1-Pad3)")
  (net 26 "Net-(RV2-Pad3)")
  (net 27 3.3V_FILT)
  (net 28 /VCO)
  (net 29 "Net-(P3-Pad4)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3.3V)
    (add_net /IF_I)
    (add_net /IF_Q)
    (add_net /OUT_I)
    (add_net /OUT_Q)
    (add_net /VCO)
    (add_net 3.3V_FILT)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C10-Pad1)")
    (add_net "Net-(C12-Pad1)")
    (add_net "Net-(C12-Pad2)")
    (add_net "Net-(C13-Pad1)")
    (add_net "Net-(C14-Pad2)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(C5-Pad2)")
    (add_net "Net-(C6-Pad1)")
    (add_net "Net-(C7-Pad2)")
    (add_net "Net-(C8-Pad1)")
    (add_net "Net-(C9-Pad1)")
    (add_net "Net-(P3-Pad4)")
    (add_net "Net-(R13-Pad1)")
    (add_net "Net-(R16-Pad1)")
    (add_net "Net-(R4-Pad1)")
    (add_net "Net-(R7-Pad1)")
    (add_net "Net-(RV1-Pad3)")
    (add_net "Net-(RV2-Pad3)")
  )
  (module Pin_Headers:Pin_Header_Straight_1x04_Pitch2.54mm (layer F.Cu) (tedit 5B0D7551)
    (at 152.146 131.826 270)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference P3 (at 0 -2.33 270) (layer F.SilkS) hide)
    (fp_text value CONN_01X04 (at 0 9.95 270) (layer F.Fab) hide)
    (fp_text user %R (at 0.127 -1.905 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.032 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 2.032 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 2.032 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 "Net-(P3-Pad4)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x04_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module radar_amplifier_footprints:via_stitch (layer F.Cu) (tedit 5B048F0B)
    (at 151.1935 123.5075)
    (fp_text reference REF** (at 0 1.9) (layer F.SilkS) hide)
    (fp_text value via_stitch (at 0 -1.8) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.4) (layers *.Cu)
      (net 4 GND))
  )
  (module radar_amplifier_footprints:via_stitch (layer F.Cu) (tedit 5B048E7F)
    (at 145.0975 127.508)
    (fp_text reference REF** (at 0 1.9) (layer F.SilkS) hide)
    (fp_text value via_stitch (at 0 -1.8) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.4) (layers *.Cu)
      (net 4 GND))
  )
  (module radar_amplifier_footprints:via_stitch (layer F.Cu) (tedit 5B048ED4)
    (at 148.844 127.1905)
    (fp_text reference REF** (at 0 1.9) (layer F.SilkS) hide)
    (fp_text value via_stitch (at 0 -1.8) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.4) (layers *.Cu)
      (net 4 GND))
  )
  (module radar_amplifier_footprints:via_stitch (layer F.Cu) (tedit 5B048E3B)
    (at 142.748 122.2375)
    (fp_text reference REF** (at 0 1.9) (layer F.SilkS) hide)
    (fp_text value via_stitch (at 0 -1.8) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.4) (layers *.Cu)
      (net 4 GND))
  )
  (module radar_amplifier_footprints:via_stitch (layer F.Cu) (tedit 5B048E24)
    (at 142.6845 120.3325)
    (fp_text reference REF** (at 0 1.9) (layer F.SilkS) hide)
    (fp_text value via_stitch (at 0 -1.8) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.4) (layers *.Cu)
      (net 4 GND))
  )
  (module radar_amplifier_footprints:via_stitch (layer F.Cu) (tedit 5B048DD4)
    (at 142.5575 112.7125)
    (fp_text reference REF** (at 0 1.9) (layer F.SilkS) hide)
    (fp_text value via_stitch (at 0 -1.8) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.4) (layers *.Cu)
      (net 4 GND))
  )
  (module radar_amplifier_footprints:via_stitch (layer F.Cu) (tedit 5B048DF5)
    (at 153.2255 113.9825)
    (fp_text reference REF** (at 0 1.9) (layer F.SilkS) hide)
    (fp_text value via_stitch (at 0 -1.8) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.4) (layers *.Cu)
      (net 4 GND))
  )
  (module radar_amplifier_footprints:via_stitch (layer F.Cu) (tedit 5B048DF5)
    (at 157.6705 115.189)
    (fp_text reference REF** (at 0 1.9) (layer F.SilkS) hide)
    (fp_text value via_stitch (at 0 -1.8) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.4) (layers *.Cu)
      (net 4 GND))
  )
  (module radar_amplifier_footprints:via_stitch (layer F.Cu) (tedit 5B048EF2)
    (at 156.718 128.143)
    (fp_text reference REF** (at 0 1.9) (layer F.SilkS) hide)
    (fp_text value via_stitch (at 0 -1.8) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.4) (layers *.Cu)
      (net 4 GND))
  )
  (module radar_amplifier_footprints:via_stitch (layer F.Cu) (tedit 5B048EFF)
    (at 153.543 128.651)
    (fp_text reference REF** (at 0 1.9) (layer F.SilkS) hide)
    (fp_text value via_stitch (at 0 -1.8) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.4) (layers *.Cu)
      (net 4 GND))
  )
  (module radar_amplifier_footprints:via_stitch (layer F.Cu) (tedit 5B048EFF)
    (at 150.4315 128.0795)
    (fp_text reference REF** (at 0 1.9) (layer F.SilkS) hide)
    (fp_text value via_stitch (at 0 -1.8) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.4) (layers *.Cu)
      (net 4 GND))
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 5B0734CC)
    (at 150.8365 128.905 180)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C10 (at 0 0 360) (layer F.SilkS))
    (fp_text value 100uF (at 0 2.3 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.5 0 180) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(C10-Pad1)"))
    (pad 2 smd rect (at 1.5 0 180) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module radar_amplifier_footprints:via_stitch (layer F.Cu) (tedit 5B048E76)
    (at 144.399 129.2225)
    (fp_text reference REF** (at 0 1.9) (layer F.SilkS) hide)
    (fp_text value via_stitch (at 0 -1.8) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.4) (layers *.Cu)
      (net 4 GND))
  )
  (module radar_amplifier_footprints:via_stitch (layer F.Cu) (tedit 5B048E01)
    (at 148.717 116.3955)
    (fp_text reference REF** (at 0 1.9) (layer F.SilkS) hide)
    (fp_text value via_stitch (at 0 -1.8) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.4) (layers *.Cu)
      (net 4 GND))
  )
  (module radar_amplifier_footprints:via_stitch (layer F.Cu) (tedit 5B048E01)
    (at 140.7795 112.903)
    (fp_text reference REF** (at 0 1.9) (layer F.SilkS) hide)
    (fp_text value via_stitch (at 0 -1.8) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.4) (layers *.Cu)
      (net 4 GND))
  )
  (module radar_amplifier_footprints:via_stitch (layer F.Cu) (tedit 5B048E4C)
    (at 138.8745 125.349)
    (fp_text reference REF** (at 0 1.9) (layer F.SilkS) hide)
    (fp_text value via_stitch (at 0 -1.8) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.4) (layers *.Cu)
      (net 4 GND))
  )
  (module radar_amplifier_footprints:via_stitch (layer F.Cu) (tedit 5B048D0B)
    (at 142.621 108.7755)
    (fp_text reference REF** (at 0 1.9) (layer F.SilkS) hide)
    (fp_text value via_stitch (at 0 -1.8) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.4) (layers *.Cu)
      (net 4 GND))
  )
  (module radar_amplifier_footprints:via_stitch (layer F.Cu) (tedit 5B048DDA)
    (at 151.0665 113.2205)
    (fp_text reference REF** (at 0 1.9) (layer F.SilkS) hide)
    (fp_text value via_stitch (at 0 -1.8) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.4) (layers *.Cu)
      (net 4 GND))
  )
  (module radar_amplifier_footprints:via_stitch (layer F.Cu) (tedit 5B048DD4)
    (at 146.939 113.665)
    (fp_text reference REF** (at 0 1.9) (layer F.SilkS) hide)
    (fp_text value via_stitch (at 0 -1.8) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.4) (layers *.Cu)
      (net 4 GND))
  )
  (module radar_amplifier_footprints:via_stitch (layer F.Cu) (tedit 5B048DD4)
    (at 144.5895 113.411)
    (fp_text reference REF** (at 0 1.9) (layer F.SilkS) hide)
    (fp_text value via_stitch (at 0 -1.8) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.4) (layers *.Cu)
      (net 4 GND))
  )
  (module radar_amplifier_footprints:via_stitch (layer F.Cu) (tedit 5B048DF5)
    (at 152.4635 113.2205)
    (fp_text reference REF** (at 0 1.9) (layer F.SilkS) hide)
    (fp_text value via_stitch (at 0 -1.8) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.4) (layers *.Cu)
      (net 4 GND))
  )
  (module radar_amplifier_footprints:via_stitch (layer F.Cu) (tedit 5B048EF2)
    (at 155.3845 120.8405)
    (fp_text reference REF** (at 0 1.9) (layer F.SilkS) hide)
    (fp_text value via_stitch (at 0 -1.8) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.4) (layers *.Cu)
      (net 4 GND))
  )
  (module radar_amplifier_footprints:via_stitch (layer F.Cu) (tedit 5B048F0B)
    (at 156.718 125.476)
    (fp_text reference REF** (at 0 1.9) (layer F.SilkS) hide)
    (fp_text value via_stitch (at 0 -1.8) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.4) (layers *.Cu)
      (net 4 GND))
  )
  (module radar_amplifier_footprints:via_stitch (layer F.Cu) (tedit 5B048F0B)
    (at 149.6695 125.5395)
    (fp_text reference REF** (at 0 1.9) (layer F.SilkS) hide)
    (fp_text value via_stitch (at 0 -1.8) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.4) (layers *.Cu)
      (net 4 GND))
  )
  (module radar_amplifier_footprints:via_stitch (layer F.Cu) (tedit 5B048F0B)
    (at 153.416 125.603)
    (fp_text reference REF** (at 0 1.9) (layer F.SilkS) hide)
    (fp_text value via_stitch (at 0 -1.8) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.4) (layers *.Cu)
      (net 4 GND))
  )
  (module radar_amplifier_footprints:via_stitch (layer F.Cu) (tedit 5B048EF2)
    (at 158.623 124.46)
    (fp_text reference REF** (at 0 1.9) (layer F.SilkS) hide)
    (fp_text value via_stitch (at 0 -1.8) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.4) (layers *.Cu)
      (net 4 GND))
  )
  (module radar_amplifier_footprints:via_stitch (layer F.Cu) (tedit 5B048EF2)
    (at 156.718 123.698)
    (fp_text reference REF** (at 0 1.9) (layer F.SilkS) hide)
    (fp_text value via_stitch (at 0 -1.8) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.4) (layers *.Cu)
      (net 4 GND))
  )
  (module radar_amplifier_footprints:via_stitch (layer F.Cu) (tedit 5B048EF2)
    (at 158.75 127.8255)
    (fp_text reference REF** (at 0 1.9) (layer F.SilkS) hide)
    (fp_text value via_stitch (at 0 -1.8) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.4) (layers *.Cu)
      (net 4 GND))
  )
  (module radar_amplifier_footprints:via_stitch (layer F.Cu) (tedit 5B048EF2)
    (at 155.702 128.651)
    (fp_text reference REF** (at 0 1.9) (layer F.SilkS) hide)
    (fp_text value via_stitch (at 0 -1.8) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.4) (layers *.Cu)
      (net 4 GND))
  )
  (module radar_amplifier_footprints:via_stitch (layer F.Cu) (tedit 5B048EF2)
    (at 157.48 131.2545)
    (fp_text reference REF** (at 0 1.9) (layer F.SilkS) hide)
    (fp_text value via_stitch (at 0 -1.8) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.4) (layers *.Cu)
      (net 4 GND))
  )
  (module radar_amplifier_footprints:via_stitch (layer F.Cu) (tedit 5B048DF5)
    (at 156.718 116.713)
    (fp_text reference REF** (at 0 1.9) (layer F.SilkS) hide)
    (fp_text value via_stitch (at 0 -1.8) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.4) (layers *.Cu)
      (net 4 GND))
  )
  (module radar_amplifier_footprints:via_stitch (layer F.Cu) (tedit 5B048DF5)
    (at 157.5435 116.713)
    (fp_text reference REF** (at 0 1.9) (layer F.SilkS) hide)
    (fp_text value via_stitch (at 0 -1.8) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.4) (layers *.Cu)
      (net 4 GND))
  )
  (module radar_amplifier_footprints:via_stitch (layer F.Cu) (tedit 5B048DF5)
    (at 154.8765 117.348)
    (fp_text reference REF** (at 0 1.9) (layer F.SilkS) hide)
    (fp_text value via_stitch (at 0 -1.8) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.4) (layers *.Cu)
      (net 4 GND))
  )
  (module radar_amplifier_footprints:via_stitch (layer F.Cu) (tedit 5B048DF5)
    (at 156.6545 113.7285)
    (fp_text reference REF** (at 0 1.9) (layer F.SilkS) hide)
    (fp_text value via_stitch (at 0 -1.8) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.4) (layers *.Cu)
      (net 4 GND))
  )
  (module radar_amplifier_footprints:via_stitch (layer F.Cu) (tedit 5B048E06)
    (at 158.8135 110.871)
    (fp_text reference REF** (at 0 1.9) (layer F.SilkS) hide)
    (fp_text value via_stitch (at 0 -1.8) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.4) (layers *.Cu)
      (net 4 GND))
  )
  (module radar_amplifier_footprints:via_stitch (layer F.Cu) (tedit 5B048E06)
    (at 154.7495 110.744)
    (fp_text reference REF** (at 0 1.9) (layer F.SilkS) hide)
    (fp_text value via_stitch (at 0 -1.8) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.4) (layers *.Cu)
      (net 4 GND))
  )
  (module radar_amplifier_footprints:via_stitch (layer F.Cu) (tedit 5B048E0D)
    (at 157.734 109.7915)
    (fp_text reference REF** (at 0 1.9) (layer F.SilkS) hide)
    (fp_text value via_stitch (at 0 -1.8) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.4) (layers *.Cu)
      (net 4 GND))
  )
  (module radar_amplifier_footprints:via_stitch (layer F.Cu) (tedit 5B048DF5)
    (at 154.7495 108.6485)
    (fp_text reference REF** (at 0 1.9) (layer F.SilkS) hide)
    (fp_text value via_stitch (at 0 -1.8) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.4) (layers *.Cu)
      (net 4 GND))
  )
  (module radar_amplifier_footprints:via_stitch (layer F.Cu) (tedit 5B048E01)
    (at 140.716 116.586)
    (fp_text reference REF** (at 0 1.9) (layer F.SilkS) hide)
    (fp_text value via_stitch (at 0 -1.8) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.4) (layers *.Cu)
      (net 4 GND))
  )
  (module radar_amplifier_footprints:via_stitch (layer F.Cu) (tedit 5B048E01)
    (at 137.3505 117.1575)
    (fp_text reference REF** (at 0 1.9) (layer F.SilkS) hide)
    (fp_text value via_stitch (at 0 -1.8) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.4) (layers *.Cu)
      (net 4 GND))
  )
  (module radar_amplifier_footprints:via_stitch (layer F.Cu) (tedit 5B048E01)
    (at 137.3505 119.6975)
    (fp_text reference REF** (at 0 1.9) (layer F.SilkS) hide)
    (fp_text value via_stitch (at 0 -1.8) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.4) (layers *.Cu)
      (net 4 GND))
  )
  (module radar_amplifier_footprints:via_stitch (layer F.Cu) (tedit 5B048E01)
    (at 142.875 116.459)
    (fp_text reference REF** (at 0 1.9) (layer F.SilkS) hide)
    (fp_text value via_stitch (at 0 -1.8) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.4) (layers *.Cu)
      (net 4 GND))
  )
  (module radar_amplifier_footprints:via_stitch (layer F.Cu) (tedit 5B048E01)
    (at 141.5415 117.729)
    (fp_text reference REF** (at 0 1.9) (layer F.SilkS) hide)
    (fp_text value via_stitch (at 0 -1.8) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.4) (layers *.Cu)
      (net 4 GND))
  )
  (module radar_amplifier_footprints:via_stitch (layer F.Cu) (tedit 5B048E01)
    (at 148.209 119.1895)
    (fp_text reference REF** (at 0 1.9) (layer F.SilkS) hide)
    (fp_text value via_stitch (at 0 -1.8) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.4) (layers *.Cu)
      (net 4 GND))
  )
  (module radar_amplifier_footprints:via_stitch (layer F.Cu) (tedit 5B048E01)
    (at 150.876 119.1895)
    (fp_text reference REF** (at 0 1.9) (layer F.SilkS) hide)
    (fp_text value via_stitch (at 0 -1.8) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.4) (layers *.Cu)
      (net 4 GND))
  )
  (module radar_amplifier_footprints:via_stitch (layer F.Cu) (tedit 5B048E01)
    (at 152.8445 116.84)
    (fp_text reference REF** (at 0 1.9) (layer F.SilkS) hide)
    (fp_text value via_stitch (at 0 -1.8) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.4) (layers *.Cu)
      (net 4 GND))
  )
  (module radar_amplifier_footprints:via_stitch (layer F.Cu) (tedit 5B048EFF)
    (at 152.3365 127.4445)
    (fp_text reference REF** (at 0 1.9) (layer F.SilkS) hide)
    (fp_text value via_stitch (at 0 -1.8) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.4) (layers *.Cu)
      (net 4 GND))
  )
  (module radar_amplifier_footprints:via_stitch (layer F.Cu) (tedit 5B048EDE)
    (at 150.876 129.6035)
    (fp_text reference REF** (at 0 1.9) (layer F.SilkS) hide)
    (fp_text value via_stitch (at 0 -1.8) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.4) (layers *.Cu)
      (net 4 GND))
  )
  (module radar_amplifier_footprints:via_stitch (layer F.Cu) (tedit 5B048D4E)
    (at 136.8425 113.411)
    (fp_text reference REF** (at 0 1.9) (layer F.SilkS) hide)
    (fp_text value via_stitch (at 0 -1.8) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.4) (layers *.Cu)
      (net 4 GND))
  )
  (module radar_amplifier_footprints:via_stitch (layer F.Cu) (tedit 5B048E47)
    (at 137.414 122.301)
    (fp_text reference REF** (at 0 1.9) (layer F.SilkS) hide)
    (fp_text value via_stitch (at 0 -1.8) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.4) (layers *.Cu)
      (net 4 GND))
  )
  (module radar_amplifier_footprints:via_stitch (layer F.Cu) (tedit 5B048D2E)
    (at 137.922 110.871)
    (fp_text reference REF** (at 0 1.9) (layer F.SilkS) hide)
    (fp_text value via_stitch (at 0 -1.8) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.4) (layers *.Cu)
      (net 4 GND))
  )
  (module radar_amplifier_footprints:via_stitch (layer F.Cu) (tedit 5B048D53)
    (at 137.8585 114.681)
    (fp_text reference REF** (at 0 1.9) (layer F.SilkS) hide)
    (fp_text value via_stitch (at 0 -1.8) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.4) (layers *.Cu)
      (net 4 GND))
  )
  (module radar_amplifier_footprints:via_stitch (layer F.Cu) (tedit 5B048DD4)
    (at 148.717 113.157)
    (fp_text reference REF** (at 0 1.9) (layer F.SilkS) hide)
    (fp_text value via_stitch (at 0 -1.8) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.4) (layers *.Cu)
      (net 4 GND))
  )
  (module radar_amplifier_footprints:via_stitch (layer F.Cu) (tedit 5B048DF5)
    (at 153.2255 111.633)
    (fp_text reference REF** (at 0 1.9) (layer F.SilkS) hide)
    (fp_text value via_stitch (at 0 -1.8) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.4) (layers *.Cu)
      (net 4 GND))
  )
  (module radar_amplifier_footprints:via_stitch (layer F.Cu) (tedit 5B048E15)
    (at 156.6545 108.712)
    (fp_text reference REF** (at 0 1.9) (layer F.SilkS) hide)
    (fp_text value via_stitch (at 0 -1.8) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.4) (layers *.Cu)
      (net 4 GND))
  )
  (module radar_amplifier_footprints:via_stitch (layer F.Cu) (tedit 5B048E0D)
    (at 158.8135 108.9025)
    (fp_text reference REF** (at 0 1.9) (layer F.SilkS) hide)
    (fp_text value via_stitch (at 0 -1.8) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.4) (layers *.Cu)
      (net 4 GND))
  )
  (module radar_amplifier_footprints:via_stitch (layer F.Cu) (tedit 5B048E7F)
    (at 146.431 125.73)
    (fp_text reference REF** (at 0 1.9) (layer F.SilkS) hide)
    (fp_text value via_stitch (at 0 -1.8) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.4) (layers *.Cu)
      (net 4 GND))
  )
  (module radar_amplifier_footprints:via_stitch (layer F.Cu) (tedit 5B048E7B)
    (at 145.161 125.73)
    (fp_text reference REF** (at 0 1.9) (layer F.SilkS) hide)
    (fp_text value via_stitch (at 0 -1.8) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.4) (layers *.Cu)
      (net 4 GND))
  )
  (module radar_amplifier_footprints:via_stitch (layer F.Cu) (tedit 5B048F0B)
    (at 158.242 126.1745)
    (fp_text reference REF** (at 0 1.9) (layer F.SilkS) hide)
    (fp_text value via_stitch (at 0 -1.8) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.4) (layers *.Cu)
      (net 4 GND))
  )
  (module radar_amplifier_footprints:via_stitch (layer F.Cu) (tedit 5B048D27)
    (at 139.0015 110.1725)
    (fp_text reference REF** (at 0 1.9) (layer F.SilkS) hide)
    (fp_text value via_stitch (at 0 -1.8) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.4) (layers *.Cu)
      (net 4 GND))
  )
  (module radar_amplifier_footprints:via_stitch (layer F.Cu) (tedit 5B048E2E)
    (at 143.891 120.904)
    (fp_text reference REF** (at 0 1.9) (layer F.SilkS) hide)
    (fp_text value via_stitch (at 0 -1.8) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.4) (layers *.Cu)
      (net 4 GND))
  )
  (module radar_amplifier_footprints:via_stitch (layer F.Cu) (tedit 5B048E29)
    (at 141.7955 121.285)
    (fp_text reference REF** (at 0 1.9) (layer F.SilkS) hide)
    (fp_text value via_stitch (at 0 -1.8) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.4) (layers *.Cu)
      (net 4 GND))
  )
  (module radar_amplifier_footprints:via_stitch (layer F.Cu) (tedit 5B048E24)
    (at 140.843 120.396)
    (fp_text reference REF** (at 0 1.9) (layer F.SilkS) hide)
    (fp_text value via_stitch (at 0 -1.8) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.4) (layers *.Cu)
      (net 4 GND))
  )
  (module radar_amplifier_footprints:via_stitch (layer F.Cu) (tedit 5B048E32)
    (at 141.7955 123.19)
    (fp_text reference REF** (at 0 1.9) (layer F.SilkS) hide)
    (fp_text value via_stitch (at 0 -1.8) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.4) (layers *.Cu)
      (net 4 GND))
  )
  (module radar_amplifier_footprints:via_stitch (layer F.Cu) (tedit 5B048E3B)
    (at 140.7795 122.3645)
    (fp_text reference REF** (at 0 1.9) (layer F.SilkS) hide)
    (fp_text value via_stitch (at 0 -1.8) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.4) (layers *.Cu)
      (net 4 GND))
  )
  (module radar_amplifier_footprints:via_stitch (layer F.Cu) (tedit 5B048E4C)
    (at 137.795 124.587)
    (fp_text reference REF** (at 0 1.9) (layer F.SilkS) hide)
    (fp_text value via_stitch (at 0 -1.8) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.4) (layers *.Cu)
      (net 4 GND))
  )
  (module radar_amplifier_footprints:via_stitch (layer F.Cu) (tedit 5B048E52)
    (at 137.922 126.111)
    (fp_text reference REF** (at 0 1.9) (layer F.SilkS) hide)
    (fp_text value via_stitch (at 0 -1.8) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.4) (layers *.Cu)
      (net 4 GND))
  )
  (module radar_amplifier_footprints:via_stitch (layer F.Cu) (tedit 5B048EF6)
    (at 158.259 129.582)
    (fp_text reference REF** (at 0 1.9) (layer F.SilkS) hide)
    (fp_text value via_stitch (at 0 -1.8) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.4) (layers *.Cu)
      (net 4 GND))
  )
  (module radar_amplifier_footprints:via_stitch (layer F.Cu) (tedit 5B048EF2)
    (at 158.75 132.207)
    (fp_text reference REF** (at 0 1.9) (layer F.SilkS) hide)
    (fp_text value via_stitch (at 0 -1.8) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.4) (layers *.Cu)
      (net 4 GND))
  )
  (module radar_amplifier_footprints:via_stitch (layer F.Cu) (tedit 5B048EED)
    (at 156.1465 132.207)
    (fp_text reference REF** (at 0 1.9) (layer F.SilkS) hide)
    (fp_text value via_stitch (at 0 -1.8) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.4) (layers *.Cu)
      (net 4 GND))
  )
  (module radar_amplifier_footprints:via_stitch (layer F.Cu) (tedit 5B048EE8)
    (at 154.759 131.332)
    (fp_text reference REF** (at 0 1.9) (layer F.SilkS) hide)
    (fp_text value via_stitch (at 0 -1.8) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.4) (layers *.Cu)
      (net 4 GND))
  )
  (module radar_amplifier_footprints:via_stitch (layer F.Cu) (tedit 5B048ED4)
    (at 147.8915 129.4765)
    (fp_text reference REF** (at 0 1.9) (layer F.SilkS) hide)
    (fp_text value via_stitch (at 0 -1.8) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.4) (layers *.Cu)
      (net 4 GND))
  )
  (module radar_amplifier_footprints:via_stitch (layer F.Cu) (tedit 5B048E41)
    (at 140.843 124.333)
    (fp_text reference REF** (at 0 1.9) (layer F.SilkS) hide)
    (fp_text value via_stitch (at 0 -1.8) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.4) (layers *.Cu)
      (net 4 GND))
  )
  (module radar_amplifier_footprints:via_stitch (layer F.Cu) (tedit 5B048E5D)
    (at 140.7795 125.857)
    (fp_text reference REF** (at 0 1.9) (layer F.SilkS) hide)
    (fp_text value via_stitch (at 0 -1.8) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.4) (layers *.Cu)
      (net 4 GND))
  )
  (module radar_amplifier_footprints:via_stitch (layer F.Cu) (tedit 5B048E57)
    (at 138.8745 127.254)
    (fp_text reference REF** (at 0 1.9) (layer F.SilkS) hide)
    (fp_text value via_stitch (at 0 -1.8) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.4) (layers *.Cu)
      (net 4 GND))
  )
  (module radar_amplifier_footprints:via_stitch (layer F.Cu) (tedit 5B048E6C)
    (at 138.557 128.7145)
    (fp_text reference REF** (at 0 1.9) (layer F.SilkS) hide)
    (fp_text value via_stitch (at 0 -1.8) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.4) (layers *.Cu)
      (net 4 GND))
  )
  (module radar_amplifier_footprints:via_stitch (layer F.Cu) (tedit 5B048E8F)
    (at 140.759 129.582)
    (fp_text reference REF** (at 0 1.9) (layer F.SilkS) hide)
    (fp_text value via_stitch (at 0 -1.8) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.4) (layers *.Cu)
      (net 4 GND))
  )
  (module radar_amplifier_footprints:via_stitch (layer F.Cu) (tedit 5B048E9A)
    (at 139.6365 130.556)
    (fp_text reference REF** (at 0 1.9) (layer F.SilkS) hide)
    (fp_text value via_stitch (at 0 -1.8) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.4) (layers *.Cu)
      (net 4 GND))
  )
  (module radar_amplifier_footprints:via_stitch (layer F.Cu) (tedit 5B048E8A)
    (at 136.906 129.794)
    (fp_text reference REF** (at 0 1.9) (layer F.SilkS) hide)
    (fp_text value via_stitch (at 0 -1.8) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.4) (layers *.Cu)
      (net 4 GND))
  )
  (module radar_amplifier_footprints:via_stitch (layer F.Cu) (tedit 5B048E95)
    (at 135.509 130.457)
    (fp_text reference REF** (at 0 1.9) (layer F.SilkS) hide)
    (fp_text value via_stitch (at 0 -1.8) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.4) (layers *.Cu)
      (net 4 GND))
  )
  (module radar_amplifier_footprints:via_stitch (layer F.Cu) (tedit 5B048EAC)
    (at 142.509 132.207)
    (fp_text reference REF** (at 0 1.9) (layer F.SilkS) hide)
    (fp_text value via_stitch (at 0 -1.8) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.4) (layers *.Cu)
      (net 4 GND))
  )
  (module radar_amplifier_footprints:via_stitch (layer F.Cu) (tedit 5B048EB1)
    (at 140.7795 130.556)
    (fp_text reference REF** (at 0 1.9) (layer F.SilkS) hide)
    (fp_text value via_stitch (at 0 -1.8) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.4) (layers *.Cu)
      (net 4 GND))
  )
  (module radar_amplifier_footprints:via_stitch (layer F.Cu) (tedit 5B048EA8)
    (at 139.009 132.207)
    (fp_text reference REF** (at 0 1.9) (layer F.SilkS) hide)
    (fp_text value via_stitch (at 0 -1.8) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.4) (layers *.Cu)
      (net 4 GND))
  )
  (module radar_amplifier_footprints:via_stitch (layer F.Cu) (tedit 5B048E9E)
    (at 137.259 131.332)
    (fp_text reference REF** (at 0 1.9) (layer F.SilkS) hide)
    (fp_text value via_stitch (at 0 -1.8) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.4) (layers *.Cu)
      (net 4 GND))
  )
  (module radar_amplifier_footprints:via_stitch (layer F.Cu) (tedit 5B048EA3)
    (at 135.509 132.207)
    (fp_text reference REF** (at 0 1.9) (layer F.SilkS) hide)
    (fp_text value via_stitch (at 0 -1.8) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.4) (layers *.Cu)
      (net 4 GND))
  )
  (module radar_amplifier_footprints:via_stitch (layer F.Cu) (tedit 5B048D46)
    (at 137.6045 112.649)
    (fp_text reference REF** (at 0 1.9) (layer F.SilkS) hide)
    (fp_text value via_stitch (at 0 -1.8) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.4) (layers *.Cu)
      (net 4 GND))
  )
  (module radar_amplifier_footprints:via_stitch (layer F.Cu) (tedit 5B048D3F)
    (at 135.509 112.593)
    (fp_text reference REF** (at 0 1.9) (layer F.SilkS) hide)
    (fp_text value via_stitch (at 0 -1.8) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.4) (layers *.Cu)
      (net 4 GND))
  )
  (module radar_amplifier_footprints:via_stitch (layer F.Cu) (tedit 5B048D3B)
    (at 137.259 111.718)
    (fp_text reference REF** (at 0 1.9) (layer F.SilkS) hide)
    (fp_text value via_stitch (at 0 -1.8) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.4) (layers *.Cu)
      (net 4 GND))
  )
  (module radar_amplifier_footprints:via_stitch (layer F.Cu) (tedit 5B048D33)
    (at 135.509 110.843)
    (fp_text reference REF** (at 0 1.9) (layer F.SilkS) hide)
    (fp_text value via_stitch (at 0 -1.8) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.4) (layers *.Cu)
      (net 4 GND))
  )
  (module radar_amplifier_footprints:via_stitch (layer F.Cu) (tedit 5B048D22)
    (at 140.9065 111.0615)
    (fp_text reference REF** (at 0 1.9) (layer F.SilkS) hide)
    (fp_text value via_stitch (at 0 -1.8) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.4) (layers *.Cu)
      (net 4 GND))
  )
  (module radar_amplifier_footprints:via_stitch (layer F.Cu) (tedit 5B048D0B)
    (at 139.009 109.093)
    (fp_text reference REF** (at 0 1.9) (layer F.SilkS) hide)
    (fp_text value via_stitch (at 0 -1.8) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.4) (layers *.Cu)
      (net 4 GND))
  )
  (module radar_amplifier_footprints:via_stitch (layer F.Cu) (tedit 5B048D16)
    (at 137.259 109.968)
    (fp_text reference REF** (at 0 1.9) (layer F.SilkS) hide)
    (fp_text value via_stitch (at 0 -1.8) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.4) (layers *.Cu)
      (net 4 GND))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5B043F95)
    (at 139.446 115.57 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at 1.778 -0.508 360) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.9 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 13 /IF_Q))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5B0440B5)
    (at 149.86 113.03 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at 1.778 0 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.9 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5B0441BD)
    (at 152.4 119.253 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C5 (at 1.778 0 180) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.9 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C5-Pad1)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C5-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5B044ABC)
    (at 141.732 112.776 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C7 (at -1.7145 0 360) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.9 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 19 /OUT_Q))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C7-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5B046D46)
    (at 139.192 121.412 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C8 (at -1.778 0 270) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.9 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(C8-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 /IF_I))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5B0462AE)
    (at 145.923 127.5715 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C9 (at -1.8415 0.0635 360) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.9 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(C9-Pad1)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5B046EB1)
    (at 152.4 123.063 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C12 (at 1.905 0 360) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.9 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(C12-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(C12-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5B047AB9)
    (at 156.845 122.809 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C14 (at -1.905 0.0635 270) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.9 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 10 /OUT_I))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(C14-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5B0440A4)
    (at 139.065 117.348)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at 1.778 0 90) (layer F.SilkS))
    (fp_text value 33k (at 0 1.9) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 +3.3V))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5B04401C)
    (at 139.319 113.792 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at 1.7145 0 450) (layer F.SilkS))
    (fp_text value 33k (at 0 1.9 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5B04409F)
    (at 148.082 114.808 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at -2.032 0 180) (layer F.SilkS))
    (fp_text value 470 (at 0 1.9 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5B044117)
    (at 149.7965 115.824 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at -0.762 1.2065 90) (layer F.SilkS))
    (fp_text value 1.7K (at 0 1.9 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(R4-Pad1)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C3-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5B046BA4)
    (at 154.2415 119.761 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at 1.651 0 180) (layer F.SilkS))
    (fp_text value 47k (at 0 1.9 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 +3.3V))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C5-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5B046BA7)
    (at 156.718 117.729)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R6 (at 1.778 0 90) (layer F.SilkS))
    (fp_text value 47k (at 0 1.9) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C5-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5B044E25)
    (at 143.383 112.649 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R7 (at -1.5875 -0.0635 180) (layer F.SilkS))
    (fp_text value 2.2k (at 0 1.9 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(R7-Pad1)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C6-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5B044997)
    (at 142.494 115.316)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R8 (at -0.508 1.27 180) (layer F.SilkS))
    (fp_text value 100k (at 0 1.9) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C7-Pad2)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(R7-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5B044DA6)
    (at 139.319 112.014 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R9 (at 0.5715 1.143 180) (layer F.SilkS))
    (fp_text value 47k (at 0 1.9 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 19 /OUT_Q))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5B046D40)
    (at 139.065 119.634)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R10 (at 1.7145 -0.254 270) (layer F.SilkS))
    (fp_text value 33k (at 0 1.9) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 +3.3V))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(C8-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5B047044)
    (at 139.065 123.19 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R11 (at -1.7145 -0.127 270) (layer F.SilkS))
    (fp_text value 33k (at 0 1.9 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(C8-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5B046F4C)
    (at 147.574 127.5715 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R12 (at -1.778 0 360) (layer F.SilkS))
    (fp_text value 470 (at 0 1.9 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(C9-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(C8-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5B046EAE)
    (at 150.622 126.873)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R13 (at 0 -1.143 180) (layer F.SilkS))
    (fp_text value 1.7K (at 0 1.9) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(R13-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(C10-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5B046EB5)
    (at 154.2415 122.555 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R14 (at 1.778 0 360) (layer F.SilkS))
    (fp_text value 47k (at 0 1.9 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 +3.3V))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(C12-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5B04741C)
    (at 156.718 124.46)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R15 (at 1.9685 0.6985 180) (layer F.SilkS))
    (fp_text value 47k (at 0 1.9) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(C12-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5B0474EA)
    (at 144.3355 127.508 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R16 (at -1.778 0.381 360) (layer F.SilkS))
    (fp_text value 2.2k (at 0 1.9 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(R16-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(C13-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5B047253)
    (at 142.1765 127)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R17 (at 0 -1.2065) (layer F.SilkS))
    (fp_text value 100k (at 0 1.9) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(C14-Pad2)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(R16-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5B04756A)
    (at 156.972 121.158 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R18 (at -1.778 0 450) (layer F.SilkS))
    (fp_text value 47k (at 0 1.9 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 10 /OUT_I))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module radar_amplifier_footprints:Bourns_Trimpot_TC33 (layer F.Cu) (tedit 5B047251)
    (at 155.448 113.919 180)
    (fp_text reference RV1 (at -2.4765 0 270) (layer F.SilkS))
    (fp_text value 50k (at 0 -3.5 180) (layer F.Fab) hide)
    (pad 2 smd rect (at 0 -1.45 180) (size 1.6 1.5) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C5-Pad2)"))
    (pad 1 smd rect (at -1 1.8 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(R4-Pad1)"))
    (pad 3 smd rect (at 1 1.8 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(RV1-Pad3)"))
  )
  (module radar_amplifier_footprints:Bourns_Trimpot_TC33 (layer F.Cu) (tedit 5B047439)
    (at 155.448 128.27)
    (fp_text reference RV2 (at 2.4765 0 270) (layer F.SilkS))
    (fp_text value 50k (at 0 -3.5) (layer F.Fab) hide)
    (pad 2 smd rect (at 0 -1.45) (size 1.6 1.5) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(C12-Pad2)"))
    (pad 1 smd rect (at -1 1.8) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(R13-Pad1)"))
    (pad 3 smd rect (at 1 1.8) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(RV2-Pad3)"))
  )
  (module SMD_Packages:SOIC-14_N locked (layer F.Cu) (tedit 5B0807DB)
    (at 146.304 121.285 180)
    (descr "Module CMS SOJ 14 pins Large")
    (tags "CMS SOJ")
    (attr smd)
    (fp_text reference U1 (at -5.842 0.127 180) (layer F.SilkS))
    (fp_text value MAX414 (at 0 1.27 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -3.81 3.302 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C5-Pad2)"))
    (pad 2 smd rect (at -2.54 3.302 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(R4-Pad1)"))
    (pad 3 smd rect (at -1.27 3.302 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 4 smd rect (at 0 3.302 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 27 3.3V_FILT))
    (pad 5 smd rect (at 1.27 3.302 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C5-Pad1)"))
    (pad 6 smd rect (at 2.54 3.302 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(R7-Pad1)"))
    (pad 7 smd rect (at 3.81 3.302 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C7-Pad2)"))
    (pad 8 smd rect (at 3.81 -3.048 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(C14-Pad2)"))
    (pad 9 smd rect (at 2.54 -3.048 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(R16-Pad1)"))
    (pad 11 smd rect (at 0 -3.048 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 12 smd rect (at -1.27 -3.048 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(C9-Pad1)"))
    (pad 13 smd rect (at -2.54 -3.048 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(R13-Pad1)"))
    (pad 14 smd rect (at -3.81 -3.048 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(C12-Pad2)"))
    (pad 10 smd rect (at 1.27 -3.048 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(C12-Pad1)"))
    (model SMD_Packages.3dshapes/SOIC-14_N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.4 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module radar_amplifier_footprints:via_stitch (layer F.Cu) (tedit 5B048D03)
    (at 135.509 109.093)
    (fp_text reference REF** (at 0 1.9) (layer F.SilkS) hide)
    (fp_text value via_stitch (at 0 -1.8) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.4) (layers *.Cu)
      (net 4 GND))
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5B06E11A)
    (at 156.718 119.4435)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R19 (at 1.778 0 90) (layer F.SilkS))
    (fp_text value 47k (at 0 1.9) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 +3.3V))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 10 /OUT_I))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5B06E116)
    (at 140.831 109.9185 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R20 (at 0 1.143 360) (layer F.SilkS))
    (fp_text value 47k (at 0 1.9 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 +3.3V))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 19 /OUT_Q))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 5B07326C)
    (at 151.765 113.1965 90)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C3 (at -0.024 0 270) (layer F.SilkS))
    (fp_text value 100uF (at 0 2.3 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.5 0 90) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 1.5 0 90) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 5B073279)
    (at 146.7485 112.014)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C6 (at 0 0) (layer F.SilkS))
    (fp_text value 100uF (at 0 2.3) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.5 0) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C6-Pad1)"))
    (pad 2 smd rect (at 1.5 0) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 5B08117B)
    (at 141.1845 128.9685 180)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C13 (at 0 0 180) (layer F.SilkS))
    (fp_text value 100uF (at 0 2.3 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.5 0 180) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(C13-Pad1)"))
    (pad 2 smd rect (at 1.5 0 180) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5B0D6E62)
    (at 146.558 115.57 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C4 (at 1.778 -0.4445 180) (layer F.SilkS))
    (fp_text value 100uF (at 0 1.9 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 27 3.3V_FILT))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5B0D7478)
    (at 145.034 115.558 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference FB1 (at 0.012 1.016 450) (layer F.SilkS))
    (fp_text value FILTER (at 0 1.9 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 6 +3.3V))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 27 3.3V_FILT))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x05_Pitch2.54mm (layer B.Cu) (tedit 5B0D7405)
    (at 135.89 115.57 180)
    (descr "Through hole straight socket strip, 1x05, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x05 2.54mm single row")
    (fp_text reference P1 (at 0 2.33 180) (layer B.SilkS))
    (fp_text value CONN_01X05 (at 0 -12.49 180) (layer B.Fab) hide)
    (fp_text user %R (at 0 1.9685 180) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /IF_Q))
    (pad 2 thru_hole oval (at 0 -2.54 180) (size 2.032 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 +3.3V))
    (pad 3 thru_hole oval (at 0 -5.08 180) (size 2.032 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /IF_I))
    (pad 4 thru_hole oval (at 0 -7.62 180) (size 2.032 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 5 thru_hole oval (at 0 -10.16 180) (size 2.032 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 /VCO))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x05_Pitch2.54mm.wrl
      (at (xyz 0 -0.2 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04_Pitch2.54mm (layer F.Cu) (tedit 5B0D7447)
    (at 152.146 109.474 270)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference P2 (at 0 -2.33 270) (layer F.SilkS))
    (fp_text value CONN_01X04 (at 0 9.95 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 3.81 360) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /OUT_I))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.032 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 2.032 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 +3.3V))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 2.032 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 /OUT_Q))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x04_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58307A47)
    (at 136.3465 128.3335 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R21 (at 0.5835 -1.3335 180) (layer F.SilkS))
    (fp_text value 0 (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(P3-Pad4)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 28 /VCO))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "rev. 1.1" (at 148.0185 111.887) (layer B.SilkS))
  (gr_line (start 134.366 107.95) (end 134.366 133.35) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 159.766 107.95) (end 159.766 133.35) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 134.366 133.35) (end 159.766 133.35) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 134.366 107.95) (end 159.766 107.95) (layer Edge.Cuts) (width 0.15))
  (zone (net 4) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 134.366 107.95) (xy 159.766 107.95) (xy 159.766 133.35) (xy 134.366 133.35)
      )
    )
  )
  (zone (net 4) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 134.366 107.95) (xy 159.766 107.95) (xy 159.766 133.35) (xy 134.366 133.35)
      )
    )
  )
)
