<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<board>
<plain>
<wire x1="7" y1="0" x2="81.001" y2="0" width="0" layer="20"/>
<wire x1="81.001" y1="0" x2="88.001" y2="7" width="0" layer="20" curve="90"/>
<wire x1="88.001" y1="7" x2="88.001" y2="56.995953125" width="0" layer="20"/>
<wire x1="88.001" y1="56.995953125" x2="81.001675" y2="63.995953125" width="0" layer="20" curve="89.994475"/>
<wire x1="81.001675" y1="63.995953125" x2="7.000675" y2="64.00308125" width="0" layer="20"/>
<wire x1="7.000675" y1="64.00308125" x2="0" y2="57.00308125" width="0" layer="20" curve="89.960068"/>
<wire x1="0" y1="57.00308125" x2="0" y2="7" width="0" layer="20"/>
<wire x1="0" y1="7" x2="7" y2="0" width="0" layer="20" curve="90"/>
<text>B (RST)</text>
<text>RX</text>
<text>TX</text>
<text>VCC</text>
<text>A</text>
<text>GND</text>
<text>Rly GND</text>
<text>Rly +12v</text>
<text>Brake SW</text>
<text>Kickstand</text>
<text>Light +5</text>
<text>Clock</text>
<text>Light</text>
<text>+12V</text>
<text>GND</text>
<text>Motorcycle Keyless Ignition System</text>
<text>v1.0</text>
<text>D:/A Moving Bin/Silk.bmp</text>
<text>D:/A Moving Bin/Silk.bmp</text>
<text>D:/A Moving Bin/Silk.bmp</text>
<text>GND</text>
<text>SCL</text>
<text>SDA</text>
<text>VCC</text>
<text>GND</text>
<hole x="5" y="4" drill="4"/>
<hole x="5" y="60" drill="4"/>
<hole x="83" y="60" drill="4"/>
<hole x="83" y="4" drill="4"/>
<text>GND</text>
</plain>
<libraries>
<library name="Assys Complex">
<packages>
<package name="R_THM">
<description>Through Hole Resistor&lt;br&gt;
Drill: 0.8 mm &lt;br&gt;
Lead Spacing: 10 mm</description>
</package>
<package name="TO-92">
<description>TO-92 &lt;br&gt;
Pin pitch: 1.27 mm (Modified due to narrow spacing)</description>
</package>
<package name="C_H5">
<description>Radial Leaded Multilayer Ceramic Capacitor (H5)&lt;br&gt;
Lead Spacing: 5 mm&lt;br&gt;
Drill: 0.7 mm &lt;br&gt;

Datsheet: &lt;a href="mouser.com/datasheet/2/427/kseries-1763315.pdf "&gt;K-Series Capacitors&lt;/a&gt;</description>
</package>
<package name="TO220">
<description>TRANSISTOR &lt;br&gt;
Lenght: 10.36 mm &lt;br&gt;
Width: 4.57 mm &lt;br&gt;
Lead Spacing: 2.54 mm &lt;br&gt;
Lead Diameter: 0.6 mm &lt;br&gt;</description>
</package>
<package name="BUZZER-12">
<description>Footprint Diameter: 12 mm &lt;br&gt;
Lead Diameter: 0.6 mm&lt;br&gt;
Lead Spacing: 6.5 mm &lt;br&gt;</description>
</package>
<package name="DO-204AC_(DO-15)">
<description>Length (B): 7.6 mm &lt;br&gt;
Width (D): 3.6 mm &lt;br&gt;
Lead Diameter (C): 0.86 mm &lt;br&gt;
Drill: 1 mm &lt;br&gt;</description>
</package>
<package name="FB-5.23">
<description>Ferrite Bead Package for: 28L0138-80R-10 &lt;br&gt;
Lenght (C):  5.23 mm &lt;br&gt;
Width (A): 3.51 mm &lt;br&gt;
Lead Diameter: 0.51 mm &lt;br&gt;
Drill: 8 mm &lt;br&gt;</description>
</package>
<package name="DO-201AD">
<description>DIODE &lt;br&gt;
Lenght: 9.5 mm &lt;br&gt;
Width: 5.3 mm &lt;br&gt;
Lead Diameter: 1.32 mm &lt;br&gt;</description>
</package>
<package name="DO35-7A_ZENER">
<description>&lt;B&gt;DIODE&lt;/B&gt;&lt;p&gt;
diameter 2 mm, horizontal, grid 7.62 mm</description>
</package>
<package name="C_UBT_8">
<description>CAPACITOR &lt;br&gt;
Diameter: 8 mm &lt;br&gt;
Lead Spacing: 4 mm&lt;br&gt;
Lead diameter: 0.6 mm &lt;br&gt;</description>
</package>
<package name="DO-204AL_(DO-41)">
<description>DIODE &lt;br&gt;
Length: 5.2 mm &lt;br&gt;
Width: 2.7 mm &lt;br&gt;
Lead Diameter: 0.86 mm &lt;br&gt;</description>
</package>
<package name="PE-526">
<description>INDUCTOR &lt;br&gt;
Lenght:  18 mm&lt;br&gt;
Width: 18 mm &lt;br&gt;
Lead Diameter: 0.63 mm &lt;br&gt;
Lead Vertical Spacing: 15.24 mm &lt;br&gt;
Lead Horizontal Spacing: 10.16 mm &lt;br&gt;</description>
</package>
<package name="C_UBT_10">
<description>CAPACITOR &lt;br&gt;
Diameter: 10 mm &lt;br&gt;
Lead Spacing: 5 mm&lt;br&gt;
Lead diameter: 0.6 mm &lt;br&gt;</description>
</package>
<package name="LTF-D">
<description>INDUCTOR &lt;BR&gt;
Width/Length: 5mm &lt;br&gt;
Pad Size: 3.2 mm (Increased to aid in soldering)&lt;br&gt;</description>
</package>
<package name="DIL08">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="HC-49USX">
<description>QUARTZ CRYSTAL OSCILLATOR &lt;br&gt;
Lenght: 11.35 mm &lt;br&gt;
Width: 4.65 mm &lt;br&gt;
Lead Spacing: 4.88 mm &lt;br&gt;
Lead Diameter: 0.43 mm &lt;br&gt;</description>
</package>
<package name="DIP28">
<description>Standard 28-pin DIP package.&lt;br&gt;
IC needs to have legs bent before insertion.</description>
</package>
<package name="1X06_FTDI">
</package>
<package name="KK254_1X4">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="ASSYS_COMP_LOGO_V5">
<description>Make sure line widht is =&gt; 2 mil, otherwise Oshpark won't be able to print it. &lt;br&gt;
In the script dialolog increase the scale factor by 2.</description>
</package>
<package name="ASSYS_COMP_LOGO_V6">
<description>10 mm</description>
</package>
<package name="1X021">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X08">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="DO-41_(DO-204AL)">
<description>From Vishay&lt;br&gt;
Lenght: 5.2 mm &lt;br&gt;
Width: 2.7 &lt;br&gt;
Lead Diameter: 0.8 mm &lt;br&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="Q3" library="Assys Complex" package="TO220" value="IPP80N03S4L-04">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="Assys Complex" package="R_THM" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="Assys Complex" package="R_THM" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="Assys Complex" package="C_H5" value="0.1µF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q5" library="Assys Complex" package="TO-92" value="2N7000">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R17" library="Assys Complex" package="R_THM" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R13" library="Assys Complex" package="R_THM" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="BZ1" library="Assys Complex" package="BUZZER-12" value="BUZZER_254-EMB15-RO">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R14" library="Assys Complex" package="R_THM" value="56">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TVS1" library="Assys Complex" package="DO-204AC_(DO-15)" value="P6KE24CA">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="FB2" library="Assys Complex" package="FB-5.23" value="28L0138">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="Assys Complex" package="DO-201AD" value="SB560">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="FB1" library="Assys Complex" package="FB-5.23" value="28L0138">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Z1" library="Assys Complex" package="DO35-7A_ZENER" value="1N5233">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="Assys Complex" package="R_THM" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="Assys Complex" package="R_THM" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="Assys Complex" package="R_THM" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q1" library="Assys Complex" package="TO-92" value="2N7000">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q2" library="Assys Complex" package="TO220" value="SPP15P10PL_H">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="Assys Complex" package="C_UBT_8" value="22µF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D3" library="Assys Complex" package="DO-204AL_(DO-41)" value="1N5819">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L1" library="Assys Complex" package="PE-526" value="680µH">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="Assys Complex" package="C_UBT_10" value="220µF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L2" library="Assys Complex" package="LTF-D" value="22µH">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC1" library="Assys Complex" package="DIL08" value="LM2574">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C12" library="Assys Complex" package="C_H5" value="0.1µF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C10" library="Assys Complex" package="C_H5" value="0.1µF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="XTAL1" library="Assys Complex" package="HC-49USX" value="16MHZ">
<attribute name="FREQUENCY" value="16 MHZ"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C9" library="Assys Complex" package="C_H5" value="22pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C11" library="Assys Complex" package="C_H5" value="22pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC2" library="Assys Complex" package="DIP28" value="328P">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="IC-09136"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="Assys Complex" package="C_H5" value="0.1µF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q4" library="Assys Complex" package="TO-92" value="2N7000">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="Assys Complex" package="R_THM" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="Assys Complex" package="R_THM" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R11" library="Assys Complex" package="R_THM" value="220">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="Assys Complex" package="C_H5" value="0.1µF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="Assys Complex" package="R_THM" value="220">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C13" library="Assys Complex" package="C_H5" value="0.1µF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R16" library="Assys Complex" package="R_THM" value="220">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R15" library="Assys Complex" package="R_THM" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP4" library="Assys Complex" package="1X06_FTDI" value="USB-to-TTL Serial Adapter">
<attribute name="VALUE"/>
</element>
<element name="R12" library="Assys Complex" package="R_THM" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="Assys Complex" package="R_THM" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP2" library="Assys Complex" package="KK254_1X4" value="NFC Reader">
<attribute name="VALUE"/>
</element>
<element name="U$1" library="Assys Complex" package="ASSYS_COMP_LOGO_V5" value=""/>
<element name="U$2" library="Assys Complex" package="ASSYS_COMP_LOGO_V6" value=""/>
<element name="R1" library="Assys Complex" package="R_THM" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="Assys Complex" package="C_H5" value="0.01µF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="Assys Complex" package="1X021" value="Power Entry">
<attribute name="VALUE"/>
</element>
<element name="C8" library="Assys Complex" package="C_UBT_8" value="22µF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="Assys Complex" package="C_H5" value="0.1µF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP3" library="Assys Complex" package="1X08" value="I/O and Accesories">
<attribute name="VALUE"/>
</element>
<element name="D2" library="Assys Complex" package="DO-41_(DO-204AL)" value="1N4007">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$5">
<contactref element="D1" pad="C"/>
<contactref element="Z1" pad="C"/>
<contactref element="Q2" pad="3"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="R3" pad="1"/>
<contactref element="Q2" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="Z1" pad="A"/>
<contactref element="R3" pad="2"/>
<contactref element="R2" pad="1"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="GND">
<contactref element="R8" pad="1"/>
<contactref element="Q3" pad="3"/>
<contactref element="C6" pad="2"/>
<contactref element="R17" pad="1"/>
<contactref element="Q5" pad="1"/>
<contactref element="C12" pad="2"/>
<contactref element="C10" pad="2"/>
<contactref element="C9" pad="2"/>
<contactref element="C11" pad="2"/>
<contactref element="R9" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="C13" pad="2"/>
<contactref element="JP4" pad="1"/>
<contactref element="JP4" pad="2"/>
<contactref element="TVS1" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="FB2" pad="2"/>
<contactref element="C4" pad="-"/>
<contactref element="D3" pad="A"/>
<contactref element="C7" pad="-"/>
<contactref element="IC1" pad="2"/>
<contactref element="IC1" pad="3"/>
<contactref element="IC1" pad="4"/>
<contactref element="IC1" pad="6"/>
<contactref element="IC1" pad="8"/>
<contactref element="Q1" pad="1"/>
<contactref element="Q4" pad="1"/>
<contactref element="R5" pad="1"/>
<contactref element="IC2" pad="8"/>
<contactref element="IC2" pad="22"/>
<contactref element="C2" pad="2"/>
<contactref element="C8" pad="-"/>
<contactref element="C3" pad="2"/>
<contactref element="JP3" pad="5"/>
</signal>
<signal name="RELAY_+12V">
<contactref element="C6" pad="1"/>
<contactref element="Q2" pad="2"/>
<contactref element="C4" pad="+"/>
<contactref element="IC1" pad="5"/>
<contactref element="JP3" pad="2"/>
<contactref element="D2" pad="C"/>
</signal>
<signal name="N$12">
<contactref element="D3" pad="C"/>
<contactref element="L1" pad="1"/>
<contactref element="IC1" pad="7"/>
</signal>
<signal name="N$13">
<contactref element="L1" pad="2"/>
<contactref element="C7" pad="+"/>
<contactref element="L2" pad="2"/>
<contactref element="IC1" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="XTAL1" pad="1"/>
<contactref element="C9" pad="1"/>
<contactref element="IC2" pad="9"/>
</signal>
<signal name="N$14">
<contactref element="XTAL1" pad="2"/>
<contactref element="C11" pad="1"/>
<contactref element="IC2" pad="10"/>
</signal>
<signal name="N$16">
<contactref element="R6" pad="2"/>
<contactref element="Q3" pad="1"/>
<contactref element="R8" pad="2"/>
</signal>
<signal name="+5V">
<contactref element="R15" pad="2"/>
<contactref element="R14" pad="2"/>
<contactref element="R12" pad="1"/>
<contactref element="L2" pad="1"/>
<contactref element="C12" pad="1"/>
<contactref element="IC2" pad="7"/>
<contactref element="IC2" pad="20"/>
<contactref element="IC2" pad="21"/>
<contactref element="JP2" pad="3"/>
<contactref element="C8" pad="+"/>
<contactref element="C3" pad="1"/>
<contactref element="JP3" pad="4"/>
</signal>
<signal name="N$10">
<contactref element="R13" pad="1"/>
<contactref element="R17" pad="2"/>
<contactref element="Q5" pad="2"/>
</signal>
<signal name="N$18">
<contactref element="Q5" pad="3"/>
<contactref element="BZ1" pad="-"/>
</signal>
<signal name="CLOCK">
<contactref element="R10" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="IC2" pad="6"/>
</signal>
<signal name="SDA">
<contactref element="IC2" pad="27"/>
<contactref element="JP2" pad="2"/>
</signal>
<signal name="SCL">
<contactref element="IC2" pad="28"/>
<contactref element="JP2" pad="1"/>
</signal>
<signal name="CLOCK_OUT">
<contactref element="R10" pad="2"/>
<contactref element="JP3" pad="7"/>
</signal>
<signal name="N$20">
<contactref element="C1" pad="1"/>
<contactref element="FB1" pad="2"/>
<contactref element="D1" pad="A"/>
<contactref element="TVS1" pad="1"/>
<contactref element="C2" pad="1"/>
</signal>
<signal name="N$17">
<contactref element="R9" pad="1"/>
<contactref element="R7" pad="2"/>
<contactref element="Q4" pad="2"/>
</signal>
<signal name="LIGHT_GND">
<contactref element="R11" pad="1"/>
<contactref element="JP3" pad="8"/>
</signal>
<signal name="NFC_GND">
<contactref element="R11" pad="2"/>
<contactref element="Q4" pad="3"/>
<contactref element="JP2" pad="4"/>
</signal>
<signal name="KICKSTAND_SW_OUT">
<contactref element="R16" pad="2"/>
<contactref element="JP3" pad="6"/>
</signal>
<signal name="RESET">
<contactref element="C10" pad="1"/>
<contactref element="IC2" pad="1"/>
<contactref element="JP4" pad="6"/>
<contactref element="R12" pad="2"/>
</signal>
<signal name="KICKSTAND_SW">
<contactref element="IC2" pad="4"/>
<contactref element="R16" pad="1"/>
<contactref element="R15" pad="1"/>
<contactref element="C13" pad="1"/>
</signal>
<signal name="POWER_CTRL">
<contactref element="R4" pad="1"/>
<contactref element="IC2" pad="19"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="BRAKE_SW">
<contactref element="R2" pad="2"/>
<contactref element="Q1" pad="3"/>
<contactref element="JP3" pad="3"/>
</signal>
<signal name="+12V_IN">
<contactref element="FB1" pad="1"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="GND_IN">
<contactref element="FB2" pad="1"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="RX">
<contactref element="JP4" pad="4"/>
<contactref element="IC2" pad="2"/>
</signal>
<signal name="TX">
<contactref element="JP4" pad="5"/>
<contactref element="IC2" pad="3"/>
</signal>
<signal name="RELAY_GND">
<contactref element="Q3" pad="2"/>
<contactref element="JP3" pad="1"/>
<contactref element="D2" pad="A"/>
</signal>
<signal name="N$2">
<contactref element="Q1" pad="2"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="RELAY_DRIVER">
<contactref element="IC2" pad="11"/>
<contactref element="R6" pad="1"/>
</signal>
<signal name="READER_LSCANNER_DRIVER">
<contactref element="IC2" pad="13"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="BUZZER_DRIVER">
<contactref element="IC2" pad="18"/>
<contactref element="R13" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="R14" pad="1"/>
<contactref element="BZ1" pad="+"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
