(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "GND")
  (net 2 "Net-(Q1-Pad1)")
  (net 3 "+24V")
  (net 4 "-12V")
  (net 5 "GND1")
  (net 6 "Net-(D1-Pad1)")
  (net 7 "Net-(J3-Pad1)")
  (net 8 "Net-(J4-Pad1)")
  (net 9 "Net-(J5-Pad1)")
  (net 10 "Net-(H1-Pad1)")
  (net 11 "Net-(R3-Pad1)")
  (net 12 "Net-(R4-Pad1)")
  (net 13 "Net-(R7-Pad1)")
  (net 14 "Net-(R9-Pad1)")
  (net 15 "Net-(R15-Pad1)")
  (net 16 "Net-(R23-Pad1)")
  (net 17 "Net-(R23-Pad2)")
  (net 18 "unconnected-(U2-Pad1)")
  (net 19 "unconnected-(U2-Pad3)")
  (net 20 "unconnected-(U2-Pad6)")
  (net 21 "unconnected-(U2-Pad8)")
  (net 22 "unconnected-(U2-Pad9)")
  (net 23 "unconnected-(U2-Pad14)")
  (net 24 "unconnected-(U2-Pad16)")
  (net 25 "unconnected-(U3-Pad1)")
  (net 26 "unconnected-(U3-Pad3)")
  (net 27 "unconnected-(U3-Pad6)")
  (net 28 "unconnected-(U3-Pad8)")
  (net 29 "unconnected-(U3-Pad9)")
  (net 30 "unconnected-(U3-Pad14)")
  (net 31 "unconnected-(U3-Pad16)")
  (net 32 "unconnected-(U4-Pad1)")
  (net 33 "unconnected-(U4-Pad3)")
  (net 34 "unconnected-(U4-Pad6)")
  (net 35 "unconnected-(U4-Pad8)")
  (net 36 "unconnected-(U4-Pad9)")
  (net 37 "unconnected-(U4-Pad14)")
  (net 38 "unconnected-(U4-Pad16)")
  (net 39 "Net-(J6-Pad1)")
  (net 40 "Net-(R10-Pad2)")
  (net 41 "Net-(R11-Pad1)")
  (net 42 "Net-(R4-Pad2)")
  (net 43 "Net-(R5-Pad2)")
  (net 44 "Net-(R6-Pad1)")
  (net 45 "Net-(R9-Pad2)")
  (net 46 "Net-(R12-Pad1)")
  (net 47 "Net-(R13-Pad1)")
  (net 48 "Net-(R13-Pad2)")
  (net 49 "Net-(R14-Pad2)")
  (net 50 "Net-(R19-Pad1)")
  (net 51 "Net-(R20-Pad1)")
  (net 52 "Net-(R20-Pad2)")
  (net 53 "Net-(R21-Pad2)")
  (net 54 "Net-(R22-Pad1)")
  (net 55 "unconnected-(U1-Pad5)")
  (net 56 "unconnected-(U5-Pad1)")
  (net 57 "unconnected-(U5-Pad3)")
  (net 58 "unconnected-(U5-Pad6)")
  (net 59 "unconnected-(U5-Pad8)")
  (net 60 "unconnected-(U5-Pad9)")
  (net 61 "unconnected-(U5-Pad14)")
  (net 62 "unconnected-(U5-Pad16)")
  (net 63 "Net-(R24-Pad1)")
  (net 64 "Net-(R24-Pad2)")
  (net 65 "Net-(R25-Pad1)")
  (net 66 "Net-(Q1-Pad3)")
  (net 67 "Net-(R25-Pad2)")
  (net 68 "Net-(R26-Pad2)")
  (footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 146.05 92.195 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "MOSFET transfer function measurement v1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C6" (at 3.175 0 180) (layer "F.SilkS"))
    (fp_text value "0.1u" (at 0 1.85 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0 90) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 4 "-12V") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0 90) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 5 "GND1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "_es_RLC:Potentiometer_Nidec_ST4_Vertical" (layer "F.Cu")
    (tedit 620D450F)
    (at 104.648 101.092)
    (descr "Potentiometer, vertical, Vishay TS53YJ, https://www.vishay.com/docs/51008/ts53.pdf")
    (tags "Potentiometer vertical Vishay TS53YJ")
    (property "Sheetfile" "MOSFET transfer function measurement v1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "RV1" (at 0 -3.75) (layer "F.SilkS"))
    (fp_text value "1k" (at 0 3.75) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2) (layer "F.Fab"))
    (pad "1" smd rect (at 2 -1.15) (size 2 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 64 "Net-(R24-Pad2)") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect (at -2 0) (size 2 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "+24V") (pinfunction "2") (pintype "passive"))
    (pad "3" smd rect (at 2 1.15) (size 2 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "Net-(R23-Pad1)") (pinfunction "3") (pintype "passive"))
    (model "${STIERS_3DMODEL_DIR}/ST-4ETA2k_(202).stp"
      (offset (xyz 0 0 2.286))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 184.785 108.585)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "MOSFET transfer function measurement v1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R14" (at -3.175 0 90) (layer "F.SilkS"))
    (fp_text value "49.9" (at 0 1.82) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 9 "Net-(J5-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 49 "Net-(R14-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 137.795 100.965 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "MOSFET transfer function measurement v1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R9" (at 3.175 0) (layer "F.SilkS"))
    (fp_text value "DNP" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 90) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 14 "Net-(R9-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 90) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 45 "Net-(R9-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "_es_Connector:BNC_Horizontal_ThruHole" (layer "F.Cu")
    (tedit 62A0B0B9)
    (at 187.96 113.03 180)
    (property "MPN" "031-5431-10RFX")
    (property "Manufacturer" "Amphenol RF")
    (property "Sheetfile" "MOSFET transfer function measurement v1.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J5" (at 8.636 -2.286 90 unlocked) (layer "F.SilkS"))
    (fp_text value "Is" (at 0 -3.81 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.54 unlocked) (layer "F.Fab"))
    (pad "" thru_hole oval (at -5.08 -5.08 180) (size 3.5 7) (drill 2.01) (layers *.Cu *.Mask))
    (pad "" thru_hole oval (at 5.08 -5.08 180) (size 3.5 7) (drill 2.01) (layers *.Cu *.Mask))
    (pad "1" thru_hole oval (at 0 0 180) (size 1.6 2.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 9 "Net-(J5-Pad1)") (pinfunction "In") (pintype "passive"))
    (pad "2" thru_hole oval (at -2.54 0 180) (size 1.6 2.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 5 "GND1") (pinfunction "Ext") (pintype "passive"))
    (model "${STIERS_3DMODEL_DIR}/31-5431-10RFX.stp"
      (offset (xyz 0 -1.3462 0.9144))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 -90))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 127.635 108.585)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "MOSFET transfer function measurement v1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R10" (at -3.175 0 90) (layer "F.SilkS"))
    (fp_text value "49.9" (at 0 1.82) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 8 "Net-(J4-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 40 "Net-(R10-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 156.845 101.085 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "MOSFET transfer function measurement v1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R4" (at 3.175 0 180) (layer "F.SilkS"))
    (fp_text value "DNP" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 90) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 12 "Net-(R4-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 90) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 42 "Net-(R4-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_2816_7142Metric_Pad3.20x4.45mm_HandSolder" (layer "F.Cu")
    (tedit 5F6BB4CA)
    (at 171.45 74.93 180)
    (descr "Resistor SMD 2816 (7142 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size from: https://www.vishay.com/docs/30100/wsl.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "MOSFET transfer function measurement v1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R17" (at -7.62 -5.08 90) (layer "F.SilkS"))
    (fp_text value "10m" (at 0 3.18) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.6 0 180) (size 3.2 4.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.078125)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 2.6 0 180) (size 3.2 4.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.078125)
      (net 66 "Net-(Q1-Pad3)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_2816_7142Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3_DIN965" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 193.04 43.561)
    (descr "Mounting Hole 3.2mm, no annular, M3, DIN965")
    (tags "mounting hole 3.2mm no annular m3 din965")
    (property "Sheetfile" "MOSFET transfer function measurement v1.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H4" (at 0 -11.43) (layer "F.SilkS") hide)
    (fp_text value "MountingHole" (at 0 3.8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 147.955 74.93)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "MOSFET transfer function measurement v1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R8" (at 0 -1.905 180) (layer "F.SilkS"))
    (fp_text value "20" (at 0 1.82) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 67 "Net-(R25-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 2 "Net-(Q1-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 110.744 102.235)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "MOSFET transfer function measurement v1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R23" (at -1.27 1.778) (layer "F.SilkS"))
    (fp_text value "4.53k" (at 0 1.82) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 16 "Net-(R23-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 17 "Net-(R23-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 122.682 101.346 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "MOSFET transfer function measurement v1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C4" (at 3.175 0) (layer "F.SilkS"))
    (fp_text value "0.1u" (at 0 1.85 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0 90) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 4 "-12V") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0 90) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 5 "GND1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "_es_IC:SOIC127P1030X265-16N" (layer "F.Cu")
    (tedit 629F626F)
    (at 130.81 100.965 -90)
    (property "Sheetfile" "MOSFET transfer function measurement v1.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U3" (at -6.35 -5.08 180) (layer "F.SilkS"))
    (fp_text value "INA114" (at 0 4.553949 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -4.64 -4.445 270) (size 2.06 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 25 "unconnected-(U3-Pad1)") (pinfunction "NC") (pintype "no_connect"))
    (pad "2" smd roundrect (at -4.64 -3.175 270) (size 2.06 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 45 "Net-(R9-Pad2)") (pinfunction "Rg") (pintype "passive"))
    (pad "3" smd roundrect (at -4.64 -1.905 270) (size 2.06 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 26 "unconnected-(U3-Pad3)") (pinfunction "NC") (pintype "no_connect"))
    (pad "4" smd roundrect (at -4.64 -0.635 270) (size 2.06 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 41 "Net-(R11-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "5" smd roundrect (at -4.64 0.635 270) (size 2.06 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 13 "Net-(R7-Pad1)") (pinfunction "+") (pintype "input"))
    (pad "6" smd roundrect (at -4.64 1.905 270) (size 2.06 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 27 "unconnected-(U3-Pad6)") (pinfunction "NC") (pintype "no_connect"))
    (pad "7" smd roundrect (at -4.64 3.175 270) (size 2.06 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 4 "-12V") (pinfunction "V-") (pintype "power_in"))
    (pad "8" smd roundrect (at -4.64 4.445 270) (size 2.06 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 28 "unconnected-(U3-Pad8)") (pinfunction "NC") (pintype "no_connect"))
    (pad "9" smd roundrect (at 4.64 4.445 270) (size 2.06 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 29 "unconnected-(U3-Pad9)") (pinfunction "NC") (pintype "no_connect"))
    (pad "10" smd roundrect (at 4.64 3.175 270) (size 2.06 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 5 "GND1") (pinfunction "Ref") (pintype "passive"))
    (pad "11" smd roundrect (at 4.64 1.905 270) (size 2.06 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 40 "Net-(R10-Pad2)") (pintype "output"))
    (pad "12" smd roundrect (at 4.64 0.635 270) (size 2.06 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 40 "Net-(R10-Pad2)") (pinfunction "FB") (pintype "input"))
    (pad "13" smd roundrect (at 4.64 -0.635 270) (size 2.06 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 3 "+24V") (pinfunction "V+") (pintype "power_in"))
    (pad "14" smd roundrect (at 4.64 -1.905 270) (size 2.06 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 30 "unconnected-(U3-Pad14)") (pinfunction "NC") (pintype "no_connect"))
    (pad "15" smd roundrect (at 4.64 -3.175 270) (size 2.06 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 14 "Net-(R9-Pad1)") (pinfunction "Rg") (pintype "passive"))
    (pad "16" smd roundrect (at 4.64 -4.445 270) (size 2.06 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 31 "unconnected-(U3-Pad16)") (pinfunction "NC") (pintype "no_connect"))
    (model "${STIERS_3DMODEL_DIR}/INA114AU_1K.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 171.45 108.585 180)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "MOSFET transfer function measurement v1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C11" (at -3.048 -0.127 90) (layer "F.SilkS"))
    (fp_text value "0.1u" (at 0 1.85) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0 180) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 5 "GND1") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0 180) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 3 "+24V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "_es_Connector:BNC_Horizontal_ThruHole" (layer "F.Cu")
    (tedit 62A0B0B9)
    (at 130.81 113.03 180)
    (property "MPN" "031-5431-10RFX")
    (property "Manufacturer" "Amphenol RF")
    (property "Sheetfile" "MOSFET transfer function measurement v1.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J4" (at 8.636 -2.286 90 unlocked) (layer "F.SilkS"))
    (fp_text value "Ig" (at 0 -3.81 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.54 unlocked) (layer "F.Fab"))
    (pad "" thru_hole oval (at -5.08 -5.08 180) (size 3.5 7) (drill 2.01) (layers *.Cu *.Mask))
    (pad "" thru_hole oval (at 5.08 -5.08 180) (size 3.5 7) (drill 2.01) (layers *.Cu *.Mask))
    (pad "1" thru_hole oval (at 0 0 180) (size 1.6 2.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 8 "Net-(J4-Pad1)") (pinfunction "In") (pintype "passive"))
    (pad "2" thru_hole oval (at -2.54 0 180) (size 1.6 2.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 5 "GND1") (pinfunction "Ext") (pintype "passive"))
    (model "${STIERS_3DMODEL_DIR}/31-5431-10RFX.stp"
      (offset (xyz 0 -1.3462 0.9144))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 -90))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 152.4 93.472)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "MOSFET transfer function measurement v1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R6" (at 1.778 -1.524 180) (layer "F.SilkS"))
    (fp_text value "100" (at 0 1.82) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 44 "Net-(R6-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 66 "Net-(Q1-Pad3)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 120.65 48.895 180)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "MOSFET transfer function measurement v1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C2" (at -1.905 1.905 180) (layer "F.SilkS"))
    (fp_text value "10u" (at 0 1.85) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0 180) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 5 "GND1") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0 180) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 4 "-12V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 113.665 95.885)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "MOSFET transfer function measurement v1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C3" (at 0 -1.905 180) (layer "F.SilkS"))
    (fp_text value "0.1u" (at 0 1.85) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 5 "GND1") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 3 "+24V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 165.735 108.585)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "MOSFET transfer function measurement v1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R21" (at -3.302 0.127 90) (layer "F.SilkS"))
    (fp_text value "49.9" (at 0 1.82) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 39 "Net-(J6-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 53 "Net-(R21-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 132.08 92.075 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "MOSFET transfer function measurement v1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R11" (at 3.175 0) (layer "F.SilkS"))
    (fp_text value "100" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 90) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 41 "Net-(R11-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 90) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 2 "Net-(Q1-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 165.1 92.075 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "MOSFET transfer function measurement v1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C12" (at 3.048 -0.127 180) (layer "F.SilkS"))
    (fp_text value "0.1u" (at 0 1.85 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0 90) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 4 "-12V") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0 90) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 5 "GND1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 148.59 92.195 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "MOSFET transfer function measurement v1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R3" (at 3.175 0 180) (layer "F.SilkS"))
    (fp_text value "100" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 90) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 11 "Net-(R3-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 90) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 2 "Net-(Q1-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 146.685 108.705)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "MOSFET transfer function measurement v1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R5" (at -3.175 0 90) (layer "F.SilkS"))
    (fp_text value "49.9" (at 0 1.82) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 7 "Net-(J3-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 43 "Net-(R5-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 133.35 108.585 180)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "MOSFET transfer function measurement v1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C7" (at -3.175 0 90) (layer "F.SilkS"))
    (fp_text value "0.1u" (at 0 1.85) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0 180) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 5 "GND1") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0 180) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 3 "+24V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 127 92.075 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "MOSFET transfer function measurement v1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C8" (at 3.175 0 180) (layer "F.SilkS"))
    (fp_text value "0.1u" (at 0 1.85 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0 90) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 4 "-12V") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0 90) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 5 "GND1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 184.15 92.075 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "MOSFET transfer function measurement v1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C10" (at 3.175 0 180) (layer "F.SilkS"))
    (fp_text value "0.1u" (at 0 1.85 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0 90) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 4 "-12V") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0 90) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 5 "GND1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 167.64 92.075 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "MOSFET transfer function measurement v1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R19" (at 3.048 -0.127 180) (layer "F.SilkS"))
    (fp_text value "100" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 90) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 50 "Net-(R19-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 90) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 10 "Net-(H1-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 113.03 105.918)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "MOSFET transfer function measurement v1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R1" (at -3.175 0 90) (layer "F.SilkS"))
    (fp_text value "49.9" (at 0 1.82) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 5 "GND1") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 6 "Net-(D1-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 120.65 51.435 180)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "MOSFET transfer function measurement v1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C14" (at -1.905 -1.905) (layer "F.SilkS"))
    (fp_text value "0.1u" (at 0 1.85) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0 180) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 5 "GND1") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0 180) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 4 "-12V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 194.945 100.965 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "MOSFET transfer function measurement v1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R13" (at 3.175 0 180) (layer "F.SilkS"))
    (fp_text value "DNP" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 90) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 47 "Net-(R13-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 90) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 48 "Net-(R13-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 120.142 101.346 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "MOSFET transfer function measurement v1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R25" (at 3.048 0 180) (layer "F.SilkS"))
    (fp_text value "500" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 90) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 65 "Net-(R25-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 90) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 67 "Net-(R25-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_2816_7142Metric_Pad3.20x4.45mm_HandSolder" (layer "F.Cu")
    (tedit 5F6BB4CA)
    (at 171.45 80.01 180)
    (descr "Resistor SMD 2816 (7142 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size from: https://www.vishay.com/docs/30100/wsl.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "MOSFET transfer function measurement v1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R16" (at -5.14 0 90) (layer "F.SilkS"))
    (fp_text value "10m" (at 0 3.18) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.6 0 180) (size 3.2 4.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.078125)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 2.6 0 180) (size 3.2 4.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.078125)
      (net 66 "Net-(Q1-Pad3)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_2816_7142Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 189.23 92.075 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "MOSFET transfer function measurement v1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R15" (at 3.175 0) (layer "F.SilkS"))
    (fp_text value "100" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 90) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 15 "Net-(R15-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 90) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 186.69 92.075 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "MOSFET transfer function measurement v1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R12" (at 3.175 0) (layer "F.SilkS"))
    (fp_text value "100" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 90) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 46 "Net-(R12-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 90) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 66 "Net-(Q1-Pad3)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "_es_Connector:BNC_Horizontal_ThruHole" (layer "F.Cu")
    (tedit 62A0B0B9)
    (at 149.86 113.15 180)
    (property "MPN" "031-5431-10RFX")
    (property "Manufacturer" "Amphenol RF")
    (property "Sheetfile" "MOSFET transfer function measurement v1.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J3" (at 8.9408 -2.2676 90 unlocked) (layer "F.SilkS"))
    (fp_text value "Vgs" (at 0 -3.81 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.54 unlocked) (layer "F.Fab"))
    (pad "" thru_hole oval (at 5.08 -5.08 180) (size 3.5 7) (drill 2.01) (layers *.Cu *.Mask))
    (pad "" thru_hole oval (at -5.08 -5.08 180) (size 3.5 7) (drill 2.01) (layers *.Cu *.Mask))
    (pad "1" thru_hole oval (at 0 0 180) (size 1.6 2.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 7 "Net-(J3-Pad1)") (pinfunction "In") (pintype "passive"))
    (pad "2" thru_hole oval (at -2.54 0 180) (size 1.6 2.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 5 "GND1") (pinfunction "Ext") (pintype "passive"))
    (model "${STIERS_3DMODEL_DIR}/31-5431-10RFX.stp"
      (offset (xyz 0 -1.3462 0.9144))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 -90))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 106.68 51.435 180)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "MOSFET transfer function measurement v1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C13" (at 1.27 -1.85) (layer "F.SilkS"))
    (fp_text value "0.1u" (at 0 1.85) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0 180) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 3 "+24V") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0 180) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 5 "GND1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3_DIN965" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 125.73 43.561)
    (descr "Mounting Hole 3.2mm, no annular, M3, DIN965")
    (tags "mounting hole 3.2mm no annular m3 din965")
    (property "Sheetfile" "MOSFET transfer function measurement v1.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H3" (at 0 -11.684) (layer "F.SilkS") hide)
    (fp_text value "MountingHole" (at 0 3.8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 116.84 107.188 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "MOSFET transfer function measurement v1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R26" (at 0 1.778 90) (layer "F.SilkS"))
    (fp_text value "500" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 90) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 6 "Net-(D1-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 90) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 68 "Net-(R26-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "_es_IC:SOIC127P1030X265-16N" (layer "F.Cu")
    (tedit 629F626F)
    (at 168.91 100.965 -90)
    (property "Sheetfile" "MOSFET transfer function measurement v1.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U5" (at -6.35 -5.08 180) (layer "F.SilkS"))
    (fp_text value "INA114" (at 0 4.445 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -4.64 -4.445 270) (size 2.06 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 56 "unconnected-(U5-Pad1)") (pinfunction "NC") (pintype "no_connect"))
    (pad "2" smd roundrect (at -4.64 -3.175 270) (size 2.06 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 52 "Net-(R20-Pad2)") (pinfunction "Rg") (pintype "passive"))
    (pad "3" smd roundrect (at -4.64 -1.905 270) (size 2.06 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 57 "unconnected-(U5-Pad3)") (pinfunction "NC") (pintype "no_connect"))
    (pad "4" smd roundrect (at -4.64 -0.635 270) (size 2.06 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 54 "Net-(R22-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "5" smd roundrect (at -4.64 0.635 270) (size 2.06 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 50 "Net-(R19-Pad1)") (pinfunction "+") (pintype "input"))
    (pad "6" smd roundrect (at -4.64 1.905 270) (size 2.06 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 58 "unconnected-(U5-Pad6)") (pinfunction "NC") (pintype "no_connect"))
    (pad "7" smd roundrect (at -4.64 3.175 270) (size 2.06 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 4 "-12V") (pinfunction "V-") (pintype "power_in"))
    (pad "8" smd roundrect (at -4.64 4.445 270) (size 2.06 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 59 "unconnected-(U5-Pad8)") (pinfunction "NC") (pintype "no_connect"))
    (pad "9" smd roundrect (at 4.64 4.445 270) (size 2.06 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 60 "unconnected-(U5-Pad9)") (pinfunction "NC") (pintype "no_connect"))
    (pad "10" smd roundrect (at 4.64 3.175 270) (size 2.06 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 5 "GND1") (pinfunction "Ref") (pintype "passive"))
    (pad "11" smd roundrect (at 4.64 1.905 270) (size 2.06 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 53 "Net-(R21-Pad2)") (pintype "output"))
    (pad "12" smd roundrect (at 4.64 0.635 270) (size 2.06 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 53 "Net-(R21-Pad2)") (pinfunction "FB") (pintype "input"))
    (pad "13" smd roundrect (at 4.64 -0.635 270) (size 2.06 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 3 "+24V") (pinfunction "V+") (pintype "power_in"))
    (pad "14" smd roundrect (at 4.64 -1.905 270) (size 2.06 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 61 "unconnected-(U5-Pad14)") (pinfunction "NC") (pintype "no_connect"))
    (pad "15" smd roundrect (at 4.64 -3.175 270) (size 2.06 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 51 "Net-(R20-Pad1)") (pinfunction "Rg") (pintype "passive"))
    (pad "16" smd roundrect (at 4.64 -4.445 270) (size 2.06 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 62 "unconnected-(U5-Pad16)") (pinfunction "NC") (pintype "no_connect"))
    (model "${STIERS_3DMODEL_DIR}/INA114AU_1K.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "Resistor_SMD:R_2816_7142Metric_Pad3.20x4.45mm_HandSolder" (layer "F.Cu")
    (tedit 5F6BB4CA)
    (at 171.45 69.85 180)
    (descr "Resistor SMD 2816 (7142 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size from: https://www.vishay.com/docs/30100/wsl.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "MOSFET transfer function measurement v1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R18" (at -5.14 0 90) (layer "F.SilkS"))
    (fp_text value "10m" (at 0 3.18) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.6 0 180) (size 3.2 4.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.078125)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 2.6 0 180) (size 3.2 4.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.078125)
      (net 66 "Net-(Q1-Pad3)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_2816_7142Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 129.54 92.075 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "MOSFET transfer function measurement v1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R7" (at 3.175 0 180) (layer "F.SilkS"))
    (fp_text value "100" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 90) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 13 "Net-(R7-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 90) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 67 "Net-(R25-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 190.5 108.585 180)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "MOSFET transfer function measurement v1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C9" (at -3.048 0 90) (layer "F.SilkS"))
    (fp_text value "0.1u" (at 0 1.85) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0 180) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 5 "GND1") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0 180) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 3 "+24V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 184.785 74.93 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "MOSFET transfer function measurement v1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R2" (at 0 1.905 180) (layer "F.SilkS"))
    (fp_text value "0" (at 0 1.82) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 180) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 5 "GND1") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 180) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 106.68 48.895 180)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "MOSFET transfer function measurement v1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C1" (at 1.905 1.905) (layer "F.SilkS"))
    (fp_text value "10u" (at 0 1.85) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0 180) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 3 "+24V") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0 180) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 5 "GND1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 152.4 108.705 180)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "MOSFET transfer function measurement v1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C5" (at -3.175 0 90) (layer "F.SilkS"))
    (fp_text value "0.1u" (at 0 1.85) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0 180) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 5 "GND1") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0 180) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 3 "+24V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical_SMD_Pin1Right" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 113.03 43.18 90)
    (descr "surface-mounted straight pin header, 1x04, 2.54mm pitch, single row, style 2 (pin 1 right)")
    (tags "Surface mounted pin header SMD 1x04 2.54mm single row style2 pin1 right")
    (property "Sheetfile" "MOSFET transfer function measurement v1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "J1" (at 0 -6.14 90) (layer "F.SilkS"))
    (fp_text value "PWR" (at 0 6.14 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd rect (at 1.655 -3.81 90) (size 2.51 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "+24V") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" smd rect (at -1.655 -1.27 90) (size 2.51 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "GND1") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" smd rect (at 1.655 1.27 90) (size 2.51 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "GND1") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" smd rect (at -1.655 3.81 90) (size 2.51 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "-12V") (pinfunction "Pin_4") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical_SMD_Pin1Right.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "_es_Connector:BNC_Horizontal_ThruHole" (layer "F.Cu")
    (tedit 62A0B0B9)
    (at 168.91 113.03 180)
    (property "MPN" "031-5431-10RFX")
    (property "Manufacturer" "Amphenol RF")
    (property "Sheetfile" "MOSFET transfer function measurement v1.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J6" (at 8.636 -2.286 90 unlocked) (layer "F.SilkS"))
    (fp_text value "Vds" (at 0 -3.81 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.54 unlocked) (layer "F.Fab"))
    (pad "" thru_hole oval (at 5.08 -5.08 180) (size 3.5 7) (drill 2.01) (layers *.Cu *.Mask))
    (pad "" thru_hole oval (at -5.08 -5.08 180) (size 3.5 7) (drill 2.01) (layers *.Cu *.Mask))
    (pad "1" thru_hole oval (at 0 0 180) (size 1.6 2.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 39 "Net-(J6-Pad1)") (pinfunction "In") (pintype "passive"))
    (pad "2" thru_hole oval (at -2.54 0 180) (size 1.6 2.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 5 "GND1") (pinfunction "Ext") (pintype "passive"))
    (model "${STIERS_3DMODEL_DIR}/31-5431-10RFX.stp"
      (offset (xyz 0 -1.3462 0.9144))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 -90))
    )
  )
  (footprint "_es_IC:SOIC127P1030X265-16N" (layer "F.Cu")
    (tedit 629F626F)
    (at 149.86 101.085 -90)
    (property "Sheetfile" "MOSFET transfer function measurement v1.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U2" (at -5.835 -6.096 180) (layer "F.SilkS"))
    (fp_text value "INA114" (at 0 4.445 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -4.64 -4.445 270) (size 2.06 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 18 "unconnected-(U2-Pad1)") (pinfunction "NC") (pintype "no_connect"))
    (pad "2" smd roundrect (at -4.64 -3.175 270) (size 2.06 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 42 "Net-(R4-Pad2)") (pinfunction "Rg") (pintype "passive"))
    (pad "3" smd roundrect (at -4.64 -1.905 270) (size 2.06 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 19 "unconnected-(U2-Pad3)") (pinfunction "NC") (pintype "no_connect"))
    (pad "4" smd roundrect (at -4.64 -0.635 270) (size 2.06 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 44 "Net-(R6-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "5" smd roundrect (at -4.64 0.635 270) (size 2.06 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 11 "Net-(R3-Pad1)") (pinfunction "+") (pintype "input"))
    (pad "6" smd roundrect (at -4.64 1.905 270) (size 2.06 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 20 "unconnected-(U2-Pad6)") (pinfunction "NC") (pintype "no_connect"))
    (pad "7" smd roundrect (at -4.64 3.175 270) (size 2.06 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 4 "-12V") (pinfunction "V-") (pintype "power_in"))
    (pad "8" smd roundrect (at -4.64 4.445 270) (size 2.06 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 21 "unconnected-(U2-Pad8)") (pinfunction "NC") (pintype "no_connect"))
    (pad "9" smd roundrect (at 4.64 4.445 270) (size 2.06 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 22 "unconnected-(U2-Pad9)") (pinfunction "NC") (pintype "no_connect"))
    (pad "10" smd roundrect (at 4.64 3.175 270) (size 2.06 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 5 "GND1") (pinfunction "Ref") (pintype "passive"))
    (pad "11" smd roundrect (at 4.64 1.905 270) (size 2.06 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 43 "Net-(R5-Pad2)") (pintype "output"))
    (pad "12" smd roundrect (at 4.64 0.635 270) (size 2.06 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 43 "Net-(R5-Pad2)") (pinfunction "FB") (pintype "input"))
    (pad "13" smd roundrect (at 4.64 -0.635 270) (size 2.06 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 3 "+24V") (pinfunction "V+") (pintype "power_in"))
    (pad "14" smd roundrect (at 4.64 -1.905 270) (size 2.06 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 23 "unconnected-(U2-Pad14)") (pinfunction "NC") (pintype "no_connect"))
    (pad "15" smd roundrect (at 4.64 -3.175 270) (size 2.06 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 12 "Net-(R4-Pad1)") (pinfunction "Rg") (pintype "passive"))
    (pad "16" smd roundrect (at 4.64 -4.445 270) (size 2.06 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 24 "unconnected-(U2-Pad16)") (pinfunction "NC") (pintype "no_connect"))
    (model "${STIERS_3DMODEL_DIR}/INA114AU_1K.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "Diode_SMD:D_1206_3216Metric_Pad1.42x1.75mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 113.03 108.458 180)
    (descr "Diode SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "diode handsolder")
    (property "Sheetfile" "MOSFET transfer function measurement v1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D1" (at 3.048 0 90) (layer "F.SilkS"))
    (fp_text value "DNP" (at 0 1.82) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.4875 0 180) (size 1.425 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.175439)
      (net 6 "Net-(D1-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4875 0 180) (size 1.425 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.175439)
      (net 5 "GND1") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "_es_Transistors:TO-264_SMD" (layer "F.Cu")
    (tedit 626843E4)
    (at 159.385 62.5725)
    (property "Sheetfile" "MOSFET transfer function measurement v1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Q1" (at 0 -22.86 unlocked) (layer "F.SilkS"))
    (fp_text value "IXTK200N10L2" (at 0 -15.24 unlocked) (layer "F.Fab"))
    (fp_text user "S" (at 5.715 -1.27 unlocked) (layer "F.Fab"))
    (fp_text user "G" (at -5.715 -1.27 unlocked) (layer "F.Fab"))
    (fp_text user "D" (at 0 -1.27 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -12.7 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at -5.461 12.065) (size 3.81 20.32) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "Net-(Q1-Pad1)") (pinfunction "G") (pintype "input"))
    (pad "2" smd roundrect (at 0 12.065) (size 3.81 20.32) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "Net-(H1-Pad1)") (pinfunction "D") (pintype "passive"))
    (pad "3" smd roundrect (at 5.461 12.065) (size 3.81 20.32) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 66 "Net-(Q1-Pad3)") (pinfunction "S") (pintype "passive"))
    (model "${STIERS_3DMODEL_DIR}/IXTK200N10L2 MOSFET.stp"
      (offset (xyz -9.906 0 -1.5875))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 90))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 170.18 92.075 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "MOSFET transfer function measurement v1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R22" (at 3.048 -0.127 180) (layer "F.SilkS"))
    (fp_text value "100" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 90) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 54 "Net-(R22-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 90) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 66 "Net-(Q1-Pad3)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "_es_IC:SOIC127P1030X265-16N" (layer "F.Cu")
    (tedit 629F626F)
    (at 187.96 100.965 -90)
    (property "Sheetfile" "MOSFET transfer function measurement v1.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U4" (at -6.35 -5.08 180) (layer "F.SilkS"))
    (fp_text value "INA114" (at -0.108949 4.553949 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -4.64 -4.445 270) (size 2.06 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 32 "unconnected-(U4-Pad1)") (pinfunction "NC") (pintype "no_connect"))
    (pad "2" smd roundrect (at -4.64 -3.175 270) (size 2.06 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 48 "Net-(R13-Pad2)") (pinfunction "Rg") (pintype "passive"))
    (pad "3" smd roundrect (at -4.64 -1.905 270) (size 2.06 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 33 "unconnected-(U4-Pad3)") (pinfunction "NC") (pintype "no_connect"))
    (pad "4" smd roundrect (at -4.64 -0.635 270) (size 2.06 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 15 "Net-(R15-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "5" smd roundrect (at -4.64 0.635 270) (size 2.06 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 46 "Net-(R12-Pad1)") (pinfunction "+") (pintype "input"))
    (pad "6" smd roundrect (at -4.64 1.905 270) (size 2.06 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 34 "unconnected-(U4-Pad6)") (pinfunction "NC") (pintype "no_connect"))
    (pad "7" smd roundrect (at -4.64 3.175 270) (size 2.06 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 4 "-12V") (pinfunction "V-") (pintype "power_in"))
    (pad "8" smd roundrect (at -4.64 4.445 270) (size 2.06 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 35 "unconnected-(U4-Pad8)") (pinfunction "NC") (pintype "no_connect"))
    (pad "9" smd roundrect (at 4.64 4.445 270) (size 2.06 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 36 "unconnected-(U4-Pad9)") (pinfunction "NC") (pintype "no_connect"))
    (pad "10" smd roundrect (at 4.64 3.175 270) (size 2.06 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 5 "GND1") (pinfunction "Ref") (pintype "passive"))
    (pad "11" smd roundrect (at 4.64 1.905 270) (size 2.06 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 49 "Net-(R14-Pad2)") (pintype "output"))
    (pad "12" smd roundrect (at 4.64 0.635 270) (size 2.06 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 49 "Net-(R14-Pad2)") (pinfunction "FB") (pintype "input"))
    (pad "13" smd roundrect (at 4.64 -0.635 270) (size 2.06 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 3 "+24V") (pinfunction "V+") (pintype "power_in"))
    (pad "14" smd roundrect (at 4.64 -1.905 270) (size 2.06 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 37 "unconnected-(U4-Pad14)") (pinfunction "NC") (pintype "no_connect"))
    (pad "15" smd roundrect (at 4.64 -3.175 270) (size 2.06 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 47 "Net-(R13-Pad1)") (pinfunction "Rg") (pintype "passive"))
    (pad "16" smd roundrect (at 4.64 -4.445 270) (size 2.06 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 38 "unconnected-(U4-Pad16)") (pinfunction "NC") (pintype "no_connect"))
    (model "${STIERS_3DMODEL_DIR}/INA114AU_1K.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 175.895 100.965 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "MOSFET transfer function measurement v1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R20" (at 3.175 0 180) (layer "F.SilkS"))
    (fp_text value "DNP" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 90) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 51 "Net-(R20-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 90) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 52 "Net-(R20-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 110.744 99.695 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "MOSFET transfer function measurement v1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R24" (at 1.27 1.778) (layer "F.SilkS"))
    (fp_text value "4.53k" (at 0 1.82) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 180) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 63 "Net-(R24-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 180) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 64 "Net-(R24-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.7mm_M2.5_Pad_TopBottom" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 159.385 88.9)
    (descr "Mounting Hole 2.7mm, M2.5")
    (tags "mounting hole 2.7mm m2.5")
    (property "Sheetfile" "MOSFET transfer function measurement v1.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H1" (at 45.085 0) (layer "F.SilkS") hide)
    (fp_text value "PWR+" (at 0 3.7) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" connect circle (at 0 0) (size 5.4 5.4) (layers "B.Cu" "B.Mask")
      (net 10 "Net-(H1-Pad1)") (pinfunction "1") (pintype "input"))
    (pad "1" connect circle (at 0 0) (size 5.4 5.4) (layers "F.Cu" "F.Mask")
      (net 10 "Net-(H1-Pad1)") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at 0 0) (size 3.1 3.1) (drill 2.7) (layers *.Cu *.Mask)
      (net 10 "Net-(H1-Pad1)") (pinfunction "1") (pintype "input"))
  )
  (footprint "_es_IC:SOIC-8_MS-012-AA" (layer "F.Cu")
    (tedit 5D9F72B1)
    (at 116.205 100.965 90)
    (descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "Sheetfile" "MOSFET transfer function measurement v1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U1" (at -3.175 -3.429) (layer "F.SilkS"))
    (fp_text value "OP27" (at 0 3.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.475 -1.905 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 17 "Net-(R23-Pad2)") (pinfunction "Vos") (pintype "input"))
    (pad "2" smd roundrect (at -2.475 -0.635 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 65 "Net-(R25-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "3" smd roundrect (at -2.475 0.635 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 68 "Net-(R26-Pad2)") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at -2.475 1.905 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "-12V") (pinfunction "V-") (pintype "power_in"))
    (pad "5" smd roundrect (at 2.475 1.905 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 55 "unconnected-(U1-Pad5)") (pinfunction "NC") (pintype "no_connect"))
    (pad "6" smd roundrect (at 2.475 0.635 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 67 "Net-(R25-Pad2)") (pintype "output"))
    (pad "7" smd roundrect (at 2.475 -0.635 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "+24V") (pinfunction "V+") (pintype "power_in"))
    (pad "8" smd roundrect (at 2.475 -1.905 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 63 "Net-(R24-Pad1)") (pinfunction "Vos") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.7mm_M2.5_Pad_TopBottom" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 179.07 74.93)
    (descr "Mounting Hole 2.7mm, M2.5")
    (tags "mounting hole 2.7mm m2.5")
    (property "Sheetfile" "MOSFET transfer function measurement v1.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H2" (at 25.4 0 90) (layer "F.SilkS") hide)
    (fp_text value "PWR-" (at 3.81 -0.635 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 3.1 3.1) (drill 2.7) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "1") (pintype "input"))
    (pad "1" connect circle (at 0 0) (size 5.4 5.4) (layers "B.Cu" "B.Mask")
      (net 1 "GND") (pinfunction "1") (pintype "input"))
    (pad "1" connect circle (at 0 0) (size 5.4 5.4) (layers "F.Cu" "F.Mask")
      (net 1 "GND") (pinfunction "1") (pintype "input"))
  )
  (footprint "_es_Connector:BNC_Horizontal_ThruHole" (layer "F.Cu")
    (tedit 62A0B0B9)
    (at 111.76 113.03 180)
    (property "MPN" "031-5431-10RFX")
    (property "Manufacturer" "Amphenol RF")
    (property "Sheetfile" "MOSFET transfer function measurement v1.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J2" (at 8.636 -2.286 90 unlocked) (layer "F.SilkS"))
    (fp_text value "Vin" (at 0 -3.81 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.54 unlocked) (layer "F.Fab"))
    (pad "" thru_hole oval (at 5.08 -5.08 180) (size 3.5 7) (drill 2.01) (layers *.Cu *.Mask))
    (pad "" thru_hole oval (at -5.08 -5.08 180) (size 3.5 7) (drill 2.01) (layers *.Cu *.Mask))
    (pad "1" thru_hole oval (at 0 0 180) (size 1.6 2.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 6 "Net-(D1-Pad1)") (pinfunction "In") (pintype "passive"))
    (pad "2" thru_hole oval (at -2.54 0 180) (size 1.6 2.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 5 "GND1") (pinfunction "Ext") (pintype "passive"))
    (model "${STIERS_3DMODEL_DIR}/31-5431-10RFX.stp"
      (offset (xyz 0 -1.3462 0.9144))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 -90))
    )
  )
  (gr_line (start 173.989999 35.559999) (end 196.85 35.56) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 102.87 125.203949) (mid 101.073949 124.46) (end 100.33 122.663949) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 149.86 63.500001) (end 168.910001 63.500002) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 102.87 35.56) (end 144.779999 35.560001) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 171.450001 60.960001) (end 171.449999 38.099999) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 100.33 122.663949) (end 100.33 38.1) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 149.86 63.500001) (mid 148.063949 62.756052) (end 147.32 60.960001) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 144.78 35.559999) (mid 146.576051 36.303948) (end 147.32 38.099999) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 171.449999 38.099999) (mid 172.193948 36.303948) (end 173.989999 35.559999) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 199.39 122.663949) (mid 198.646051 124.46) (end 196.85 125.203949) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 199.39 38.1) (end 199.39 122.663949) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 196.85 125.203949) (end 102.87 125.203949) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 147.32 38.099999) (end 147.32 60.960001) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 171.450001 60.960001) (mid 170.706052 62.756052) (end 168.910001 63.500001) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 196.85 35.56) (mid 198.646051 36.303949) (end 199.39 38.1) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 100.33 38.1) (mid 101.073949 36.303949) (end 102.87 35.56) (layer "Edge.Cuts") (width 0.1))
  (gr_text "-12V" (at 116.84 38.1 270) (layer "F.SilkS"))
  (gr_text "GND" (at 111.76 38.1 270) (layer "F.SilkS"))
  (gr_text "GND" (at 114.3 38.1 270) (layer "F.SilkS"))
  (gr_text "+24V" (at 109.22 38.1 270) (layer "F.SilkS"))
  (gr_text "Vgs" (at 140.8684 111.6076 90) (layer "F.SilkS"))
  (gr_text "Vin" (at 103.124 111.76 90) (layer "F.SilkS"))
  (gr_text "Vds" (at 160.274 111.506 90) (layer "F.SilkS"))
  (gr_text "POWER" (at 118.745 43.18 90) (layer "F.SilkS"))
  (gr_text "PWR+" (at 159.385 92.71) (layer "F.SilkS"))
  (gr_text "Ig" (at 121.666 112.268 90) (layer "F.SilkS"))
  (gr_text "Is" (at 179.324 112.268 90) (layer "F.SilkS"))
  (gr_text "MOSFET Transfer Function Measurement, v1\n8 June 2022, E. Stiers" (at 125.984 69.088) (layer "F.SilkS"))
  (gr_text "PWR-" (at 181.61 70.485 90) (layer "F.SilkS"))
  (zone (net 1) (net_name "GND") (layers F&B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 2.54))
    (polygon
      (pts
        (xy 182.245 73.66)
        (xy 182.245 76.2)
        (xy 175.895 82.55)
        (xy 172.085 82.55)
        (xy 172.085 67.31)
        (xy 175.895 67.31)
      )
    )
  )
  (zone (net 5) (net_name "GND1") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 2.54))
    (polygon
      (pts
        (xy 200.66 126.365)
        (xy 99.06 126.365)
        (xy 99.06 34.29)
        (xy 200.66 34.29)
      )
    )
  )
  (zone (net 66) (net_name "Net-(Q1-Pad3)") (layers F&B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 2.54))
    (polygon
      (pts
        (xy 170.434 67.691)
        (xy 170.434 82.296)
        (xy 166.751 84.836)
        (xy 162.941 84.836)
        (xy 162.941 64.516)
        (xy 166.751 64.516)
      )
    )
  )
)
