(kicad_pcb (version 20171130) (host pcbnew "(5.1.4)-1")
  (general
    (thickness 1.6)
    (drawings 5)
    (tracks 147)
    (zones 0)
    (modules 34)
    (nets 26)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.3048)
    (user_trace_width 0.1524)
    (user_trace_width 0.254)
    (user_trace_width 0.3048)
    (user_trace_width 0.4064)
    (user_trace_width 0.508)
    (user_trace_width 0.6096)
    (user_trace_width 0.762)
    (user_trace_width 1.016)
    (user_trace_width 1.27)
    (user_trace_width 2.54)
    (trace_clearance 0.1524)
    (zone_clearance 0.1524)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.508)
    (via_drill 0.254)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (user_via 0.508 0.254)
    (user_via 0.6096 0.3048)
    (user_via 0.762 0.508)
    (user_via 1.016 0.508)
    (user_via 1.524 0.762)
    (user_via 2.032 1.016)
    (user_via 2.032 1.524)
    (user_via 2.54 1.524)
    (user_via 2.54 2.032)
    (uvia_size 2)
    (uvia_drill 1)
    (uvias_allowed no)
    (uvia_min_size 1)
    (uvia_min_drill 1)
    (edge_width 0.15)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.0508)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 /5VA)
  (net 2 "Net-(D1-Pad2)")
  (net 3 /VIN)
  (net 4 /SCLK)
  (net 5 /SDO)
  (net 6 /CS)
  (net 7 /SIG_IN)
  (net 8 GND)
  (net 9 VCC)
  (net 10 /PD)
  (net 11 "Net-(R3-Pad2)")
  (net 12 /3.3VA)
  (net 13 /GPIO14)
  (net 14 /GPIO3)
  (net 15 /GPIO2)
  (net 16 /GPIO22)
  (net 17 /GPIO23)
  (net 18 "Net-(R2-Pad3)")
  (net 19 "Net-(U1-Pad4)")
  (net 20 /TRIG_PI)
  (net 21 /GPIO15)
  (net 22 /GPIO18)
  (net 23 /TRIG_EXT)
  (net 24 "Net-(R7-Pad1)")
  (net 25 "Net-(U3-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.508)
    (via_drill 0.254)
    (uvia_dia 2)
    (uvia_drill 1)
    (add_net /3.3VA)
    (add_net /5VA)
    (add_net /CS)
    (add_net /GPIO14)
    (add_net /GPIO15)
    (add_net /GPIO18)
    (add_net /GPIO2)
    (add_net /GPIO22)
    (add_net /GPIO23)
    (add_net /GPIO3)
    (add_net /PD)
    (add_net /SCLK)
    (add_net /SDO)
    (add_net /SIG_IN)
    (add_net /TRIG_EXT)
    (add_net /TRIG_PI)
    (add_net /VIN)
    (add_net GND)
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(R2-Pad3)")
    (add_net "Net-(R3-Pad2)")
    (add_net "Net-(R7-Pad1)")
    (add_net "Net-(U1-Pad4)")
    (add_net "Net-(U3-Pad2)")
    (add_net VCC)
  )
  (module TO_SOT_Packages_SMD:SOT-353_SC-70-5_Handsoldering (layer B.Cu) (tedit 5E2FD7FC)
    (at 116.4336 50.3174 180)
    (descr "SOT-353, SC-70-5, Handsoldering")
    (tags "SOT-353 SC-70-5 Handsoldering")
    (attr smd)
    (fp_text reference U4 (at 3.4036 -0.4826 180) (layer B.SilkS))
    (fp_text value 74LVC1G32 (at 0 -2 180) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 5 smd rect (at 1.33 0.65 180) (size 1.5 0.4) (layers B.Cu B.Paste B.Mask)
      (net 9 VCC))
    (pad 4 smd rect (at 1.33 -0.65 180) (size 1.5 0.4) (layers B.Cu B.Paste B.Mask)
      (net 25 "Net-(U3-Pad2)"))
    (pad 3 smd rect (at -1.33 -0.65 180) (size 1.5 0.4) (layers B.Cu B.Paste B.Mask)
      (net 8 GND))
    (pad 2 smd rect (at -1.33 0 180) (size 1.5 0.4) (layers B.Cu B.Paste B.Mask)
      (net 23 /TRIG_EXT))
    (pad 1 smd rect (at -1.33 0.65 180) (size 1.5 0.4) (layers B.Cu B.Paste B.Mask)
      (net 20 /TRIG_PI))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-353_SC-70-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 58AA848B)
    (at 103.6066 53.7972 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C3 (at 3.2512 0.1016 270) (layer B.SilkS))
    (fp_text value 4.7u (at 0 -1.5 270) (layer B.Fab))
    (fp_text user %R (at 0 1.25 270) (layer B.Fab))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 12 /3.3VA))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SamacSys_Parts:SOT95P280X145-6N (layer F.Cu) (tedit 5E2EADCD)
    (at 115.7732 56.896 270)
    (descr "DBV (R-PDSO-G6)")
    (tags "Integrated Circuit")
    (attr smd)
    (fp_text reference IC1 (at 3.683 -1.016 270) (layer F.SilkS))
    (fp_text value ADS7886SDBVT (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.25 -0.95) (size 0.6 1.2) (layers F.Cu F.Paste F.Mask)
      (net 12 /3.3VA))
    (pad 2 smd rect (at -1.25 0) (size 0.6 1.2) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 3 smd rect (at -1.25 0.95) (size 0.6 1.2) (layers F.Cu F.Paste F.Mask)
      (net 3 /VIN))
    (pad 4 smd rect (at 1.25 0.95) (size 0.6 1.2) (layers F.Cu F.Paste F.Mask)
      (net 4 /SCLK))
    (pad 5 smd rect (at 1.25 0) (size 0.6 1.2) (layers F.Cu F.Paste F.Mask)
      (net 5 /SDO))
    (pad 6 smd rect (at 1.25 -0.95) (size 0.6 1.2) (layers F.Cu F.Paste F.Mask)
      (net 6 /CS))
    (model "C:/Users/Jonathan Chandler/Documents/SamacSys_PCB_Library/KiCad/3D_Models/ADS7886SBDBVT.step"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SamacSys_Parts2:TC33X-2_1 (layer F.Cu) (tedit 5E2EACF1)
    (at 102.4636 54.3814)
    (descr TC33X-2_1)
    (tags Resistor)
    (attr smd)
    (fp_text reference R2 (at -3.4036 2.2098) (layer F.SilkS))
    (fp_text value TC33X-2-101E (at -0.337 0.209) (layer F.SilkS) hide)
    (fp_text user %R (at -0.337 0.209) (layer F.Fab))
    (pad 3 smd rect (at 1 1.7 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(R2-Pad3)"))
    (pad 2 smd rect (at 0 -1.55 90) (size 1.5 1.6) (layers F.Cu F.Paste F.Mask)
      (net 3 /VIN))
    (pad 1 smd rect (at -1 1.7 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 10 /PD))
    (model C:\SamacSys_PCB_Library\KiCad\SamacSys_Parts.3dshapes\TC33X-2-101E.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_2.7mm_M2.5 (layer F.Cu) (tedit 56D1B4CB)
    (at 98.7552 43.0022)
    (descr "Mounting Hole 2.7mm, no annular, M2.5")
    (tags "mounting hole 2.7mm no annular m2.5")
    (attr virtual)
    (fp_text reference M2.5 (at -1.2192 -2.1082 180) (layer F.SilkS))
    (fp_text value MountingHole_2.7mm_M2.5 (at 0 3.7) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_2.7mm_M2.5 (layer F.Cu) (tedit 56D1B4CB)
    (at 121.7168 43.0276)
    (descr "Mounting Hole 2.7mm, no annular, M2.5")
    (tags "mounting hole 2.7mm no annular m2.5")
    (attr virtual)
    (fp_text reference M2.5 (at 1.1938 -2.159 180) (layer F.SilkS))
    (fp_text value MountingHole_2.7mm_M2.5 (at 0 3.7) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 118.2624 56.7436 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at 3.302 0 90) (layer F.SilkS))
    (fp_text value 10k (at 0 1.55 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 9 VCC))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 /CS))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 58AA848B)
    (at 117.0432 57.5564 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C5 (at -3.048 0 270) (layer B.SilkS))
    (fp_text value 1n (at 0 -1.5 270) (layer B.Fab))
    (fp_text user %R (at 0 1.25 270) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 6 /CS))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 8 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 115.1128 57.3786 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at -3.048 0.1524 270) (layer B.SilkS))
    (fp_text value 100 (at 0 -1.55 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 6 /CS))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 11 "Net-(R3-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 58AA848B)
    (at 116.7384 42.2656 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at -0.1016 -1.4224 90) (layer F.SilkS))
    (fp_text value 4.7u (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.25 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 /5VA))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23-5_HandSoldering (layer B.Cu) (tedit 58CE4E7E)
    (at 116.459 53.594 180)
    (descr "5-pin SOT23 package")
    (tags "SOT-23-5 hand-soldering")
    (attr smd)
    (fp_text reference U3 (at 3.429 1.397 180) (layer B.SilkS))
    (fp_text value 74LVC1G14 (at 0 -2.9 180) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 5 smd rect (at 1.35 0.95 180) (size 1.56 0.65) (layers B.Cu B.Paste B.Mask)
      (net 9 VCC))
    (pad 4 smd rect (at 1.35 -0.95 180) (size 1.56 0.65) (layers B.Cu B.Paste B.Mask)
      (net 11 "Net-(R3-Pad2)"))
    (pad 3 smd rect (at -1.35 -0.95 180) (size 1.56 0.65) (layers B.Cu B.Paste B.Mask)
      (net 8 GND))
    (pad 2 smd rect (at -1.35 0 180) (size 1.56 0.65) (layers B.Cu B.Paste B.Mask)
      (net 25 "Net-(U3-Pad2)"))
    (pad 1 smd rect (at -1.35 0.95 180) (size 1.56 0.65) (layers B.Cu B.Paste B.Mask))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes\SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 113.6904 46.2534 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R6 (at -0.5334 -1.4224 270) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.55 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 23 /TRIG_EXT))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 58AA848B)
    (at 117.7544 46.863 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C6 (at 2.794 0 270) (layer B.SilkS))
    (fp_text value 4.7u (at 0 -1.5 270) (layer B.Fab))
    (fp_text user %R (at 0 1.25 270) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 9 VCC))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 8 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 114.7572 61.0108 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at 2.8702 0.5842 90) (layer F.SilkS))
    (fp_text value 10k (at 0 1.55 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 /SCLK))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 58AA848B)
    (at 102.1334 49.7332 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C4 (at 2.921 0 90) (layer F.SilkS))
    (fp_text value 1n (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.25 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 /VIN))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 103.6574 49.5808 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at 2.921 0 90) (layer F.SilkS))
    (fp_text value 100k (at 0 1.55 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 /VIN))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 58AA848B)
    (at 116.3828 53.8734 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at 1.3208 1.2446) (layer F.SilkS))
    (fp_text value 4.7u (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 -1.25) (layer F.Fab))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 12 /3.3VA))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 102.489 58.0136)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference D1 (at -1.0668 1.524) (layer F.SilkS))
    (fp_text value BAT_63-02V_H6327 (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 10 /PD))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SamacSys_Parts:SHDR8W60P254_2X4_1016X508X850P (layer F.Cu) (tedit 5DCDE698)
    (at 120.4722 47.9044 270)
    (descr 2214S-8)
    (tags Connector)
    (fp_text reference J1 (at 3.8354 2.3368 90) (layer F.SilkS))
    (fp_text value 2214S-08SG-85 (at 0 0 90) (layer F.SilkS) hide)
    (pad 8 thru_hole circle (at 7.62 -2.54) (size 1.575 1.575) (drill 1.05) (layers *.Cu *.Mask F.SilkS)
      (net 13 /GPIO14))
    (pad 7 thru_hole circle (at 7.62 0) (size 1.575 1.575) (drill 1.05) (layers *.Cu *.Mask F.SilkS)
      (net 20 /TRIG_PI))
    (pad 6 thru_hole circle (at 5.08 -2.54) (size 1.575 1.575) (drill 1.05) (layers *.Cu *.Mask F.SilkS)
      (net 8 GND))
    (pad 5 thru_hole circle (at 5.08 0) (size 1.575 1.575) (drill 1.05) (layers *.Cu *.Mask F.SilkS)
      (net 14 /GPIO3))
    (pad 4 thru_hole circle (at 2.54 -2.54) (size 1.575 1.575) (drill 1.05) (layers *.Cu *.Mask F.SilkS)
      (net 1 /5VA))
    (pad 3 thru_hole circle (at 2.54 0) (size 1.575 1.575) (drill 1.05) (layers *.Cu *.Mask F.SilkS)
      (net 15 /GPIO2))
    (pad 2 thru_hole circle (at 0 -2.54) (size 1.575 1.575) (drill 1.05) (layers *.Cu *.Mask F.SilkS)
      (net 1 /5VA))
    (pad 1 thru_hole rect (at 0 0) (size 1.575 1.575) (drill 1.05) (layers *.Cu *.Mask F.SilkS)
      (net 9 VCC))
  )
  (module SamacSys_Parts:SHDR8W60P254_2X4_1016X508X850P (layer F.Cu) (tedit 5DCDE698)
    (at 120.4722 58.0644 270)
    (descr 2214S-8)
    (tags Connector)
    (fp_text reference J2 (at 8.001 2.2098 90) (layer F.SilkS))
    (fp_text value 2214S-08SG-85 (at 0 0 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.575 1.575) (drill 1.05) (layers *.Cu *.Mask F.SilkS)
      (net 8 GND))
    (pad 2 thru_hole circle (at 0 -2.54) (size 1.575 1.575) (drill 1.05) (layers *.Cu *.Mask F.SilkS)
      (net 21 /GPIO15))
    (pad 3 thru_hole circle (at 2.54 0) (size 1.575 1.575) (drill 1.05) (layers *.Cu *.Mask F.SilkS)
      (net 5 /SDO))
    (pad 4 thru_hole circle (at 2.54 -2.54) (size 1.575 1.575) (drill 1.05) (layers *.Cu *.Mask F.SilkS)
      (net 22 /GPIO18))
    (pad 5 thru_hole circle (at 5.08 0) (size 1.575 1.575) (drill 1.05) (layers *.Cu *.Mask F.SilkS)
      (net 4 /SCLK))
    (pad 6 thru_hole circle (at 5.08 -2.54) (size 1.575 1.575) (drill 1.05) (layers *.Cu *.Mask F.SilkS)
      (net 8 GND))
    (pad 7 thru_hole circle (at 7.62 0) (size 1.575 1.575) (drill 1.05) (layers *.Cu *.Mask F.SilkS)
      (net 16 /GPIO22))
    (pad 8 thru_hole circle (at 7.62 -2.54) (size 1.575 1.575) (drill 1.05) (layers *.Cu *.Mask F.SilkS)
      (net 17 /GPIO23))
  )
  (module TO_SOT_Packages_SMD:SOT-23-5_HandSoldering (layer F.Cu) (tedit 58CE4E7E)
    (at 113.6142 42.291 180)
    (descr "5-pin SOT23 package")
    (tags "SOT-23-5 hand-soldering")
    (attr smd)
    (fp_text reference U1 (at 1.6764 -2.413 90) (layer F.SilkS))
    (fp_text value LP5907MFX-3.3 (at 0 2.9) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 -0.95 180) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 /5VA))
    (pad 2 smd rect (at -1.35 0 180) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 3 smd rect (at -1.35 0.95 180) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 /5VA))
    (pad 4 smd rect (at 1.35 0.95 180) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(U1-Pad4)"))
    (pad 5 smd rect (at 1.35 -0.95 180) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 12 /3.3VA))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes\SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23-6_Handsoldering (layer B.Cu) (tedit 58CE4E7E)
    (at 102.5652 58.039 90)
    (descr "6-pin SOT-23 package, Handsoldering")
    (tags "SOT-23-6 Handsoldering")
    (attr smd)
    (fp_text reference U2 (at -3.3274 -1.016 270) (layer B.SilkS))
    (fp_text value OPA355NA (at 0 -2.9 270) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 5 smd rect (at 1.35 0 90) (size 1.56 0.65) (layers B.Cu B.Paste B.Mask)
      (net 12 /3.3VA))
    (pad 6 smd rect (at 1.35 0.95 90) (size 1.56 0.65) (layers B.Cu B.Paste B.Mask)
      (net 12 /3.3VA))
    (pad 4 smd rect (at 1.35 -0.95 90) (size 1.56 0.65) (layers B.Cu B.Paste B.Mask)
      (net 24 "Net-(R7-Pad1)"))
    (pad 3 smd rect (at -1.35 -0.95 90) (size 1.56 0.65) (layers B.Cu B.Paste B.Mask)
      (net 7 /SIG_IN))
    (pad 2 smd rect (at -1.35 0 90) (size 1.56 0.65) (layers B.Cu B.Paste B.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -1.35 0.95 90) (size 1.56 0.65) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Measurement_Points:Measurement_Point_Round-TH_Small (layer F.Cu) (tedit 56C35F63)
    (at 109.8042 44.4754)
    (descr "Mesurement Point, Square, Trough Hole,  DM 1.5mm, Drill 0.8mm,")
    (tags "Mesurement Point Round Trough Hole 1.5mm Drill 0.8mm")
    (attr virtual)
    (fp_text reference 3V3 (at 0 -2) (layer F.SilkS))
    (fp_text value TestPoint_Alt (at 0 2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 /3.3VA))
  )
  (module Measurement_Points:Measurement_Point_Round-TH_Small (layer F.Cu) (tedit 56C35F63)
    (at 115.5446 64.2112 180)
    (descr "Mesurement Point, Square, Trough Hole,  DM 1.5mm, Drill 0.8mm,")
    (tags "Mesurement Point Round Trough Hole 1.5mm Drill 0.8mm")
    (attr virtual)
    (fp_text reference CS1 (at -1.8034 0.7112 90) (layer F.SilkS))
    (fp_text value TestPoint_Alt (at 0 2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 /CS))
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 98.6536 49.022)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J3 (at -1.778 -2.4892) (layer F.SilkS))
    (fp_text value Conn_01x03_Female (at 0 7.41) (layer F.Fab))
    (fp_text user %R (at 0 2.54 90) (layer F.Fab))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 GND))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 /TRIG_EXT))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 98.6282 59.055)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J4 (at -1.7272 7.3914) (layer F.SilkS))
    (fp_text value Conn_01x03_Female (at 0 7.41) (layer F.Fab))
    (fp_text user %R (at 0 2.54 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 GND))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /SIG_IN))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Measurement_Points:Measurement_Point_Round-TH_Small (layer F.Cu) (tedit 56C35F63)
    (at 103.3272 44.4754)
    (descr "Mesurement Point, Square, Trough Hole,  DM 1.5mm, Drill 0.8mm,")
    (tags "Mesurement Point Round Trough Hole 1.5mm Drill 0.8mm")
    (attr virtual)
    (fp_text reference PD1 (at 0 -2) (layer F.SilkS))
    (fp_text value TestPoint_Alt (at 0 2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 /PD))
  )
  (module SamacSys_Parts2:2.54+0603resistorpad (layer F.Cu) (tedit 5E2E9541)
    (at 116.9162 46.7106 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R_Term1 (at -0.6604 1.1938 270) (layer F.SilkS))
    (fp_text value 50 (at 0 1.550001 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 thru_hole circle (at 1.27 -1.397 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 8 GND))
    (pad 1 thru_hole circle (at -1.27 -1.397 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 23 /TRIG_EXT))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 23 /TRIG_EXT))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SamacSys_Parts2:2.54+0603resistorpad (layer F.Cu) (tedit 5E2E9541)
    (at 101.6254 62.7888 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R_Term2 (at 0.1524 1.143 270) (layer F.SilkS))
    (fp_text value 50 (at 0 1.55 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 /SIG_IN))
    (pad 1 thru_hole circle (at -1.27 -1.397 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 7 /SIG_IN))
    (pad 2 thru_hole circle (at 1.27 -1.397 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 8 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Measurement_Points:Measurement_Point_Round-TH_Small (layer F.Cu) (tedit 56C35F63)
    (at 106.4768 44.4754)
    (descr "Mesurement Point, Square, Trough Hole,  DM 1.5mm, Drill 0.8mm,")
    (tags "Mesurement Point Round Trough Hole 1.5mm Drill 0.8mm")
    (attr virtual)
    (fp_text reference VIN1 (at 0 -2) (layer F.SilkS))
    (fp_text value TestPoint_Alt (at 0 2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 /VIN))
  )
  (module SamacSys_Parts2:733910070 (layer F.Cu) (tedit 5E2E97A3)
    (at 109.22 51.562)
    (descr 73391-0070-1)
    (tags Connector)
    (fp_text reference J5 (at 0 -0.28) (layer F.SilkS))
    (fp_text value Conn_Coaxial (at 0 -0.28) (layer F.SilkS) hide)
    (pad 2 thru_hole circle (at 2.54 -2.54 90) (size 2.4 2.4) (drill 1.6) (layers *.Cu *.Mask F.SilkS)
      (net 8 GND))
    (pad 2 thru_hole circle (at 2.54 2.54 90) (size 2.4 2.4) (drill 1.6) (layers *.Cu *.Mask F.SilkS)
      (net 8 GND))
    (pad 2 thru_hole circle (at -2.54 2.54 90) (size 2.4 2.4) (drill 1.6) (layers *.Cu *.Mask F.SilkS)
      (net 8 GND))
    (pad 2 thru_hole circle (at -2.54 -2.54 90) (size 2.4 2.4) (drill 1.6) (layers *.Cu *.Mask F.SilkS)
      (net 8 GND))
    (pad 1 thru_hole circle (at 0 0 90) (size 2.4 2.4) (drill 1.6) (layers *.Cu *.Mask F.SilkS)
      (net 23 /TRIG_EXT))
    (model "C:/Users/Jonathan Chandler/Documents/SamacSys_PCB_Library/KiCad/3D_Models/5-1814832-1.step"
      (offset (xyz 0 0 8.890000000000001))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SamacSys_Parts2:733910070 (layer F.Cu) (tedit 5E2E97A3)
    (at 109.22 61.595)
    (descr 73391-0070-1)
    (tags Connector)
    (fp_text reference J6 (at 0 -0.28) (layer F.SilkS))
    (fp_text value Conn_Coaxial (at 0 -0.28) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0 90) (size 2.4 2.4) (drill 1.6) (layers *.Cu *.Mask F.SilkS)
      (net 7 /SIG_IN))
    (pad 2 thru_hole circle (at -2.54 -2.54 90) (size 2.4 2.4) (drill 1.6) (layers *.Cu *.Mask F.SilkS)
      (net 8 GND))
    (pad 2 thru_hole circle (at -2.54 2.54 90) (size 2.4 2.4) (drill 1.6) (layers *.Cu *.Mask F.SilkS)
      (net 8 GND))
    (pad 2 thru_hole circle (at 2.54 2.54 90) (size 2.4 2.4) (drill 1.6) (layers *.Cu *.Mask F.SilkS)
      (net 8 GND))
    (pad 2 thru_hole circle (at 2.54 -2.54 90) (size 2.4 2.4) (drill 1.6) (layers *.Cu *.Mask F.SilkS)
      (net 8 GND))
    (model "C:/Users/Jonathan Chandler/Documents/SamacSys_PCB_Library/KiCad/3D_Models/5-1814832-1.step"
      (offset (xyz 0 0 8.890000000000001))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 101.4222 53.6702 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R7 (at 3.1496 -0.0254 90) (layer B.SilkS))
    (fp_text value Inf (at 0 -1.55 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 24 "Net-(R7-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 98.7552 56.5404)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R8 (at -1.778 -1.1684) (layer B.SilkS))
    (fp_text value 0 (at 0 -1.55) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 10 /PD))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 24 "Net-(R7-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "ADC Pi Hat 0.3" (at 107.696 66.6242) (layer F.SilkS))
  (gr_line (start 95.758 40.0558) (end 124.714 40.0558) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 95.758 67.31) (end 95.758 40.0558) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 124.714 67.31) (end 95.758 67.31) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 124.714 40.0558) (end 124.714 67.31) (layer Edge.Cuts) (width 0.15))
  (zone (net 8) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.3048) (thermal_bridge_width 0.3048))
    (polygon
      (pts
        (xy 124.333 40.4622) (xy 96.139 40.4622) (xy 96.139 66.929) (xy 124.333 66.929)
      )
    )
  )
  (zone (net 8) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.3048) (thermal_bridge_width 0.3048))
    (polygon
      (pts
        (xy 124.333 40.4622) (xy 96.139 40.4622) (xy 96.139 66.929) (xy 124.333 66.929)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 113.3348 67.31) (xy 113.3348 57.3532) (xy 117.7798 57.3532) (xy 117.77345 57.5056) (xy 113.49355 57.5056)
        (xy 113.5126 67.31)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 121.6235 47.0662) (xy 121.6235 47.2186) (xy 117.2801 47.2186) (xy 117.2801 47.0662)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 116.459 58.293) (xy 116.3066 58.293) (xy 116.3066 40.068419) (xy 116.459 40.068419)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 115.4684 65.0748) (xy 115.6208 65.0748) (xy 115.6208 67.3354) (xy 115.4684 67.3354)
      )
    )
  )
)
