<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="39.37" y2="0" width="0" layer="20"/>
<wire x1="39.37" y1="0" x2="39.37" y2="25.4" width="0" layer="20"/>
<wire x1="39.37" y1="25.4" x2="0" y2="25.4" width="0" layer="20"/>
<wire x1="0" y1="25.4" x2="0" y2="0" width="0" layer="20"/>
<text>luislab</text>
<text>5.5V</text>
<text>LTC3106
Solar-Supercapacitor
Energy Harvester</text>
<text>v1.0</text>
<text>GND</text>
<text>PGOOD</text>
<text>VOUT</text>
<text>GND</text>
<text>PGOOD</text>
<text>VOUT</text>
<text>-SOLAR+</text>
<text>+CHARGE-</text>
</plain>
<libraries>
<library name="LuisLab-PowerManagement">
<description>&lt;a href="http://luislab.com"&gt;LuisLab.com&lt;/a&gt; &lt;span style="color:#FF1493"&gt;&lt;b&gt;Power Management&lt;/b&gt;&lt;/span&gt; library
&lt;br /&gt;
&lt;table&gt;
  &lt;tr&gt;&lt;td&gt;&lt;strong&gt;RAD&lt;strong&gt;&lt;/td&gt;&lt;td&gt;Radial Lead Type&lt;/td&gt;&lt;/tr&gt;
  &lt;tr&gt;&lt;td&gt;&lt;strong&gt;POL&lt;strong&gt;&lt;/td&gt;&lt;td&gt;Polarized&lt;/td&gt;&lt;/tr&gt;
  &lt;tr&gt;&lt;td&gt;&lt;strong&gt;&lt;acronym title="Plated Through Hole"&gt;&lt;abbr title="Plated Through Hole"&gt;PTH&lt;/abbr&gt;&lt;/acronym&gt;&lt;strong&gt;&lt;/td&gt;&lt;td&gt;Plated Through Hole&lt;/td&gt;&lt;/tr&gt;
  &lt;tr&gt;&lt;td&gt;&lt;strong&gt;D&lt;strong&gt;&lt;/td&gt;&lt;td&gt;Diameter&lt;/td&gt;&lt;/tr&gt;
  &lt;tr&gt;&lt;td&gt;&lt;strong&gt;LS&lt;strong&gt;&lt;/td&gt;&lt;td&gt;Lead space&lt;/td&gt;&lt;/tr&gt;
  &lt;tr&gt;&lt;td&gt;&lt;strong&gt;TA&lt;strong&gt;&lt;/td&gt;&lt;td&gt;Top Adjust&lt;/td&gt;&lt;/tr&gt;
  &lt;tr&gt;&lt;td&gt;&lt;strong&gt;SA&lt;strong&gt;&lt;/td&gt;&lt;td&gt;Side Adjust&lt;/td&gt;&lt;/tr&gt;
&lt;/table&gt;</description>
<packages>
<package name="QFN-20-3X4MM">
<description>&lt;h2&gt;UDC Package&lt;br/&gt;
20-Lead Plastic QFN (3mm x 4mm)&lt;/h2&gt;
&lt;p style="color:red"&gt;&lt;strong&gt;Note:&lt;/strong&gt; Not a JEDEC package outline.&lt;/p&gt;
&lt;br /&gt;
&lt;img src="http://cds.linear.com/image/34160.png" alt="LTC3106 Package Drawing" height="420"&gt;
&lt;br /&gt;
http://cds.linear.com/docs/en/packaging/QFN_20_05-08-1742.pdf</description>
</package>
</packages>
</library>
<library name="LuisLab-Connectors">
<description>&lt;a href="http://funarduino.com"&gt;FunArduino.com&lt;/a&gt; &lt;span style="color:#FF1493"&gt;&lt;b&gt;Connectors&lt;/b&gt;&lt;/span&gt; library
&lt;br /&gt;
&lt;table&gt;
  &lt;tr&gt;&lt;td&gt;&lt;strong&gt;HDR&lt;strong&gt;&lt;/td&gt;&lt;td&gt;Header&lt;/td&gt;&lt;/tr&gt;
  &lt;tr&gt;&lt;td&gt;&lt;strong&gt;&lt;acronym title="Plated Through Hole"&gt;&lt;abbr title="Plated Through Hole"&gt;PTH&lt;/abbr&gt;&lt;/acronym&gt;&lt;strong&gt;&lt;/td&gt;&lt;td&gt;Plated Through Hole&lt;/td&gt;&lt;/tr&gt;
  &lt;tr&gt;&lt;td&gt;&lt;strong&gt;RA&lt;strong&gt;&lt;/td&gt;&lt;td&gt;Right Angle&lt;/td&gt;&lt;/tr&gt;
  &lt;tr&gt;&lt;td&gt;&lt;strong&gt;STR&lt;strong&gt;&lt;/td&gt;&lt;td&gt;Straight&lt;/td&gt;&lt;/tr&gt;
  &lt;tr&gt;&lt;td&gt;&lt;strong&gt;BC&lt;strong&gt;&lt;/td&gt;&lt;td&gt;Breadboard Compatible&lt;/td&gt;&lt;/tr&gt;
  &lt;tr&gt;&lt;td&gt;&lt;strong&gt;G[#,..,#]&lt;strong&gt;&lt;/td&gt;&lt;td&gt;Ground pads[pin number]&lt;/td&gt;&lt;/tr&gt;
&lt;/table&gt;</description>
<packages>
<package name="PIN_2X03_0.1&quot;_PTH_STR_G[1,6]">
<description>&lt;h2&gt;Pin Header 2x03, 0.1", Straight, &lt;acronym title="Plated Through Hole"&gt;&lt;abbr title="Plated Through Hole"&gt;PTH&lt;/abbr&gt;&lt;/acronym&gt;&lt;/h2&gt;
&lt;ul&gt;
&lt;li&gt;Pitch: 0.1" (2.54mm)&lt;/li&gt;
&lt;li&gt;Straight pin&lt;/li&gt;
&lt;li&gt;Through hole&lt;/li&gt;
&lt;li&gt;Ground pins: 1, 6&lt;/li&gt;&lt;/ul&gt;
&lt;p style="color:ForestGreen; text-decoration: underline;"&gt;Rev 1.1 - 11-Aug-2017&lt;/p&gt;</description>
</package>
<package name="PIN_1X02_0.1&quot;_PTH_STR_G[0]">
<description>Pin Header 1x02, 0.1" Pitch (2.54mm), Straight Pin, &lt;acronym title="Plated Through Hole"&gt;&lt;abbr title="Plated Through Hole"&gt;PTH&lt;/abbr&gt;&lt;/acronym&gt;&lt;br /&gt;
No Ground Pin
&lt;p style="color:ForestGreen; text-decoration: underline;"&gt;Rev 1.1 - 17-Jul-2017&lt;/p&gt;</description>
</package>
<package name="PIN_1X03_0.1&quot;_PTH_STR_G[1]">
<description>Pin Header 1x03, 0.1" Pitch (2.54mm), Straight Pin, &lt;acronym title="Plated Through Hole"&gt;&lt;abbr title="Plated Through Hole"&gt;PTH&lt;/abbr&gt;&lt;/acronym&gt;&lt;br /&gt;
Ground pin 1
&lt;p style="color:ForestGreen; text-decoration: underline;"&gt;Rev 1.1 - 13-Jul-2017&lt;/p&gt;</description>
</package>
<package name="PIN_1X03_0.1&quot;_PTH_STR_G[0]">
<description>Pin Header 1x03, 0.1" Pitch (2.54mm), Straight Pin, &lt;acronym title="Plated Through Hole"&gt;&lt;abbr title="Plated Through Hole"&gt;PTH&lt;/abbr&gt;&lt;/acronym&gt;&lt;br /&gt;
No Ground Pin
&lt;p style="color:ForestGreen; text-decoration: underline;"&gt;Rev 1.1 - 17-Jul-2017&lt;/p&gt;</description>
</package>
<package name="PIN_1X02_0.1&quot;_PTH_STR_G[1]">
<description>Pin Header 1x02, 0.1" Pitch (2.54mm), Straight Pin, &lt;acronym title="Plated Through Hole"&gt;&lt;abbr title="Plated Through Hole"&gt;PTH&lt;/abbr&gt;&lt;/acronym&gt;&lt;br /&gt;
Ground Pin 1
&lt;p style="color:ForestGreen; text-decoration: underline;"&gt;Rev 1.1 - 27-Jul-2017&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="LuisLab-Pasives">
<description>&lt;a href="http://luislab.com"&gt;LuisLab.com&lt;/a&gt; &lt;span style="color:#FF1493"&gt;&lt;b&gt;Discrete Components&lt;/b&gt;&lt;/span&gt; library
&lt;br /&gt;
&lt;table&gt;
  &lt;tr&gt;&lt;td&gt;&lt;strong&gt;RAD&lt;strong&gt;&lt;/td&gt;&lt;td&gt;Radial Lead Type&lt;/td&gt;&lt;/tr&gt;
  &lt;tr&gt;&lt;td&gt;&lt;strong&gt;POL&lt;strong&gt;&lt;/td&gt;&lt;td&gt;Polarized&lt;/td&gt;&lt;/tr&gt;
  &lt;tr&gt;&lt;td&gt;&lt;strong&gt;&lt;acronym title="Plated Through Hole"&gt;&lt;abbr title="Plated Through Hole"&gt;PTH&lt;/abbr&gt;&lt;/acronym&gt;&lt;strong&gt;&lt;/td&gt;&lt;td&gt;Plated Through Hole&lt;/td&gt;&lt;/tr&gt;
  &lt;tr&gt;&lt;td&gt;&lt;strong&gt;D&lt;strong&gt;&lt;/td&gt;&lt;td&gt;Diameter&lt;/td&gt;&lt;/tr&gt;
  &lt;tr&gt;&lt;td&gt;&lt;strong&gt;LS&lt;strong&gt;&lt;/td&gt;&lt;td&gt;Lead space&lt;/td&gt;&lt;/tr&gt;
  &lt;tr&gt;&lt;td&gt;&lt;strong&gt;TA&lt;strong&gt;&lt;/td&gt;&lt;td&gt;Top Adjust&lt;/td&gt;&lt;/tr&gt;
  &lt;tr&gt;&lt;td&gt;&lt;strong&gt;SA&lt;strong&gt;&lt;/td&gt;&lt;td&gt;Side Adjust&lt;/td&gt;&lt;/tr&gt;
&lt;/table&gt;</description>
<packages>
<package name="0603[1608]">
<description>&lt;acronym title="Surface-Mount Device"&gt;&lt;abbr title="Surface-Mount Device"&gt;SMD&lt;/abbr&gt;&lt;/acronym&gt; 0603 [1008 Metric] Chip Resistors and Chip Capacitors Package
&lt;p style="color:ForestGreen; text-decoration: underline;"&gt;Rev 1.1 - 27-Jul-2017&lt;/p&gt;</description>
</package>
<package name="INDUCTOR_TY_NR_50">
<description>Inductor SMD. Fits Taiyo Youden NR/NRS 50 Series
&lt;br /&gt;
&lt;br /&gt;Fits
&lt;table&gt;
  &lt;tr&gt;&lt;td&gt;Taiyo Yuden &lt;strong&gt;NRS5014T100MMGG&lt;/strong&gt;&lt;/td&gt;&lt;td&gt;&lt;/td&gt;&lt;/tr&gt;
&lt;/table&gt;</description>
</package>
<package name="CAP_POL_PTH_COIN_5.0MM_D19.0MM_V">
<description>&lt;h2&gt;Polarized Capacitor&lt;/h2&gt;
&lt;ul&gt;
&lt;li&gt;Trough Hole&lt;/li&gt;
&lt;li&gt;Coin&lt;/li&gt;
&lt;li&gt;Vertical terminal&lt;/li&gt;
&lt;li&gt;Body Diameter: &lt;strong&gt;19mm&lt;/strong&gt;&lt;/li&gt;
&lt;li&gt;Lead space:  &lt;strong&gt;5.0mm&lt;/strong&gt;&lt;/li&gt;&lt;/ul&gt;
&lt;p style="color:ForestGreen; text-decoration: underline;"&gt;Rev 1.1 - 18-Jul-2017&lt;/p&gt;</description>
</package>
<package name="TRIMPOT_3296W_TA_PTH">
<description>&lt;h2&gt;Trimpot 3296W&lt;/h2&gt;
&lt;ul&gt;
&lt;li&gt;Top Adjust&lt;/li&gt;
&lt;li&gt;Multiturn&lt;/li&gt;&lt;/ul&gt;
&lt;br /&gt;
&lt;img id="ctl50_ctl00_ctl00_DataRepeater_DataFieldsRepeater_17_ProductImage_2" src="http://www.bourns.com/images/Products/resistive-products/3296.gif?sfvrsn=eef3ad9e_0" alt="Trimpot 3296 series"&gt;
&lt;br /&gt;
https://www.bourns.com/pdfs/3296.pdf
&lt;p style="color:ForestGreen; text-decoration: underline;"&gt;Rev 1.1 - 19-Jul-2017&lt;/p&gt;</description>
</package>
<package name="CAP_POL_PTH_RAD_2.5MM_D6.3MM_V">
<description>&lt;h2&gt;Polarized Capacitor&lt;/h2&gt;
&lt;ul&gt;
&lt;li&gt;Trough Hole&lt;/li&gt;
&lt;li&gt;Radial&lt;/li&gt;
&lt;li&gt;Vertical mount&lt;/li&gt;
&lt;li&gt;Body Diameter: &lt;strong&gt;6.5mm&lt;/strong&gt;&lt;/li&gt;
&lt;li&gt;Lead space:  &lt;strong&gt;2.5mm&lt;/strong&gt;&lt;/li&gt;
&lt;li&gt;Lead Diameter: &lt;strong&gt;0.5mm&lt;/strong&gt;&lt;/li&gt;&lt;/ul&gt;
&lt;p style="color:ForestGreen; text-decoration: underline;"&gt;Rev 1.1 - 20-Jul-2017&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="LuisLab-Semiconductors">
<description>&lt;a href="http://funarduino.com"&gt;FunArduino.com&lt;/a&gt; &lt;span style="color:#FF1493"&gt;&lt;b&gt;Discrete Components&lt;/b&gt;&lt;/span&gt; library</description>
<packages>
<package name="SOD-323(SC-76)">
<description>&lt;h2&gt;&lt;acronym title="Small Outline Diode"&gt;&lt;abbr title="Small Outline Diode"&gt;SOD&lt;/abbr&gt;&lt;/acronym&gt;323 (JEITA SC-76)&lt;/h2&gt;
JEITA package outline code SC-76
&lt;br /&gt;
&lt;img src="http://cache.nxp.com/assets/images/en/chip-images/sod323_3d.gif" alt="SOD323 plastic surface-mounted package" style="max-width:687px;max-height:360px"&gt;
&lt;br /&gt;
http://www.nxp.com/docs/en/package-information/SOD323.pdf
&lt;p style="color:ForestGreen; text-decoration: underline;"&gt;Rev 1.1 - 13-Sep-2017&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U1" library="LuisLab-PowerManagement" package="QFN-20-3X4MM" value="">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="JP1" library="LuisLab-Connectors" package="PIN_2X03_0.1&quot;_PTH_STR_G[1,6]" value="">
<attribute name="MOUNTING" value="PTH"/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP3" library="LuisLab-Connectors" package="PIN_2X03_0.1&quot;_PTH_STR_G[1,6]" value="">
<attribute name="MOUNTING" value="PTH"/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP6" library="LuisLab-Connectors" package="PIN_1X02_0.1&quot;_PTH_STR_G[0]" value="">
<attribute name="MOUNTING" value="PTH"/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C9" library="LuisLab-Pasives" package="0603[1608]" value="1μF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L1" library="LuisLab-Pasives" package="INDUCTOR_TY_NR_50" value="10μH">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="C2" library="LuisLab-Pasives" package="0603[1608]" value="2.2uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="LuisLab-Semiconductors" package="SOD-323(SC-76)" value="ZLLS400">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="LuisLab-Pasives" package="0603[1608]" value="0.1μF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="LuisLab-Pasives" package="0603[1608]" value="1μF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C10" library="LuisLab-Pasives" package="CAP_POL_PTH_COIN_5.0MM_D19.0MM_V" value="1F">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="LuisLab-Pasives" package="0603[1608]" value="1M">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP2" library="LuisLab-Connectors" package="PIN_1X03_0.1&quot;_PTH_STR_G[0]" value="">
<attribute name="MOUNTING" value=""/>
<attribute name="PITCH" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="LuisLab-Pasives" package="0603[1608]" value="820K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="VR2" library="LuisLab-Pasives" package="TRIMPOT_3296W_TA_PTH" value="2M">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="R3" library="LuisLab-Pasives" package="0603[1608]" value="33Ω">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D2" library="LuisLab-Semiconductors" package="SOD-323(SC-76)" value="5.1V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="LuisLab-Pasives" package="CAP_POL_PTH_RAD_2.5MM_D6.3MM_V" value="330μF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="LuisLab-Pasives" package="CAP_POL_PTH_RAD_2.5MM_D6.3MM_V" value="330μF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="LuisLab-Pasives" package="CAP_POL_PTH_RAD_2.5MM_D6.3MM_V" value="100μF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="LuisLab-Pasives" package="CAP_POL_PTH_RAD_2.5MM_D6.3MM_V" value="47μF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="LuisLab-Pasives" package="CAP_POL_PTH_RAD_2.5MM_D6.3MM_V" value="330μF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP4" library="LuisLab-Connectors" package="PIN_1X03_0.1&quot;_PTH_STR_G[1]" value="">
<attribute name="MOUNTING" value=""/>
<attribute name="PITCH" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="VR1" library="LuisLab-Pasives" package="TRIMPOT_3296W_TA_PTH" value="2M">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="JP5" library="LuisLab-Connectors" package="PIN_1X03_0.1&quot;_PTH_STR_G[0]" value="">
<attribute name="MOUNTING" value=""/>
<attribute name="PITCH" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="LuisLab-Connectors" package="PIN_1X02_0.1&quot;_PTH_STR_G[1]" value="-SOLAR+">
<attribute name="MOUNTING" value="PTH"/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="LuisLab-Connectors" package="PIN_1X02_0.1&quot;_PTH_STR_G[1]" value="+CHARGE-">
<attribute name="MOUNTING" value="PTH"/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J3" library="LuisLab-Connectors" package="PIN_1X03_0.1&quot;_PTH_STR_G[1]" value="">
<attribute name="MOUNTING" value=""/>
<attribute name="PITCH" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="U1" pad="15"/>
<contactref element="U1" pad="21"/>
<contactref element="JP1" pad="1"/>
<contactref element="JP1" pad="6"/>
<contactref element="JP3" pad="1"/>
<contactref element="JP3" pad="6"/>
<contactref element="C9" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="U1" pad="1"/>
<contactref element="U1" pad="11"/>
<contactref element="C7" pad="1"/>
<contactref element="C10" pad="-"/>
<contactref element="R2" pad="2"/>
<contactref element="D2" pad="+"/>
<contactref element="C5" pad="-"/>
<contactref element="C8" pad="-"/>
<contactref element="C4" pad="-"/>
<contactref element="C1" pad="-"/>
<contactref element="C6" pad="-"/>
<contactref element="JP4" pad="1"/>
<contactref element="VR1" pad="CCW"/>
<contactref element="J3" pad="1"/>
<contactref element="J2" pad="1"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="FDT">
</signal>
<signal name="N$1">
</signal>
<signal name="OS1">
<contactref element="U1" pad="5"/>
<contactref element="JP1" pad="5"/>
</signal>
<signal name="OS2">
<contactref element="U1" pad="6"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="VCC">
<contactref element="U1" pad="4"/>
<contactref element="JP1" pad="4"/>
<contactref element="JP1" pad="3"/>
<contactref element="JP3" pad="3"/>
<contactref element="JP3" pad="4"/>
<contactref element="C3" pad="2"/>
<contactref element="JP2" pad="1"/>
<contactref element="JP4" pad="3"/>
</signal>
<signal name="SS2">
<contactref element="U1" pad="9"/>
<contactref element="JP3" pad="2"/>
</signal>
<signal name="SS1">
<contactref element="U1" pad="10"/>
<contactref element="JP3" pad="5"/>
</signal>
<signal name="VSTORE">
<contactref element="JP5" pad="1"/>
<contactref element="U1" pad="14"/>
<contactref element="U1" pad="19"/>
<contactref element="JP6" pad="1"/>
<contactref element="J2" pad="2"/>
</signal>
<signal name="VCAP">
<contactref element="U1" pad="20"/>
<contactref element="C9" pad="2"/>
<contactref element="C8" pad="+"/>
<contactref element="JP6" pad="2"/>
</signal>
<signal name="SW1">
<contactref element="L1" pad="1"/>
<contactref element="U1" pad="18"/>
</signal>
<signal name="SW2">
<contactref element="L1" pad="2"/>
<contactref element="U1" pad="17"/>
<contactref element="D1" pad="+"/>
</signal>
<signal name="VAUX">
<contactref element="U1" pad="3"/>
<contactref element="C2" pad="2"/>
<contactref element="D1" pad="-"/>
</signal>
<signal name="VOUT">
<contactref element="C10" pad="+"/>
<contactref element="C1" pad="+"/>
<contactref element="U1" pad="2"/>
<contactref element="R1" pad="2"/>
<contactref element="J3" pad="3"/>
</signal>
<signal name="VIN">
<contactref element="U1" pad="16"/>
<contactref element="C7" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="D2" pad="-"/>
<contactref element="C5" pad="+"/>
<contactref element="C4" pad="+"/>
<contactref element="C6" pad="+"/>
<contactref element="JP5" pad="3"/>
</signal>
<signal name="PGOOD">
<contactref element="U1" pad="7"/>
<contactref element="R1" pad="1"/>
<contactref element="J3" pad="2"/>
</signal>
<signal name="N$10">
<contactref element="JP2" pad="3"/>
<contactref element="VR2" pad="CW"/>
</signal>
<signal name="N$9">
<contactref element="VR2" pad="CCW"/>
<contactref element="VR2" pad="W"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="MPP">
<contactref element="JP2" pad="2"/>
<contactref element="U1" pad="8"/>
</signal>
<signal name="ILIMSEL">
<contactref element="U1" pad="12"/>
<contactref element="JP4" pad="2"/>
</signal>
<signal name="RUN">
<contactref element="U1" pad="13"/>
<contactref element="VR1" pad="W"/>
</signal>
<signal name="N$7">
<contactref element="JP5" pad="2"/>
<contactref element="VR1" pad="CW"/>
</signal>
<signal name="N$2">
<contactref element="J1" pad="2"/>
<contactref element="R3" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
