(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 51)
    (no_connects 0)
    (area 106.831381 45.644999 176.859001 90.526619)
    (thickness 1.6)
    (drawings 6)
    (tracks 89)
    (zones 0)
    (modules 17)
    (nets 34)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.254)
    (trace_clearance 0.254)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.254)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 4.064 4.064)
    (pad_drill 3.302)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue false)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory GERBERS/))
  )
  (net 0 "")
  (net 1 VIN)
  (net 2 GND)
  (net 3 V33)
  (net 4 "Net-(J1-Pad1)")
  (net 5 "Net-(J1-Pad2)")
  (net 6 "Net-(J1-Pad3)")
  (net 7 "Net-(J1-Pad4)")
  (net 8 "Net-(J1-Pad5)")
  (net 9 "Net-(J1-Pad6)")
  (net 10 "Net-(J2-Pad1)")
  (net 11 "Net-(J2-Pad2)")
  (net 12 "Net-(J2-Pad3)")
  (net 13 "Net-(J2-Pad4)")
  (net 14 "Net-(J2-Pad5)")
  (net 15 "Net-(J2-Pad6)")
  (net 16 "Net-(J2-Pad7)")
  (net 17 "Net-(J2-Pad8)")
  (net 18 "Net-(J2-Pad9)")
  (net 19 "Net-(J2-Pad10)")
  (net 20 "Net-(J2-Pad11)")
  (net 21 "Net-(J3-Pad1)")
  (net 22 "Net-(J4-Pad2)")
  (net 23 "Net-(J4-Pad3)")
  (net 24 VFO_CLK)
  (net 25 AUX_CLK)
  (net 26 BFO_CLK)
  (net 27 I2C_SDA)
  (net 28 I2C_SCL)
  (net 29 "Net-(C2-Pad1)")
  (net 30 "Net-(J1-Pad9)")
  (net 31 "Net-(J1-Pad10)")
  (net 32 "Net-(J1-Pad11)")
  (net 33 "Net-(J1-Pad12)")
  (net_class Default "This is the default net class."
    (clearance 0.254)
    (trace_width 0.254)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net AUX_CLK)
    (add_net BFO_CLK)
    (add_net GND)
    (add_net I2C_SCL)
    (add_net I2C_SDA)
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad10)")
    (add_net "Net-(J1-Pad11)")
    (add_net "Net-(J1-Pad12)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J1-Pad9)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J2-Pad10)")
    (add_net "Net-(J2-Pad11)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J2-Pad4)")
    (add_net "Net-(J2-Pad5)")
    (add_net "Net-(J2-Pad6)")
    (add_net "Net-(J2-Pad7)")
    (add_net "Net-(J2-Pad8)")
    (add_net "Net-(J2-Pad9)")
    (add_net "Net-(J3-Pad1)")
    (add_net "Net-(J4-Pad2)")
    (add_net "Net-(J4-Pad3)")
    (add_net V33)
    (add_net VFO_CLK)
    (add_net VIN)
  )
  (module kc1fsz-footprint-library:Adafruit_SI5351a_Module (layer F.Cu) (tedit 5B0DFB99)
    (at 157.48 73.025 270)
    (fp_text reference U3 (at 5.207 3.302 270) (layer F.SilkS))
    (fp_text value Adafruit_SI5351a (at 0 -5.08 270) (layer F.Fab))
    (fp_text user CLK0 (at -7.493 1.778 270) (layer F.SilkS))
    (fp_text user CLK1 (at -5.08 -1.651 270) (layer F.SilkS))
    (fp_text user CLK2 (at -2.286 1.778 270) (layer F.SilkS))
    (fp_text user SCL (at 0 -1.778 270) (layer F.SilkS))
    (fp_text user SDA (at 2.54 1.778 270) (layer F.SilkS))
    (fp_text user GND (at 5.207 -1.778 270) (layer F.SilkS))
    (fp_text user VIN (at 7.62 1.778 270) (layer F.SilkS))
    (pad 7 thru_hole circle (at -7.62 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 24 VFO_CLK))
    (pad 6 thru_hole circle (at -5.08 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 25 AUX_CLK))
    (pad 5 thru_hole circle (at -2.54 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 26 BFO_CLK))
    (pad 4 thru_hole circle (at 0 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 28 I2C_SCL))
    (pad 3 thru_hole circle (at 2.54 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 27 I2C_SDA))
    (pad 2 thru_hole circle (at 5.08 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole rect (at 7.62 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 3 V33))
    (pad "" thru_hole circle (at -12.7 0 270) (size 4.064 4.064) (drill 3.302) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 12.7 0 270) (size 4.064 4.064) (drill 3.302) (layers *.Cu *.Mask))
  )
  (module Pin_Headers:Pin_Header_Straight_1x11_Pitch2.54mm (layer F.Cu) (tedit 5B0F47F7)
    (at 121.285 85.725 90)
    (descr "Through hole straight pin header, 1x11, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x11 2.54mm single row")
    (fp_text reference J2 (at 2.54 1.27 90) (layer F.SilkS))
    (fp_text value Conn_01x11 (at 0 27.73 90) (layer F.Fab))
    (fp_text user %R (at 0 12.7 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(J2-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(J2-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(J2-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(J2-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(J2-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(J2-Pad6)"))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(J2-Pad7)"))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(J2-Pad8)"))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(J2-Pad9)"))
    (pad 10 thru_hole oval (at 0 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(J2-Pad10)"))
    (pad 11 thru_hole oval (at 0 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(J2-Pad11)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x11_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01_Pitch2.54mm (layer F.Cu) (tedit 5B0F44FE)
    (at 117.475 85.725)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference J3 (at -2.54 -1.905) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 2.33) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(J3-Pad1)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x01_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 5B0DFE4A)
    (at 151.765 65.405)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J5 (at 1.397 -2.159) (layer F.SilkS))
    (fp_text value Conn_01x03 (at 0 7.41) (layer F.Fab))
    (fp_text user %R (at 0 2.54 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 VFO_CLK))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 AUX_CLK))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 BFO_CLK))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module kc1fsz-footprint-library:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5B0DF17D)
    (at 127 55.753 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R1 (at 3.81 0 90) (layer F.SilkS))
    (fp_text value 10 (at 3.81 1.86 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 29 "Net-(C2-Pad1)"))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 VIN))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module teensy:Teensy30_31_32_LC (layer F.Cu) (tedit 5B0F47E4)
    (at 130.175 73.025)
    (fp_text reference U1 (at 0 -10.16) (layer F.SilkS))
    (fp_text value Teensy3.2 (at 0 10.16) (layer F.Fab) hide)
    (fp_text user T3.2 (at -10.16 -2.54 90) (layer F.SilkS))
    (fp_text user T3.1 (at -6.35 -2.54 90) (layer F.SilkS))
    (pad 17 thru_hole circle (at 16.51 0) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
    (pad 18 thru_hole circle (at 16.51 -2.54) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
    (pad 19 thru_hole circle (at 16.51 -5.08) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(J1-Pad1)"))
    (pad 20 thru_hole circle (at 16.51 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(J1-Pad2)"))
    (pad 16 thru_hole circle (at 16.51 2.54) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 3 V33))
    (pad 15 thru_hole circle (at 16.51 5.08) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
    (pad 14 thru_hole circle (at 16.51 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 20 "Net-(J2-Pad11)"))
    (pad 21 thru_hole circle (at 13.97 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(J1-Pad3)"))
    (pad 22 thru_hole circle (at 11.43 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(J1-Pad4)"))
    (pad 23 thru_hole circle (at 8.89 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(J1-Pad5)"))
    (pad 24 thru_hole circle (at 6.35 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(J1-Pad6)"))
    (pad 25 thru_hole circle (at 3.81 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 27 I2C_SDA))
    (pad 26 thru_hole circle (at 1.27 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 28 I2C_SCL))
    (pad 27 thru_hole circle (at -1.27 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 30 "Net-(J1-Pad9)"))
    (pad 28 thru_hole circle (at -3.81 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 31 "Net-(J1-Pad10)"))
    (pad 29 thru_hole circle (at -6.35 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 32 "Net-(J1-Pad11)"))
    (pad 30 thru_hole circle (at -8.89 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 33 "Net-(J1-Pad12)"))
    (pad 31 thru_hole circle (at -11.43 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
    (pad 32 thru_hole circle (at -13.97 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(J4-Pad3)"))
    (pad 33 thru_hole circle (at -16.51 -7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(J4-Pad2)"))
    (pad 34 thru_hole circle (at -13.97 -5.08) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
    (pad 35 thru_hole circle (at -8.89 -5.08) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
    (pad 36 thru_hole circle (at -6.35 -5.08) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
    (pad 37 thru_hole circle (at -3.81 -5.08) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
    (pad 13 thru_hole circle (at 13.97 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(J2-Pad10)"))
    (pad 12 thru_hole circle (at 11.43 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 18 "Net-(J2-Pad9)"))
    (pad 11 thru_hole circle (at 8.89 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(J2-Pad8)"))
    (pad 10 thru_hole circle (at 6.35 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(J2-Pad7)"))
    (pad 9 thru_hole circle (at 3.81 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(J2-Pad6)"))
    (pad 8 thru_hole circle (at 1.27 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(J2-Pad5)"))
    (pad 7 thru_hole circle (at -1.27 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(J2-Pad4)"))
    (pad 6 thru_hole circle (at -3.81 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(J2-Pad3)"))
    (pad 5 thru_hole circle (at -6.35 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(J2-Pad2)"))
    (pad 4 thru_hole circle (at -8.89 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(J2-Pad1)"))
    (pad 3 thru_hole circle (at -11.43 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
    (pad 2 thru_hole circle (at -13.97 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
    (pad 1 thru_hole rect (at -16.51 7.62) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 38 thru_hole circle (at -1.27 0) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask))
    (pad 39 thru_hole circle (at 1.27 0) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask))
    (pad 40 thru_hole circle (at 3.81 0) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask))
    (pad 41 thru_hole circle (at 6.35 0) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask))
    (pad 42 thru_hole circle (at 8.89 0) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask))
    (pad 43 thru_hole circle (at 11.43 0) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask))
    (pad 44 thru_hole circle (at 13.97 0) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask))
    (pad 45 thru_hole circle (at 13.97 -2.54) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask))
    (pad 46 thru_hole circle (at 11.43 -2.54) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask))
    (pad 47 thru_hole circle (at 8.89 -2.54) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask))
    (pad 48 thru_hole circle (at 6.35 -2.54) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask))
    (pad 49 thru_hole circle (at 3.81 -2.54) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask))
    (pad 50 thru_hole circle (at 1.27 -2.54) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask))
    (pad 51 thru_hole circle (at -1.27 -2.54) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask))
    (pad 52 thru_hole circle (at -6.35 0) (size 1.9 1.9) (drill 0.5) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(J3-Pad1)"))
    (pad 52 thru_hole circle (at -10.16 0) (size 1.9 1.9) (drill 0.5) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(J3-Pad1)"))
  )
  (module Pin_Headers:Pin_Header_Straight_1x04_Pitch2.54mm (layer F.Cu) (tedit 5B0DF1B2)
    (at 151.765 82.55 180)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference U2 (at 0 -3.175 180) (layer F.SilkS))
    (fp_text value OLED_128x64 (at 0 9.95 180) (layer F.Fab))
    (fp_text user %R (at 0 3.81 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 V33))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 I2C_SCL))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 I2C_SDA))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x04_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04_Pitch2.54mm (layer F.Cu) (tedit 5B0F44E9)
    (at 111.633 48.895)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference J4 (at 2.54 0) (layer F.SilkS))
    (fp_text value Conn_01x04 (at 0 9.95) (layer F.Fab) hide)
    (fp_text user %R (at 0 3.81 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 VIN))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(J4-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(J4-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x04_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:CP_Radial_D10.0mm_P5.00mm (layer F.Cu) (tedit 5B0F4679)
    (at 117.094 52.451)
    (descr "CP, Radial series, Radial, pin pitch=5.00mm, , diameter=10mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 5.00mm  diameter 10mm Electrolytic Capacitor")
    (fp_text reference C1 (at 0.381 -2.921) (layer F.SilkS))
    (fp_text value 220u (at 2.5 6.31) (layer F.Fab))
    (fp_text user %R (at 2.5 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 VIN))
    (pad 2 thru_hole circle (at 5 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D10.0mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:CP_Radial_D10.0mm_P5.00mm (layer F.Cu) (tedit 5B0F467D)
    (at 131.826 52.324)
    (descr "CP, Radial series, Radial, pin pitch=5.00mm, , diameter=10mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 5.00mm  diameter 10mm Electrolytic Capacitor")
    (fp_text reference C2 (at 0.889 -2.794) (layer F.SilkS))
    (fp_text value 220u (at 2.5 6.31) (layer F.Fab))
    (fp_text user %R (at 2.5 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 29 "Net-(C2-Pad1)"))
    (pad 2 thru_hole circle (at 5 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D10.0mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module kc1fsz-footprint-library:C_Disc_D4.7mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 5B0F4697)
    (at 141.859 50.419 270)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=4.7*2.5mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 4.7mm width 2.5mm Capacitor")
    (fp_text reference C3 (at 2.286 0.254 270) (layer F.SilkS))
    (fp_text value 0.1u (at 2.5 2.56 270) (layer F.Fab))
    (fp_text user %R (at 2.5 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "Net-(C2-Pad1)"))
    (pad 2 thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D4.7mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:CP_Radial_D5.0mm_P2.50mm (layer F.Cu) (tedit 597BC7C2)
    (at 148.717 55.245 180)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor")
    (fp_text reference C4 (at 1.25 -3.81 180) (layer F.SilkS))
    (fp_text value 10u (at 1.25 3.81 180) (layer F.Fab))
    (fp_text user %R (at 1.25 0 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 V33))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D5.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-220_Vertical (layer F.Cu) (tedit 5B0F468A)
    (at 147.066 49.403)
    (descr "TO-220, Vertical, RM 2.54mm")
    (tags "TO-220 Vertical RM 2.54mm")
    (fp_text reference U4 (at 9.144 0.127) (layer F.SilkS))
    (fp_text value LM1117-3.3 (at 2.54 3.92) (layer F.Fab))
    (fp_text user %R (at 9.144 -0.508) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 3 V33))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 29 "Net-(C2-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-220_Vertical.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x12_Pitch2.54mm (layer F.Cu) (tedit 5B0F423C)
    (at 149.225 60.579 270)
    (descr "Through hole straight pin header, 1x12, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x12 2.54mm single row")
    (fp_text reference J1 (at 0 -2.33 270) (layer F.SilkS))
    (fp_text value Conn_01x12 (at 0 30.27 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 13.97 360) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(J1-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(J1-Pad6)"))
    (pad 7 thru_hole oval (at 0 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 I2C_SDA))
    (pad 8 thru_hole oval (at 0 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 I2C_SCL))
    (pad 9 thru_hole oval (at 0 20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 "Net-(J1-Pad9)"))
    (pad 10 thru_hole oval (at 0 22.86 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 "Net-(J1-Pad10)"))
    (pad 11 thru_hole oval (at 0 25.4 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 "Net-(J1-Pad11)"))
    (pad 12 thru_hole oval (at 0 27.94 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 "Net-(J1-Pad12)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x12_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors:1pin (layer F.Cu) (tedit 5B0F4569)
    (at 156.845 53.34)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.302) (layers *.Cu *.Mask))
  )
  (module Connectors:1pin (layer F.Cu) (tedit 5B0F4573)
    (at 112.395 85.725)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.302) (layers *.Cu *.Mask))
  )
  (module Connectors:1pin (layer F.Cu) (tedit 5B0F456E)
    (at 112.395 60.96)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.302) (layers *.Cu *.Mask))
  )
  (gr_line (start 109.22 88.9) (end 160.655 88.9) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 160.655 88.9) (end 160.655 45.72) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 160.655 45.72) (end 109.22 45.72) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 109.22 45.72) (end 109.22 88.9) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text KC1FSZ (at 133.35 76.835) (layer B.SilkS))
  (gr_text "2018-05 v1" (at 119.761 76.708) (layer B.SilkS))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 160.02 87.63) (xy 109.22 87.63) (xy 109.22 46.99) (xy 160.02 46.99)
      )
    )
  )
)
