(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
  )
  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "GND")
  (net 2 "VCC")
  (net 3 "/SCL")
  (net 4 "/SDA")
  (net 5 "/ANT")
  (net 6 "VDD")
  (net 7 "unconnected-(GS1-GS-Pad1)")
  (net 8 "Net-(U3-OUT)")
  (net 9 "/PZR")
  (net 10 "unconnected-(U1-FD-Pad4)")
  (net 11 "unconnected-(U2-GPO-Pad7)")
  (net 12 "unconnected-(U4-PD4-Pad1)")
  (net 13 "unconnected-(U4-PD5-Pad2)")
  (net 14 "unconnected-(U4-PD6-Pad3)")
  (net 15 "unconnected-(U4-PC0-Pad10)")
  (net 16 "unconnected-(U4-PC1-Pad11)")
  (net 17 "unconnected-(U4-PD2-Pad19)")
  (net 18 "unconnected-(U4-PD3-Pad20)")
  (net 19 "/R")
  (net 20 "/G")
  (net 21 "/B")
  (net 22 "/PZ+")
  (net 23 "/PZ-")
  (net 24 "/RED")
  (net 25 "/GREEN")
  (net 26 "/BLUE")
  (net 27 "unconnected-(U4-PC7-Pad17)")
  (net 28 "unconnected-(U4-PC6-Pad16)")
  (net 29 "unconnected-(U4-PC5-Pad15)")
  (net 30 "/~{RST}")
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (at 120.65 92.075 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "D:/boards/nfc-tst/nfc-tst/nfc-tst.sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R3" (at 0 2.54 -180) (layer "F.SilkS") hide)
    (fp_text value "100" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "VDD") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "VCC") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (at 123.825 92.075 180)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "Sheetfile" "D:/boards/nfc-tst/nfc-tst/nfc-tst.sch")
    (property "Sheetname" "")
    (property "ki_description" "Current Sense Amp")
    (attr smd)
    (fp_text reference "U3" (at -3.175 0) (layer "F.SilkS") hide)
    (fp_text value "MAX9634" (at 0 2.4) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.1375 -0.95 180) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "2" smd roundrect (at -1.1375 0 180) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95 180) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "Net-(U3-OUT)") (pinfunction "OUT") (pintype "output"))
    (pad "4" smd roundrect (at 1.1375 0.95 180) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "VDD") (pinfunction "RS-") (pintype "input"))
    (pad "5" smd roundrect (at 1.1375 -0.95 180) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "VCC") (pinfunction "RS+") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "B.Cu")
    (at 128.27 84.455 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "D:/boards/nfc-tst/nfc-tst/nfc-tst.sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C1" (at -2.413 0 90) (layer "B.SilkS"))
    (fp_text value "1uF" (at 0 -1.43 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.775 0 270) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 6 "VDD") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 270) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_JST:JST_SH_SM04B-SRSS-TB_1x04-1MP_P1.00mm_Horizontal" (layer "B.Cu")
    (at 133.35 79.375)
    (descr "JST SH series connector, SM04B-SRSS-TB (http://www.jst-mfg.com/product/pdf/eng/eSH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST SH top entry")
    (property "Sheetfile" "D:/boards/nfc-tst/nfc-tst/nfc-tst.sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connectable mounting pin connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr smd)
    (fp_text reference "QWIIC1" (at 0 0) (layer "B.SilkS") hide)
    (fp_text value "Conn_01x04_MountingPin" (at 0 -3.98) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.5 2) (size 0.6 1.55) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" smd roundrect (at -0.5 2) (size 0.6 1.55) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "VCC") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" smd roundrect (at 0.5 2) (size 0.6 1.55) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 4 "/SDA") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" smd roundrect (at 1.5 2) (size 0.6 1.55) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 3 "/SCL") (pinfunction "Pin_4") (pintype "passive"))
    (pad "MP" smd roundrect (at -2.8 -1.875) (size 1.2 1.8) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 1 "GND") (pinfunction "MountPin") (pintype "passive"))
    (pad "MP" smd roundrect (at 2.8 -1.875) (size 1.2 1.8) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 1 "GND") (pinfunction "MountPin") (pintype "passive"))
    (model "${KISYS3DMOD}/Connector_JST.3dshapes/JST_SH_SM04B-SRSS-TB_1x04-1MP_P1.00mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprint:banana" (layer "B.Cu")
    (at 120.65 101.6)
    (property "Field4" "XXX-00000")
    (property "Sheetfile" "D:/boards/nfc-tst/nfc-tst/nfc-tst.sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J4" (at 0 -0.5) (layer "B.SilkS"))
    (fp_text value "BANANA_CONN" (at 0 0.5) (layer "B.Fab"))
    (pad "1" thru_hole custom (at 0 0) (size 6.35 6.35) (drill 4.064) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "1") (pintype "passive") (zone_connect 0) (thermal_bridge_angle 45)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly
          (pts
            (xy 0 -3.175)
            (xy 0 3.175)
            (xy -6.35 3.175)
            (xy -6.35 -3.175)
          )
          (width 0) (fill yes))
      ))
  )
  (footprint "footprint:banana" (layer "B.Cu")
    (at 120.65 82.55)
    (property "Field4" "XXX-00000")
    (property "Sheetfile" "D:/boards/nfc-tst/nfc-tst/nfc-tst.sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J5" (at 0 -0.5) (layer "B.SilkS"))
    (fp_text value "BANANA_CONN" (at 0 0.5) (layer "B.Fab"))
    (pad "1" thru_hole custom (at 0 0) (size 6.35 6.35) (drill 4.064) (layers "*.Cu" "*.Mask")
      (net 6 "VDD") (pinfunction "1") (pintype "passive") (zone_connect 0) (thermal_bridge_angle 45)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly
          (pts
            (xy 0 -3.175)
            (xy 0 3.175)
            (xy -6.35 3.175)
            (xy -6.35 -3.175)
          )
          (width 0) (fill yes))
      ))
  )
  (footprint "Buzzer_Beeper:Buzzer_Murata_PKMCS0909E4000-R1" (layer "B.Cu")
    (at 119.38 92.075 90)
    (descr "Murata Buzzer http://www.murata.com/en-us/api/pdfdownloadapi?cate=&partno=PKMCS0909E4000-R1")
    (tags "Murata Buzzer Beeper")
    (property "Sheetfile" "D:/boards/nfc-tst/nfc-tst/nfc-tst.sch")
    (property "Sheetname" "")
    (property "ki_description" "Crystal speaker/transducer")
    (property "ki_keywords" "crystal speaker ultrasonic transducer")
    (attr smd)
    (fp_text reference "PIEZO1" (at 2.286 0 180) (layer "B.SilkS") hide)
    (fp_text value "Speaker_Crystal" (at 0 -5.5 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd rect (at -4.35 0 90) (size 1.3 3.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 9 "/PZR") (pinfunction "1") (pintype "input"))
    (pad "2" smd rect (at 4.35 0 90) (size 1.3 3.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 23 "/PZ-") (pinfunction "2") (pintype "input"))
    (model "${KISYS3DMOD}/Buzzer_Beeper.3dshapes/Buzzer_Murata_PKMCS0909E4000-R1.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprint:banana" (layer "B.Cu")
    (at 120.65 120.65)
    (property "Field4" "XXX-00000")
    (property "Sheetfile" "D:/boards/nfc-tst/nfc-tst/nfc-tst.sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J3" (at 0 -0.5) (layer "B.SilkS"))
    (fp_text value "BANANA_CONN" (at 0 0.5) (layer "B.Fab"))
    (pad "1" thru_hole custom (at 0 0) (size 6.35 6.35) (drill 4.064) (layers "*.Cu" "*.Mask")
      (net 8 "Net-(U3-OUT)") (pinfunction "1") (pintype "passive") (zone_connect 0) (thermal_bridge_angle 45)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly
          (pts
            (xy 0 -3.175)
            (xy 0 3.175)
            (xy -6.35 3.175)
            (xy -6.35 -3.175)
          )
          (width 0) (fill yes))
      ))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "B.Cu")
    (at 134.62 91.44 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "D:/boards/nfc-tst/nfc-tst/nfc-tst.sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R1" (at 0 -1.27 90) (layer "B.SilkS"))
    (fp_text value "10K" (at 0 -1.43 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.825 0 90) (size 0.8 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "VCC") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 90) (size 0.8 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 3 "/SCL") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "B.Cu")
    (at 132.08 91.44 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "D:/boards/nfc-tst/nfc-tst/nfc-tst.sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R2" (at 0 -1.27 90) (layer "B.SilkS"))
    (fp_text value "10K" (at 0 -1.43 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.825 0 90) (size 0.8 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "VCC") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 90) (size 0.8 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 4 "/SDA") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "B.Cu")
    (at 127 86.995)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "D:/boards/nfc-tst/nfc-tst/nfc-tst.sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R4" (at -0.635 -1.524) (layer "B.SilkS"))
    (fp_text value "100" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.825 0) (size 0.8 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 9 "/PZR") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0) (size 0.8 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 22 "/PZ+") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "B.Cu")
    (at 141.605 97.155 -90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "D:/boards/nfc-tst/nfc-tst/nfc-tst.sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C4" (at 0 -1.651 90) (layer "B.SilkS"))
    (fp_text value "DNP" (at 0 -1.16 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.48 0 270) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 5 "/ANT") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 270) (size 0.56 0.62) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 5 "/ANT") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Symbol:KiCad-Logo2_8mm_Copper" locked (layer "B.Cu")
    (at 133.35 113.665 90)
    (descr "KiCad Logo")
    (tags "Logo KiCad")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 6.35 90) (layer "B.SilkS") hide)
    (fp_text value "KiCad-Logo2_8mm_Copper" (at 0 -7.62 90) (layer "B.Fab") hide)
  )
  (footprint "Symbol:KiCad-Logo2_8mm_SilkScreen" locked (layer "B.Cu")
    (at 133.35 113.665 90)
    (descr "KiCad Logo")
    (tags "Logo KiCad")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 6.35 90) (layer "B.SilkS") hide)
    (fp_text value "KiCad-Logo2_8mm_SilkScreen" (at 0 -7.62 90) (layer "B.Fab") hide)
  )
  (footprint "footprint:gs_logo_200mil" (layer "B.Cu")
    (at 119.38 111.125 90)
    (property "Sheetfile" "D:/boards/nfc-tst/nfc-tst/nfc-tst.sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "GS1" (at 0 3.175 90) (layer "B.SilkS") hide)
    (fp_text value "GS_logo" (at 0 0.5 90) (layer "B.Fab"))
    (pad "1" smd custom (at 0 0 90) (size 5.08 5.08) (layers "B.Cu")
      (net 7 "unconnected-(GS1-GS-Pad1)") (pinfunction "GS") (pintype "unspecified") (zone_connect 0) (thermal_bridge_angle 45)
      (options (clearance outline) (anchor circle))
      (primitives
      ))
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "B.Cu")
    (at 136.525 91.44 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "D:/boards/nfc-tst/nfc-tst/nfc-tst.sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C2" (at 0 1.43 90) (layer "B.SilkS"))
    (fp_text value "DNP" (at 0 -1.43 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.775 0 90) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "VCC") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 90) (size 0.9 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_Kingbright_AAA3528ESGCT" (layer "B.Cu")
    (at 139.79 79.245 -90)
    (descr "Kingbright, dual LED, 3.5 x 2.8 mm Surface Mount LED Lamp (http://www.kingbrightusa.com/images/catalog/SPEC/AAA3528ESGCT.pdf)")
    (tags "dual led smd")
    (property "Sheetfile" "D:/boards/nfc-tst/nfc-tst/nfc-tst.sch")
    (property "Sheetname" "")
    (property "ki_description" "RGB LED, red/anode/green/blue")
    (property "ki_keywords" "LED RGB diode")
    (attr smd)
    (fp_text reference "D1" (at 0 -0.037) (layer "B.SilkS"))
    (fp_text value "LED_RAGB" (at 0 -2.5 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd rect (at -1.4 0.725 270) (size 1.2 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 19 "/R") (pinfunction "RK") (pintype "passive"))
    (pad "2" smd rect (at 1.4 0.725 270) (size 1.2 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 6 "VDD") (pinfunction "A") (pintype "passive"))
    (pad "3" smd rect (at 1.4 -0.725 270) (size 1.2 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 20 "/G") (pinfunction "GK") (pintype "passive"))
    (pad "4" smd rect (at -1.4 -0.725 270) (size 1.2 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 21 "/B") (pinfunction "BK") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_Kingbright_AAA3528ESGCT.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Button_Switch_SMD:SW_Push_1P1T_NO_Vertical_Wuerth_434133025816" (layer "B.Cu")
    (at 127 90.805 -90)
    (descr "https://katalog.we-online.com/em/datasheet/434133025816.pdf")
    (tags "tactile switch Wurth Wuerth")
    (property "Sheetfile" "D:/boards/nfc-tst/nfc-tst/nfc-tst.sch")
    (property "Sheetname" "")
    (property "ki_description" "Push button switch, generic, two pins")
    (property "ki_keywords" "switch normally-open pushbutton push-button")
    (attr smd)
    (fp_text reference "SW1" (at 0 0 90) (layer "B.SilkS"))
    (fp_text value "SW_Push" (at 0 -2.55 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0.05 0 90) (layer "B.Fab"))
    (pad "1" smd rect (at -2.075 1.075 270) (size 1.05 0.65) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND") (pinfunction "1") (pintype "passive"))
    (pad "1" smd rect (at 2.075 1.075 270) (size 1.05 0.65) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GND") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect (at -2.075 -1.075 270) (size 1.05 0.65) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 30 "/~{RST}") (pinfunction "2") (pintype "passive"))
    (pad "2" smd rect (at 2.05 -1.075 270) (size 1.05 0.65) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 30 "/~{RST}") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/SW_Push_1P1T_NO_Vertical_Wuerth_434133025816.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "B.Cu")
    (at 139.7 86.36 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "D:/boards/nfc-tst/nfc-tst/nfc-tst.sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R6" (at -2.794 0) (layer "B.SilkS"))
    (fp_text value "250" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 20 "/G") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 25 "/GREEN") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm" (layer "B.Cu")
    (at 133.35 86.36)
    (descr "TSSOP, 20 Pin (JEDEC MO-153 Var AC https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "TSSOP SO")
    (property "Sheetfile" "D:/boards/nfc-tst/nfc-tst/nfc-tst.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U4" (at 0 0) (layer "B.SilkS"))
    (fp_text value "CH32V003F4P6" (at 0 -4.2) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -2.8625 2.925) (size 1.475 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 12 "unconnected-(U4-PD4-Pad1)") (pinfunction "PD4") (pintype "bidirectional"))
    (pad "2" smd roundrect (at -2.8625 2.275) (size 1.475 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 13 "unconnected-(U4-PD5-Pad2)") (pinfunction "PD5") (pintype "bidirectional"))
    (pad "3" smd roundrect (at -2.8625 1.625) (size 1.475 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 14 "unconnected-(U4-PD6-Pad3)") (pinfunction "PD6") (pintype "bidirectional"))
    (pad "4" smd roundrect (at -2.8625 0.975) (size 1.475 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 30 "/~{RST}") (pinfunction "PD7") (pintype "bidirectional"))
    (pad "5" smd roundrect (at -2.8625 0.325) (size 1.475 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 22 "/PZ+") (pinfunction "PA1") (pintype "bidirectional"))
    (pad "6" smd roundrect (at -2.8625 -0.325) (size 1.475 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 23 "/PZ-") (pinfunction "PA2") (pintype "bidirectional"))
    (pad "7" smd roundrect (at -2.8625 -0.975) (size 1.475 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "8" smd roundrect (at -2.8625 -1.625) (size 1.475 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 4 "/SDA") (pinfunction "PD0") (pintype "bidirectional"))
    (pad "9" smd roundrect (at -2.8625 -2.275) (size 1.475 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 6 "VDD") (pinfunction "VDD") (pintype "power_in"))
    (pad "10" smd roundrect (at -2.8625 -2.925) (size 1.475 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 15 "unconnected-(U4-PC0-Pad10)") (pinfunction "PC0") (pintype "bidirectional"))
    (pad "11" smd roundrect (at 2.8625 -2.925) (size 1.475 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 16 "unconnected-(U4-PC1-Pad11)") (pinfunction "PC1") (pintype "bidirectional"))
    (pad "12" smd roundrect (at 2.8625 -2.275) (size 1.475 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 24 "/RED") (pinfunction "PC2") (pintype "bidirectional"))
    (pad "13" smd roundrect (at 2.8625 -1.625) (size 1.475 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 25 "/GREEN") (pinfunction "PC3") (pintype "bidirectional"))
    (pad "14" smd roundrect (at 2.8625 -0.975) (size 1.475 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 26 "/BLUE") (pinfunction "PC4") (pintype "bidirectional"))
    (pad "15" smd roundrect (at 2.8625 -0.325) (size 1.475 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 29 "unconnected-(U4-PC5-Pad15)") (pinfunction "PC5") (pintype "bidirectional"))
    (pad "16" smd roundrect (at 2.8625 0.325) (size 1.475 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 28 "unconnected-(U4-PC6-Pad16)") (pinfunction "PC6") (pintype "bidirectional"))
    (pad "17" smd roundrect (at 2.8625 0.975) (size 1.475 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 27 "unconnected-(U4-PC7-Pad17)") (pinfunction "PC7") (pintype "bidirectional"))
    (pad "18" smd roundrect (at 2.8625 1.625) (size 1.475 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 3 "/SCL") (pinfunction "PD1") (pintype "bidirectional"))
    (pad "19" smd roundrect (at 2.8625 2.275) (size 1.475 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 17 "unconnected-(U4-PD2-Pad19)") (pinfunction "PD2") (pintype "bidirectional"))
    (pad "20" smd roundrect (at 2.8625 2.925) (size 1.475 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 18 "unconnected-(U4-PD3-Pad20)") (pinfunction "PD3") (pintype "bidirectional"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/TSSOP-20_4.4x6.5mm_P0.65mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "B.Cu")
    (at 139.7 84.455 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "D:/boards/nfc-tst/nfc-tst/nfc-tst.sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R5" (at -2.794 0) (layer "B.SilkS"))
    (fp_text value "750" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 19 "/R") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 24 "/RED") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "B.Cu")
    (at 139.7 88.265 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "D:/boards/nfc-tst/nfc-tst/nfc-tst.sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, US symbol")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R7" (at -2.794 0) (layer "B.SilkS"))
    (fp_text value "250" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 21 "/B") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 26 "/BLUE") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SO-8_3.9x4.9mm_P1.27mm" (layer "B.Cu")
    (at 130.81 97.155 180)
    (descr "SO, 8 Pin (https://www.nxp.com/docs/en/data-sheet/PCF8523.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SO SO")
    (property "Sheetfile" "D:/boards/nfc-tst/nfc-tst/nfc-tst.sch")
    (property "Sheetname" "")
    (property "ki_description" "NFC/I2C EEPROM, SOIC-8/TSSOP-8/DFN-8")
    (property "ki_keywords" "NFC/I2C EEPROM")
    (attr smd)
    (fp_text reference "U2" (at 0 0) (layer "B.SilkS"))
    (fp_text value "ST25DVXXKC" (at 0 -3.4) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -2.575 1.905 180) (size 1.75 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "VCC") (pinfunction "V_EH") (pintype "input"))
    (pad "2" smd roundrect (at -2.575 0.635 180) (size 1.75 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 5 "/ANT") (pinfunction "AC0") (pintype "input"))
    (pad "3" smd roundrect (at -2.575 -0.635 180) (size 1.75 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 5 "/ANT") (pinfunction "AC1") (pintype "input"))
    (pad "4" smd roundrect (at -2.575 -1.905 180) (size 1.75 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "5" smd roundrect (at 2.575 -1.905 180) (size 1.75 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 4 "/SDA") (pinfunction "SDA") (pintype "bidirectional"))
    (pad "6" smd roundrect (at 2.575 -0.635 180) (size 1.75 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 3 "/SCL") (pinfunction "SCL") (pintype "input"))
    (pad "7" smd roundrect (at 2.575 0.635 180) (size 1.75 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 11 "unconnected-(U2-GPO-Pad7)") (pinfunction "GPO") (pintype "input"))
    (pad "8" smd roundrect (at 2.575 1.905 180) (size 1.75 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "VCC") (pinfunction "VCC") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SO-8_3.9x4.9mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SO-8_3.9x4.9mm_P1.27mm" (layer "B.Cu")
    (at 137.795 97.155 90)
    (descr "SO, 8 Pin (https://www.nxp.com/docs/en/data-sheet/PCF8523.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SO SO")
    (property "Sheetfile" "D:/boards/nfc-tst/nfc-tst/nfc-tst.sch")
    (property "Sheetname" "")
    (property "ki_description" "NFC/I2C EEPROM, SOIC-8/TSSOP-8/DFN-8")
    (property "ki_keywords" "NFC/I2C EEPROM")
    (attr smd)
    (fp_text reference "U1" (at 0 0 180) (layer "B.SilkS"))
    (fp_text value "NT3H2111" (at 0 -3.4 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -2.575 1.905 90) (size 1.75 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 5 "/ANT") (pinfunction "LA") (pintype "input"))
    (pad "2" smd roundrect (at -2.575 0.635 90) (size 1.75 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "VSS") (pintype "input"))
    (pad "3" smd roundrect (at -2.575 -0.635 90) (size 1.75 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 3 "/SCL") (pinfunction "SCL") (pintype "input"))
    (pad "4" smd roundrect (at -2.575 -1.905 90) (size 1.75 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 10 "unconnected-(U1-FD-Pad4)") (pinfunction "FD") (pintype "power_in"))
    (pad "5" smd roundrect (at 2.575 -1.905 90) (size 1.75 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 4 "/SDA") (pinfunction "SDA") (pintype "bidirectional"))
    (pad "6" smd roundrect (at 2.575 -0.635 90) (size 1.75 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "VCC") (pinfunction "VCC") (pintype "input"))
    (pad "7" smd roundrect (at 2.575 0.635 90) (size 1.75 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "VCC") (pinfunction "VOUT") (pintype "input"))
    (pad "8" smd roundrect (at 2.575 1.905 90) (size 1.75 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 5 "/ANT") (pinfunction "LB") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SO-8_3.9x4.9mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_arc (start 114.3 79.375) (mid 115.229936 77.129936) (end 117.475 76.2)
    (layer "Edge.Cuts"))
  (gr_arc (start 117.475 127) (mid 115.229936 126.070064) (end 114.3 123.825)
    (layer "Edge.Cuts"))
  (gr_arc (start 177.8 123.825) (mid 176.870064 126.070064) (end 174.625 127)
    (layer "Edge.Cuts"))
  (gr_line (start 177.8 79.375) (end 177.8 123.825)
    (layer "Edge.Cuts"))
  (gr_arc (start 174.625 76.2) (mid 176.870064 77.129936) (end 177.8 79.375)
    (layer "Edge.Cuts"))
  (gr_line (start 174.625 127) (end 133.35 127)
    (layer "Edge.Cuts"))
  (gr_line (start 117.475 76.2) (end 174.625 76.2)
    (layer "Edge.Cuts"))
  (gr_line (start 114.3 123.825) (end 114.3 79.375)
    (layer "Edge.Cuts"))
  (gr_line (start 133.35 127) (end 117.475 127)
    (layer "Edge.Cuts"))
  (gr_text "BUZZER" (at 119.38 92.075) (layer "B.SilkS"))
  (gr_text "Beeping\nBlinking\nBanana plug \nNFC test \nBattle Board\n" (at 175.26 86.995) (layer "B.SilkS"))
  (gr_text "B5" (at 159.512 116.84) (layer "B.SilkS"))
  (gr_text "GND" (at 125.095 101.6 -90) (layer "F.SilkS"))
  (gr_text "VDD" (at 119.634 87.63) (layer "F.SilkS"))
  (gr_text "Vcur\n" (at 125.095 120.65 270) (layer "F.SilkS"))
  (gr_text "VCC" (at 119.634 96.52) (layer "F.SilkS"))
  (gr_text "Vload" (at 125.095 82.55 270) (layer "F.SilkS"))
  (zone (net 1) (net_name "GND") (layer "F.Cu") (hatch edge 0.5)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.254) (thermal_bridge_width 0.3048))
    (polygon
      (pts
        (xy 116.205 76.835)
        (xy 141.605 76.835)
        (xy 141.605 126.365)
        (xy 116.205 126.365)
        (xy 114.935 125.095)
        (xy 114.935 78.105)
      )
    )
  )
)
