(kicad_pcb (version 20171130) (host pcbnew "(5.0.1)-3")
  (general
    (thickness 1.6)
    (drawings 12)
    (tracks 40)
    (zones 0)
    (modules 2)
    (nets 6)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 -BATT)
  (net 2 T)
  (net 3 D)
  (net 4 C)
  (net 5 +BATT)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net C)
    (add_net D)
    (add_net T)
  )
  (net_class Power ""
    (clearance 0.2)
    (trace_width 0.5)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +BATT)
    (add_net -BATT)
  )
  (module Connector_JST:JST_GH_BM05B-GHS-TBT_1x05-1MP_P1.25mm_Vertical (layer F.Cu) (tedit 5C23A0C8)
    (at 137.0076 80.01)
    (descr "JST GH series connector, BM05B-GHS-TBT (http://www.jst-mfg.com/product/pdf/eng/eGH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST GH side entry")
    (attr smd)
    (fp_text reference J2 (at 0 -4.0386) (layer F.SilkS))
    (fp_text value Conn_01x05 (at 0 4) (layer F.Fab))
    (fp_text user %R (at 0 -1.5) (layer F.Fab))
    (pad 1 smd roundrect (at -2.5 1.95) (size 0.6 1.7) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 -BATT))
    (pad 2 smd roundrect (at -1.25 1.95) (size 0.6 1.7) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 T))
    (pad 3 smd roundrect (at 0 1.95) (size 0.6 1.7) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 D))
    (pad 4 smd roundrect (at 1.25 1.95) (size 0.6 1.7) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 C))
    (pad 5 smd roundrect (at 2.5 1.95) (size 0.6 1.7) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 +BATT))
    (pad MP smd roundrect (at -4.35 -1.4) (size 1 2.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad MP smd roundrect (at 4.35 -1.4) (size 1 2.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_GH_BM05B-GHS-TBT_1x05-1MP_P1.25mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module HDRV10W70P500_300_5X2_2702X980X895 (layer F.Cu) (tedit 5C23A514)
    (at 136.9314 99.3648 90)
    (fp_text reference J1 (at -12.4968 -4.0132 90) (layer F.SilkS))
    (fp_text value 5787444-1 (at 0.0254 3.81 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -10 1.5 90) (size 1.56 1.56) (drill 1.04) (layers *.Cu *.Mask)
      (net 1 -BATT))
    (pad 1.1 thru_hole rect (at -10 -1.5 90) (size 1.56 1.56) (drill 1.04) (layers *.Cu *.Mask)
      (net 1 -BATT))
    (pad 2 thru_hole circle (at -5 1.5 90) (size 1.56 1.56) (drill 1.04) (layers *.Cu *.Mask)
      (net 2 T))
    (pad 2.1 thru_hole circle (at -5 -1.5 90) (size 1.56 1.56) (drill 1.04) (layers *.Cu *.Mask)
      (net 2 T))
    (pad 3 thru_hole circle (at 0 1.5 90) (size 1.56 1.56) (drill 1.04) (layers *.Cu *.Mask)
      (net 3 D))
    (pad 3.1 thru_hole circle (at 0 -1.5 90) (size 1.56 1.56) (drill 1.04) (layers *.Cu *.Mask)
      (net 3 D))
    (pad 4 thru_hole circle (at 5 1.5 90) (size 1.56 1.56) (drill 1.04) (layers *.Cu *.Mask)
      (net 4 C))
    (pad 4.1 thru_hole circle (at 5 -1.5 90) (size 1.56 1.56) (drill 1.04) (layers *.Cu *.Mask)
      (net 4 C))
    (pad 5 thru_hole circle (at 10 1.5 90) (size 1.56 1.56) (drill 1.04) (layers *.Cu *.Mask)
      (net 5 +BATT))
    (pad 5.1 thru_hole circle (at 10 -1.5 90) (size 1.56 1.56) (drill 1.04) (layers *.Cu *.Mask)
      (net 5 +BATT))
  )
  (gr_line (start 143.0274 71.3994) (end 143.0274 72.0598) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 131.064 71.3994) (end 131.064 72.0852) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 131.064 117.1702) (end 131.064 117.8306) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 143.002 117.1194) (end 143.002 117.8052) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 131.064 117.1702) (end 131.064 72.0598) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 143.002 117.8052) (end 131.064 117.8306) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 143.0274 72.0598) (end 143.002 117.1448) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 131.064 71.3994) (end 143.0274 71.3994) (layer Edge.Cuts) (width 0.15))
  (gr_circle (center 137.033 115.035144) (end 138.3538 115.847944) (layer Edge.Cuts) (width 0.2))
  (gr_circle (center 136.9568 74.0664) (end 138.2776 74.8792) (layer Edge.Cuts) (width 0.2))
  (gr_text Batt- (at 134.7216 84.3788 90) (layer F.SilkS))
  (gr_text Batt+ (at 140.081 84.3788 90) (layer F.SilkS))
)
