<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="73.73" x2="0" y2="7.54" width="0" layer="20"/>
<wire x1="0" y1="7.54" x2="5" y2="2.54" width="0" layer="20" curve="90"/>
<wire x1="5" y1="2.54" x2="39.12" y2="2.54" width="0" layer="20"/>
<wire x1="39.12" y1="2.54" x2="44.12" y2="7.54" width="0" layer="20" curve="90"/>
<wire x1="44.12" y1="7.54" x2="44.12" y2="73.73" width="0" layer="20"/>
<wire x1="44.12" y1="73.73" x2="39.12" y2="78.73" width="0" layer="20" curve="90"/>
<wire x1="39.12" y1="78.73" x2="5" y2="78.73" width="0" layer="20"/>
<wire x1="5" y1="78.73" x2="0" y2="73.73" width="0" layer="20" curve="90"/>
<text>VIN</text>
<text>GND</text>
<text>SC7</text>
<text>0</text>
<text>1</text>
<text>2</text>
<text>3</text>
<text>4</text>
<text>5</text>
<text>6</text>
<text>7</text>
<text>I2C IN</text>
<text>VIN</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>SC1</text>
<text>SD2</text>
<text>SD1</text>
<text>SC2</text>
<text>SD7</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>TCA9548A</text>
<text>VCC-2</text>
<text>VIN to I2C IN</text>
<text>VIN to VCC-2</text>
<text>IC2 IN to VCC-2</text>
<text>OMSI 5/24/2017</text>
<text>TCA9548A</text>
<text>OMSI 5/24/2017</text>
<text>TCA9548A</text>
<text>TCA9548A</text>
<text>ADAFRUIT #2717</text>
<text>ADAFRUIT #2717</text>
<text>I2C MULTIPLEXER</text>
<text>I2C MULTIPLEXER</text>
<text>ADAFRUIT #2717</text>
<text>THOMAS HUDSON</text>
<text>THOMAS HUDSON</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X12_NO_SILK">
</package>
<package name="MOLEX-1X2">
</package>
<package name="MOLEX-1X4">
</package>
</packages>
</library>
<library name="th_libraries">
<packages>
<package name="STANDOFF-ELECTRICAL">
<description>#8 screw hole, 170mill, 0.30 mask</description>
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
<package name="PAD-JUMPER-2-NC_BY_PASTE_YES_SILK">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J1" library="SparkFun-Connectors" package="1X12_NO_SILK" value=""/>
<element name="J2" library="SparkFun-Connectors" package="1X12_NO_SILK" value=""/>
<element name="S1" library="th_libraries" package="STANDOFF-ELECTRICAL" value="STANDOFF_ELECTRICAL"/>
<element name="S2" library="th_libraries" package="STANDOFF-ELECTRICAL" value="STANDOFF_ELECTRICAL"/>
<element name="S3" library="th_libraries" package="STANDOFF-ELECTRICAL" value="STANDOFF_ELECTRICAL"/>
<element name="S4" library="th_libraries" package="STANDOFF-ELECTRICAL" value="STANDOFF_ELECTRICAL"/>
<element name="R2" library="SparkFun-Passives" package="0805" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="SparkFun-Passives" package="0805" value="10k">
<attribute name="VALUE"/>
</element>
<element name="R4" library="SparkFun-Passives" package="0805" value="10k">
<attribute name="VALUE"/>
</element>
<element name="R5" library="SparkFun-Passives" package="0805" value="10k">
<attribute name="VALUE"/>
</element>
<element name="R6" library="SparkFun-Passives" package="0805" value="10k">
<attribute name="VALUE"/>
</element>
<element name="R7" library="SparkFun-Passives" package="0805" value="10k">
<attribute name="VALUE"/>
</element>
<element name="R8" library="SparkFun-Passives" package="0805" value="10k">
<attribute name="VALUE"/>
</element>
<element name="R9" library="SparkFun-Passives" package="0805" value="10k">
<attribute name="VALUE"/>
</element>
<element name="R10" library="SparkFun-Passives" package="0805" value="10k">
<attribute name="VALUE"/>
</element>
<element name="R11" library="SparkFun-Passives" package="0805" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R12" library="SparkFun-Passives" package="0805" value="10k">
<attribute name="VALUE"/>
</element>
<element name="R13" library="SparkFun-Passives" package="0805" value="10k">
<attribute name="VALUE"/>
</element>
<element name="R14" library="SparkFun-Passives" package="0805" value="10k">
<attribute name="VALUE"/>
</element>
<element name="R15" library="SparkFun-Passives" package="0805" value="10k">
<attribute name="VALUE"/>
</element>
<element name="R16" library="SparkFun-Passives" package="0805" value="10k">
<attribute name="VALUE"/>
</element>
<element name="R17" library="SparkFun-Passives" package="0805" value="10k">
<attribute name="VALUE"/>
</element>
<element name="J3" library="SparkFun-Connectors" package="MOLEX-1X2" value=""/>
<element name="J4" library="SparkFun-Connectors" package="MOLEX-1X4" value=""/>
<element name="R18" library="SparkFun-Passives" package="0805" value="10k">
<attribute name="VALUE"/>
</element>
<element name="R19" library="SparkFun-Passives" package="0805" value="10k">
<attribute name="VALUE"/>
</element>
<element name="J5" library="SparkFun-Connectors" package="MOLEX-1X2" value=""/>
<element name="JP1" library="SparkFun-Passives" package="PAD-JUMPER-2-NC_BY_PASTE_YES_SILK" value="JUMPER-PAD-2-NC_BY_PASTE"/>
<element name="JP2" library="SparkFun-Passives" package="PAD-JUMPER-2-NC_BY_PASTE_YES_SILK" value="JUMPER-PAD-2-NC_BY_PASTE"/>
<element name="JP3" library="SparkFun-Passives" package="PAD-JUMPER-2-NC_BY_PASTE_YES_SILK" value="JUMPER-PAD-2-NC_BY_PASTE"/>
<element name="J6" library="SparkFun-Connectors" package="MOLEX-1X4" value=""/>
<element name="J7" library="SparkFun-Connectors" package="MOLEX-1X4" value=""/>
<element name="J8" library="SparkFun-Connectors" package="MOLEX-1X4" value=""/>
<element name="J9" library="SparkFun-Connectors" package="MOLEX-1X4" value=""/>
<element name="J10" library="SparkFun-Connectors" package="MOLEX-1X4" value=""/>
<element name="J11" library="SparkFun-Connectors" package="MOLEX-1X4" value=""/>
<element name="J12" library="SparkFun-Connectors" package="MOLEX-1X4" value=""/>
<element name="J13" library="SparkFun-Connectors" package="MOLEX-1X4" value=""/>
</elements>
<signals>
<signal name="GND">
<contactref element="J1" pad="11"/>
<contactref element="J3" pad="1"/>
<contactref element="J4" pad="1"/>
<contactref element="J5" pad="1"/>
<contactref element="J6" pad="1"/>
<contactref element="J7" pad="1"/>
<contactref element="J8" pad="1"/>
<contactref element="J9" pad="1"/>
<contactref element="J10" pad="1"/>
<contactref element="J11" pad="1"/>
<contactref element="J12" pad="1"/>
<contactref element="J13" pad="1"/>
</signal>
<signal name="SDA">
<contactref element="J1" pad="10"/>
<contactref element="J4" pad="3"/>
<contactref element="R18" pad="1"/>
</signal>
<signal name="SCL">
<contactref element="J1" pad="9"/>
<contactref element="J4" pad="4"/>
<contactref element="R19" pad="1"/>
</signal>
<signal name="RST">
<contactref element="J1" pad="8"/>
</signal>
<signal name="A0">
<contactref element="J1" pad="7"/>
</signal>
<signal name="A1">
<contactref element="J1" pad="6"/>
</signal>
<signal name="A2">
<contactref element="J1" pad="5"/>
</signal>
<signal name="SD0">
<contactref element="J1" pad="4"/>
<contactref element="R2" pad="1"/>
<contactref element="J6" pad="3"/>
</signal>
<signal name="SC0">
<contactref element="J1" pad="3"/>
<contactref element="R3" pad="1"/>
<contactref element="J6" pad="4"/>
</signal>
<signal name="SD1">
<contactref element="J1" pad="2"/>
<contactref element="R4" pad="1"/>
<contactref element="J7" pad="3"/>
</signal>
<signal name="SC1">
<contactref element="J1" pad="1"/>
<contactref element="R5" pad="1"/>
<contactref element="J7" pad="4"/>
</signal>
<signal name="SD2">
<contactref element="J2" pad="12"/>
<contactref element="R6" pad="1"/>
<contactref element="J8" pad="3"/>
</signal>
<signal name="SC2">
<contactref element="J2" pad="11"/>
<contactref element="R7" pad="1"/>
<contactref element="J8" pad="4"/>
</signal>
<signal name="SD3">
<contactref element="J2" pad="10"/>
<contactref element="R8" pad="1"/>
<contactref element="J9" pad="3"/>
</signal>
<signal name="SC3">
<contactref element="J2" pad="9"/>
<contactref element="R9" pad="1"/>
<contactref element="J9" pad="4"/>
</signal>
<signal name="SD4">
<contactref element="J2" pad="8"/>
<contactref element="R10" pad="1"/>
<contactref element="J10" pad="3"/>
</signal>
<signal name="SC4">
<contactref element="J2" pad="7"/>
<contactref element="R11" pad="1"/>
<contactref element="J10" pad="4"/>
</signal>
<signal name="SD5">
<contactref element="J2" pad="6"/>
<contactref element="R12" pad="1"/>
<contactref element="J11" pad="3"/>
</signal>
<signal name="SC5">
<contactref element="J2" pad="5"/>
<contactref element="R13" pad="1"/>
<contactref element="J11" pad="4"/>
</signal>
<signal name="SD6">
<contactref element="J2" pad="4"/>
<contactref element="R14" pad="1"/>
<contactref element="J12" pad="3"/>
</signal>
<signal name="SC6">
<contactref element="J2" pad="3"/>
<contactref element="R15" pad="1"/>
<contactref element="J12" pad="4"/>
</signal>
<signal name="SD7">
<contactref element="J2" pad="2"/>
<contactref element="R16" pad="1"/>
<contactref element="J13" pad="3"/>
</signal>
<signal name="SC7">
<contactref element="J2" pad="1"/>
<contactref element="R17" pad="1"/>
<contactref element="J13" pad="4"/>
</signal>
<signal name="VIN">
<contactref element="J1" pad="12"/>
<contactref element="J5" pad="2"/>
<contactref element="JP1" pad="2"/>
<contactref element="JP2" pad="2"/>
</signal>
<signal name="VCC_2">
<contactref element="R2" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="R4" pad="2"/>
<contactref element="R5" pad="2"/>
<contactref element="R6" pad="2"/>
<contactref element="R7" pad="2"/>
<contactref element="R8" pad="2"/>
<contactref element="R9" pad="2"/>
<contactref element="R10" pad="2"/>
<contactref element="R11" pad="2"/>
<contactref element="R12" pad="2"/>
<contactref element="R13" pad="2"/>
<contactref element="R14" pad="2"/>
<contactref element="R15" pad="2"/>
<contactref element="R16" pad="2"/>
<contactref element="R17" pad="2"/>
<contactref element="J3" pad="2"/>
<contactref element="JP2" pad="1"/>
<contactref element="JP3" pad="2"/>
<contactref element="J6" pad="2"/>
<contactref element="J7" pad="2"/>
<contactref element="J8" pad="2"/>
<contactref element="J9" pad="2"/>
<contactref element="J10" pad="2"/>
<contactref element="J11" pad="2"/>
<contactref element="J12" pad="2"/>
<contactref element="J13" pad="2"/>
</signal>
<signal name="VCC_1">
<contactref element="R18" pad="2"/>
<contactref element="R19" pad="2"/>
<contactref element="J4" pad="2"/>
<contactref element="JP1" pad="1"/>
<contactref element="JP3" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
