(kicad_pcb (version 20171130) (host pcbnew "(5.1.7)-1")
  (general
    (thickness 1.6)
    (drawings 21)
    (tracks 126)
    (zones 0)
    (modules 27)
    (nets 13)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 0.9906 0.9906)
    (pad_drill 0.9906)
    (pad_to_mask_clearance 0.0508)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 SYS_SWCLK)
  (net 3 SYS_SWDIO)
  (net 4 V_IN)
  (net 5 I2C1_SDA)
  (net 6 I2C1_SCl)
  (net 7 "Net-(R2-Pad1)")
  (net 8 GPIO_Input_2)
  (net 9 V_IN_2)
  (net 10 GPIO_Input_2_2)
  (net 11 GPIO_Input_1)
  (net 12 "Net-(R6-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net GPIO_Input_1)
    (add_net GPIO_Input_2)
    (add_net GPIO_Input_2_2)
    (add_net I2C1_SCl)
    (add_net I2C1_SDA)
    (add_net "Net-(R2-Pad1)")
    (add_net "Net-(R6-Pad1)")
    (add_net SYS_SWCLK)
    (add_net SYS_SWDIO)
    (add_net V_IN)
    (add_net V_IN_2)
  )
  (module "" (layer F.Cu) (tedit 0)
    (at 60.2 79.7)
    (fp_text reference "" (at 50.2 93.6) (layer F.SilkS))
    (fp_text value "" (at 50.2 93.6) (layer F.SilkS))
    (fp_text user GND (at 50.15 93.5 90) (layer B.SilkS))
  )
  (module "" (layer F.Cu) (tedit 0)
    (at 61.4 83.5)
    (fp_text reference "" (at 50.2 93.6) (layer F.SilkS))
    (fp_text value "" (at 50.2 93.6) (layer F.SilkS))
    (fp_text user GND (at 50.15 93.5 90) (layer B.SilkS))
  )
  (module "" (layer F.Cu) (tedit 0)
    (at 0.25 0.5)
    (fp_text reference "" (at 50.2 93.6) (layer F.SilkS))
    (fp_text value "" (at 50.2 93.6) (layer F.SilkS))
  )
  (module "" (layer F.Cu) (tedit 0)
    (at 60.2 79.7)
    (fp_text reference "" (at 50.2 93.6) (layer F.SilkS))
    (fp_text value "" (at 50.2 93.6) (layer F.SilkS))
    (fp_text user GND (at 50.15 93.5 90) (layer B.SilkS))
  )
  (module footprints:0.5mm_by_8mm_slot (layer F.Cu) (tedit 5F8F7D17)
    (at 50.2 93.6)
    (fp_text reference Slot (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value 0.5mm_by_8mm_slot (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole oval (at 0 -0.15) (size 7 0.508) (drill oval 7 0.508) (layers *.Cu *.Mask))
  )
  (module footprints:0.5mm_by_8mm_slot (layer F.Cu) (tedit 5F8F7D17)
    (at 69.85 86.7)
    (fp_text reference Slot (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value 0.5mm_by_8mm_slot (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole oval (at 0 -0.15) (size 7 0.508) (drill oval 7 0.508) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.2mm_M2 (layer F.Cu) (tedit 56D1B4CB)
    (at 49.7 95.8)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2 (at 0 3.2) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3_DIN965_Pad (layer F.Cu) (tedit 56D1B4CB)
    (at 53.7 99)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (attr virtual)
    (fp_text reference H1 (at 0 -3.8) (layer F.SilkS) hide)
    (fp_text value MountingHole_Pad (at 0 3.8) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.6 5.6) (drill 3.2) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module MountingHole:MountingHole_2.2mm_M2 (layer F.Cu) (tedit 56D1B4CB)
    (at 70.3 84.2)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2 (at 0 3.2) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3_DIN965_Pad (layer F.Cu) (tedit 56D1B4CB)
    (at 66.3 81)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (attr virtual)
    (fp_text reference H2 (at 0 -3.8) (layer F.SilkS) hide)
    (fp_text value MountingHole_Pad (at 0 3.8) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.6 5.6) (drill 3.2) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Connector_JST:JST_SH_SM04B-SRSS-TB_1x04-1MP_P1.00mm_Horizontal (layer F.Cu) (tedit 5B78AD87)
    (at 59.9 79.175 180)
    (descr "JST SH series connector, SM04B-SRSS-TB (http://www.jst-mfg.com/product/pdf/eng/eSH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST SH top entry")
    (attr smd)
    (fp_text reference J1 (at 0.2 0.3 180) (layer F.SilkS) hide)
    (fp_text value Conn_01x04 (at 0 3.98 180) (layer F.Fab) hide)
    (pad MP smd roundrect (at 2.8 1.875 180) (size 1.2 1.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333))
    (pad MP smd roundrect (at -2.8 1.875 180) (size 1.2 1.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333))
    (pad 4 smd roundrect (at 1.5 -2 180) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 I2C1_SCl))
    (pad 3 smd roundrect (at 0.5 -2 180) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 I2C1_SDA))
    (pad 2 smd roundrect (at -0.5 -2 180) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.5 -2 180) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 V_IN))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_SH_SM04B-SRSS-TB_1x04-1MP_P1.00mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector:Tag-Connect_TC2030-IDC-NL_2x03_P1.27mm_Vertical (layer B.Cu) (tedit 5A29CEA9)
    (at 59.9 81.7)
    (descr "Tag-Connect programming header; http://www.tag-connect.com/Materials/TC2030-IDC-NL.pdf")
    (tags "tag connect programming header pogo pins")
    (attr virtual)
    (fp_text reference J2 (at 0 -2.7) (layer B.SilkS) hide)
    (fp_text value Conn_02x03_Counter_Clockwise (at 0 2.3) (layer B.Fab) hide)
    (fp_text user KEEPOUT (at 0 0) (layer Cmts.User) hide)
    (fp_text user %R (at 0 0) (layer B.Fab) hide)
    (pad 6 connect circle (at 1.27 0.635) (size 0.7874 0.7874) (layers B.Cu B.Mask)
      (net 1 GND))
    (pad 5 connect circle (at 1.27 -0.635) (size 0.7874 0.7874) (layers B.Cu B.Mask)
      (net 4 V_IN))
    (pad 4 connect circle (at 0 0.635) (size 0.7874 0.7874) (layers B.Cu B.Mask)
      (net 4 V_IN))
    (pad 3 connect circle (at 0 -0.635) (size 0.7874 0.7874) (layers B.Cu B.Mask)
      (net 1 GND))
    (pad 2 connect circle (at -1.27 0.635) (size 0.7874 0.7874) (layers B.Cu B.Mask)
      (net 2 SYS_SWCLK))
    (pad 1 connect circle (at -1.27 -0.635) (size 0.7874 0.7874) (layers B.Cu B.Mask)
      (net 3 SYS_SWDIO))
    (pad "" np_thru_hole circle (at -2.54 0) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 2.54 -1.016) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 2.54 1.016) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask))
  )
  (module footprints:QRD1114 (layer B.Cu) (tedit 0)
    (at 70.19 91.3)
    (fp_text reference U3 (at 0.01 -1.27 90) (layer B.SilkS) hide)
    (fp_text value QRD1114 (at 1.055 -1.27 90) (layer B.SilkS))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User) hide)
    (fp_text user * (at 0 0) (layer B.SilkS))
    (fp_text user * (at 0 0) (layer B.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.27 1.27) (drill 0.762) (layers *.Cu *.Mask)
      (net 10 GPIO_Input_2_2))
    (pad 2 thru_hole circle (at 0 -2.54) (size 1.27 1.27) (drill 0.762) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole circle (at 2.11 -2.54) (size 1.27 1.27) (drill 0.762) (layers *.Cu *.Mask)
      (net 12 "Net-(R6-Pad1)"))
    (pad 4 thru_hole circle (at 2.11 0) (size 1.27 1.27) (drill 0.762) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Connector_Wire:SolderWirePad_1x01_SMD_1x2mm (layer F.Cu) (tedit 5DD6EB27)
    (at 62.4 102.5)
    (descr "Wire Pad, Square, SMD Pad,  5mm x 10mm,")
    (tags "MesurementPoint Square SMDPad 5mmx10mm ")
    (attr virtual)
    (fp_text reference GPIO (at 0 -2.2 90) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 2.54) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 1 smd roundrect (at 0 0) (size 1 2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 GPIO_Input_2_2))
  )
  (module Connector_Wire:SolderWirePad_1x01_SMD_1x2mm (layer B.Cu) (tedit 5DD6EB27)
    (at 60 77.5)
    (descr "Wire Pad, Square, SMD Pad,  5mm x 10mm,")
    (tags "MesurementPoint Square SMDPad 5mmx10mm ")
    (attr virtual)
    (fp_text reference J7 (at 0 2.54) (layer B.SilkS) hide)
    (fp_text value Conn_01x01 (at 0 -2.54) (layer B.Fab) hide)
    (fp_text user GND (at 0.05 1.8 90) (layer B.SilkS))
    (pad 1 smd roundrect (at 0 0) (size 1 2) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
  )
  (module Connector_Wire:SolderWirePad_1x01_SMD_1x2mm (layer F.Cu) (tedit 5DD6EB27)
    (at 58.6 102.5)
    (descr "Wire Pad, Square, SMD Pad,  5mm x 10mm,")
    (tags "MesurementPoint Square SMDPad 5mmx10mm ")
    (attr virtual)
    (fp_text reference VIN (at 0 -2 90) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 2.54) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 1 smd roundrect (at 0 0) (size 1 2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 V_IN_2))
  )
  (module Connector_Wire:SolderWirePad_1x01_SMD_1x2mm (layer B.Cu) (tedit 5DD6EB27)
    (at 58.1 77.5)
    (descr "Wire Pad, Square, SMD Pad,  5mm x 10mm,")
    (tags "MesurementPoint Square SMDPad 5mmx10mm ")
    (attr virtual)
    (fp_text reference J5 (at 0 2.54) (layer B.SilkS) hide)
    (fp_text value Conn_01x01 (at 0.1 -2.5) (layer B.Fab) hide)
    (fp_text user GPIO (at 0.1 1.8 90) (layer B.SilkS))
    (pad 1 smd roundrect (at 0 0) (size 1 2) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 8 GPIO_Input_2))
  )
  (module Connector_Wire:SolderWirePad_1x01_SMD_1x2mm (layer F.Cu) (tedit 5DD6EB27)
    (at 60.5 102.5)
    (descr "Wire Pad, Square, SMD Pad,  5mm x 10mm,")
    (tags "MesurementPoint Square SMDPad 5mmx10mm ")
    (attr virtual)
    (fp_text reference GND (at 0 -2.1 90) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 2.54) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 1 smd roundrect (at 0 0) (size 1 2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
  )
  (module Connector_Wire:SolderWirePad_1x01_SMD_1x2mm (layer B.Cu) (tedit 5DD6EB27)
    (at 61.9 77.5)
    (descr "Wire Pad, Square, SMD Pad,  5mm x 10mm,")
    (tags "MesurementPoint Square SMDPad 5mmx10mm ")
    (attr virtual)
    (fp_text reference J3 (at 0 2.54) (layer B.SilkS) hide)
    (fp_text value Conn_01x01 (at 0 -2.54) (layer B.Fab) hide)
    (fp_text user VIN (at 0.1 1.75 270) (layer B.SilkS))
    (pad 1 smd roundrect (at 0 0) (size 1 2) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 V_IN))
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer F.Cu) (tedit 5F68FEEE)
    (at 67 89.05 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R6 (at 0 -2 90) (layer F.SilkS))
    (fp_text value R (at 0 1.65) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1 0 180) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 9 V_IN_2))
    (pad 1 smd roundrect (at -1 0 180) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 12 "Net-(R6-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer F.Cu) (tedit 5F68FEEE)
    (at 67 91 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R5 (at 0 1.95 90) (layer F.SilkS))
    (fp_text value R (at 0 1.65) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1 0 180) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 9 V_IN_2))
    (pad 1 smd roundrect (at -1 0 180) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 10 GPIO_Input_2_2))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:QRD1114 (layer F.Cu) (tedit 0)
    (at 49.81 91.24 180)
    (fp_text reference U2 (at 0.01 1.24 270) (layer F.SilkS) hide)
    (fp_text value QRD1114 (at 1.055 1.27 270) (layer F.SilkS))
    (fp_text user * (at 0 0) (layer F.Fab) hide)
    (fp_text user * (at 0 0) (layer F.SilkS) hide)
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
    (pad 4 thru_hole circle (at 2.11 0 180) (size 1.27 1.27) (drill 0.762) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole circle (at 2.11 2.54 180) (size 1.27 1.27) (drill 0.762) (layers *.Cu *.Mask)
      (net 7 "Net-(R2-Pad1)"))
    (pad 2 thru_hole circle (at 0 2.54 180) (size 1.27 1.27) (drill 0.762) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.27 1.27) (drill 0.762) (layers *.Cu *.Mask)
      (net 11 GPIO_Input_1))
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer F.Cu) (tedit 5F68FEEE)
    (at 48.6 85.8 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R4 (at 0 -0.1 270) (layer F.SilkS))
    (fp_text value R (at 0 1.65) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1 0 180) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 4 V_IN))
    (pad 1 smd roundrect (at -1 0 180) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 5 I2C1_SDA))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer F.Cu) (tedit 5F68FEEE)
    (at 53 88.3 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R3 (at 0 0 90) (layer F.SilkS))
    (fp_text value R (at 0 1.65) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1 0 180) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 6 I2C1_SCl))
    (pad 1 smd roundrect (at -1 0 180) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 4 V_IN))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer F.Cu) (tedit 5F68FEEE)
    (at 53 92.1)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R2 (at 0 0 90) (layer F.SilkS))
    (fp_text value R (at 0 1.65) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1 0) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 4 V_IN))
    (pad 1 smd roundrect (at -1 0) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 7 "Net-(R2-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer F.Cu) (tedit 5F68FEEE)
    (at 53 90.2)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R1 (at 0 0 90) (layer F.SilkS))
    (fp_text value R (at 0 1.65) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1 0) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 4 V_IN))
    (pad 1 smd roundrect (at -1 0) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 11 GPIO_Input_1))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:STM32G030J6M6 (layer F.Cu) (tedit 0)
    (at 52.452204 82.045821 45)
    (fp_text reference 30J6M6 (at -0.216645 0.001397 315) (layer F.SilkS))
    (fp_text value STM32G0 (at 0.631883 0.001397 135) (layer F.SilkS))
    (fp_text user * (at -1.6256 -2.4257 45) (layer F.Fab) hide)
    (fp_text user * (at -2.9337 -3.606 45) (layer F.SilkS) hide)
    (fp_text user 0.061in/1.538mm (at -2.6797 4.9149 45) (layer Dwgs.User))
    (fp_text user 0.211in/5.359mm (at 0 -4.9149 45) (layer Dwgs.User))
    (fp_text user 0.022in/0.558mm (at 5.7277 -1.905 45) (layer Dwgs.User))
    (fp_text user 0.05in/1.27mm (at -5.7277 -1.27 45) (layer Dwgs.User))
    (fp_text user * (at -1.6256 -2.4257 45) (layer F.Fab) hide)
    (fp_text user * (at -2.9337 -3.606 45) (layer F.SilkS) hide)
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0 45) (layer Cmts.User))
    (pad 8 smd rect (at 2.6797 -1.905 45) (size 1.538199 0.558) (layers F.Cu F.Paste F.Mask)
      (net 2 SYS_SWCLK))
    (pad 7 smd rect (at 2.6797 -0.635 45) (size 1.538199 0.558) (layers F.Cu F.Paste F.Mask)
      (net 3 SYS_SWDIO))
    (pad 6 smd rect (at 2.6797 0.635 45) (size 1.538199 0.558) (layers F.Cu F.Paste F.Mask)
      (net 5 I2C1_SDA))
    (pad 5 smd rect (at 2.6797 1.905 45) (size 1.538199 0.558) (layers F.Cu F.Paste F.Mask)
      (net 6 I2C1_SCl))
    (pad 4 smd rect (at -2.6797 1.905 45) (size 1.538199 0.558) (layers F.Cu F.Paste F.Mask)
      (net 11 GPIO_Input_1))
    (pad 3 smd rect (at -2.6797 0.635 45) (size 1.538199 0.558) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -2.6797 -0.635 45) (size 1.538199 0.558) (layers F.Cu F.Paste F.Mask)
      (net 4 V_IN))
    (pad 1 smd rect (at -2.6797 -1.905 45) (size 1.538199 0.558) (layers F.Cu F.Paste F.Mask)
      (net 8 GPIO_Input_2))
  )
  (gr_text VIN (at 59.8 83.1) (layer B.SilkS))
  (gr_text GND (at 61.3 83.1) (layer B.SilkS))
  (gr_text V+ (at 47.7 87.3 90) (layer F.SilkS))
  (gr_text GND (at 49.9 87.2 90) (layer F.SilkS))
  (gr_text GND (at 47.7 92.8 90) (layer F.SilkS))
  (gr_text V+ (at 72.4 87.2 90) (layer B.SilkS))
  (gr_text GND (at 70.2 87.2 90) (layer B.SilkS))
  (gr_text GND (at 72.3 92.9 90) (layer B.SilkS))
  (gr_text SWCLK (at 56.9 82.5) (layer B.SilkS))
  (gr_text SWDIO (at 56.9 81) (layer B.SilkS))
  (gr_line (start 54.9 83.9) (end 54.9 93.2) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 65.1 86.8) (end 65.1 96.1) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 53.9 93.2) (end 54.9 93.2) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 53.9 96.1) (end 53.9 93.2) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 54.9 96.1) (end 53.9 96.1) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 66.1 86.8) (end 65.1 86.8) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 66.1 83.9) (end 66.1 86.8) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 65.1 83.9) (end 66.1 83.9) (layer Edge.Cuts) (width 0.05))
  (gr_circle (center 60 90) (end 74 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 65.1 83.9) (end 54.9 83.9) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 54.9 96.1) (end 65.1 96.1) (layer Edge.Cuts) (width 0.05))
)
