<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.5.0">
<drawing>
<board>
<plain>
<wire x1="15.2" y1="19.5" x2="15.2" y2="24.4" width="0.3048" layer="20"/>
<wire x1="15.2" y1="24.4" x2="15.45" y2="24.65" width="0.3048" layer="20" curve="-90"/>
<wire x1="15.45" y1="24.65" x2="15.45" y2="25.525" width="0.3048" layer="20"/>
<wire x1="15.45" y1="25.525" x2="14.9" y2="26.075" width="0.3048" layer="20"/>
<wire x1="14.9" y1="26.075" x2="14" y2="27.675" width="0.3048" layer="20"/>
<wire x1="14" y1="27.675" x2="13.95" y2="30.3" width="0.3048" layer="20"/>
<wire x1="13.95" y1="30.3" x2="14.675" y2="32" width="0.3048" layer="20"/>
<wire x1="14.675" y1="32" x2="15.9" y2="33.45" width="0.3048" layer="20"/>
<wire x1="15.9" y1="33.45" x2="17.025" y2="34.375" width="0.3048" layer="20"/>
<wire x1="17.025" y1="34.375" x2="18.75" y2="35" width="0.3048" layer="20"/>
<wire x1="18.75" y1="35" x2="21" y2="35.025" width="0.3048" layer="20"/>
<wire x1="21" y1="35.025" x2="22.525" y2="34.35" width="0.3048" layer="20"/>
<wire x1="22.525" y1="34.35" x2="23.35" y2="33.4" width="0.3048" layer="20"/>
<wire x1="23.35" y1="33.4" x2="23.425" y2="33.2" width="0.3048" layer="20"/>
<wire x1="23.425" y1="33.2" x2="24.075" y2="33.225" width="0.3048" layer="20"/>
<wire x1="24.075" y1="33.225" x2="27.575" y2="34" width="0.3048" layer="20"/>
<wire x1="27.575" y1="34" x2="29.775" y2="34" width="0.3048" layer="20"/>
<wire x1="29.775" y1="34" x2="29.8" y2="34" width="0.3048" layer="20"/>
<wire x1="15.2" y1="19.475" x2="16.125" y2="16.975" width="0.3048" layer="20"/>
<wire x1="16.125" y1="16.975" x2="17.375" y2="15.275" width="0.3048" layer="20"/>
<wire x1="17.375" y1="15.275" x2="19.225" y2="14.175" width="0.3048" layer="20"/>
<wire x1="19.225" y1="14.175" x2="21.2" y2="13.45" width="0.3048" layer="20"/>
<wire x1="21.2" y1="13.45" x2="23.45" y2="13.025" width="0.3048" layer="20"/>
<wire x1="23.45" y1="13.025" x2="25.225" y2="12.875" width="0.3048" layer="20"/>
<wire x1="25.225" y1="12.875" x2="29.875" y2="12.875" width="0.3048" layer="20"/>
<wire x1="29.875" y1="12.875" x2="29.925" y2="12.875" width="0.3048" layer="20"/>
<wire x1="44.65" y1="19.475" x2="44.65" y2="24.375" width="0.3048" layer="20"/>
<wire x1="44.65" y1="24.375" x2="44.4" y2="24.625" width="0.3048" layer="20" curve="90"/>
<wire x1="44.4" y1="24.625" x2="44.4" y2="25.5" width="0.3048" layer="20"/>
<wire x1="44.4" y1="25.5" x2="44.95" y2="26.05" width="0.3048" layer="20"/>
<wire x1="44.95" y1="26.05" x2="45.85" y2="27.65" width="0.3048" layer="20"/>
<wire x1="45.85" y1="27.65" x2="45.9" y2="30.275" width="0.3048" layer="20"/>
<wire x1="45.9" y1="30.275" x2="45.175" y2="31.975" width="0.3048" layer="20"/>
<wire x1="45.175" y1="31.975" x2="43.95" y2="33.425" width="0.3048" layer="20"/>
<wire x1="43.95" y1="33.425" x2="42.825" y2="34.35" width="0.3048" layer="20"/>
<wire x1="42.825" y1="34.35" x2="41.1" y2="34.975" width="0.3048" layer="20"/>
<wire x1="41.1" y1="34.975" x2="38.85" y2="35" width="0.3048" layer="20"/>
<wire x1="38.85" y1="35" x2="37.325" y2="34.325" width="0.3048" layer="20"/>
<wire x1="37.325" y1="34.325" x2="36.5" y2="33.375" width="0.3048" layer="20"/>
<wire x1="36.5" y1="33.375" x2="36.425" y2="33.175" width="0.3048" layer="20"/>
<wire x1="36.425" y1="33.175" x2="35.775" y2="33.2" width="0.3048" layer="20"/>
<wire x1="35.775" y1="33.2" x2="32.275" y2="33.975" width="0.3048" layer="20"/>
<wire x1="32.275" y1="33.975" x2="29.775" y2="34" width="0.3048" layer="20"/>
<wire x1="44.65" y1="19.45" x2="43.725" y2="16.95" width="0.3048" layer="20"/>
<wire x1="43.725" y1="16.95" x2="42.475" y2="15.25" width="0.3048" layer="20"/>
<wire x1="42.475" y1="15.25" x2="40.625" y2="14.15" width="0.3048" layer="20"/>
<wire x1="40.625" y1="14.15" x2="38.65" y2="13.425" width="0.3048" layer="20"/>
<wire x1="38.65" y1="13.425" x2="36.4" y2="13" width="0.3048" layer="20"/>
<wire x1="36.4" y1="13" x2="34.625" y2="12.85" width="0.3048" layer="20"/>
<wire x1="34.625" y1="12.85" x2="29.875" y2="12.875" width="0.3048" layer="20"/>
<text>M.Cagri Baydemir
    08.09.2016</text>
<text> Aspilsan
08.09.2016</text>
</plain>
<libraries>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805-CAP">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="CHIP-LED0603">
<description>&lt;b&gt;Hyper CHIPLED Hyper-Bright LED&lt;/b&gt;&lt;p&gt;
LB Q993&lt;br&gt;
Source: http://www.osram.convergy.de/ ... Lb_q993.pdf</description>
</package>
<package name="CR1220-SMD">
</package>
</packages>
</library>
<library name="semicon-smd-ipc">
<description>&lt;b&gt;IPC Standard SMD Semiconductors&lt;/b&gt;&lt;p&gt;
A few devices defined according to the IPC standard.&lt;p&gt;
Based on:&lt;p&gt;
IPC-SM-782&lt;br&gt;
IRevision A, August 1993&lt;br&gt;
Includes Amendment 1, October 1996&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOT23">
<description>&lt;b&gt;SOT-23&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="SparkFun-Capacitors" package="0805-CAP" value="1.0uF">
<attribute name="PROD_ID" value="CAP-11625"/>
<attribute name="NAME"/>
</element>
<element name="C2" library="SparkFun-Capacitors" package="0805-CAP" value="1.0uF">
<attribute name="PROD_ID" value="CAP-11625"/>
<attribute name="NAME"/>
</element>
<element name="LED1" library="adafruit" package="CHIP-LED0603" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED2" library="adafruit" package="CHIP-LED0603" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q1" library="semicon-smd-ipc" package="SOT23" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q2" library="semicon-smd-ipc" package="SOT23" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="0603" value="1.5KOHM">
<attribute name="PROD_ID" value="RES-08306"/>
<attribute name="NAME"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="0603" value="1.5KOHM">
<attribute name="PROD_ID" value="RES-08306"/>
<attribute name="NAME"/>
</element>
<element name="R3" library="SparkFun-Resistors" package="0603" value="1.5KOHM">
<attribute name="PROD_ID" value="RES-08306"/>
<attribute name="NAME"/>
</element>
<element name="R4" library="SparkFun-Resistors" package="0603" value="1.5KOHM">
<attribute name="PROD_ID" value="RES-08306"/>
<attribute name="NAME"/>
</element>
<element name="BATTERY" library="adafruit" package="CR1220-SMD" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="Q2" pad="3"/>
<contactref element="C1" pad="1"/>
<contactref element="LED1" pad="C"/>
</signal>
<signal name="N$4">
<contactref element="Q1" pad="3"/>
<contactref element="C2" pad="2"/>
<contactref element="LED2" pad="C"/>
</signal>
<signal name="N$5">
<contactref element="R1" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="R4" pad="2"/>
<contactref element="BATTERY" pad="-"/>
</signal>
<signal name="GND">
<contactref element="Q2" pad="2"/>
<contactref element="Q1" pad="2"/>
<contactref element="BATTERY" pad="+$1"/>
</signal>
<signal name="N$6">
<contactref element="LED1" pad="A"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="LED2" pad="A"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="R3" pad="1"/>
<contactref element="C1" pad="2"/>
<contactref element="Q1" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="R4" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="Q2" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
