(kicad_pcb (version 4) (host pcbnew 4.0.5)
  (general
    (links 44)
    (no_connects 0)
    (area 91.124999 70.024999 135.875001 85.175001)
    (thickness 1.6)
    (drawings 20)
    (tracks 211)
    (zones 0)
    (modules 15)
    (nets 40)
  )
  (page A4)
  (layers
    (0 Front signal hide)
    (31 Bottom signal)
    (32 B.Adhes user)
    (33 F.Adhes user hide)
    (34 B.Paste user)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user hide)
    (38 B.Mask user)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.4)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 131.7 74.1)
    (visible_elements 7FFEBDDF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 GND)
  (net 3 "Net-(C2-Pad1)")
  (net 4 +5V)
  (net 5 +3V3)
  (net 6 "Net-(F1-Pad2)")
  (net 7 CE)
  (net 8 CSN)
  (net 9 SCK)
  (net 10 MOSI)
  (net 11 MISO)
  (net 12 "Net-(J1-Pad8)")
  (net 13 "Net-(J2-Pad1)")
  (net 14 D-)
  (net 15 "Net-(R1-Pad2)")
  (net 16 D+)
  (net 17 "Net-(R2-Pad2)")
  (net 18 "Net-(U1-Pad1)")
  (net 19 "Net-(U1-Pad8)")
  (net 20 "Net-(U1-Pad12)")
  (net 21 "Net-(U1-Pad13)")
  (net 22 "Net-(U1-Pad18)")
  (net 23 "Net-(U1-Pad19)")
  (net 24 "Net-(U1-Pad20)")
  (net 25 "Net-(U1-Pad21)")
  (net 26 "Net-(U1-Pad22)")
  (net 27 "Net-(U1-Pad25)")
  (net 28 "Net-(U1-Pad28)")
  (net 29 "Net-(U1-Pad29)")
  (net 30 "Net-(U1-Pad30)")
  (net 31 "Net-(U1-Pad31)")
  (net 32 "Net-(U1-Pad32)")
  (net 33 "Net-(U1-Pad36)")
  (net 34 "Net-(U1-Pad37)")
  (net 35 "Net-(U1-Pad38)")
  (net 36 "Net-(U1-Pad39)")
  (net 37 "Net-(U1-Pad40)")
  (net 38 "Net-(U1-Pad41)")
  (net 39 "Net-(U1-Pad42)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net +5V)
    (add_net CE)
    (add_net CSN)
    (add_net D+)
    (add_net D-)
    (add_net GND)
    (add_net MISO)
    (add_net MOSI)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(F1-Pad2)")
    (add_net "Net-(J1-Pad8)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(R1-Pad2)")
    (add_net "Net-(R2-Pad2)")
    (add_net "Net-(U1-Pad1)")
    (add_net "Net-(U1-Pad12)")
    (add_net "Net-(U1-Pad13)")
    (add_net "Net-(U1-Pad18)")
    (add_net "Net-(U1-Pad19)")
    (add_net "Net-(U1-Pad20)")
    (add_net "Net-(U1-Pad21)")
    (add_net "Net-(U1-Pad22)")
    (add_net "Net-(U1-Pad25)")
    (add_net "Net-(U1-Pad28)")
    (add_net "Net-(U1-Pad29)")
    (add_net "Net-(U1-Pad30)")
    (add_net "Net-(U1-Pad31)")
    (add_net "Net-(U1-Pad32)")
    (add_net "Net-(U1-Pad36)")
    (add_net "Net-(U1-Pad37)")
    (add_net "Net-(U1-Pad38)")
    (add_net "Net-(U1-Pad39)")
    (add_net "Net-(U1-Pad40)")
    (add_net "Net-(U1-Pad41)")
    (add_net "Net-(U1-Pad42)")
    (add_net "Net-(U1-Pad8)")
    (add_net SCK)
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer Bottom) (tedit 58C56088)
    (at 104.9 73.2 180)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C1 (at 0 0 180) (layer B.SilkS))
    (fp_text value 16pF (at 0 -2 180) (layer B.Fab))
    (fp_text user %R (at 0 1.75 180) (layer B.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.6) (layers Bottom B.Paste B.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 2 0 180) (size 2 1.6) (layers Bottom B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer Front) (tedit 58C568AF)
    (at 104.3 79.5 90)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C2 (at 0 0 90) (layer F.SilkS))
    (fp_text value 16pF (at 0 1.8 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.6) (layers Front F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 2 0 90) (size 2 1.6) (layers Front F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer Bottom) (tedit 58C5608D)
    (at 110.6 73.3 90)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C3 (at 0.1 0.1 90) (layer B.SilkS))
    (fp_text value 10uF (at 0 -2 90) (layer B.Fab))
    (fp_text user %R (at 0 1.75 90) (layer B.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.6) (layers Bottom B.Paste B.Mask)
      (net 4 +5V))
    (pad 2 smd rect (at 2 0 90) (size 2 1.6) (layers Bottom B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer Bottom) (tedit 58C56090)
    (at 113.4 73.3 90)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C4 (at 0.1 0 90) (layer B.SilkS))
    (fp_text value 10uF (at 0 -2 90) (layer B.Fab))
    (fp_text user %R (at 0 1.75 90) (layer B.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.6) (layers Bottom B.Paste B.Mask)
      (net 5 +3V3))
    (pad 2 smd rect (at 2 0 90) (size 2 1.6) (layers Bottom B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer Front) (tedit 58C568B6)
    (at 104.9 73.2 180)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C5 (at 0 0 180) (layer F.SilkS))
    (fp_text value 0.1uF (at -0.5 1.7 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.6) (layers Front F.Paste F.Mask)
      (net 5 +3V3))
    (pad 2 smd rect (at 2 0 180) (size 2 1.6) (layers Front F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Fuse_Holders_and_Fuses:Fuse_SMD1206_HandSoldering (layer Bottom) (tedit 58C56080)
    (at 104.9 81.8 180)
    (descr "Fuse, Sicherung, SMD1206, Littlefuse-Wickmann 433 Series, Hand Soldering,")
    (tags "Fuse Sicherung SMD1206 Littlefuse-Wickmann 433 Series Hand Soldering ")
    (attr smd)
    (fp_text reference F1 (at 0 0 180) (layer B.SilkS))
    (fp_text value 500mA (at -0.15 -2.5 180) (layer B.Fab))
    (pad 1 smd rect (at -2.09 0 90) (size 2.03 2.65) (layers Bottom B.Paste B.Mask)
      (net 4 +5V))
    (pad 2 smd rect (at 2.09 0 90) (size 2.03 2.65) (layers Bottom B.Paste B.Mask)
      (net 6 "Net-(F1-Pad2)"))
  )
  (module Pin_Headers:Pin_Header_Straight_2x04_Pitch2.54mm (layer Front) (tedit 58C5682A)
    (at 131.7 71.5)
    (descr "Through hole straight pin header, 2x04, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x04 2.54mm double row")
    (fp_text reference J1 (at 1.27 -2.39) (layer F.SilkS) hide)
    (fp_text value CONN_02X04 (at 3.1 11) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 +3V3))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 CE))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 CSN))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 SCK))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 MOSI))
    (pad 7 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 MISO))
    (pad 8 thru_hole oval (at 2.54 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(J1-Pad8)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x04_Pitch2.54mm.wrl
      (at (xyz 0.05 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Connect:GS2 (layer Bottom) (tedit 58C560AE)
    (at 116.5 75.2)
    (descr "2-pin solder bridge")
    (tags "solder bridge")
    (attr smd)
    (fp_text reference J2 (at 1.78 0 90) (layer B.SilkS) hide)
    (fp_text value GS2 (at -1.8 0 270) (layer B.Fab))
    (pad 1 smd rect (at 0 0.64) (size 1.27 0.97) (layers Bottom B.Paste B.Mask)
      (net 13 "Net-(J2-Pad1)"))
    (pad 2 smd rect (at 0 -0.64) (size 1.27 0.97) (layers Bottom B.Paste B.Mask)
      (net 2 GND))
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer Bottom) (tedit 58C56085)
    (at 104.7 78.7 180)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R1 (at 0 0 180) (layer B.SilkS))
    (fp_text value 22R (at 0 -1.9 180) (layer B.Fab))
    (fp_text user %R (at 0 1.85 180) (layer B.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers Bottom B.Paste B.Mask)
      (net 14 D-))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers Bottom B.Paste B.Mask)
      (net 15 "Net-(R1-Pad2)"))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer Bottom) (tedit 58C56087)
    (at 104.7 75.9 180)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R2 (at 0 0 180) (layer B.SilkS))
    (fp_text value 22R (at 0 -1.9 180) (layer B.Fab))
    (fp_text user %R (at 0 1.85 180) (layer B.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers Bottom B.Paste B.Mask)
      (net 16 D+))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers Bottom B.Paste B.Mask)
      (net 17 "Net-(R2-Pad2)"))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer Bottom) (tedit 58C560B4)
    (at 116.5 81.3 90)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R3 (at 0 0 90) (layer B.SilkS))
    (fp_text value 10K (at 0 -1.9 90) (layer B.Fab))
    (fp_text user %R (at 0 1.85 90) (layer B.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers Bottom B.Paste B.Mask)
      (net 4 +5V))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers Bottom B.Paste B.Mask)
      (net 13 "Net-(J2-Pad1)"))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT89-3_Housing_Handsoldering (layer Bottom) (tedit 58C560A7)
    (at 111.7 80.4 270)
    (descr "SOT89-3, Housing, Handsoldering,")
    (tags "SOT89-3 Housing Handsoldering ")
    (attr smd)
    (fp_text reference REG1 (at 0.5 1.7 270) (layer B.SilkS))
    (fp_text value HT7333 (at 0.5 -3.15 270) (layer B.Fab))
    (pad 1 smd rect (at -1.98 1.5) (size 1 2.5) (layers Bottom B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -1.98 0) (size 1 2.5) (layers Bottom B.Paste B.Mask)
      (net 4 +5V))
    (pad 3 smd rect (at -1.98 -1.5) (size 1 2.5) (layers Bottom B.Paste B.Mask)
      (net 5 +3V3))
    (pad 2 smd rect (at 1.98 0) (size 2 4) (layers Bottom B.Paste B.Mask)
      (net 4 +5V))
    (pad 2 smd trapezoid (at -0.37 0 180) (size 1.5 0.75) (rect_delta 0 -0.5 ) (layers Bottom B.Paste B.Mask)
      (net 4 +5V))
    (model TO_SOT_Packages_SMD.3dshapes/SOT89-3_Housing_Handsoldering.wrl
      (at (xyz 0.02 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 90))
    )
  )
  (module Housings_QFP:TQFP-44_10x10mm_Pitch0.8mm (layer Front) (tedit 58C568D8)
    (at 122 77.6 180)
    (descr "44-Lead Plastic Thin Quad Flatpack (PT) - 10x10x1.0 mm Body [TQFP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFP 0.8")
    (attr smd)
    (fp_text reference U1 (at 3.7 -4.1 180) (layer F.SilkS))
    (fp_text value ATMEGA32U4-AU (at 0 0.1 315) (layer F.Fab))
    (fp_text user %R (at 1.6 -2 180) (layer F.Fab))
    (pad 1 smd rect (at -5.7 -4 180) (size 1.5 0.55) (layers Front F.Paste F.Mask)
      (net 18 "Net-(U1-Pad1)"))
    (pad 2 smd rect (at -5.7 -3.2 180) (size 1.5 0.55) (layers Front F.Paste F.Mask)
      (net 4 +5V))
    (pad 3 smd rect (at -5.7 -2.4 180) (size 1.5 0.55) (layers Front F.Paste F.Mask)
      (net 14 D-))
    (pad 4 smd rect (at -5.7 -1.6 180) (size 1.5 0.55) (layers Front F.Paste F.Mask)
      (net 16 D+))
    (pad 5 smd rect (at -5.7 -0.8 180) (size 1.5 0.55) (layers Front F.Paste F.Mask)
      (net 2 GND))
    (pad 6 smd rect (at -5.7 0 180) (size 1.5 0.55) (layers Front F.Paste F.Mask)
      (net 5 +3V3))
    (pad 7 smd rect (at -5.7 0.8 180) (size 1.5 0.55) (layers Front F.Paste F.Mask)
      (net 4 +5V))
    (pad 8 smd rect (at -5.7 1.6 180) (size 1.5 0.55) (layers Front F.Paste F.Mask)
      (net 19 "Net-(U1-Pad8)"))
    (pad 9 smd rect (at -5.7 2.4 180) (size 1.5 0.55) (layers Front F.Paste F.Mask)
      (net 9 SCK))
    (pad 10 smd rect (at -5.7 3.2 180) (size 1.5 0.55) (layers Front F.Paste F.Mask)
      (net 10 MOSI))
    (pad 11 smd rect (at -5.7 4 180) (size 1.5 0.55) (layers Front F.Paste F.Mask)
      (net 11 MISO))
    (pad 12 smd rect (at -4 5.7 270) (size 1.5 0.55) (layers Front F.Paste F.Mask)
      (net 20 "Net-(U1-Pad12)"))
    (pad 13 smd rect (at -3.2 5.7 270) (size 1.5 0.55) (layers Front F.Paste F.Mask)
      (net 21 "Net-(U1-Pad13)"))
    (pad 14 smd rect (at -2.4 5.7 270) (size 1.5 0.55) (layers Front F.Paste F.Mask)
      (net 4 +5V))
    (pad 15 smd rect (at -1.6 5.7 270) (size 1.5 0.55) (layers Front F.Paste F.Mask)
      (net 2 GND))
    (pad 16 smd rect (at -0.8 5.7 270) (size 1.5 0.55) (layers Front F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 17 smd rect (at 0 5.7 270) (size 1.5 0.55) (layers Front F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 18 smd rect (at 0.8 5.7 270) (size 1.5 0.55) (layers Front F.Paste F.Mask)
      (net 22 "Net-(U1-Pad18)"))
    (pad 19 smd rect (at 1.6 5.7 270) (size 1.5 0.55) (layers Front F.Paste F.Mask)
      (net 23 "Net-(U1-Pad19)"))
    (pad 20 smd rect (at 2.4 5.7 270) (size 1.5 0.55) (layers Front F.Paste F.Mask)
      (net 24 "Net-(U1-Pad20)"))
    (pad 21 smd rect (at 3.2 5.7 270) (size 1.5 0.55) (layers Front F.Paste F.Mask)
      (net 25 "Net-(U1-Pad21)"))
    (pad 22 smd rect (at 4 5.7 270) (size 1.5 0.55) (layers Front F.Paste F.Mask)
      (net 26 "Net-(U1-Pad22)"))
    (pad 23 smd rect (at 5.7 4 180) (size 1.5 0.55) (layers Front F.Paste F.Mask)
      (net 2 GND))
    (pad 24 smd rect (at 5.7 3.2 180) (size 1.5 0.55) (layers Front F.Paste F.Mask)
      (net 4 +5V))
    (pad 25 smd rect (at 5.7 2.4 180) (size 1.5 0.55) (layers Front F.Paste F.Mask)
      (net 27 "Net-(U1-Pad25)"))
    (pad 26 smd rect (at 5.7 1.6 180) (size 1.5 0.55) (layers Front F.Paste F.Mask)
      (net 7 CE))
    (pad 27 smd rect (at 5.7 0.8 180) (size 1.5 0.55) (layers Front F.Paste F.Mask)
      (net 8 CSN))
    (pad 28 smd rect (at 5.7 0 180) (size 1.5 0.55) (layers Front F.Paste F.Mask)
      (net 28 "Net-(U1-Pad28)"))
    (pad 29 smd rect (at 5.7 -0.8 180) (size 1.5 0.55) (layers Front F.Paste F.Mask)
      (net 29 "Net-(U1-Pad29)"))
    (pad 30 smd rect (at 5.7 -1.6 180) (size 1.5 0.55) (layers Front F.Paste F.Mask)
      (net 30 "Net-(U1-Pad30)"))
    (pad 31 smd rect (at 5.7 -2.4 180) (size 1.5 0.55) (layers Front F.Paste F.Mask)
      (net 31 "Net-(U1-Pad31)"))
    (pad 32 smd rect (at 5.7 -3.2 180) (size 1.5 0.55) (layers Front F.Paste F.Mask)
      (net 32 "Net-(U1-Pad32)"))
    (pad 33 smd rect (at 5.7 -4 180) (size 1.5 0.55) (layers Front F.Paste F.Mask)
      (net 13 "Net-(J2-Pad1)"))
    (pad 34 smd rect (at 4 -5.7 270) (size 1.5 0.55) (layers Front F.Paste F.Mask)
      (net 4 +5V))
    (pad 35 smd rect (at 3.2 -5.7 270) (size 1.5 0.55) (layers Front F.Paste F.Mask)
      (net 2 GND))
    (pad 36 smd rect (at 2.4 -5.7 270) (size 1.5 0.55) (layers Front F.Paste F.Mask)
      (net 33 "Net-(U1-Pad36)"))
    (pad 37 smd rect (at 1.6 -5.7 270) (size 1.5 0.55) (layers Front F.Paste F.Mask)
      (net 34 "Net-(U1-Pad37)"))
    (pad 38 smd rect (at 0.8 -5.7 270) (size 1.5 0.55) (layers Front F.Paste F.Mask)
      (net 35 "Net-(U1-Pad38)"))
    (pad 39 smd rect (at 0 -5.7 270) (size 1.5 0.55) (layers Front F.Paste F.Mask)
      (net 36 "Net-(U1-Pad39)"))
    (pad 40 smd rect (at -0.8 -5.7 270) (size 1.5 0.55) (layers Front F.Paste F.Mask)
      (net 37 "Net-(U1-Pad40)"))
    (pad 41 smd rect (at -1.6 -5.7 270) (size 1.5 0.55) (layers Front F.Paste F.Mask)
      (net 38 "Net-(U1-Pad41)"))
    (pad 42 smd rect (at -2.4 -5.7 270) (size 1.5 0.55) (layers Front F.Paste F.Mask)
      (net 39 "Net-(U1-Pad42)"))
    (pad 43 smd rect (at -3.2 -5.7 270) (size 1.5 0.55) (layers Front F.Paste F.Mask)
      (net 2 GND))
    (pad 44 smd rect (at -4 -5.7 270) (size 1.5 0.55) (layers Front F.Paste F.Mask)
      (net 4 +5V))
    (model Housings_QFP.3dshapes/TQFP-44_10x10mm_Pitch0.8mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module customs.pretty:usb-PCB (layer Front) (tedit 542BB0AF)
    (at 91.2 77.6 270)
    (attr virtual)
    (fp_text reference USB1 (at 0.13 -7.85 270) (layer F.SilkS) hide)
    (fp_text value USB_PLUG (at 0.29 -10.13 270) (layer F.SilkS) hide)
    (pad 1 connect rect (at 3.81 -4.9 270) (size 1.9 8) (layers Front F.Mask)
      (net 6 "Net-(F1-Pad2)"))
    (pad 4 connect rect (at -3.81 -4.9 270) (size 1.9 8) (layers Front F.Mask)
      (net 2 GND))
    (pad 3 connect rect (at -1.3 -5.15 270) (size 2 7.5) (layers Front F.Mask)
      (net 17 "Net-(R2-Pad2)"))
    (pad 2 connect rect (at 1.3 -5.15 270) (size 2 7.5) (layers Front F.Mask)
      (net 15 "Net-(R1-Pad2)"))
  )
  (module Crystals:Crystal_SMD_HC49-SD (layer Front) (tedit 58C568C9)
    (at 111.1 77.6 270)
    (descr "SMD Crystal HC-49-SD http://cdn-reichelt.de/documents/datenblatt/B400/xxx-HC49-SMD.pdf, 11.4x4.7mm^2 package")
    (tags "SMD SMT crystal")
    (attr smd)
    (fp_text reference Y1 (at 0 -0.1 270) (layer F.SilkS))
    (fp_text value 16Mhz (at -0.2 3.3 270) (layer F.Fab))
    (pad 1 smd rect (at -4.25 0 270) (size 4.5 2) (layers Front F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 4.25 0 270) (size 4.5 2) (layers Front F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (model Crystals.3dshapes/Crystal_SMD_HC49-SD.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "WirelessController\nv0.1" (at 120.7 77.6 90) (layer B.SilkS))
  (gr_line (start 103.6 85.1) (end 135.8 85.1) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 135.8 70.1) (end 103.6 70.1) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 135.8 70.1) (end 135.8 85.1) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 103.2 83.9) (end 103.2 84.7) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 103.6 84.7) (end 103.6 85.1) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 103.2 70.5) (end 103.2 71.3) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 103.6 70.5) (end 103.2 70.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 102.9 71.6) (end 91.2 71.6) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 91.2 83.6) (end 102.9 83.6) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 102.9 83.9) (end 102.9 83.6) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 102.9 71.3) (end 103.2 71.3) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 91.2 83.6) (end 91.2 71.6) (angle 90) (layer Edge.Cuts) (width 0.15))
  (dimension 9.1 (width 0.3) (layer Eco1.User)
    (gr_text "9.100 mm" (at 95.75 53.25) (layer Eco1.User))
    (feature1 (pts (xy 100.3 83.7) (xy 100.3 51.9)))
    (feature2 (pts (xy 91.2 83.7) (xy 91.2 51.9)))
    (crossbar (pts (xy 91.2 54.6) (xy 100.3 54.6)))
    (arrow1a (pts (xy 100.3 54.6) (xy 99.173496 55.186421)))
    (arrow1b (pts (xy 100.3 54.6) (xy 99.173496 54.013579)))
    (arrow2a (pts (xy 91.2 54.6) (xy 92.326504 55.186421)))
    (arrow2b (pts (xy 91.2 54.6) (xy 92.326504 54.013579)))
  )
  (dimension 15 (width 0.3) (layer Eco1.User)
    (gr_text "15.000 mm" (at 159.95 77.6 270) (layer Eco1.User))
    (feature1 (pts (xy 91.2 85.1) (xy 161.3 85.1)))
    (feature2 (pts (xy 91.2 70.1) (xy 161.3 70.1)))
    (crossbar (pts (xy 158.6 70.1) (xy 158.6 85.1)))
    (arrow1a (pts (xy 158.6 85.1) (xy 158.013579 83.973496)))
    (arrow1b (pts (xy 158.6 85.1) (xy 159.186421 83.973496)))
    (arrow2a (pts (xy 158.6 70.1) (xy 158.013579 71.226504)))
    (arrow2b (pts (xy 158.6 70.1) (xy 159.186421 71.226504)))
  )
  (dimension 12 (width 0.3) (layer Eco1.User)
    (gr_text "12.000 mm" (at 97.8 64.5) (layer Eco1.User))
    (feature1 (pts (xy 103.2 75.8) (xy 103.2 63.2)))
    (feature2 (pts (xy 91.2 75.8) (xy 91.2 63.2)))
    (crossbar (pts (xy 91.2 65.9) (xy 103.2 65.9)))
    (arrow1a (pts (xy 103.2 65.9) (xy 102.073496 66.486421)))
    (arrow1b (pts (xy 103.2 65.9) (xy 102.073496 65.313579)))
    (arrow2a (pts (xy 91.2 65.9) (xy 92.326504 66.486421)))
    (arrow2b (pts (xy 91.2 65.9) (xy 92.326504 65.313579)))
  )
  (zone (net 4) (net_name +5V) (layer Bottom) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 100.3 70.1) (xy 126.7 70.1) (xy 126.7 85.1) (xy 100.3 85.1)
      )
    )
  )
  (zone (net 5) (net_name +3V3) (layer Bottom) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 129.1 70.1) (xy 129.1 85.1) (xy 135.8 85.1) (xy 135.8 70.1)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer Front) (hatch edge 0.508)
    (connect_pads (clearance 0.4))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 135.8 85.1) (xy 100.3 85.1) (xy 100.3 70.1) (xy 135.8 70.1)
      )
    )
  )
)
