<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<board>
<plain>
<wire x1="0" y1="114.3" x2="0" y2="-14.1986" width="0" layer="20"/>
<wire x1="0" y1="-14.1986" x2="20.066" y2="-14.1986" width="0" layer="20"/>
<wire x1="20.066" y1="-14.1986" x2="20.066" y2="114.3" width="0" layer="20"/>
<wire x1="20.066" y1="114.3" x2="0" y2="114.3" width="0" layer="20"/>
<text>Energia</text>
<text>Vastus</text>
<text>Noise Engineering</text>
<text>EV 02</text>
<hole x="12.579984375" y="-11.19975" drill="3.2004"/>
<hole x="7.499528125" y="111.30000625" drill="3.2004"/>
<hole x="12.579528125" y="111.30000625" drill="3.2004"/>
<hole x="7.499984375" y="-11.19975" drill="3.2004"/>
<hole x="2.419528125" y="111.30000625" drill="3.2004"/>
<hole x="17.659528125" y="111.30000625" drill="3.2004"/>
<hole x="2.419984375" y="-11.19975" drill="3.2004"/>
<hole x="17.659984375" y="-11.19975" drill="3.2004"/>
<text>-12 .5A</text>
<text>+12 .5A</text>
<text>+5 1A</text>
<text>www.noiseengineering.us</text>
</plain>
<libraries>
<library name="_mylib">
<description>stephen's parts</description>
<packages>
<package name="EURORACK_POWER_PLUS">
<description>eurorack power plus cv/gate</description>
</package>
<package name="R1225">
</package>
<package name="HEADER_2_PIN_SMALL">
</package>
<package name="TEST_POINT">
</package>
<package name="FIDUCIAL_1MM">
</package>
<package name="EURORACK_POWER">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="_mylib" package="EURORACK_POWER_PLUS" value="EURORACK_POWER_PLUSHEADER"/>
<element name="R1" library="_mylib" package="R1225" value="100"/>
<element name="R2" library="_mylib" package="R1225" value="100"/>
<element name="R3" library="_mylib" package="R1225" value="100"/>
<element name="R4" library="_mylib" package="R1225" value="100"/>
<element name="R5" library="_mylib" package="R1225" value="100"/>
<element name="R6" library="_mylib" package="R1225" value="100"/>
<element name="R7" library="_mylib" package="R1225" value="100"/>
<element name="R8" library="_mylib" package="R1225" value="100"/>
<element name="R9" library="_mylib" package="R1225" value="20"/>
<element name="R10" library="_mylib" package="R1225" value="20"/>
<element name="JP12" library="_mylib" package="HEADER_2_PIN_SMALL" value="HEADER_2_PINSMALL"/>
<element name="JN12" library="_mylib" package="HEADER_2_PIN_SMALL" value="HEADER_2_PINSMALL"/>
<element name="J5" library="_mylib" package="HEADER_2_PIN_SMALL" value="HEADER_2_PINSMALL"/>
<element name="TP-12" library="_mylib" package="TEST_POINT" value="TEST_POINTTE"/>
<element name="TP+12" library="_mylib" package="TEST_POINT" value="TEST_POINTTE"/>
<element name="TP+5" library="_mylib" package="TEST_POINT" value="TEST_POINTTE"/>
<element name="TPGND" library="_mylib" package="TEST_POINT" value="TEST_POINTTE"/>
<element name="R11" library="_mylib" package="R1225" value="20"/>
<element name="R12" library="_mylib" package="R1225" value="20"/>
<element name="U$2" library="_mylib" package="FIDUCIAL_1MM" value="FIDUCIAL"/>
<element name="U$3" library="_mylib" package="FIDUCIAL_1MM" value="FIDUCIAL"/>
<element name="U$4" library="_mylib" package="EURORACK_POWER" value="EURORACK_POWERHEADER"/>
</elements>
<signals>
<signal name="GND">
<contactref element="R1" pad="1"/>
<contactref element="R2" pad="1"/>
<contactref element="R3" pad="1"/>
<contactref element="R4" pad="1"/>
<contactref element="R5" pad="1"/>
<contactref element="R6" pad="1"/>
<contactref element="R7" pad="1"/>
<contactref element="R8" pad="1"/>
<contactref element="U$1" pad="13"/>
<contactref element="U$1" pad="12"/>
<contactref element="U$1" pad="11"/>
<contactref element="U$1" pad="9"/>
<contactref element="U$1" pad="10"/>
<contactref element="U$1" pad="14"/>
<contactref element="R10" pad="1"/>
<contactref element="R9" pad="1"/>
<contactref element="TPGND" pad="0"/>
<contactref element="R11" pad="1"/>
<contactref element="R12" pad="1"/>
<contactref element="U$4" pad="GND1" route="any" routetag="GND"/>
<contactref element="U$4" pad="GND2" route="any" routetag="GND"/>
<contactref element="U$4" pad="GND3" route="any" routetag="GND"/>
<contactref element="U$4" pad="GND0" route="any" routetag="GND"/>
<contactref element="U$4" pad="GND5" route="any" routetag="GND"/>
<contactref element="U$4" pad="GND4" route="any" routetag="GND"/>
</signal>
<signal name="-12VIN">
<contactref element="U$1" pad="15"/>
<contactref element="U$1" pad="16"/>
<contactref element="JN12" pad="2"/>
<contactref element="TP-12" pad="0"/>
<contactref element="U$4" pad="-12V0"/>
<contactref element="U$4" pad="-12V1"/>
</signal>
<signal name="+5VIN">
<contactref element="U$1" pad="5"/>
<contactref element="U$1" pad="6"/>
<contactref element="J5" pad="2"/>
<contactref element="TP+5" pad="0"/>
</signal>
<signal name="N$1">
<contactref element="R8" pad="2"/>
<contactref element="R7" pad="2"/>
<contactref element="R6" pad="2"/>
<contactref element="R5" pad="2"/>
<contactref element="JN12" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="R4" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="R1" pad="2"/>
<contactref element="JP12" pad="1"/>
</signal>
<signal name="+12VIN">
<contactref element="U$1" pad="7"/>
<contactref element="U$1" pad="8"/>
<contactref element="JP12" pad="2"/>
<contactref element="TP+12" pad="0"/>
<contactref element="U$4" pad="+12V0"/>
<contactref element="U$4" pad="+12V1"/>
</signal>
<signal name="N$3">
<contactref element="R9" pad="2"/>
<contactref element="R10" pad="2"/>
<contactref element="J5" pad="1"/>
<contactref element="R11" pad="2"/>
<contactref element="R12" pad="2"/>
</signal>
<signal name="N$4">
</signal>
<signal name="N$5">
</signal>
</signals>
</board>
</drawing>
</eagle>
