(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 34)
    (no_connects 0)
    (area 91.339999 75.924999 132.355001 129.025001)
    (thickness 1.6)
    (drawings 29)
    (tracks 159)
    (zones 0)
    (modules 8)
    (nets 56)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.508)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.1524)
    (pcb_text_size 0.762 0.762)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 0.6)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 +3V3)
  (net 2 /HIPPOT)
  (net 3 GNDA)
  (net 4 /THIGHPOT)
  (net 5 /KNEEPOT)
  (net 6 +5V)
  (net 7 /CALFPOT5V)
  (net 8 GND)
  (net 9 /CALFPOT3V3)
  (net 10 "Net-(U1-Pad2)")
  (net 11 "Net-(U1-Pad3)")
  (net 12 "Net-(U1-Pad5)")
  (net 13 "Net-(U1-Pad6)")
  (net 14 "Net-(U1-Pad7)")
  (net 15 "Net-(U1-Pad8)")
  (net 16 "Net-(U1-Pad9)")
  (net 17 "Net-(U1-Pad10)")
  (net 18 "Net-(U1-Pad11)")
  (net 19 /HIP0)
  (net 20 "Net-(U1-Pad13)")
  (net 21 /FB2)
  (net 22 /THIGH1)
  (net 23 /KNEE0)
  (net 24 /FB4)
  (net 25 "Net-(U1-Pad18)")
  (net 26 "Net-(U1-Pad19)")
  (net 27 /FB6)
  (net 28 "Net-(U1-Pad22)")
  (net 29 "Net-(U1-Pad23)")
  (net 30 "Net-(U1-Pad24)")
  (net 31 "Net-(U1-Pad25)")
  (net 32 /KNEE1)
  (net 33 /THIGH0)
  (net 34 /HIP1)
  (net 35 /MDISABLE)
  (net 36 "Net-(U1-Pad30)")
  (net 37 "Net-(U1-Pad31)")
  (net 38 "Net-(U1-Pad32)")
  (net 39 "Net-(U1-Pad33)")
  (net 40 "Net-(U1-Pad34)")
  (net 41 "Net-(U1-Pad35)")
  (net 42 "Net-(U1-Pad38)")
  (net 43 "Net-(U2-Pad20)")
  (net 44 "Net-(U2-Pad14)")
  (net 45 "Net-(U2-Pad25)")
  (net 46 "Net-(U2-Pad26)")
  (net 47 "Net-(U2-Pad28)")
  (net 48 "Net-(U2-Pad29)")
  (net 49 "Net-(U2-Pad30)")
  (net 50 /M1EN)
  (net 51 "Net-(U2-Pad9)")
  (net 52 /M2EN)
  (net 53 "Net-(U2-Pad2)")
  (net 54 /SPI_CLK)
  (net 55 /SPI_DO)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net +5V)
    (add_net /CALFPOT3V3)
    (add_net /CALFPOT5V)
    (add_net /FB2)
    (add_net /FB4)
    (add_net /FB6)
    (add_net /HIP0)
    (add_net /HIP1)
    (add_net /HIPPOT)
    (add_net /KNEE0)
    (add_net /KNEE1)
    (add_net /KNEEPOT)
    (add_net /M1EN)
    (add_net /M2EN)
    (add_net /MDISABLE)
    (add_net /SPI_CLK)
    (add_net /SPI_DO)
    (add_net /THIGH0)
    (add_net /THIGH1)
    (add_net /THIGHPOT)
    (add_net GND)
    (add_net GNDA)
    (add_net "Net-(U1-Pad10)")
    (add_net "Net-(U1-Pad11)")
    (add_net "Net-(U1-Pad13)")
    (add_net "Net-(U1-Pad18)")
    (add_net "Net-(U1-Pad19)")
    (add_net "Net-(U1-Pad2)")
    (add_net "Net-(U1-Pad22)")
    (add_net "Net-(U1-Pad23)")
    (add_net "Net-(U1-Pad24)")
    (add_net "Net-(U1-Pad25)")
    (add_net "Net-(U1-Pad3)")
    (add_net "Net-(U1-Pad30)")
    (add_net "Net-(U1-Pad31)")
    (add_net "Net-(U1-Pad32)")
    (add_net "Net-(U1-Pad33)")
    (add_net "Net-(U1-Pad34)")
    (add_net "Net-(U1-Pad35)")
    (add_net "Net-(U1-Pad38)")
    (add_net "Net-(U1-Pad5)")
    (add_net "Net-(U1-Pad6)")
    (add_net "Net-(U1-Pad7)")
    (add_net "Net-(U1-Pad8)")
    (add_net "Net-(U1-Pad9)")
    (add_net "Net-(U2-Pad14)")
    (add_net "Net-(U2-Pad2)")
    (add_net "Net-(U2-Pad20)")
    (add_net "Net-(U2-Pad25)")
    (add_net "Net-(U2-Pad26)")
    (add_net "Net-(U2-Pad28)")
    (add_net "Net-(U2-Pad29)")
    (add_net "Net-(U2-Pad30)")
    (add_net "Net-(U2-Pad9)")
  )
  (module teensy:Teensy30_31_32_LC_NO_INNER_OUTER (layer F.Cu) (tedit 5AFA2C97)
    (at 113.03 95.25 270)
    (fp_text reference U2 (at 0 -10.16 270) (layer F.SilkS))
    (fp_text value Teensy3.2_no_outer_inner (at 0 10.16 270) (layer F.Fab))
    (fp_text user T3.2 (at -10.16 -2.54 360) (layer F.SilkS))
    (fp_text user T3.1 (at -6.35 -2.54 360) (layer F.SilkS))
    (pad 20 thru_hole circle (at 16.51 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 43 "Net-(U2-Pad20)"))
    (pad 14 thru_hole circle (at 16.51 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 44 "Net-(U2-Pad14)"))
    (pad 21 thru_hole circle (at 13.97 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 54 /SPI_CLK))
    (pad 22 thru_hole circle (at 11.43 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 5 /KNEEPOT))
    (pad 23 thru_hole circle (at 8.89 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 9 /CALFPOT3V3))
    (pad 24 thru_hole circle (at 6.35 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 4 /THIGHPOT))
    (pad 25 thru_hole circle (at 3.81 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 45 "Net-(U2-Pad25)"))
    (pad 26 thru_hole circle (at 1.27 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 46 "Net-(U2-Pad26)"))
    (pad 27 thru_hole circle (at -1.27 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 2 /HIPPOT))
    (pad 28 thru_hole circle (at -3.81 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 47 "Net-(U2-Pad28)"))
    (pad 29 thru_hole circle (at -6.35 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 48 "Net-(U2-Pad29)"))
    (pad 30 thru_hole circle (at -8.89 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 49 "Net-(U2-Pad30)"))
    (pad 31 thru_hole circle (at -11.43 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 1 +3V3))
    (pad 32 thru_hole circle (at -13.97 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 3 GNDA))
    (pad 33 thru_hole circle (at -16.51 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 6 +5V))
    (pad 13 thru_hole circle (at 13.97 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 55 /SPI_DO))
    (pad 12 thru_hole circle (at 11.43 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 34 /HIP1))
    (pad 11 thru_hole circle (at 8.89 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 19 /HIP0))
    (pad 10 thru_hole circle (at 6.35 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 50 /M1EN))
    (pad 9 thru_hole circle (at 3.81 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 51 "Net-(U2-Pad9)"))
    (pad 8 thru_hole circle (at 1.27 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 32 /KNEE1))
    (pad 7 thru_hole circle (at -1.27 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 23 /KNEE0))
    (pad 6 thru_hole circle (at -3.81 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 22 /THIGH1))
    (pad 5 thru_hole circle (at -6.35 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 33 /THIGH0))
    (pad 4 thru_hole circle (at -8.89 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 52 /M2EN))
    (pad 3 thru_hole circle (at -11.43 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 35 /MDISABLE))
    (pad 2 thru_hole circle (at -13.97 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 53 "Net-(U2-Pad2)"))
    (pad 1 thru_hole rect (at -16.51 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 8 GND))
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5874F706)
    (at 107.95 122.555)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R1 (at 5.08 -2.31) (layer F.SilkS))
    (fp_text value 560 (at 5.08 2.31) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 /CALFPOT5V))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 /CALFPOT3V3))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5874F706)
    (at 118.11 118.11 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R2 (at 5.08 -2.31 180) (layer F.SilkS))
    (fp_text value 1K (at 5.08 2.31 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 /CALFPOT3V3))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 GND))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module leg_thing:MOLEX6PIN (layer F.Cu) (tedit 5B0608AA)
    (at 128.905 93.345)
    (fp_text reference J1 (at 1.905 -4.445 90) (layer F.SilkS))
    (fp_text value HIPCALF (at 1.905 2.54 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 -6.35) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 GNDA))
    (pad 2 thru_hole circle (at 0 -3.81) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 /HIPPOT))
    (pad 3 thru_hole circle (at 0 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (pad 4 thru_hole circle (at 0 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 7 /CALFPOT5V))
    (pad 5 thru_hole circle (at 0 3.81) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 6 +5V))
    (pad 6 thru_hole circle (at 0 6.35) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 8 GND))
  )
  (module leg_thing:MOLEX6PIN (layer F.Cu) (tedit 5B0608AA)
    (at 128.905 112.395)
    (fp_text reference J2 (at 1.905 -4.445 90) (layer F.SilkS))
    (fp_text value THIGHKNEE (at 1.905 2.54 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 -6.35) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (pad 2 thru_hole circle (at 0 -3.81) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 GNDA))
    (pad 3 thru_hole circle (at 0 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 4 /THIGHPOT))
    (pad 4 thru_hole circle (at 0 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 5 /KNEEPOT))
    (pad 5 thru_hole circle (at 0 3.81) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (pad 6 thru_hole circle (at 0 6.35) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 GNDA))
  )
  (module leg_thing:ESP32THINGPOWERSHIELD (layer F.Cu) (tedit 5B060959)
    (at 113.03 104.14)
    (fp_text reference U1 (at 0 0.5) (layer F.SilkS))
    (fp_text value ESP32THINGPOWERSHIELD (at 0 -0.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 11.43 -25.4) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 8 GND))
    (pad 2 thru_hole circle (at 11.43 -22.86) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 10 "Net-(U1-Pad2)"))
    (pad 3 thru_hole circle (at 11.43 -20.32) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 11 "Net-(U1-Pad3)"))
    (pad 4 thru_hole circle (at 11.43 -17.78) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 8 GND))
    (pad 5 thru_hole circle (at 11.43 -15.24) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 12 "Net-(U1-Pad5)"))
    (pad 6 thru_hole circle (at 11.43 -12.7) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 13 "Net-(U1-Pad6)"))
    (pad 7 thru_hole circle (at 11.43 -10.16) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 14 "Net-(U1-Pad7)"))
    (pad 8 thru_hole circle (at 11.43 -7.62) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 15 "Net-(U1-Pad8)"))
    (pad 9 thru_hole circle (at 11.43 -5.08) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 16 "Net-(U1-Pad9)"))
    (pad 10 thru_hole circle (at 11.43 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 17 "Net-(U1-Pad10)"))
    (pad 11 thru_hole circle (at 11.43 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 18 "Net-(U1-Pad11)"))
    (pad 12 thru_hole circle (at 11.43 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 19 /HIP0))
    (pad 13 thru_hole circle (at 11.43 5.08) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 20 "Net-(U1-Pad13)"))
    (pad 14 thru_hole circle (at 11.43 7.62) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 21 /FB2))
    (pad 15 thru_hole circle (at 11.43 10.16) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 22 /THIGH1))
    (pad 16 thru_hole circle (at 11.43 12.7) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 23 /KNEE0))
    (pad 17 thru_hole circle (at 11.43 15.24) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 24 /FB4))
    (pad 18 thru_hole circle (at 11.43 17.78) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 25 "Net-(U1-Pad18)"))
    (pad 19 thru_hole circle (at 11.43 20.32) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 26 "Net-(U1-Pad19)"))
    (pad 20 thru_hole circle (at 11.43 22.86) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 27 /FB6))
    (pad 21 thru_hole circle (at -11.43 22.86) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 8 GND))
    (pad 22 thru_hole circle (at -11.43 20.32) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 28 "Net-(U1-Pad22)"))
    (pad 23 thru_hole circle (at -11.43 17.78) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 29 "Net-(U1-Pad23)"))
    (pad 24 thru_hole circle (at -11.43 15.24) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 30 "Net-(U1-Pad24)"))
    (pad 25 thru_hole circle (at -11.43 12.7) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 31 "Net-(U1-Pad25)"))
    (pad 26 thru_hole circle (at -11.43 10.16) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 32 /KNEE1))
    (pad 27 thru_hole circle (at -11.43 7.62) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 33 /THIGH0))
    (pad 28 thru_hole circle (at -11.43 5.08) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 34 /HIP1))
    (pad 29 thru_hole circle (at -11.43 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 35 /MDISABLE))
    (pad 30 thru_hole circle (at -11.43 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 36 "Net-(U1-Pad30)"))
    (pad 31 thru_hole circle (at -11.43 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 37 "Net-(U1-Pad31)"))
    (pad 32 thru_hole circle (at -11.43 -5.08) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 38 "Net-(U1-Pad32)"))
    (pad 33 thru_hole circle (at -11.43 -7.62) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 39 "Net-(U1-Pad33)"))
    (pad 34 thru_hole circle (at -11.43 -10.16) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 40 "Net-(U1-Pad34)"))
    (pad 35 thru_hole circle (at -11.43 -12.7) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 41 "Net-(U1-Pad35)"))
    (pad 36 thru_hole circle (at -11.43 -15.24) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (pad 37 thru_hole circle (at -11.43 -17.78) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 8 GND))
    (pad 38 thru_hole circle (at -11.43 -20.32) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 42 "Net-(U1-Pad38)"))
    (pad 39 thru_hole circle (at -11.43 -22.86) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 6 +5V))
    (pad 40 thru_hole circle (at -11.43 -25.4) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 8 GND))
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 5B0AA8AE)
    (at 115.57 127 270)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J3 (at 0 -2.33 270) (layer F.SilkS))
    (fp_text value SPI (at 0 7.41 270) (layer F.Fab))
    (fp_text user %R (at 0 2.54 360) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 GND))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 54 /SPI_CLK))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 55 /SPI_DO))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 112.3 85.09 180)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R3 (at 0 -1.85 180) (layer F.SilkS))
    (fp_text value 1K (at 0 1.9 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 35 /MDISABLE))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text V1 (at 128.27 102.87) (layer F.SilkS))
  (gr_text K1 (at 103.378 114.3) (layer F.SilkS))
  (gr_text T0 (at 103.378 111.76) (layer F.SilkS))
  (gr_text H1 (at 103.378 109.22) (layer F.SilkS))
  (gr_text MD (at 103.378 106.68) (layer F.SilkS))
  (gr_text K0 (at 122.936 116.84) (layer F.SilkS))
  (gr_text T1 (at 122.936 114.3) (layer F.SilkS))
  (gr_text H0 (at 122.936 106.68) (layer F.SilkS))
  (gr_text G (at 125.73 118.872) (layer F.SilkS))
  (gr_text 3 (at 125.73 116.332) (layer F.SilkS))
  (gr_text K (at 125.73 113.792) (layer F.SilkS))
  (gr_text T (at 125.73 110.998) (layer F.SilkS))
  (gr_text G (at 125.73 108.458) (layer F.SilkS))
  (gr_text 3 (at 125.73 105.918) (layer F.SilkS))
  (gr_text G (at 125.73 87.122) (layer F.SilkS))
  (gr_text H (at 125.73 89.662) (layer F.SilkS))
  (gr_text 3 (at 125.73 92.202) (layer F.SilkS))
  (gr_text C (at 125.73 94.742) (layer F.SilkS))
  (gr_text 5 (at 125.73 97.282) (layer F.SilkS))
  (gr_text G (at 125.73 99.822) (layer F.SilkS))
  (gr_line (start 99.695 128.905) (end 99.695 76.835) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 126.365 128.905) (end 99.695 128.905) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 126.365 120.65) (end 126.365 128.905) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 130.81 120.65) (end 126.365 120.65) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 130.81 85.09) (end 130.81 120.65) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 126.365 85.09) (end 130.81 85.09) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 126.365 76.835) (end 126.365 85.09) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 99.695 76.835) (end 126.365 76.835) (layer Edge.Cuts) (width 0.1))
  (zone (net 8) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 125.984 93.472) (xy 130.302 93.472) (xy 130.302 100.838) (xy 125.984 100.838) (xy 125.984 128.524)
        (xy 100.076 128.524) (xy 100.076 77.216) (xy 125.984 77.216)
      )
    )
  )
  (zone (net 3) (net_name GNDA) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 130.302 85.598) (xy 130.302 92.964) (xy 126.492 92.964) (xy 126.492 85.598)
      )
    )
  )
  (zone (net 3) (net_name GNDA) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 126.492 104.902) (xy 130.302 104.902) (xy 130.302 120.142) (xy 126.492 120.142)
      )
    )
  )
)
