(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 0)
    (no_connects 4)
    (area 130.514288 93.1 162.145 114.491)
    (thickness 1.6)
    (drawings 7)
    (tracks 81)
    (zones 0)
    (modules 14)
    (nets 10)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.508)
    (user_trace_width 0.1524)
    (user_trace_width 0.254)
    (user_trace_width 0.508)
    (user_trace_width 2.032)
    (trace_clearance 0.2)
    (zone_clearance 0.25)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 0.6 0.6)
    (pad_drill 0.3)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (grid_origin 151.6 101.4)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue false)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerber-TOF/))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(J1-Pad1)")
  (net 3 "Net-(J1-Pad2)")
  (net 4 +2V8)
  (net 5 "Net-(J2-Pad3)")
  (net 6 "Net-(J2-Pad1)")
  (net 7 +BATT)
  (net 8 /DI)
  (net 9 /DO)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +2V8)
    (add_net +BATT)
    (add_net /DI)
    (add_net /DO)
    (add_net GND)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J2-Pad3)")
  )
  (module footprints:via (layer F.Cu) (tedit 59EDACEE)
    (at 156.6 99.9)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value via (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module footprints:via (layer F.Cu) (tedit 59EDACEE)
    (at 143.85 100.65)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value via (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module footprints:via (layer F.Cu) (tedit 59EDACEE)
    (at 152.6 111.15)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value via (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module penguiconbadge2:LED5050 (layer F.Cu) (tedit 59EDABF8)
    (at 146.507 109.098)
    (fp_text reference U3 (at 0.254 4.318) (layer F.SilkS) hide)
    (fp_text value WS2812 (at 0.508 -3.81) (layer F.Fab))
    (pad 5 smd rect (at 2.4 0) (size 2 1.1) (layers F.Cu F.Paste F.Mask)
      (net 7 +BATT))
    (pad 2 smd rect (at -2.4 0) (size 2 1.1) (layers F.Cu F.Paste F.Mask)
      (net 8 /DI))
    (pad 4 smd rect (at 2.4 1.7) (size 2 1.1) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at 2.4 -1.7) (size 2 1.1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -2.4 1.7) (size 2 1.1) (layers F.Cu F.Paste F.Mask)
      (net 7 +BATT))
    (pad 1 smd rect (at -2.4 -1.7) (size 2 1.1) (layers F.Cu F.Paste F.Mask)
      (net 9 /DO))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59EDADAD)
    (at 155.029 101.539 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at 2.4 0 270) (layer F.SilkS) hide)
    (fp_text value 4.7uF (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +2V8))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59EDADAA)
    (at 153.759 101.539 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at 2.54 0 270) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +2V8))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module _sensors:VL53L0X (layer F.Cu) (tedit 57CEB927)
    (at 150.038 101.616)
    (descr VL53L0X)
    (tags "TOF distance sensor")
    (fp_text reference U1 (at 0 0) (layer F.SilkS) hide)
    (fp_text value VL53L0X (at 0 0) (layer F.Fab) hide)
    (pad 1 smd rect (at 1.6 0.8) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 4 +2V8))
    (pad 2 smd rect (at 0.8 0.8) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 0 0.8) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at -1.6 0.8) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J1-Pad1)"))
    (pad 4 smd rect (at -0.8 0.8) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -1.6 0) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 11 smd rect (at 1.6 -0.8) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 4 +2V8))
    (pad 10 smd rect (at 0.8 -0.8) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(J2-Pad3)"))
    (pad 9 smd rect (at 0 -0.8) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(J2-Pad1)"))
    (pad 8 smd rect (at -0.8 -0.8) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask))
    (pad 7 smd rect (at -1.6 -0.8) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J1-Pad2)"))
    (pad 12 smd rect (at 1.6 0) (size 0.5 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KIPRJMOD}/kicad-lib/3Dmodels/Sensors/ST-VL53L0X.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59EDADA3)
    (at 155.295 107.242 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C3 (at 0 -1.5 180) (layer F.SilkS) hide)
    (fp_text value 10uF (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 +BATT))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59EDADB1)
    (at 150.965 104.194 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C4 (at 0 -1.5 180) (layer F.SilkS) hide)
    (fp_text value 10uF (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +2V8))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_JST:JST_SH_SM02B-SRSS-TB_02x1.00mm_Angled (layer F.Cu) (tedit 59EDADB8)
    (at 144.2665 102.013 270)
    (descr http://www.jst-mfg.com/product/pdf/eng/eSH.pdf)
    (tags "connector jst sh")
    (attr smd)
    (fp_text reference J1 (at -0.5 -4 270) (layer F.SilkS) hide)
    (fp_text value Conn_01x02 (at 0 4.5 270) (layer F.Fab))
    (pad 1 smd rect (at -0.5 -1.9375 270) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J1-Pad1)"))
    (pad 2 smd rect (at 0.5 -1.9375 270) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J1-Pad2)"))
    (pad "" smd rect (at -1.8 1.9375 270) (size 1.2 1.8) (layers F.Cu F.Paste F.Mask))
    (pad "" smd rect (at 1.8 1.9375 270) (size 1.2 1.8) (layers F.Cu F.Paste F.Mask))
  )
  (module Connectors_JST:JST_SH_SM05B-SRSS-TB_05x1.00mm_Angled (layer B.Cu) (tedit 59EDADD8)
    (at 144.4555 105.877 90)
    (descr http://www.jst-mfg.com/product/pdf/eng/eSH.pdf)
    (tags "connector jst sh")
    (attr smd)
    (fp_text reference J2 (at -2 4 90) (layer B.SilkS) hide)
    (fp_text value Conn_01x05 (at 0 -4.5 90) (layer B.Fab))
    (pad 1 smd rect (at -2 1.9375 90) (size 0.6 1.55) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(J2-Pad1)"))
    (pad 2 smd rect (at -1 1.9375 90) (size 0.6 1.55) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 0 1.9375 90) (size 0.6 1.55) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(J2-Pad3)"))
    (pad 4 smd rect (at 1 1.9375 90) (size 0.6 1.55) (layers B.Cu B.Paste B.Mask)
      (net 7 +BATT))
    (pad 5 smd rect (at 2 1.9375 90) (size 0.6 1.55) (layers B.Cu B.Paste B.Mask)
      (net 8 /DI))
    (pad "" smd rect (at -3.3 -1.9375 90) (size 1.2 1.8) (layers B.Cu B.Paste B.Mask))
    (pad "" smd rect (at 3.3 -1.9375 90) (size 1.2 1.8) (layers B.Cu B.Paste B.Mask))
  )
  (module Connectors_JST:JST_SH_SM05B-SRSS-TB_05x1.00mm_Angled (layer B.Cu) (tedit 59EDADD4)
    (at 153.7915 105.877 270)
    (descr http://www.jst-mfg.com/product/pdf/eng/eSH.pdf)
    (tags "connector jst sh")
    (attr smd)
    (fp_text reference J3 (at -2 4 270) (layer B.SilkS) hide)
    (fp_text value Conn_01x05 (at 0 -4.5 270) (layer B.Fab))
    (pad 1 smd rect (at -2 1.9375 270) (size 0.6 1.55) (layers B.Cu B.Paste B.Mask)
      (net 9 /DO))
    (pad 2 smd rect (at -1 1.9375 270) (size 0.6 1.55) (layers B.Cu B.Paste B.Mask)
      (net 7 +BATT))
    (pad 3 smd rect (at 0 1.9375 270) (size 0.6 1.55) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(J2-Pad3)"))
    (pad 4 smd rect (at 1 1.9375 270) (size 0.6 1.55) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 2 1.9375 270) (size 0.6 1.55) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(J2-Pad1)"))
    (pad "" smd rect (at -3.3 -1.9375 270) (size 1.2 1.8) (layers B.Cu B.Paste B.Mask))
    (pad "" smd rect (at 3.3 -1.9375 270) (size 1.2 1.8) (layers B.Cu B.Paste B.Mask))
  )
  (module TO_SOT_Packages_SMD:SOT-23-5 (layer F.Cu) (tedit 59EDADA6)
    (at 154.945 104.763 180)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U2 (at 0 -6.637 180) (layer F.SilkS) hide)
    (fp_text value AP2125K-2.8TRG1 (at 0 2.9 180) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 7 +BATT))
    (pad 2 smd rect (at -1.1 0 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -1.1 0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 7 +BATT))
    (pad 4 smd rect (at 1.1 0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 1.1 -0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 4 +2V8))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:via (layer F.Cu) (tedit 59EDACEE)
    (at 146.35 108.9)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value via (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (gr_text "DWC\nTOF\nV3" (at 152.35 110.15) (layer F.SilkS))
  (dimension 14 (width 0.3) (layer Dwgs.User)
    (gr_text "0.5512 in" (at 136.050001 106 270) (layer Dwgs.User))
    (feature1 (pts (xy 140.8 113) (xy 134.700001 113)))
    (feature2 (pts (xy 140.8 99) (xy 134.700001 99)))
    (crossbar (pts (xy 137.400001 99) (xy 137.400001 113)))
    (arrow1a (pts (xy 137.400001 113) (xy 136.81358 111.873496)))
    (arrow1b (pts (xy 137.400001 113) (xy 137.986422 111.873496)))
    (arrow2a (pts (xy 137.400001 99) (xy 136.81358 100.126504)))
    (arrow2b (pts (xy 137.400001 99) (xy 137.986422 100.126504)))
  )
  (dimension 16.4 (width 0.3) (layer Dwgs.User)
    (gr_text "0.6457 in" (at 149.2 94.45) (layer Dwgs.User))
    (feature1 (pts (xy 157.4 98.4) (xy 157.4 93.1)))
    (feature2 (pts (xy 141 98.4) (xy 141 93.1)))
    (crossbar (pts (xy 141 95.8) (xy 157.4 95.8)))
    (arrow1a (pts (xy 157.4 95.8) (xy 156.273496 96.386421)))
    (arrow1b (pts (xy 157.4 95.8) (xy 156.273496 95.213579)))
    (arrow2a (pts (xy 141 95.8) (xy 142.126504 96.386421)))
    (arrow2b (pts (xy 141 95.8) (xy 142.126504 95.213579)))
  )
  (gr_line (start 140.97 113.03) (end 140.97 99.06) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 157.48 113.03) (end 140.97 113.03) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 157.48 99.06) (end 157.48 113.03) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 140.97 99.06) (end 157.48 99.06) (layer Edge.Cuts) (width 0.1))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.25))
    (min_thickness 0.25)
    (fill yes (arc_segments 32) (thermal_gap 0.25) (thermal_bridge_width 0.25))
    (polygon
      (pts
        (xy 139.7 97.79) (xy 158.115 97.79) (xy 158.115 114.3) (xy 139.7 114.3)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.25))
    (min_thickness 0.25)
    (fill yes (arc_segments 32) (thermal_gap 0.25) (thermal_bridge_width 0.25))
    (polygon
      (pts
        (xy 139.5 97.904246) (xy 157.915 97.904246) (xy 157.915 114.414246) (xy 139.5 114.414246)
      )
    )
  )
)
