(kicad_pcb (version 20171130) (host pcbnew "(5.1.7)-1")
  (general
    (thickness 1.6)
    (drawings 54)
    (tracks 351)
    (zones 0)
    (modules 23)
    (nets 45)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.1524)
    (user_trace_width 0.2032)
    (user_trace_width 0.8128)
    (trace_clearance 0.1524)
    (zone_clearance 0.254)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.0508)
    (solder_mask_min_width 0.1016)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 /SCL)
  (net 2 /SDA)
  (net 3 VCC)
  (net 4 GND)
  (net 5 /SDB)
  (net 6 /AD)
  (net 7 /R_EXT)
  (net 8 /OUT1)
  (net 9 /OUT2)
  (net 10 /OUT3)
  (net 11 /OUT4)
  (net 12 /OUT5)
  (net 13 /OUT6)
  (net 14 /OUT7)
  (net 15 /OUT8)
  (net 16 /OUT9)
  (net 17 /OUT10)
  (net 18 /OUT11)
  (net 19 /OUT12)
  (net 20 /OUT13)
  (net 21 /OUT14)
  (net 22 /OUT15)
  (net 23 /OUT16)
  (net 24 /OUT17)
  (net 25 /OUT18)
  (net 26 /OUT19)
  (net 27 /OUT20)
  (net 28 /OUT21)
  (net 29 /OUT22)
  (net 30 /OUT23)
  (net 31 /OUT24)
  (net 32 /OUT25)
  (net 33 /OUT26)
  (net 34 /OUT27)
  (net 35 /OUT28)
  (net 36 /OUT29)
  (net 37 /OUT30)
  (net 38 /OUT31)
  (net 39 /OUT32)
  (net 40 /OUT33)
  (net 41 /OUT34)
  (net 42 /OUT35)
  (net 43 /OUT36)
  (net 44 +3V3)
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.25)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net /AD)
    (add_net /OUT1)
    (add_net /OUT10)
    (add_net /OUT11)
    (add_net /OUT12)
    (add_net /OUT13)
    (add_net /OUT14)
    (add_net /OUT15)
    (add_net /OUT16)
    (add_net /OUT17)
    (add_net /OUT18)
    (add_net /OUT19)
    (add_net /OUT2)
    (add_net /OUT20)
    (add_net /OUT21)
    (add_net /OUT22)
    (add_net /OUT23)
    (add_net /OUT24)
    (add_net /OUT25)
    (add_net /OUT26)
    (add_net /OUT27)
    (add_net /OUT28)
    (add_net /OUT29)
    (add_net /OUT3)
    (add_net /OUT30)
    (add_net /OUT31)
    (add_net /OUT32)
    (add_net /OUT33)
    (add_net /OUT34)
    (add_net /OUT35)
    (add_net /OUT36)
    (add_net /OUT4)
    (add_net /OUT5)
    (add_net /OUT6)
    (add_net /OUT7)
    (add_net /OUT8)
    (add_net /OUT9)
    (add_net /R_EXT)
    (add_net /SCL)
    (add_net /SDA)
    (add_net /SDB)
    (add_net GND)
    (add_net VCC)
  )
  (module Connectors_JST:JST_SH_SM04B-SRSS-TB_04x1.00mm_Angled (layer F.Cu) (tedit 56B07436)
    (at 38.354 46.99 270)
    (descr http://www.jst-mfg.com/product/pdf/eng/eSH.pdf)
    (tags "connector jst sh")
    (attr smd)
    (fp_text reference J1 (at -1.5 -4 90) (layer F.SilkS))
    (fp_text value Conn_01x04 (at 0 4.5 90) (layer F.Fab))
    (pad "" smd rect (at 2.8 1.9375 270) (size 1.2 1.8) (layers F.Cu F.Paste F.Mask))
    (pad "" smd rect (at -2.8 1.9375 270) (size 1.2 1.8) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at 1.5 -1.9375 270) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 1 /SCL))
    (pad 3 smd rect (at 0.5 -1.9375 270) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 2 /SDA))
    (pad 2 smd rect (at -0.5 -1.9375 270) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 44 +3V3))
    (pad 1 smd rect (at -1.5 -1.9375 270) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
  )
  (module Connectors_JST:JST_SH_SM04B-SRSS-TB_04x1.00mm_Angled (layer F.Cu) (tedit 56B07436)
    (at 98.806 46.99 90)
    (descr http://www.jst-mfg.com/product/pdf/eng/eSH.pdf)
    (tags "connector jst sh")
    (attr smd)
    (fp_text reference J2 (at 3.048 -2.54 90) (layer F.SilkS))
    (fp_text value Conn_01x04 (at 0 4.5 90) (layer F.Fab))
    (pad 1 smd rect (at -1.5 -1.9375 90) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 2 smd rect (at -0.5 -1.9375 90) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 44 +3V3))
    (pad 3 smd rect (at 0.5 -1.9375 90) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 2 /SDA))
    (pad 4 smd rect (at 1.5 -1.9375 90) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 1 /SCL))
    (pad "" smd rect (at -2.8 1.9375 90) (size 1.2 1.8) (layers F.Cu F.Paste F.Mask))
    (pad "" smd rect (at 2.8 1.9375 90) (size 1.2 1.8) (layers F.Cu F.Paste F.Mask))
  )
  (module is31fl3236a:QFN-44-1EP_5x5mm_P0.4mm_EP2.45x2.45mm (layer F.Cu) (tedit 5E07AD5A)
    (at 71.882 46.99 90)
    (descr "QFN, 44 Pin (http://ww1.microchip.com/downloads/en/DeviceDoc/2512S.pdf#page=17), generated with kicad-footprint-generator ipc_noLead_generator.py")
    (tags "QFN NoLead")
    (attr smd)
    (fp_text reference U1 (at 0 -3.82 90) (layer F.SilkS))
    (fp_text value IS31FL3236A (at 0 3.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 45 smd roundrect (at 0 0 90) (size 2.45 2.45) (layers F.Cu F.Mask) (roundrect_rratio 0.102041)
      (net 4 GND))
    (pad "" smd roundrect (at -0.61 -0.61 90) (size 0.99 0.99) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.61 0.61 90) (size 0.99 0.99) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.61 -0.61 90) (size 0.99 0.99) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.61 0.61 90) (size 0.99 0.99) (layers F.Paste) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -2.5375 -2 90) (size 0.675 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 /OUT3))
    (pad 2 smd roundrect (at -2.4375 -1.6 90) (size 0.875 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 /OUT4))
    (pad 3 smd roundrect (at -2.4375 -1.2 90) (size 0.875 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 /OUT5))
    (pad 4 smd roundrect (at -2.4375 -0.8 90) (size 0.875 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 /OUT6))
    (pad 5 smd roundrect (at -2.4375 -0.4 90) (size 0.875 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 /OUT7))
    (pad 6 smd roundrect (at -2.4375 0 90) (size 0.875 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 /OUT8))
    (pad 7 smd roundrect (at -2.4375 0.4 90) (size 0.875 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 16 /OUT9))
    (pad 8 smd roundrect (at -2.4375 0.8 90) (size 0.875 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 /OUT10))
    (pad 9 smd roundrect (at -2.4375 1.2 90) (size 0.875 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 /OUT11))
    (pad 10 smd roundrect (at -2.4375 1.6 90) (size 0.875 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 /OUT12))
    (pad 11 smd roundrect (at -2.5375 2 90) (size 0.675 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 /OUT13))
    (pad 12 smd roundrect (at -2 2.5375 90) (size 0.2 0.675) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 /OUT14))
    (pad 13 smd roundrect (at -1.6 2.4375 90) (size 0.2 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 /OUT15))
    (pad 14 smd roundrect (at -1.2 2.4375 90) (size 0.2 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 23 /OUT16))
    (pad 15 smd roundrect (at -0.8 2.4375 90) (size 0.2 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 /OUT17))
    (pad 16 smd roundrect (at -0.4 2.4375 90) (size 0.2 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 25 /OUT18))
    (pad 17 smd roundrect (at 0 2.4375 90) (size 0.2 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (pad 18 smd roundrect (at 0.4 2.4375 90) (size 0.2 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 /OUT19))
    (pad 19 smd roundrect (at 0.8 2.4375 90) (size 0.2 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 27 /OUT20))
    (pad 20 smd roundrect (at 1.2 2.4375 90) (size 0.2 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 28 /OUT21))
    (pad 21 smd roundrect (at 1.6 2.4375 90) (size 0.2 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 29 /OUT22))
    (pad 22 smd roundrect (at 2 2.5375 90) (size 0.2 0.675) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 30 /OUT23))
    (pad 23 smd roundrect (at 2.5375 2 90) (size 0.675 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 31 /OUT24))
    (pad 24 smd roundrect (at 2.4375 1.6 90) (size 0.875 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 32 /OUT25))
    (pad 25 smd roundrect (at 2.4375 1.2 90) (size 0.875 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 33 /OUT26))
    (pad 26 smd roundrect (at 2.4375 0.8 90) (size 0.875 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 34 /OUT27))
    (pad 27 smd roundrect (at 2.4375 0.4 90) (size 0.875 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 35 /OUT28))
    (pad 28 smd roundrect (at 2.4375 0 90) (size 0.875 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 36 /OUT29))
    (pad 29 smd roundrect (at 2.4375 -0.4 90) (size 0.875 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 37 /OUT30))
    (pad 30 smd roundrect (at 2.4375 -0.8 90) (size 0.875 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 38 /OUT31))
    (pad 31 smd roundrect (at 2.4375 -1.2 90) (size 0.875 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 39 /OUT32))
    (pad 32 smd roundrect (at 2.4375 -1.6 90) (size 0.875 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 40 /OUT33))
    (pad 33 smd roundrect (at 2.5375 -2 90) (size 0.675 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 41 /OUT34))
    (pad 34 smd roundrect (at 2 -2.5375 90) (size 0.2 0.675) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 42 /OUT35))
    (pad 35 smd roundrect (at 1.6 -2.4375 90) (size 0.2 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 43 /OUT36))
    (pad 36 smd roundrect (at 1.2 -2.4375 90) (size 0.2 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 /SDB))
    (pad 37 smd roundrect (at 0.8 -2.4375 90) (size 0.2 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 /AD))
    (pad 38 smd roundrect (at 0.4 -2.4375 90) (size 0.2 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 VCC))
    (pad 39 smd roundrect (at 0 -2.4375 90) (size 0.2 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (pad 40 smd roundrect (at -0.4 -2.4375 90) (size 0.2 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 /R_EXT))
    (pad 41 smd roundrect (at -0.8 -2.4375 90) (size 0.2 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 /SDA))
    (pad 42 smd roundrect (at -1.2 -2.4375 90) (size 0.2 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 /SCL))
    (pad 43 smd roundrect (at -1.6 -2.4375 90) (size 0.2 0.875) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 /OUT1))
    (pad 44 smd roundrect (at -2 -2.5375 90) (size 0.2 0.675) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 /OUT2))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/QFN-44-1EP_5x5mm_P0.4mm_EP2.45x2.45mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x21_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 43.18 55.88 90)
    (descr "Through hole straight pin header, 1x21, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x21 2.54mm single row")
    (fp_text reference J3 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value Conn_01x21 (at 0 53.13 90) (layer F.Fab))
    (fp_text user %R (at 0 25.4) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /SCL))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /SDA))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /SDB))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 10 thru_hole oval (at 0 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 11 thru_hole oval (at 0 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 12 thru_hole oval (at 0 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 13 thru_hole oval (at 0 30.48 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 14 thru_hole oval (at 0 33.02 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 15 thru_hole oval (at 0 35.56 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 16 thru_hole oval (at 0 38.1 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 17 thru_hole oval (at 0 40.64 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 18 thru_hole oval (at 0 43.18 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 19 thru_hole oval (at 0 45.72 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 20 thru_hole oval (at 0 48.26 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 21 thru_hole oval (at 0 50.8 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 VCC))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x21_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x21_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 43.18 40.64 90)
    (descr "Through hole straight pin header, 1x21, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x21 2.54mm single row")
    (fp_text reference J4 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value Conn_01x21 (at 0 53.13 90) (layer F.Fab))
    (fp_text user %R (at 0 25.4) (layer F.Fab))
    (pad 21 thru_hole oval (at 0 50.8 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 /OUT16))
    (pad 20 thru_hole oval (at 0 48.26 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 /OUT17))
    (pad 19 thru_hole oval (at 0 45.72 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 /OUT18))
    (pad 18 thru_hole oval (at 0 43.18 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 /OUT19))
    (pad 17 thru_hole oval (at 0 40.64 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 /OUT20))
    (pad 16 thru_hole oval (at 0 38.1 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 /OUT21))
    (pad 15 thru_hole oval (at 0 35.56 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 /OUT22))
    (pad 14 thru_hole oval (at 0 33.02 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 /OUT23))
    (pad 13 thru_hole oval (at 0 30.48 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 /OUT24))
    (pad 12 thru_hole oval (at 0 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 /OUT25))
    (pad 11 thru_hole oval (at 0 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 /OUT26))
    (pad 10 thru_hole oval (at 0 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 /OUT27))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 /OUT28))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 /OUT29))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 /OUT30))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 /OUT31))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 /OUT32))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 /OUT33))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 /OUT34))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 /OUT35))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 /OUT36))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x21_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x21_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 43.18 38.1 90)
    (descr "Through hole straight pin header, 1x21, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x21 2.54mm single row")
    (fp_text reference J5 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value Conn_01x21 (at 0 53.13 90) (layer F.Fab))
    (fp_text user %R (at 0 25.4) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 10 thru_hole oval (at 0 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 11 thru_hole oval (at 0 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 12 thru_hole oval (at 0 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 13 thru_hole oval (at 0 30.48 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 14 thru_hole oval (at 0 33.02 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 15 thru_hole oval (at 0 35.56 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 16 thru_hole oval (at 0 38.1 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 17 thru_hole oval (at 0 40.64 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 18 thru_hole oval (at 0 43.18 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 19 thru_hole oval (at 0 45.72 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 20 thru_hole oval (at 0 48.26 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 21 thru_hole oval (at 0 50.8 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 VCC))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x21_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x15_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 58.42 53.34 90)
    (descr "Through hole straight pin header, 1x15, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x15 2.54mm single row")
    (fp_text reference J6 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value Conn_01x15 (at 0 37.89 90) (layer F.Fab))
    (fp_text user %R (at 0 17.78) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /OUT1))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /OUT2))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /OUT3))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /OUT4))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /OUT5))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /OUT6))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /OUT7))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 /OUT8))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /OUT9))
    (pad 10 thru_hole oval (at 0 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 /OUT10))
    (pad 11 thru_hole oval (at 0 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 /OUT11))
    (pad 12 thru_hole oval (at 0 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 /OUT12))
    (pad 13 thru_hole oval (at 0 30.48 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 /OUT13))
    (pad 14 thru_hole oval (at 0 33.02 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 /OUT14))
    (pad 15 thru_hole oval (at 0 35.56 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 /OUT15))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x15_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_DIN965_Pad (layer F.Cu) (tedit 56D1B4CB)
    (at 99.06 39.37)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (fp_text reference H1 (at 0 -3.8) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 3.8) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.6 5.6) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_DIN965_Pad (layer F.Cu) (tedit 56D1B4CB)
    (at 99.06 54.61)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (fp_text reference H2 (at 0 -3.8) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 3.8) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.6 5.6) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_DIN965_Pad (layer F.Cu) (tedit 56D1B4CB)
    (at 38.1 54.61)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (fp_text reference H3 (at 0 -3.8) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 3.8) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.6 5.6) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_DIN965_Pad (layer F.Cu) (tedit 56D1B4CB)
    (at 38.1 39.37)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (fp_text reference H4 (at 0 -3.8) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 3.8) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.6 5.6) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 64.135 47.371 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C1 (at -2.413 0 180) (layer F.SilkS))
    (fp_text value 10u (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 3 VCC))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 66.167 47.371 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C2 (at -2.413 0 180) (layer F.SilkS))
    (fp_text value 100n (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 VCC))
    (pad 2 smd roundrect (at 0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Jumper:SolderJumper-2_P1.3mm_Bridged_RoundedPad1.0x1.5mm (layer B.Cu) (tedit 5C745284)
    (at 45.72 52.959 270)
    (descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, bridged with 1 copper strip")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP1 (at -2.921 0 90) (layer B.SilkS))
    (fp_text value SolderJumper_2_Bridged (at 0 -1.9 90) (layer B.Fab))
    (pad 2 smd custom (at 0.65 0 270) (size 1 0.5) (layers B.Cu B.Mask)
      (net 4 GND) (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_poly (pts
           (xy 0 0.75) (xy -0.5 0.75) (xy -0.5 -0.75) (xy 0 -0.75)) (width 0))
      ))
    (pad 1 smd custom (at -0.65 0 270) (size 1 0.5) (layers B.Cu B.Mask)
      (net 6 /AD) (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_poly (pts
           (xy 0 0.75) (xy 0.5 0.75) (xy 0.5 -0.75) (xy 0 -0.75)) (width 0))
      ))
  )
  (module Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm (layer B.Cu) (tedit 5B391E66)
    (at 43.18 52.959 270)
    (descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP2 (at -2.921 0 270) (layer B.SilkS))
    (fp_text value SolderJumper_2_Open (at 0 -1.9 270) (layer B.Fab))
    (pad 1 smd custom (at -0.65 0 270) (size 1 0.5) (layers B.Cu B.Mask)
      (net 6 /AD) (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_poly (pts
           (xy 0 0.75) (xy 0.5 0.75) (xy 0.5 -0.75) (xy 0 -0.75)) (width 0))
      ))
    (pad 2 smd custom (at 0.65 0 270) (size 1 0.5) (layers B.Cu B.Mask)
      (net 3 VCC) (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_poly (pts
           (xy 0 0.75) (xy -0.5 0.75) (xy -0.5 -0.75) (xy 0 -0.75)) (width 0))
      ))
  )
  (module Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm (layer B.Cu) (tedit 5B391E66)
    (at 48.26 52.959 270)
    (descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP3 (at -2.921 0 90) (layer B.SilkS))
    (fp_text value SolderJumper_2_Open (at 0 -1.9 90) (layer B.Fab))
    (pad 2 smd custom (at 0.65 0 270) (size 1 0.5) (layers B.Cu B.Mask)
      (net 1 /SCL) (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_poly (pts
           (xy 0 0.75) (xy -0.5 0.75) (xy -0.5 -0.75) (xy 0 -0.75)) (width 0))
      ))
    (pad 1 smd custom (at -0.65 0 270) (size 1 0.5) (layers B.Cu B.Mask)
      (net 6 /AD) (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_poly (pts
           (xy 0 0.75) (xy 0.5 0.75) (xy 0.5 -0.75) (xy 0 -0.75)) (width 0))
      ))
  )
  (module Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm (layer B.Cu) (tedit 5B391E66)
    (at 50.8 52.959 270)
    (descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP4 (at 0 -1.778 90) (layer B.SilkS))
    (fp_text value SolderJumper_2_Open (at 0 -1.9 90) (layer B.Fab))
    (pad 2 smd custom (at 0.65 0 270) (size 1 0.5) (layers B.Cu B.Mask)
      (net 2 /SDA) (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_poly (pts
           (xy 0 0.75) (xy -0.5 0.75) (xy -0.5 -0.75) (xy 0 -0.75)) (width 0))
      ))
    (pad 1 smd custom (at -0.65 0 270) (size 1 0.5) (layers B.Cu B.Mask)
      (net 6 /AD) (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_poly (pts
           (xy 0 0.75) (xy 0.5 0.75) (xy 0.5 -0.75) (xy 0 -0.75)) (width 0))
      ))
  )
  (module Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm (layer F.Cu) (tedit 5B391E66)
    (at 93.98 48.895 90)
    (descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP5 (at 0 -1.8 90) (layer F.SilkS))
    (fp_text value SolderJumper_2_Open (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd custom (at -0.65 0 90) (size 1 0.5) (layers F.Cu F.Mask)
      (net 3 VCC) (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy 0 -0.75) (xy 0.5 -0.75) (xy 0.5 0.75) (xy 0 0.75)) (width 0))
      ))
    (pad 2 smd custom (at 0.65 0 90) (size 1 0.5) (layers F.Cu F.Mask)
      (net 44 +3V3) (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy 0 -0.75) (xy -0.5 -0.75) (xy -0.5 0.75) (xy 0 0.75)) (width 0))
      ))
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder (layer F.Cu) (tedit 5F68FEEE)
    (at 55.372 46.99 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R1 (at 0 2.286) (layer F.SilkS))
    (fp_text value 2.7K (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9125 0 180) (size 0.975 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (pad 1 smd roundrect (at -0.9125 0 180) (size 0.975 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 /R_EXT))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 60.519999 46.99 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R2 (at 5.08 -2.37) (layer F.SilkS))
    (fp_text value R (at 5.08 2.37) (layer F.Fab))
    (fp_text user %R (at 5.08 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 /R_EXT))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder (layer F.Cu) (tedit 5F68FEEE)
    (at 46.863 49.53 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R3 (at -2.54 0 90) (layer F.SilkS))
    (fp_text value 4.7K (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 VCC))
    (pad 2 smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 /SDA))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder (layer F.Cu) (tedit 5F68FEEE)
    (at 45.339 49.53 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R4 (at -2.54 0 90) (layer F.SilkS))
    (fp_text value 4.7K (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 /SCL))
    (pad 1 smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 VCC))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder (layer F.Cu) (tedit 5F68FEEE)
    (at 48.387 49.53 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R5 (at -2.54 0 90) (layer F.SilkS))
    (fp_text value 4.7K (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 VCC))
    (pad 2 smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 /SDB))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "JP5 connects\nStemma 3.3 to VCC" (at 53.213 43.815) (layer B.SilkS))
  (gr_text "IS31FL3236A Breakout\nby rglenn\n01-01-2021" (at 85.471 47.117) (layer F.SilkS))
  (gr_text "I2C address\n0x3C if JP1 bridged (d)\n0x3F if JP2 bridged\n0x3D if JP3 bridged\n0x3E if JP4 bridged\nBRIDGE ONLY ONE" (at 82.55 46.99) (layer B.SilkS))
  (gr_text SDB (at 53.34 52.959 90) (layer F.SilkS))
  (gr_text SDA (at 50.8 52.959 90) (layer F.SilkS))
  (gr_text SCL (at 48.26 52.959 90) (layer F.SilkS))
  (gr_text GND (at 45.72 52.959 90) (layer F.SilkS))
  (gr_text VCC (at 43.18 52.959 90) (layer F.SilkS))
  (gr_text 1 (at 58.42 51.054) (layer F.SilkS))
  (gr_text 2 (at 60.96 51.181) (layer F.SilkS))
  (gr_text 3 (at 63.5 51.181) (layer F.SilkS))
  (gr_text 4 (at 66.04 51.181) (layer F.SilkS))
  (gr_text 5 (at 68.58 51.181) (layer F.SilkS))
  (gr_text 6 (at 71.12 51.181) (layer F.SilkS))
  (gr_text 7 (at 73.66 51.181) (layer F.SilkS))
  (gr_text 8 (at 76.2 51.181) (layer F.SilkS))
  (gr_text 9 (at 78.74 51.181) (layer F.SilkS))
  (gr_text 10 (at 81.28 51.181) (layer F.SilkS))
  (gr_text 11 (at 83.82 51.181) (layer F.SilkS))
  (gr_text 12 (at 86.36 51.181) (layer F.SilkS))
  (gr_text 13 (at 88.9 51.181) (layer F.SilkS))
  (gr_text 14 (at 91.44 51.181) (layer F.SilkS))
  (gr_text 15 (at 93.98 51.181) (layer F.SilkS))
  (gr_text 16 (at 93.98 42.926) (layer F.SilkS))
  (gr_text 17 (at 91.44 42.926) (layer F.SilkS))
  (gr_text 18 (at 88.9 42.926) (layer F.SilkS))
  (gr_text 19 (at 86.36 42.926) (layer F.SilkS))
  (gr_text 20 (at 83.82 42.926) (layer F.SilkS))
  (gr_text 21 (at 81.28 42.926) (layer F.SilkS))
  (gr_text 22 (at 78.74 42.926) (layer F.SilkS))
  (gr_text 23 (at 76.2 42.926) (layer F.SilkS))
  (gr_text 24 (at 73.66 42.926) (layer F.SilkS))
  (gr_text 25 (at 71.12 42.926) (layer F.SilkS))
  (gr_text 26 (at 68.58 42.926) (layer F.SilkS))
  (gr_text 27 (at 66.04 42.926) (layer F.SilkS))
  (gr_text 28 (at 63.5 42.926) (layer F.SilkS))
  (gr_text 29 (at 60.96 42.926) (layer F.SilkS))
  (gr_text 30 (at 58.42 42.926) (layer F.SilkS))
  (gr_text 31 (at 55.88 42.926) (layer F.SilkS))
  (gr_text 32 (at 53.34 42.926) (layer F.SilkS))
  (gr_text 33 (at 50.8 42.926) (layer F.SilkS))
  (gr_text 34 (at 48.26 42.926) (layer F.SilkS))
  (gr_text 35 (at 45.72 42.926) (layer F.SilkS))
  (gr_text 36 (at 43.18 42.926) (layer F.SilkS))
  (dimension 21.59 (width 0.15) (layer Dwgs.User)
    (gr_text "0.8500 in" (at 31.974 46.99 270) (layer Dwgs.User))
    (feature1 (pts (xy 38.1 57.785) (xy 32.687579 57.785)))
    (feature2 (pts (xy 38.1 36.195) (xy 32.687579 36.195)))
    (crossbar (pts (xy 33.274 36.195) (xy 33.274 57.785)))
    (arrow1a (pts (xy 33.274 57.785) (xy 32.687579 56.658496)))
    (arrow1b (pts (xy 33.274 57.785) (xy 33.860421 56.658496)))
    (arrow2a (pts (xy 33.274 36.195) (xy 32.687579 37.321504)))
    (arrow2b (pts (xy 33.274 36.195) (xy 33.860421 37.321504)))
  )
  (dimension 67.31 (width 0.15) (layer Dwgs.User)
    (gr_text "2.6500 in" (at 68.58 63.53) (layer Dwgs.User))
    (feature1 (pts (xy 102.235 54.991) (xy 102.235 62.816421)))
    (feature2 (pts (xy 34.925 54.991) (xy 34.925 62.816421)))
    (crossbar (pts (xy 34.925 62.23) (xy 102.235 62.23)))
    (arrow1a (pts (xy 102.235 62.23) (xy 101.108496 62.816421)))
    (arrow1b (pts (xy 102.235 62.23) (xy 101.108496 61.643579)))
    (arrow2a (pts (xy 34.925 62.23) (xy 36.051504 62.816421)))
    (arrow2b (pts (xy 34.925 62.23) (xy 36.051504 61.643579)))
  )
  (gr_line (start 38.1 36.195) (end 99.06 36.195) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 34.925 39.37) (end 34.925 54.61) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 38.1 39.37) (end 38.1 36.195) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 102.235 39.37) (end 102.235 54.61) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 99.06 39.37) (end 102.235 39.37) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 99.06 57.785) (end 38.1 57.785) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 99.06 54.61) (end 99.06 57.785) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 38.1 54.61) (end 34.925 54.61) (angle -90) (layer Edge.Cuts) (width 0.05))
  (zone (net 4) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.2032))
    (polygon
      (pts
        (xy 102.87 58.42) (xy 34.29 58.42) (xy 34.29 35.56) (xy 102.87 35.56)
      )
    )
  )
)
