(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
		(50 "User.1" user)
		(51 "User.2" user)
		(52 "User.3" user)
		(53 "User.4" user)
		(54 "User.5" user)
		(55 "User.6" user)
		(56 "User.7" user)
		(57 "User.8" user)
		(58 "User.9" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(pcbplotparams
			(layerselection 0x00010fc_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "unconnected-(J1-P2-Pad2)")
	(net 2 "unconnected-(J1-P4-Pad4)")
	(net 3 "unconnected-(J1-P3-Pad3)")
	(net 4 "unconnected-(J1-P1-Pad1)")
	(net 5 "-12V")
	(net 6 "+5V")
	(net 7 "GND")
	(net 8 "+12V")
	(net 9 "Net-(U3-BYP)")
	(net 10 "Net-(U1-BYP)")
	(net 11 "Net-(U2-BYP)")
	(net 12 "5V5")
	(net 13 "-9V5")
	(net 14 "+9V5")
	(net 15 "/adj3")
	(net 16 "/adj2")
	(net 17 "/adj1")
	(footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder"
		(layer "F.Cu")
		(at 115.062 122.174 180)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C6"
			(at 0 -1.85 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "10nF"
			(at 0 1.85 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.5625 0 180)
			(size 1.325 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.188679)
			(net 11 "Net-(U2-BYP)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.5625 0 180)
			(size 1.325 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.188679)
			(net 13 "-9V5")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 109.728 124.968 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R1"
			(at 0 -1.65 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "47k"
			(at 0 1.778 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0 90)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 12 "5V5")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0 90)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 15 "/adj3")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3_DIN965_Pad"
		(layer "F.Cu")
		(at 97.536 159.3)
		(descr "Mounting Hole 3.2mm, M3, DIN965")
		(tags "mounting hole 3.2mm m3 din965")
		(property "Reference" "H2"
			(at 0 -3.8 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_Pad"
			(at 0 3.8 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_3.2mm_M3_DIN965_Pad"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole with connection"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*Pad*")
		(sheetname "Root")
		(sheetfile "power.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 5.6 5.6)
			(drill 3.2)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 7 "GND")
			(pinfunction "1")
			(pintype "input")
		)
	)
	(footprint "PCM_Package_SO_AKL:SO-8_3.9x4.9mm_P1.27mm"
		(layer "F.Cu")
		(at 106.426 131.064 -90)
		(descr "SO, 8 Pin (https://www.nxp.com/docs/en/data-sheet/PCF8523.pdf), Alternate KiCad Library")
		(tags "SO SO")
		(property "Reference" "U3"
			(at 0 -3.5 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LT1763CS8"
			(at 0 3.4 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "PCM_Package_SO_AKL:SO-8_3.9x4.9mm_P1.27mm"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1763fh.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "SO-8 500mA Adjustable low dropout voltage regulator, Alternate KiCad Library"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.575 -1.905 270)
			(size 1.75 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 12 "5V5")
			(pinfunction "OUT")
			(pintype "power_out")
		)
		(pad "2" smd roundrect
			(at -2.575 -0.635 270)
			(size 1.75 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 15 "/adj3")
			(pinfunction "ADJ")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at -2.575 0.635 270)
			(size 1.75 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 7 "GND")
			(pintype "power_in")
		)
		(pad "4" smd roundrect
			(at -2.575 1.905 270)
			(size 1.75 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 9 "Net-(U3-BYP)")
			(pinfunction "BYP")
			(pintype "passive")
		)
		(pad "5" smd roundrect
			(at 2.575 1.905 270)
			(size 1.75 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 8 "+12V")
			(pinfunction "~{SHDN}")
			(pintype "input")
		)
		(pad "6" smd roundrect
			(at 2.575 0.635 270)
			(size 1.75 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 7 "GND")
			(pintype "power_in")
		)
		(pad "7" smd roundrect
			(at 2.575 -0.635 270)
			(size 1.75 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 7 "GND")
			(pintype "power_in")
		)
		(pad "8" smd roundrect
			(at 2.575 -1.905 270)
			(size 1.75 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 8 "+12V")
			(pinfunction "IN")
			(pintype "power_in")
		)
		(model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder"
		(layer "F.Cu")
		(at 103.124 112.268 180)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C8"
			(at 0 -1.85 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "10uF X7R"
			(at 0 1.85 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.5625 0 180)
			(size 1.325 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.188679)
			(net 14 "+9V5")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.5625 0 180)
			(size 1.325 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.188679)
			(net 7 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder"
		(layer "F.Cu")
		(at 102.108 130.556 90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C4"
			(at 0 -1.85 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "10nF"
			(at 0 -2.286 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.5625 0 90)
			(size 1.325 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.188679)
			(net 12 "5V5")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.5625 0 90)
			(size 1.325 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.188679)
			(net 9 "Net-(U3-BYP)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 100.33 119.126 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R8"
			(at 0 -1.65 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "6k98"
			(at 0.508 -2.032 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0 90)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 17 "/adj1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0 90)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 7 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 106.934 124.968 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R2"
			(at 0 -1.65 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "13k3"
			(at 0 -1.778 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0 90)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 15 "/adj3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0 90)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 7 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3_DIN965_Pad"
		(layer "F.Cu")
		(at 117.536 136.8)
		(descr "Mounting Hole 3.2mm, M3, DIN965")
		(tags "mounting hole 3.2mm m3 din965")
		(property "Reference" "H3"
			(at 0 -3.8 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_Pad"
			(at 0 3.8 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_3.2mm_M3_DIN965_Pad"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole with connection"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*Pad*")
		(sheetname "Root")
		(sheetfile "power.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 5.6 5.6)
			(drill 3.2)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 7 "GND")
			(pinfunction "1")
			(pintype "input")
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 102.87 119.126 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R7"
			(at 0 -1.65 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "47k"
			(at 0.254 2.032 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0 90)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 14 "+9V5")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0 90)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 17 "/adj1")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3_DIN965_Pad"
		(layer "F.Cu")
		(at 97.536 114.3)
		(descr "Mounting Hole 3.2mm, M3, DIN965")
		(tags "mounting hole 3.2mm m3 din965")
		(property "Reference" "H1"
			(at -2.286 3.81 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_Pad"
			(at 0 3.8 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_3.2mm_M3_DIN965_Pad"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole with connection"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*Pad*")
		(sheetname "Root")
		(sheetfile "power.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 5.6 5.6)
			(drill 3.2)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 7 "GND")
			(pinfunction "1")
			(pintype "input")
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder"
		(layer "F.Cu")
		(at 117.348 129.286 -90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C7"
			(at 0 -1.85 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "10uF X7R"
			(at -5.842 -0.254 -90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.5625 0 270)
			(size 1.325 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.188679)
			(net 12 "5V5")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.5625 0 270)
			(size 1.325 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.188679)
			(net 7 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder"
		(layer "F.Cu")
		(at 102.87 123.698 -90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C9"
			(at 0 -1.85 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "10nF"
			(at 3.048 0.508 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(pad "1" smd roundrect
			(at -1.5625 0 270)
			(size 1.325 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.188679)
			(net 14 "+9V5")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.5625 0 270)
			(size 1.325 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.188679)
			(net 10 "Net-(U1-BYP)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 118.618 115.316 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R3"
			(at 0 -1.65 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "47k"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0 90)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 13 "-9V5")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0 90)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 16 "/adj2")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 121.412 115.316 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R4"
			(at 0 -1.65 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "6k98"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0 90)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 16 "/adj2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0 90)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 7 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "PCM_Package_SO_AKL:SO-8_3.9x4.9mm_P1.27mm"
		(layer "F.Cu")
		(at 97.79 125.222 -90)
		(descr "SO, 8 Pin (https://www.nxp.com/docs/en/data-sheet/PCF8523.pdf), Alternate KiCad Library")
		(tags "SO SO")
		(property "Reference" "U1"
			(at 0 -3.5 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LT1763CS8"
			(at 0 3.4 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "PCM_Package_SO_AKL:SO-8_3.9x4.9mm_P1.27mm"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1763fh.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "SO-8 500mA Adjustable low dropout voltage regulator, Alternate KiCad Library"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.575 -1.905 270)
			(size 1.75 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 14 "+9V5")
			(pinfunction "OUT")
			(pintype "power_out")
		)
		(pad "2" smd roundrect
			(at -2.575 -0.635 270)
			(size 1.75 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 17 "/adj1")
			(pinfunction "ADJ")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at -2.575 0.635 270)
			(size 1.75 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 7 "GND")
			(pintype "power_in")
		)
		(pad "4" smd roundrect
			(at -2.575 1.905 270)
			(size 1.75 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 10 "Net-(U1-BYP)")
			(pinfunction "BYP")
			(pintype "passive")
		)
		(pad "5" smd roundrect
			(at 2.575 1.905 270)
			(size 1.75 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 8 "+12V")
			(pinfunction "~{SHDN}")
			(pintype "input")
		)
		(pad "6" smd roundrect
			(at 2.575 0.635 270)
			(size 1.75 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 7 "GND")
			(pintype "power_in")
		)
		(pad "7" smd roundrect
			(at 2.575 -0.635 270)
			(size 1.75 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 7 "GND")
			(pintype "power_in")
		)
		(pad "8" smd roundrect
			(at 2.575 -1.905 270)
			(size 1.75 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 8 "+12V")
			(pinfunction "IN")
			(pintype "power_in")
		)
		(model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder"
		(layer "F.Cu")
		(at 120.904 111.252)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C5"
			(at 0 -1.85 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "10uF X7R"
			(at 0 1.85 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.5625 0)
			(size 1.325 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.188679)
			(net 13 "-9V5")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.5625 0)
			(size 1.325 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.188679)
			(net 7 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "PCM_Package_TO_SOT_SMD_AKL:SOT-23-5"
		(layer "F.Cu")
		(at 120.65 119.38 90)
		(descr "5-pin SOT23 package, Alternate KiCad Library")
		(tags "SOT-23-5")
		(property "Reference" "U2"
			(at 0 -2.9 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LT1964ES5-BYP"
			(at 0 2.9 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "PCM_Package_TO_SOT_SMD_AKL:SOT-23-5"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1964fb.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "SOT-23-5 200mA adjustable negative LDO voltage regulator with reference bypass Alternate KiCad Library"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.35 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.1 -0.95 90)
			(size 1.06 0.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 7 "GND")
			(pintype "power_in")
		)
		(pad "2" smd roundrect
			(at -1.1 0 90)
			(size 1.06 0.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 5 "-12V")
			(pinfunction "IN")
			(pintype "power_in")
		)
		(pad "3" smd roundrect
			(at -1.1 0.95 90)
			(size 1.06 0.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 11 "Net-(U2-BYP)")
			(pinfunction "BYP")
			(pintype "input")
		)
		(pad "4" smd roundrect
			(at 1.1 0.95 90)
			(size 1.06 0.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 16 "/adj2")
			(pinfunction "ADJ")
			(pintype "passive")
		)
		(pad "5" smd roundrect
			(at 1.1 -0.95 90)
			(size 1.06 0.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 13 "-9V5")
			(pinfunction "OUT")
			(pintype "power_out")
		)
		(model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:CP_Radial_D6.3mm_P2.50mm"
		(layer "B.Cu")
		(at 115.062 157.819621 -90)
		(descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=6.3mm, Electrolytic Capacitor")
		(tags "CP Radial series Radial pin pitch 2.50mm  diameter 6.3mm Electrolytic Capacitor")
		(property "Reference" "C3"
			(at 1.184379 -4.826 90)
			(layer "B.SilkS")
		)
		(property "Value" "22uF 25V Nichicon"
			(at 1.25 -4.4 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_THT:CP_Radial_D6.3mm_P2.50mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Polarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "Root")
		(sheetfile "power.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.25 0 90)
			(layer "B.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 7 "GND")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.5 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 5 "-12V")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D6.3mm_P2.50mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "PCM_4ms_Connector:Pins_2x08_2.54mm_TH_EuroPower_Shrouded_reducedsilk"
		(layer "B.Cu")
		(at 105.664 149.598 180)
		(property "Reference" "J1"
			(at -5.586 10.578 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "Eurorack_Power_16pin_Shrouded"
			(at -9.4752 -11.8872 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "PCM_4ms_Connector:Pins_2x08_2.54mm_TH_EuroPower_Shrouded_reducedsilk"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Header, Male Pins, 2*8, spacing 2.54mm, straight pin, shrouded and keyed"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Specifications" "Header, Male Pins, 2*8, spacing 2.54mm, straight pin, shrouded and keyed"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Cixi LanLing"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part Number" "LL1007-1 (2*8 HITEMP)"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin_Header_Straight_2X* Pin_Header_Angled_2X* Socket_Strip_Straight_2X* Socket_Strip_Angled_2X* IDC_Header_Straight_*")
		(sheetname "Root")
		(sheetfile "power.kicad_sch")
		(attr through_hole)
		(fp_text user "-12V"
			(at 0 -11.438 0)
			(layer "B.SilkS")
		)
		(pad "1" thru_hole circle
			(at -1.27 8.89 180)
			(size 1.651 1.651)
			(drill 0.9)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 4 "unconnected-(J1-P1-Pad1)")
			(pinfunction "P1")
			(pintype "passive+no_connect")
		)
		(pad "2" thru_hole circle
			(at 1.27 8.89 180)
			(size 1.651 1.651)
			(drill 0.9)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 1 "unconnected-(J1-P2-Pad2)")
			(pinfunction "P2")
			(pintype "passive+no_connect")
		)
		(pad "3" thru_hole circle
			(at -1.27 6.35 180)
			(size 1.651 1.651)
			(drill 0.9)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 3 "unconnected-(J1-P3-Pad3)")
			(pinfunction "P3")
			(pintype "passive+no_connect")
		)
		(pad "4" thru_hole circle
			(at 1.27 6.35 180)
			(size 1.651 1.651)
			(drill 0.9)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 2 "unconnected-(J1-P4-Pad4)")
			(pinfunction "P4")
			(pintype "passive+no_connect")
		)
		(pad "5" thru_hole circle
			(at -1.27 3.81 180)
			(size 1.651 1.651)
			(drill 0.9)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 6 "+5V")
			(pinfunction "+12V")
			(pintype "passive")
		)
		(pad "6" thru_hole circle
			(at 1.27 3.81 180)
			(size 1.651 1.651)
			(drill 0.9)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 6 "+5V")
			(pinfunction "P6")
			(pintype "passive")
		)
		(pad "7" thru_hole circle
			(at -1.27 1.27 180)
			(size 1.651 1.651)
			(drill 0.9)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 8 "+12V")
			(pinfunction "12V")
			(pintype "passive")
		)
		(pad "8" thru_hole circle
			(at 1.27 1.27 180)
			(size 1.651 1.651)
			(drill 0.9)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 8 "+12V")
			(pinfunction "+12V")
			(pintype "passive")
		)
		(pad "9" thru_hole circle
			(at -1.27 -1.27 180)
			(size 1.651 1.651)
			(drill 0.9)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 7 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "10" thru_hole circle
			(at 1.27 -1.27 180)
			(size 1.651 1.651)
			(drill 0.9)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 7 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "11" thru_hole circle
			(at -1.27 -3.81 180)
			(size 1.651 1.651)
			(drill 0.9)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 7 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "12" thru_hole circle
			(at 1.27 -3.81 180)
			(size 1.651 1.651)
			(drill 0.9)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 7 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "13" thru_hole circle
			(at -1.27 -6.35 180)
			(size 1.651 1.651)
			(drill 0.9)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 7 "GND")
			(pinfunction "-12")
			(pintype "passive")
		)
		(pad "14" thru_hole circle
			(at 1.27 -6.35 180)
			(size 1.651 1.651)
			(drill 0.9)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 7 "GND")
			(pinfunction "-12V")
			(pintype "passive")
		)
		(pad "15" thru_hole circle
			(at -1.27 -8.89 180)
			(size 1.651 1.651)
			(drill 0.9)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 5 "-12V")
			(pinfunction "-12V")
			(pintype "passive")
		)
		(pad "16" thru_hole circle
			(at 1.27 -8.89 180)
			(size 1.651 1.651)
			(drill 0.9)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 5 "-12V")
			(pinfunction "P16")
			(pintype "passive")
		)
		(model "${KICAD_4MS_LIBS}/packages3d/TSS-108-01-G-D.stp"
			(hide yes)
			(opacity 0.5500)
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 90)
			)
		)
		(model "${KICAD8_3RD_PARTY}/3dmodels/HTSS-108-02-L-D.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 -90)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical"
		(layer "B.Cu")
		(at 122.174 142.494 180)
		(descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x04 2.54mm single row")
		(property "Reference" "J8"
			(at 0 2.33 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_01x04_Pin"
			(at 0 -9.95 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x04, script generated"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "power.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 -3.81 90)
			(layer "B.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 6 "+5V")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 -2.54 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 8 "+12V")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 -5.08 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 7 "GND")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 -7.62 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 5 "-12V")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical"
		(layer "B.Cu")
		(at 107.706 115.316 -90)
		(descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x04 2.54mm single row")
		(property "Reference" "J5"
			(at 0 2.33 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_01x04_Pin"
			(at 0 -9.95 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x04, script generated"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "power.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 -3.81 0)
			(layer "B.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 14 "+9V5")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 -2.54 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 7 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 -5.08 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 7 "GND")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 -7.62 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 13 "-9V5")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical"
		(layer "B.Cu")
		(at 120.396 125.232 180)
		(descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x04 2.54mm single row")
		(property "Reference" "J2"
			(at 0 2.33 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_01x04_Pin"
			(at -2.921 -9.223 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x04, script generated"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "power.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 -3.81 90)
			(layer "B.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 12 "5V5")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 -2.54 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 12 "5V5")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 -5.08 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 7 "GND")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 -7.62 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 7 "GND")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:CP_Radial_D6.3mm_P2.50mm"
		(layer "B.Cu")
		(at 115.062 142.5 -90)
		(descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=6.3mm, Electrolytic Capacitor")
		(tags "CP Radial series Radial pin pitch 2.50mm  diameter 6.3mm Electrolytic Capacitor")
		(property "Reference" "C1"
			(at 3.296 -4.318 90)
			(layer "B.SilkS")
		)
		(property "Value" "68uF 25V Nichicon"
			(at 1.25 -4.4 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_THT:CP_Radial_D6.3mm_P2.50mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Polarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "Root")
		(sheetfile "power.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.25 0 90)
			(layer "B.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 6 "+5V")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.5 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 7 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D6.3mm_P2.50mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical"
		(layer "B.Cu")
		(at 96.774 151.628)
		(descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x04 2.54mm single row")
		(property "Reference" "J7"
			(at 0 2.33 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_01x04_Pin"
			(at 0 -9.95 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x04, script generated"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "power.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at -0.244 -3.556 90)
			(layer "B.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 7 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 -2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 7 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 -5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 6 "+5V")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 -7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 6 "+5V")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:CP_Radial_D6.3mm_P2.50mm"
		(layer "B.Cu")
		(at 115.062 150.5 -90)
		(descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=6.3mm, Electrolytic Capacitor")
		(tags "CP Radial series Radial pin pitch 2.50mm  diameter 6.3mm Electrolytic Capacitor")
		(property "Reference" "C2"
			(at 1.25 -4.572 90)
			(layer "B.SilkS")
		)
		(property "Value" "22uF 25V Nichicon"
			(at 1.25 -4.4 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_THT:CP_Radial_D6.3mm_P2.50mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Polarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "Root")
		(sheetfile "power.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.25 0 90)
			(layer "B.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 8 "+12V")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.5 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 7 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D6.3mm_P2.50mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical"
		(layer "B.Cu")
		(at 107.706 119.126 -90)
		(descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x04 2.54mm single row")
		(property "Reference" "J4"
			(at 0 2.33 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_01x04_Pin"
			(at 0 -9.95 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x04, script generated"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "power.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 -3.81 0)
			(layer "B.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 14 "+9V5")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 -2.54 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 7 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 -5.08 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 7 "GND")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 -7.62 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 13 "-9V5")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical"
		(layer "B.Cu")
		(at 114.3 125.232 180)
		(descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x04 2.54mm single row")
		(property "Reference" "J3"
			(at 0 2.33 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_01x04_Pin"
			(at 0 -9.95 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x04, script generated"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "power.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 -3.81 90)
			(layer "B.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 12 "5V5")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 -2.54 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 12 "5V5")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 -5.08 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 7 "GND")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 -7.62 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 7 "GND")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical"
		(layer "B.Cu")
		(at 107.706 111.506 -90)
		(descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x04 2.54mm single row")
		(property "Reference" "J6"
			(at 0 2.33 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_01x04_Pin"
			(at 0 -9.95 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x04, script generated"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "power.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 -3.81 0)
			(layer "B.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 14 "+9V5")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 -2.54 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 7 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 -5.08 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 7 "GND")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 -7.62 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 13 "-9V5")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_rect
		(start 93.98 109.474)
		(end 125.98 164.592)
		(fill none)
		(layer "Edge.Cuts")
	)
	(gr_text "+5V"
		(at 98.298 141.224 0)
		(layer "B.SilkS")
	)
	(gr_text "±9V5"
		(at 105.156 116.078 0)
		(layer "B.SilkS")
	)
	(gr_text "+5V5"
		(at 123.952 124.714 90)
		(layer "B.SilkS")
	)
	(zone
		(net 7)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 93.98 109.474) (xy 93.98 164.592) (xy 125.984 164.592) (xy 125.984 109.474)
			)
		)
	)
	(zone
		(net 7)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 1)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 93.98 109.474) (xy 93.98 164.592) (xy 125.984 164.592) (xy 125.984 109.474)
			)
		)
	)
)
