(kicad_pcb (version 4) (host pcbnew 4.0.6-e0-6349~53~ubuntu16.04.1)
  (general
    (links 28)
    (no_connects 0)
    (area 142.862299 107.302299 153.047701 120.027701)
    (thickness 1.6)
    (drawings 14)
    (tracks 128)
    (zones 0)
    (modules 12)
    (nets 11)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.254)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.0254)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.762)
    (uvia_drill 0.508)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF3F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 /LV)
  (net 2 /L1)
  (net 3 /L2)
  (net 4 /H1)
  (net 5 /H2)
  (net 6 /HV)
  (net 7 /L3)
  (net 8 /H3)
  (net 9 /L4)
  (net 10 /H4)
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.254)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
    (add_net /H1)
    (add_net /H2)
    (add_net /H3)
    (add_net /H4)
    (add_net /HV)
    (add_net /L1)
    (add_net /L2)
    (add_net /L3)
    (add_net /L4)
    (add_net /LV)
  )
  (module TO_SOT_Packages_SMD:SOT-363_SC-70-6_Handsoldering (layer F.Cu) (tedit 58DB5FEB)
    (at 147.828 116.332 270)
    (descr "SOT-363, SC-70-6, Handsoldering")
    (tags "SOT-363 SC-70-6 Handsoldering")
    (attr smd)
    (fp_text reference Q1 (at 0 -2 270) (layer F.SilkS) hide)
    (fp_text value BSS138PS (at 0 2 450) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.33 -0.65 270) (size 1.5 0.4) (layers F.Cu F.Paste F.Mask)
      (net 2 /L1))
    (pad 2 smd rect (at -1.33 0 270) (size 1.5 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 /LV))
    (pad 3 smd rect (at -1.33 0.65 270) (size 1.5 0.4) (layers F.Cu F.Paste F.Mask)
      (net 5 /H2))
    (pad 4 smd rect (at 1.33 0.65 270) (size 1.5 0.4) (layers F.Cu F.Paste F.Mask)
      (net 3 /L2))
    (pad 5 smd rect (at 1.33 0 270) (size 1.5 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 /LV))
    (pad 6 smd rect (at 1.33 -0.65 270) (size 1.5 0.4) (layers F.Cu F.Paste F.Mask)
      (net 4 /H1))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-363_SC-70-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-363_SC-70-6_Handsoldering (layer F.Cu) (tedit 58DB5FE8)
    (at 147.828 110.55 270)
    (descr "SOT-363, SC-70-6, Handsoldering")
    (tags "SOT-363 SC-70-6 Handsoldering")
    (attr smd)
    (fp_text reference Q2 (at 0 -2 270) (layer F.SilkS) hide)
    (fp_text value BSS138PS (at 0 2 450) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.33 -0.65 270) (size 1.5 0.4) (layers F.Cu F.Paste F.Mask)
      (net 7 /L3))
    (pad 2 smd rect (at -1.33 0 270) (size 1.5 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 /LV))
    (pad 3 smd rect (at -1.33 0.65 270) (size 1.5 0.4) (layers F.Cu F.Paste F.Mask)
      (net 10 /H4))
    (pad 4 smd rect (at 1.33 0.65 270) (size 1.5 0.4) (layers F.Cu F.Paste F.Mask)
      (net 9 /L4))
    (pad 5 smd rect (at 1.33 0 270) (size 1.5 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 /LV))
    (pad 6 smd rect (at 1.33 -0.65 270) (size 1.5 0.4) (layers F.Cu F.Paste F.Mask)
      (net 8 /H3))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-363_SC-70-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 58DB5FB0)
    (at 147.32 117.348 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at 0 1.45 180) (layer B.SilkS) hide)
    (fp_text value 10k (at 0 -1.55 180) (layer B.Fab))
    (fp_text user %R (at 0 1.45 180) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 1 /LV))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 2 /L1))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 58DB5FB9)
    (at 147.32 114.3 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at 0 1.45 180) (layer B.SilkS) hide)
    (fp_text value 10k (at 0 -1.55 180) (layer B.Fab))
    (fp_text user %R (at 0 1.45 180) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 1 /LV))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 3 /L2))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 58DB5FA4)
    (at 148.59 118.872)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at 0 1.45) (layer B.SilkS) hide)
    (fp_text value 10k (at 0 -1.55) (layer B.Fab))
    (fp_text user %R (at 0 1.45) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 6 /HV))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 4 /H1))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 58DB5FA8)
    (at 148.59 115.824)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at 0 1.45) (layer B.SilkS) hide)
    (fp_text value 10k (at 0 -1.55) (layer B.Fab))
    (fp_text user %R (at 0 1.45) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 6 /HV))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 5 /H2))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 58DB5FD1)
    (at 147.32 108.204 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at 0 1.45 180) (layer B.SilkS) hide)
    (fp_text value 10k (at 0 -1.55 180) (layer B.Fab))
    (fp_text user %R (at 0 1.45 180) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 1 /LV))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 9 /L4))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 58DB5FCA)
    (at 148.59 109.728)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R6 (at 0 1.45) (layer B.SilkS) hide)
    (fp_text value 10k (at 0 -1.55) (layer B.Fab))
    (fp_text user %R (at 0 1.45) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 6 /HV))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 10 /H4))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x05_Pitch2.54mm locked (layer B.Cu) (tedit 58DB5F99)
    (at 144.145 118.745)
    (descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x05 2.54mm single row")
    (fp_text reference J1 (at 0 2.33) (layer B.SilkS) hide)
    (fp_text value LV (at 0 -12.49) (layer B.Fab))
    (fp_text user %R (at 0 2.33) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /LV))
    (pad 2 thru_hole oval (at 0 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /L1))
    (pad 3 thru_hole oval (at 0 -5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /L2))
    (pad 4 thru_hole oval (at 0 -7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /L3))
    (pad 5 thru_hole oval (at 0 -10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /L4))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x05_Pitch2.54mm.wrl
      (at (xyz 0 -0.2 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x05_Pitch2.54mm locked (layer B.Cu) (tedit 58DB5F9E)
    (at 151.765 118.745)
    (descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x05 2.54mm single row")
    (fp_text reference J2 (at 0 2.33) (layer B.SilkS) hide)
    (fp_text value HV (at 0 -12.49) (layer B.Fab))
    (fp_text user %R (at 0 2.33) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /HV))
    (pad 2 thru_hole oval (at 0 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /H1))
    (pad 3 thru_hole oval (at 0 -5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /H2))
    (pad 4 thru_hole oval (at 0 -7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /H3))
    (pad 5 thru_hole oval (at 0 -10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /H4))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x05_Pitch2.54mm.wrl
      (at (xyz 0 -0.2 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 58DB5FCD)
    (at 147.32 111.252 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R7 (at 0 1.45 180) (layer B.SilkS) hide)
    (fp_text value 10k (at 0 -1.55 180) (layer B.Fab))
    (fp_text user %R (at 0 1.45 180) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 1 /LV))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 7 /L3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 58DB5FAD)
    (at 148.59 112.776)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R8 (at 0 1.45) (layer B.SilkS) hide)
    (fp_text value 10k (at 0 -1.55) (layer B.Fab))
    (fp_text user %R (at 0 1.45) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 6 /HV))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 8 /H3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text HV (at 150.368 118.745 90) (layer F.SilkS))
  (gr_text H1 (at 150.368 116.205 90) (layer F.SilkS))
  (gr_text H2 (at 150.368 113.665 90) (layer F.SilkS))
  (gr_text H3 (at 150.368 111.125 90) (layer F.SilkS))
  (gr_text H4 (at 150.368 108.585 90) (layer F.SilkS))
  (gr_text LV (at 145.542 118.745 270) (layer F.SilkS))
  (gr_text L1 (at 145.542 116.205 270) (layer F.SilkS))
  (gr_text L2 (at 145.542 113.665 270) (layer F.SilkS))
  (gr_text L3 (at 145.542 111.125 270) (layer F.SilkS))
  (gr_text L4 (at 145.542 108.585 270) (layer F.SilkS))
  (gr_line (start 142.875 120.015) (end 142.875 107.315) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 153.035 120.015) (end 142.875 120.015) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 153.035 107.315) (end 153.035 120.015) (angle 90) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 142.875 107.315) (end 153.035 107.315) (angle 90) (layer Edge.Cuts) (width 0.0254))
)
