(kicad_pcb (version 20171130) (host pcbnew 5.1.8)
  (general
    (thickness 1.6)
    (drawings 26)
    (tracks 20)
    (zones 0)
    (modules 5)
    (nets 5)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.6)
    (user_trace_width 0.4)
    (user_trace_width 0.6)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 +1V8)
  (net 2 "Net-(J1-Pad2)")
  (net 3 "Net-(J2-Pad1)")
  (net 4 +3V3)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +1V8)
    (add_net +3V3)
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J2-Pad1)")
  )
  (module Connector_PinHeader_2.54mm_edge:PinHeader_1x03_P2.45mm_edge (layer F.Cu) (tedit 5FA464C7)
    (at 101.092 34.29 270)
    (fp_text reference J2 (at 0 -5.08 90) (layer F.SilkS) hide)
    (fp_text value Conn_01x03_Male (at 0 1.27 90) (layer F.Fab))
    (pad 3 smd roundrect (at 2.54 -1.778 270) (size 1.5 3.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +1V8))
    (pad 1 smd rect (at -2.54 -1.778 270) (size 1.5 3.6) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J2-Pad1)"))
    (pad 2 smd roundrect (at 0 -1.778 270) (size 1.5 3.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 +3V3))
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer F.Cu) (tedit 5F68FEEE)
    (at 99.06 34.29 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R2 (at -2.71 -0.06 180) (layer F.SilkS))
    (fp_text value 10k (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1 0 90) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 3 "Net-(J2-Pad1)"))
    (pad 1 smd roundrect (at -1 0 90) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 4 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer F.Cu) (tedit 5F68FEEE)
    (at 92.71 34.29 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R1 (at -2.71 0.04) (layer F.SilkS))
    (fp_text value 10k (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1 0 90) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 2 "Net-(J1-Pad2)"))
    (pad 1 smd roundrect (at -1 0 90) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 1 +1V8))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer F.Cu) (tedit 5A02FF57)
    (at 95.885 34.29 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q1 (at 0 -2.5) (layer F.SilkS))
    (fp_text value BSS138 (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 3 smd rect (at 1 0 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J2-Pad1)"))
    (pad 2 smd rect (at -1 0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J1-Pad2)"))
    (pad 1 smd rect (at -1 -0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 +1V8))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm_edge:PinHeader_1x02_P2.54mm_Edge (layer F.Cu) (tedit 5FA464A1)
    (at 91.44 34.29 90)
    (fp_text reference J1 (at 0 -5.08 90) (layer F.SilkS) hide)
    (fp_text value Conn_01x02_Male (at 0 1.27 90) (layer F.Fab))
    (pad 1 smd rect (at -1.27 -1.778 90) (size 1.5 3.6) (layers F.Cu F.Paste F.Mask)
      (net 1 +1V8))
    (pad 2 smd roundrect (at 1.27 -1.778 90) (size 1.5 3.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 "Net-(J1-Pad2)"))
  )
  (gr_text VTref (at 101.8 36.85) (layer B.SilkS))
  (gr_text 3.3V (at 102 34.35) (layer B.SilkS))
  (gr_text SWDIO (at 101.5 31.8) (layer B.SilkS))
  (gr_text SWDIO (at 91 33.05) (layer B.SilkS))
  (gr_text "VDD\n(1.8V)" (at 90.45 36.35) (layer B.SilkS))
  (gr_text G&W (at 94.5 34.5 270) (layer B.SilkS))
  (gr_text "DBG\n" (at 98 34.5 90) (layer B.SilkS))
  (gr_line (start 87.5 38) (end 87.5 30.5) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 104 39) (end 88.5 39) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 105 30.5) (end 105 38) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 88.5 29.5) (end 104 29.5) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 104 38) (end 104 39) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 104 30.5) (end 105 30.5) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 88.5 38) (end 87.5 38) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 88.5 30.5) (end 88.5 29.5) (angle -90) (layer Edge.Cuts) (width 0.05))
)
