(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 231)
    (no_connects 0)
    (area 89.165715 39.24 194.044285 131.015)
    (thickness 1.6)
    (drawings 66)
    (tracks 587)
    (zones 0)
    (modules 106)
    (nets 77)
  )
  (page A4)
  (title_block
    (title "SatNOGS Rotator Controller")
    (date 2016-12-11)
    (rev v2)
    (company "Libre Space Foundation")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.6)
    (trace_clearance 0.2)
    (zone_clearance 0.6)
    (zone_45_only no)
    (trace_min 0.15)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.8)
    (via_drill 0.5)
    (via_min_size 0.4)
    (via_min_drill 0.35)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 0.8 0.8)
    (pad_drill 0.5)
    (pad_to_mask_clearance 0.05)
    (solder_mask_min_width 0.05)
    (aux_axis_origin 91.44 121.92)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ../no-git/gerber_controller/))
  )
  (net 0 "")
  (net 1 +5V)
  (net 2 GND)
  (net 3 /VIN)
  (net 4 /TX)
  (net 5 /RTS)
  (net 6 /RX)
  (net 7 /A)
  (net 8 /B)
  (net 9 /SW1)
  (net 10 /SW2)
  (net 11 /M1IN2)
  (net 12 /M1IN1)
  (net 13 /M1FB)
  (net 14 /EN)
  (net 15 /M2IN2)
  (net 16 /M2IN1)
  (net 17 /M2FB)
  (net 18 /MS1M1)
  (net 19 /MS1M2)
  (net 20 /SCL1)
  (net 21 /SDA1)
  (net 22 /2AM1)
  (net 23 /1AM1)
  (net 24 /2BM1)
  (net 25 /1BM1)
  (net 26 /2AM2)
  (net 27 /1AM2)
  (net 28 /2BM2)
  (net 29 /1BM2)
  (net 30 /A3)
  (net 31 /A2)
  (net 32 "Net-(U1-Pad3)")
  (net 33 "Net-(U1-Pad18)")
  (net 34 "Net-(U1-Pad17)")
  (net 35 +12V)
  (net 36 "Net-(F1-Pad1)")
  (net 37 /MS3M1)
  (net 38 /MS2M1)
  (net 39 /MS3M2)
  (net 40 /MS2M2)
  (net 41 /PB5)
  (net 42 /M1RST)
  (net 43 /M2RST)
  (net 44 /M1D2)
  (net 45 /M1D1)
  (net 46 "Net-(U6-Pad11)")
  (net 47 "Net-(U6-Pad12)")
  (net 48 /M2D2)
  (net 49 /M2D1)
  (net 50 "Net-(U6-Pad21)")
  (net 51 "Net-(U6-Pad22)")
  (net 52 "Net-(U6-Pad23)")
  (net 53 "Net-(U6-Pad1)")
  (net 54 "Net-(C7-Pad1)")
  (net 55 /FB)
  (net 56 "Net-(U5-Pad3)")
  (net 57 /SW_VIN)
  (net 58 /BOOT)
  (net 59 /SW)
  (net 60 /COMP)
  (net 61 /RT/CLK)
  (net 62 /SDA0)
  (net 63 /SCL0)
  (net 64 /SDA)
  (net 65 /SCL)
  (net 66 /PB4)
  (net 67 "Net-(C5-Pad1)")
  (net 68 /DTR)
  (net 69 "Net-(P2-Pad1)")
  (net 70 "Net-(P2-Pad2)")
  (net 71 "Net-(R8-Pad1)")
  (net 72 "Net-(R9-Pad2)")
  (net 73 /M1SF)
  (net 74 /M2SF)
  (net 75 "Net-(U8-Pad1)")
  (net 76 /RST)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.6)
    (via_dia 0.8)
    (via_drill 0.5)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (net_class neck ""
    (clearance 0.2)
    (trace_width 0.3)
    (via_dia 0.8)
    (via_drill 0.5)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (net_class power1 ""
    (clearance 0.2)
    (trace_width 0.6)
    (via_dia 0.8)
    (via_drill 0.5)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net GND)
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(U5-Pad3)")
    (add_net "Net-(U6-Pad1)")
  )
  (net_class power2 ""
    (clearance 0.6)
    (trace_width 1)
    (via_dia 0.8)
    (via_drill 0.5)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +12V)
    (add_net /1AM1)
    (add_net /1AM2)
    (add_net /1BM1)
    (add_net /1BM2)
    (add_net /2AM1)
    (add_net /2AM2)
    (add_net /2BM1)
    (add_net /2BM2)
    (add_net /SW)
    (add_net /SW_VIN)
    (add_net /VIN)
    (add_net "Net-(F1-Pad1)")
  )
  (net_class signal ""
    (clearance 0.2)
    (trace_width 0.4)
    (via_dia 0.8)
    (via_drill 0.5)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /A)
    (add_net /A2)
    (add_net /A3)
    (add_net /B)
    (add_net /BOOT)
    (add_net /COMP)
    (add_net /DTR)
    (add_net /EN)
    (add_net /FB)
    (add_net /M1D1)
    (add_net /M1D2)
    (add_net /M1FB)
    (add_net /M1IN1)
    (add_net /M1IN2)
    (add_net /M1RST)
    (add_net /M1SF)
    (add_net /M2D1)
    (add_net /M2D2)
    (add_net /M2FB)
    (add_net /M2IN1)
    (add_net /M2IN2)
    (add_net /M2RST)
    (add_net /M2SF)
    (add_net /MS1M1)
    (add_net /MS1M2)
    (add_net /MS2M1)
    (add_net /MS2M2)
    (add_net /MS3M1)
    (add_net /MS3M2)
    (add_net /PB4)
    (add_net /PB5)
    (add_net /RST)
    (add_net /RT/CLK)
    (add_net /RTS)
    (add_net /RX)
    (add_net /SCL)
    (add_net /SCL0)
    (add_net /SCL1)
    (add_net /SDA)
    (add_net /SDA0)
    (add_net /SDA1)
    (add_net /SW1)
    (add_net /SW2)
    (add_net /TX)
    (add_net "Net-(C7-Pad1)")
    (add_net "Net-(P2-Pad1)")
    (add_net "Net-(P2-Pad2)")
    (add_net "Net-(R8-Pad1)")
    (add_net "Net-(R9-Pad2)")
    (add_net "Net-(U1-Pad17)")
    (add_net "Net-(U1-Pad18)")
    (add_net "Net-(U1-Pad3)")
    (add_net "Net-(U6-Pad11)")
    (add_net "Net-(U6-Pad12)")
    (add_net "Net-(U6-Pad21)")
    (add_net "Net-(U6-Pad22)")
    (add_net "Net-(U6-Pad23)")
    (add_net "Net-(U8-Pad1)")
  )
  (module satnogs:Arduino_Pro_Mini (layer F.Cu) (tedit 589C8D04)
    (at 121.666 89.662 180)
    (descr "Arduino Pro-Mini")
    (tags Atmega328)
    (fp_text reference U1 (at 18.415 28.829 360) (layer F.SilkS))
    (fp_text value Arduino_Pro_Mini (at 8.89 13.335 270) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0 90) (size 1.6 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 4 /TX))
    (pad 24 thru_hole oval (at 12.319 8.763 90) (size 1.6 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 65 /SCL))
    (pad 23 thru_hole oval (at 12.319 11.303 90) (size 1.6 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 64 /SDA))
    (pad 17 thru_hole oval (at 12.319 21.717 90) (size 1.6 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 34 "Net-(U1-Pad17)"))
    (pad 18 thru_hole oval (at 12.319 19.177 90) (size 1.6 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 33 "Net-(U1-Pad18)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.6 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 6 /RX))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.6 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 32 "Net-(U1-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.6 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.6 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 5 /RTS))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.6 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 15 /M2IN2))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.6 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 10 /SW2))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.6 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 9 /SW1))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 1.6 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 74 /M2SF))
    (pad 10 thru_hole oval (at 0 22.86 90) (size 1.6 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 73 /M1SF))
    (pad 11 thru_hole oval (at 0 25.4 90) (size 1.6 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 14 /EN))
    (pad 12 thru_hole oval (at 0 27.94 90) (size 1.6 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 11 /M1IN2))
    (pad 13 thru_hole oval (at 15.24 27.94 90) (size 1.6 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 12 /M1IN1))
    (pad 14 thru_hole oval (at 15.24 25.4 90) (size 1.6 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 16 /M2IN1))
    (pad 15 thru_hole oval (at 15.24 22.86 90) (size 1.6 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 66 /PB4))
    (pad 16 thru_hole oval (at 15.24 20.32 90) (size 1.6 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 41 /PB5))
    (pad 19 thru_hole oval (at 15.24 17.78 90) (size 1.6 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 17 /M2FB))
    (pad 20 thru_hole oval (at 15.24 15.24 90) (size 1.6 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 13 /M1FB))
    (pad 21 thru_hole oval (at 15.24 12.7 90) (size 1.6 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 31 /A2))
    (pad 22 thru_hole oval (at 15.24 10.16 90) (size 1.6 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 30 /A3))
    (pad 25 thru_hole oval (at 15.24 7.62 90) (size 1.6 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 1 +5V))
    (pad 26 thru_hole oval (at 15.24 5.08 90) (size 1.6 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 76 /RST))
    (pad 27 thru_hole oval (at 15.24 2.54 90) (size 1.6 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 28 thru_hole oval (at 15.24 0 90) (size 1.6 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 67 "Net-(C5-Pad1)"))
    (model /home/azisi/Documents/SatNOGS/satnogs-rotator-controller/library/satnogs.3dshapes/Arduino_Pro_Mini.x3d
      (at (xyz -0.05 -1.15 0.035))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz -90 0 180))
    )
  )
  (module satnogs:via-0.8mm (layer F.Cu) (tedit 582DEF22)
    (at 143.51 120.65)
    (fp_text reference REF** (at 0 3.175) (layer F.SilkS) hide)
    (fp_text value via-0.8mm (at 0 -3.81) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module satnogs:via-0.8mm (layer F.Cu) (tedit 582DEF22)
    (at 164.211 109.093)
    (fp_text reference REF** (at 0 3.175) (layer F.SilkS) hide)
    (fp_text value via-0.8mm (at 0 -3.81) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module satnogs:via-0.8mm (layer F.Cu) (tedit 582DEF22)
    (at 180.594 95.25)
    (fp_text reference REF** (at 0 3.175) (layer F.SilkS) hide)
    (fp_text value via-0.8mm (at 0 -3.81) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module satnogs:via-0.8mm (layer F.Cu) (tedit 582DEF22)
    (at 186.69 92.71)
    (fp_text reference REF** (at 0 3.175) (layer F.SilkS) hide)
    (fp_text value via-0.8mm (at 0 -3.81) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module satnogs:via-0.8mm (layer F.Cu) (tedit 582DEF22)
    (at 182.88 92.71)
    (fp_text reference REF** (at 0 3.175) (layer F.SilkS) hide)
    (fp_text value via-0.8mm (at 0 -3.81) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module satnogs:via-0.8mm (layer F.Cu) (tedit 589CFF51)
    (at 168.91 67.31)
    (fp_text reference REF** (at 0 3.175) (layer F.SilkS) hide)
    (fp_text value via-0.8mm (at 0 -3.81) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module satnogs:via-0.8mm (layer F.Cu) (tedit 589CFEB7)
    (at 146.05 67.31)
    (fp_text reference REF** (at 0 3.175) (layer F.SilkS) hide)
    (fp_text value via-0.8mm (at 0 -3.81) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module satnogs:via-0.8mm (layer F.Cu) (tedit 589CFF46)
    (at 161.925 59.817)
    (fp_text reference REF** (at 0 3.175) (layer F.SilkS) hide)
    (fp_text value via-0.8mm (at 0 -3.81) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module satnogs:via-0.8mm (layer F.Cu) (tedit 589CFF3D)
    (at 132.08 44.45)
    (fp_text reference REF** (at 0 3.175) (layer F.SilkS) hide)
    (fp_text value via-0.8mm (at 0 -3.81) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module satnogs:via-0.8mm (layer F.Cu) (tedit 589CFE6D)
    (at 93.98 66.04)
    (fp_text reference REF** (at 0 3.175) (layer F.SilkS) hide)
    (fp_text value via-0.8mm (at 0 -3.81) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module satnogs:via-0.8mm (layer F.Cu) (tedit 589CFE76)
    (at 93.98 49.53)
    (fp_text reference REF** (at 0 3.175) (layer F.SilkS) hide)
    (fp_text value via-0.8mm (at 0 -3.81) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module satnogs:via-0.8mm (layer F.Cu) (tedit 589CFE67)
    (at 93.98 80.01)
    (fp_text reference REF** (at 0 3.175) (layer F.SilkS) hide)
    (fp_text value via-0.8mm (at 0 -3.81) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module satnogs:via-0.8mm (layer F.Cu) (tedit 589CFE5F)
    (at 93.98 95.25)
    (fp_text reference REF** (at 0 3.175) (layer F.SilkS) hide)
    (fp_text value via-0.8mm (at 0 -3.81) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module satnogs:via-0.8mm (layer F.Cu) (tedit 589CFE35)
    (at 93.98 109.22)
    (fp_text reference REF** (at 0 3.175) (layer F.SilkS) hide)
    (fp_text value via-0.8mm (at 0 -3.81) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module satnogs:via-0.8mm (layer F.Cu) (tedit 589CFE3F)
    (at 101.6 120.65)
    (fp_text reference REF** (at 0 3.175) (layer F.SilkS) hide)
    (fp_text value via-0.8mm (at 0 -3.81) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module satnogs:via-0.8mm (layer F.Cu) (tedit 589CFE91)
    (at 117.07 56.13)
    (fp_text reference REF** (at 0 3.175) (layer F.SilkS) hide)
    (fp_text value via-0.8mm (at 0 -3.81) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module satnogs:via-0.8mm (layer F.Cu) (tedit 582DEF22)
    (at 160.528 107.569)
    (fp_text reference REF** (at 0 3.175) (layer F.SilkS) hide)
    (fp_text value via-0.8mm (at 0 -3.81) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module satnogs:via-0.8mm (layer F.Cu) (tedit 582DEF22)
    (at 159.893 100.711)
    (fp_text reference REF** (at 0 3.175) (layer F.SilkS) hide)
    (fp_text value via-0.8mm (at 0 -3.81) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module satnogs:via-0.8mm (layer F.Cu) (tedit 582DEF22)
    (at 162.433 107.569)
    (fp_text reference REF** (at 0 3.175) (layer F.SilkS) hide)
    (fp_text value via-0.8mm (at 0 -3.81) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module satnogs:via-0.8mm (layer F.Cu) (tedit 582DEF22)
    (at 164.211 107.569)
    (fp_text reference REF** (at 0 3.175) (layer F.SilkS) hide)
    (fp_text value via-0.8mm (at 0 -3.81) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module satnogs:via-0.8mm (layer F.Cu) (tedit 582DEF22)
    (at 162.306 116.586)
    (fp_text reference REF** (at 0 3.175) (layer F.SilkS) hide)
    (fp_text value via-0.8mm (at 0 -3.81) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module satnogs:via-0.8mm (layer F.Cu) (tedit 582DEF22)
    (at 163.195 100.711)
    (fp_text reference REF** (at 0 3.175) (layer F.SilkS) hide)
    (fp_text value via-0.8mm (at 0 -3.81) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module satnogs:via-0.8mm (layer F.Cu) (tedit 582DEF22)
    (at 166.497 116.586)
    (fp_text reference REF** (at 0 3.175) (layer F.SilkS) hide)
    (fp_text value via-0.8mm (at 0 -3.81) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module satnogs:via-0.8mm (layer F.Cu) (tedit 582DEF22)
    (at 131.826 120.65)
    (fp_text reference REF** (at 0 3.175) (layer F.SilkS) hide)
    (fp_text value via-0.8mm (at 0 -3.81) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module satnogs:via-0.8mm (layer F.Cu) (tedit 582DEF22)
    (at 162.56 120.65)
    (fp_text reference REF** (at 0 3.175) (layer F.SilkS) hide)
    (fp_text value via-0.8mm (at 0 -3.81) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module satnogs:via-0.8mm (layer F.Cu) (tedit 582DEF22)
    (at 151.13 120.65)
    (fp_text reference REF** (at 0 3.175) (layer F.SilkS) hide)
    (fp_text value via-0.8mm (at 0 -3.81) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module satnogs:via-0.8mm (layer F.Cu) (tedit 582DEF22)
    (at 172.72 120.65)
    (fp_text reference REF** (at 0 3.175) (layer F.SilkS) hide)
    (fp_text value via-0.8mm (at 0 -3.81) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module satnogs:via-0.8mm (layer F.Cu) (tedit 582DEF22)
    (at 182.88 120.65)
    (fp_text reference REF** (at 0 3.175) (layer F.SilkS) hide)
    (fp_text value via-0.8mm (at 0 -3.81) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module satnogs:via-0.8mm (layer F.Cu) (tedit 582DEF22)
    (at 189.23 95.25)
    (fp_text reference REF** (at 0 3.175) (layer F.SilkS) hide)
    (fp_text value via-0.8mm (at 0 -3.81) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module satnogs:via-0.8mm (layer F.Cu) (tedit 589CFF3D)
    (at 156.21 44.45)
    (fp_text reference REF** (at 0 3.175) (layer F.SilkS) hide)
    (fp_text value via-0.8mm (at 0 -3.81) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module satnogs:via-0.8mm (layer F.Cu) (tedit 589CFF35)
    (at 180.34 44.45)
    (fp_text reference REF** (at 0 3.175) (layer F.SilkS) hide)
    (fp_text value via-0.8mm (at 0 -3.81) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module satnogs:via-0.8mm (layer F.Cu) (tedit 589CFF2D)
    (at 189.23 52.07)
    (fp_text reference REF** (at 0 3.175) (layer F.SilkS) hide)
    (fp_text value via-0.8mm (at 0 -3.81) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module satnogs:via-0.8mm (layer F.Cu) (tedit 589CFF51)
    (at 168.91 68.58)
    (fp_text reference REF** (at 0 3.175) (layer F.SilkS) hide)
    (fp_text value via-0.8mm (at 0 -3.81) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module satnogs:via-0.8mm (layer F.Cu) (tedit 589CFF1A)
    (at 189.23 66.04)
    (fp_text reference REF** (at 0 3.175) (layer F.SilkS) hide)
    (fp_text value via-0.8mm (at 0 -3.81) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module satnogs:via-0.8mm (layer F.Cu) (tedit 589CFF46)
    (at 159.004 57.15)
    (fp_text reference REF** (at 0 3.175) (layer F.SilkS) hide)
    (fp_text value via-0.8mm (at 0 -3.81) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module satnogs:via-0.8mm (layer F.Cu) (tedit 589CFEB7)
    (at 146.05 68.58)
    (fp_text reference REF** (at 0 3.175) (layer F.SilkS) hide)
    (fp_text value via-0.8mm (at 0 -3.81) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module satnogs:via-0.8mm (layer F.Cu) (tedit 589CFF0F)
    (at 189.23 80.01)
    (fp_text reference REF** (at 0 3.175) (layer F.SilkS) hide)
    (fp_text value via-0.8mm (at 0 -3.81) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module EuroBoard_Outline:EuroBoard_halb_Type-I_100mmX80mm_holes locked (layer F.Cu) (tedit 589CD045)
    (at 91.44 121.92)
    (descr "Outline, Eurocard 1/2, Type I, 100x80mm, with holes 3,5mm")
    (tags "Outline, Eurocard 1/2, Type I, 100x80mm, with holes 3,5mm")
    (fp_text reference "© Libre Space Foundation" (at 58.166 -33.909) (layer F.SilkS))
    (fp_text value EuroBoard_halb_Type-I_100mmX80mm_holes (at 53.34 7.62) (layer F.Fab) hide)
    (fp_line (start 0 0) (end 0 -79.99984) (layer Edge.Cuts) (width 0.381))
    (fp_line (start 0 -79.99984) (end 99.9998 -79.99984) (layer Edge.Cuts) (width 0.381))
    (fp_line (start 99.9998 -79.99984) (end 99.9998 0) (layer Edge.Cuts) (width 0.381))
    (fp_line (start 99.9998 0) (end 0 0) (layer Edge.Cuts) (width 0.381))
    (pad "" np_thru_hole circle (at 5.00126 -5.00126) (size 3.50012 3.50012) (drill 3.50012) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 5.00126 -75.00112) (size 3.50012 3.50012) (drill 3.50012) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 95.00108 -75.00112) (size 3.50012 3.50012) (drill 3.50012) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 95.00108 -5.00126) (size 3.50012 3.50012) (drill 3.50012) (layers *.Cu *.Mask F.SilkS))
  )
  (module satnogs:via-0.8mm (layer F.Cu) (tedit 589CFE9B)
    (at 127.635 52.07)
    (fp_text reference REF** (at 0 3.175) (layer F.SilkS) hide)
    (fp_text value via-0.8mm (at 0 -3.81) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module satnogs:satnogs_logo (layer B.Cu) (tedit 0)
    (at 156.845 101.854 180)
    (fp_text reference G*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (module satnogs:Pololu_Dual_MC33926 (layer F.Cu) (tedit 589DCD15)
    (at 178.308 82.296 180)
    (descr "Pin socket for pololu dual MC33926")
    (tags "Pin Socket")
    (fp_text reference U6 (at 0 -2.667 180) (layer F.SilkS))
    (fp_text value Pololu_Dual_MC33926 (at 7.239 -4.064 180) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0 180) (size 1.6 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 53 "Net-(U6-Pad1)"))
    (pad "" np_thru_hole circle (at 1.27 24.13 180) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 41.91 24.13 180) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask F.SilkS))
    (pad 26 thru_hole circle (at 22.8092 22.4028 270) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 35 +12V))
    (pad 27 thru_hole rect (at 19.30908 22.4028 180) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.6 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 3 thru_hole oval (at 5.08 0 180) (size 1.6 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 1 +5V))
    (pad 4 thru_hole oval (at 7.62 0 180) (size 1.6 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 11 /M1IN2))
    (pad 5 thru_hole oval (at 10.16 0 180) (size 1.6 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 12 /M1IN1))
    (pad 6 thru_hole oval (at 12.7 0 180) (size 1.6 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 44 /M1D2))
    (pad 7 thru_hole oval (at 15.24 0 180) (size 1.6 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 45 /M1D1))
    (pad 8 thru_hole oval (at 17.78 0 180) (size 1.6 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 73 /M1SF))
    (pad 9 thru_hole oval (at 20.32 0 180) (size 1.6 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 13 /M1FB))
    (pad 10 thru_hole oval (at 22.86 0 180) (size 1.6 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 14 /EN))
    (pad 11 thru_hole oval (at 25.4 0 180) (size 1.6 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 46 "Net-(U6-Pad11)"))
    (pad 12 thru_hole oval (at 27.94 0 180) (size 1.6 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 47 "Net-(U6-Pad12)"))
    (pad 13 thru_hole oval (at 30.48 0 180) (size 1.6 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 15 /M2IN2))
    (pad 14 thru_hole oval (at 33.02 0 180) (size 1.6 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 16 /M2IN1))
    (pad 15 thru_hole oval (at 35.56 0 180) (size 1.6 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 48 /M2D2))
    (pad 16 thru_hole oval (at 38.1 0 180) (size 1.6 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 49 /M2D1))
    (pad 17 thru_hole oval (at 40.64 0 180) (size 1.6 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 74 /M2SF))
    (pad 18 thru_hole oval (at 43.18 0 180) (size 1.6 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 17 /M2FB))
    (pad 19 thru_hole oval (at 38.1 2.54 180) (size 1.6 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 49 /M2D1))
    (pad 20 thru_hole oval (at 35.56 2.54 180) (size 1.6 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 48 /M2D2))
    (pad 21 thru_hole oval (at 27.94 2.54 180) (size 1.6 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 50 "Net-(U6-Pad21)"))
    (pad 22 thru_hole oval (at 25.4 2.54 180) (size 1.6 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 51 "Net-(U6-Pad22)"))
    (pad 23 thru_hole oval (at 22.86 2.54 180) (size 1.6 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 52 "Net-(U6-Pad23)"))
    (pad 24 thru_hole oval (at 15.24 2.54 180) (size 1.6 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 45 /M1D1))
    (pad 25 thru_hole oval (at 12.7 2.54 180) (size 1.6 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 44 /M1D2))
    (model /home/azisi/Documents/SatNOGS/satnogs-rotator-controller/library/satnogs.3dshapes/Pololu-Dual-MC33926.x3d
      (at (xyz 0.9379999999999999 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module satnogs:Pololu_A4988 (layer F.Cu) (tedit 589DCCEA)
    (at 154.178 63.246 270)
    (descr "Pin Socket for Pololu A4988 , Stepper Motor Driver")
    (tags "Pin Socket")
    (fp_text reference U4 (at 15.24 17.78 360) (layer F.SilkS))
    (fp_text value Pololu_A4988 (at 10.668 3.937 360) (layer F.Fab))
    (pad 1 thru_hole oval (at -0.018651 0.016285 180) (size 1.6 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole oval (at -0.018651 2.556285 180) (size 1.6 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 1 +5V))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.6 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 29 /1BM2))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.6 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 27 /1AM2))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.6 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 26 /2AM2))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 1.6 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 28 /2BM2))
    (pad 7 thru_hole oval (at 0 15.24 180) (size 1.6 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 8 thru_hole oval (at 0 17.78 180) (size 1.6 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 35 +12V))
    (pad 9 thru_hole oval (at 12.7 17.78 180) (size 1.6 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 14 /EN))
    (pad 10 thru_hole oval (at 12.7 15.24 180) (size 1.6 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 19 /MS1M2))
    (pad 11 thru_hole oval (at 12.7 12.7 180) (size 1.6 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 40 /MS2M2))
    (pad 12 thru_hole oval (at 12.7 10.16 180) (size 1.6 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 39 /MS3M2))
    (pad 13 thru_hole oval (at 12.7 7.62 180) (size 1.6 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 43 /M2RST))
    (pad 14 thru_hole oval (at 12.7 5.08 180) (size 1.6 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 43 /M2RST))
    (pad 15 thru_hole oval (at 12.7 2.54 180) (size 1.6 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 16 /M2IN1))
    (pad 16 thru_hole oval (at 12.7 0 180) (size 1.6 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 15 /M2IN2))
    (model ../../../../../home/azisi/Documents/SatNOGS/satnogs-rotator-controller/library/satnogs.3dshapes/Pololu_A4988_Headers.wrl
      (at (xyz 0.25 -0.35 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 90))
    )
  )
  (module satnogs:Pololu_A4988 (layer F.Cu) (tedit 589DCD03)
    (at 177.038 63.246 270)
    (descr "Pin Socket for Pololu A4988 , Stepper Motor Driver")
    (tags "Pin Socket")
    (fp_text reference U3 (at 15.24 17.78 360) (layer F.SilkS))
    (fp_text value Pololu_A4988 (at 10.541 4.064 360) (layer F.Fab))
    (pad 1 thru_hole oval (at -0.018651 0.016285 180) (size 1.6 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole oval (at -0.018651 2.556285 180) (size 1.6 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 1 +5V))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.6 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 25 /1BM1))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.6 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 23 /1AM1))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.6 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 22 /2AM1))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 1.6 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 24 /2BM1))
    (pad 7 thru_hole oval (at 0 15.24 180) (size 1.6 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 8 thru_hole oval (at 0 17.78 180) (size 1.6 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 35 +12V))
    (pad 9 thru_hole oval (at 12.7 17.78 180) (size 1.6 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 14 /EN))
    (pad 10 thru_hole oval (at 12.7 15.24 180) (size 1.6 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 18 /MS1M1))
    (pad 11 thru_hole oval (at 12.7 12.7 180) (size 1.6 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 38 /MS2M1))
    (pad 12 thru_hole oval (at 12.7 10.16 180) (size 1.6 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 37 /MS3M1))
    (pad 13 thru_hole oval (at 12.7 7.62 180) (size 1.6 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 42 /M1RST))
    (pad 14 thru_hole oval (at 12.7 5.08 180) (size 1.6 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 42 /M1RST))
    (pad 15 thru_hole oval (at 12.7 2.54 180) (size 1.6 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 12 /M1IN1))
    (pad 16 thru_hole oval (at 12.7 0 180) (size 1.6 1.8) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 11 /M1IN2))
    (model ../../../../../home/azisi/Documents/SatNOGS/satnogs-rotator-controller/library/satnogs.3dshapes/Pololu_A4988_Headers.wrl
      (at (xyz 0.25 -0.35 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x04 (layer F.Cu) (tedit 58741E54)
    (at 113.03 48.514 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P4 (at 4.445 -0.635 180) (layer F.SilkS) hide)
    (fp_text value I2C (at 0 -3.1 90) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 /SCL1))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 +5V))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 /SDA1))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 63 /SCL0))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 +5V))
    (pad 7 thru_hole oval (at 0 7.62 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 62 /SDA0))
    (pad 8 thru_hole oval (at 2.54 7.62 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x04_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 57ED4372)
    (at 120.65 52.324 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at -3.175 0 270) (layer B.SilkS))
    (fp_text value 4.7k (at 0 -2.1 90) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 62 /SDA0))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 57ED42B7)
    (at 111.379 100.33 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference JP7 (at -4.318 0 270) (layer B.SilkS))
    (fp_text value Jumper_NO_Small (at 0 -2.1 90) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 7 /A))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 4 /TX))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 57ED43C2)
    (at 108.712 100.33 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 3.429 0 450) (layer F.SilkS))
    (fp_text value 0.1u (at 0 2.1 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x03 (layer F.Cu) (tedit 5834D6DD)
    (at 124.46 48.514 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P2 (at 4.445 -0.635 180) (layer F.SilkS) hide)
    (fp_text value End-Stops (at 0 -3.1 90) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 69 "Net-(P2-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 70 "Net-(P2-Pad2)"))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 +5V))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 +5V))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 57ED43CF)
    (at 113.284 112.776 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 0 1.905 360) (layer F.SilkS))
    (fp_text value 120 (at 0 2.1 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 8 /B))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 7 /A))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 57ED436C)
    (at 118.11 52.324 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at -3.175 0 90) (layer B.SilkS))
    (fp_text value 4.7k (at 0 -2.1 90) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 63 /SCL0))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 57ED42FA)
    (at 159.258 72.136 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R4 (at 3.556 0 90) (layer B.SilkS))
    (fp_text value 100k (at 0 -2.1 90) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 18 /MS1M1))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 57ED4376)
    (at 113.03 52.324 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R6 (at -3.255 -0.127 270) (layer B.SilkS))
    (fp_text value 4.7k (at 0 -2.1 90) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 20 /SCL1))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 57ED42FC)
    (at 136.398 72.136 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R7 (at 3.73 0 90) (layer B.SilkS))
    (fp_text value 100k (at 0 -2.1 90) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 19 /MS1M2))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 57ED428C)
    (at 114.554 107.569 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R8 (at 0 -1.905 270) (layer F.SilkS))
    (fp_text value 10 (at 0 2.1 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 71 "Net-(R8-Pad1)"))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 8 /B))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 57ED43BA)
    (at 112.014 107.569 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R9 (at 0 -1.778 90) (layer F.SilkS))
    (fp_text value 10 (at 0 2.1 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 7 /A))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 72 "Net-(R9-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 57ED437A)
    (at 115.57 52.324 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R5 (at -3.255 -0.127 270) (layer B.SilkS))
    (fp_text value 4.7k (at 0 -2.1 90) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 21 /SDA1))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 57ED42C4)
    (at 115.189 100.33 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference JP8 (at -4.318 0 270) (layer B.SilkS))
    (fp_text value Jumper_NO_Small (at 0 -2.1 90) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 8 /B))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 6 /RX))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 57ED43DB)
    (at 138.938 103.839 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference FB1 (at -3.89 0 270) (layer F.SilkS))
    (fp_text value FILTER (at 0 2.1 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 /VIN))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(F1-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 57ED42EF)
    (at 166.878 72.136 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference JP1 (at 4.064 0 90) (layer B.SilkS))
    (fp_text value Jumper_NO_Small (at 0 -2.1 90) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 37 /MS3M1))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 57ED42F1)
    (at 164.338 72.136 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference JP2 (at 4.064 0 90) (layer B.SilkS))
    (fp_text value Jumper_NO_Small (at 0 -2.1 90) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 38 /MS2M1))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 57ED42E5)
    (at 144.018 72.136 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference JP4 (at 4.238 0 90) (layer B.SilkS))
    (fp_text value Jumper_NO_Small (at 0 -2.1 90) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 39 /MS3M2))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 57ED42E8)
    (at 141.478 72.136 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference JP5 (at 4.238 0 90) (layer B.SilkS))
    (fp_text value Jumper_NO_Small (at 0 -2.1 90) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 40 /MS2M2))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 57ED42EC)
    (at 138.938 72.136 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference JP6 (at 4.238 0 90) (layer B.SilkS))
    (fp_text value Jumper_NO_Small (at 0 -2.1 90) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 19 /MS1M2))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 57ED42F6)
    (at 161.798 72.136 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference JP3 (at 4.064 0 90) (layer B.SilkS))
    (fp_text value Jumper_NO_Small (at 0 -2.1 90) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 18 /MS1M1))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 541A9B8D)
    (at 157.861 108.839 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C6 (at 3.683 0 270) (layer F.SilkS))
    (fp_text value 100n (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 58 /BOOT))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 59 /SW))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 541A9B8D)
    (at 173.482 113.264 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C7 (at 3.429 0 270) (layer F.SilkS))
    (fp_text value 7.5n (at 4.044 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(C7-Pad1)"))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 541A9B8D)
    (at 171.196 113.264 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C8 (at 3.449 0 270) (layer F.SilkS))
    (fp_text value 10p (at 3.663 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 60 /COMP))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 54189DEE)
    (at 156.464 116.078 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R10 (at 0 -1.905 360) (layer F.SilkS))
    (fp_text value 221k (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 61 /RT/CLK))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 54189DEE)
    (at 172.546 117.348)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R11 (at 0 1.905) (layer F.SilkS))
    (fp_text value 26.7k (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 60 /COMP))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(C7-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 54189DEE)
    (at 178.562 113.364 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R12 (at -3.937 0 450) (layer F.SilkS))
    (fp_text value 147k (at -4.525 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 35 +12V))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 55 /FB))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 54189DEE)
    (at 176.276 113.364 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R13 (at 3.937 0 270) (layer F.SilkS))
    (fp_text value 10.5k (at 4.779 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 55 /FB))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58191A24)
    (at 128.27 55.499 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C10 (at 3.81 0 270) (layer F.SilkS))
    (fp_text value 0.1u (at 0 2.1 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 9 /SW1))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58191A5D)
    (at 125.984 55.519 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C11 (at -3.79 0 90) (layer F.SilkS))
    (fp_text value 0.1u (at 0 2.1 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 10 /SW2))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58191A58)
    (at 130.556 55.499 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R14 (at -3.937 0 90) (layer F.SilkS))
    (fp_text value 200 (at 0 2.1 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 9 /SW1))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 69 "Net-(P2-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58191A61)
    (at 123.698 55.499 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R15 (at 3.937 -0.254 270) (layer F.SilkS))
    (fp_text value 200 (at 0 2.1 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 70 "Net-(P2-Pad2)"))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 10 /SW2))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 54189DEE)
    (at 129.54 90.424 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference FB2 (at 0 2.0955 360) (layer F.SilkS))
    (fp_text value FILTER (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 35 +12V))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 67 "Net-(C5-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 541A9B8D)
    (at 114.554 56.134 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C12 (at 3.048 0 540) (layer F.SilkS))
    (fp_text value 0.1u (at -4.064 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 54189DEE)
    (at 113.458 78.486 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R16 (at -3.89 0 180) (layer B.SilkS))
    (fp_text value 4.7k (at 0 -2.1 180) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 64 /SDA))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 54189DEE)
    (at 113.458 80.772 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R17 (at -3.89 0 180) (layer B.SilkS))
    (fp_text value 4.7k (at 0 -2.1 180) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 65 /SCL))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:c_elec_6.3x5.3 (layer F.Cu) (tedit 57FA457B)
    (at 140.208 68.834)
    (descr "SMT capacitor, aluminium electrolytic, 6.3x5.3")
    (attr smd)
    (fp_text reference C3 (at 4.445 -2.54) (layer F.SilkS))
    (fp_text value 100u (at 0 4.445) (layer F.Fab))
    (fp_text user + (at -1.7526 -0.0762) (layer F.Fab))
    (fp_text user + (at -4.318 -2.54) (layer F.SilkS))
    (pad 1 smd rect (at -2.7 0 180) (size 3.5 1.6) (layers F.Cu F.Paste F.Mask)
      (net 35 +12V))
    (pad 2 smd rect (at 2.7 0 180) (size 3.5 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/CP_Elec_6.3x5.3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:c_elec_6.3x5.3 (layer F.Cu) (tedit 57FA457B)
    (at 163.068 68.834)
    (descr "SMT capacitor, aluminium electrolytic, 6.3x5.3")
    (attr smd)
    (fp_text reference C4 (at 4.445 -2.54) (layer F.SilkS))
    (fp_text value 100u (at 0 4.445) (layer F.Fab))
    (fp_text user + (at -1.7526 -0.0762) (layer F.Fab))
    (fp_text user + (at -4.2799 -2.54) (layer F.SilkS))
    (pad 1 smd rect (at -2.7 0 180) (size 3.5 1.6) (layers F.Cu F.Paste F.Mask)
      (net 35 +12V))
    (pad 2 smd rect (at 2.7 0 180) (size 3.5 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/CP_Elec_6.3x5.3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:c_elec_6.3x5.3 (layer F.Cu) (tedit 57FA457B)
    (at 100.711 96.393 270)
    (descr "SMT capacitor, aluminium electrolytic, 6.3x5.3")
    (attr smd)
    (fp_text reference C5 (at 4.285 2.54 540) (layer F.SilkS))
    (fp_text value 100u (at 0 -4.5593 270) (layer F.Fab))
    (fp_text user + (at -1.7526 -0.0762 270) (layer F.Fab))
    (fp_text user + (at -4.2799 3.0099 270) (layer F.SilkS))
    (pad 1 smd rect (at -2.7 0 90) (size 3.5 1.6) (layers F.Cu F.Paste F.Mask)
      (net 67 "Net-(C5-Pad1)"))
    (pad 2 smd rect (at 2.7 0 90) (size 3.5 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/CP_Elec_6.3x5.3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x04 (layer F.Cu) (tedit 5834D6E1)
    (at 101.6 48.514 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P1 (at 4.445 -0.635 180) (layer F.SilkS) hide)
    (fp_text value DEV-PINS (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 30 /A3))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 31 /A2))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 41 /PB5))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 7 thru_hole oval (at 0 7.62 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 8 thru_hole oval (at 2.54 7.62 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 66 /PB4))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x04_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Symbols:OSHW-Logo2_9.8x8mm_SilkScreen (layer F.Cu) (tedit 0)
    (at 103.886 111.125)
    (descr "Open Source Hardware Symbol")
    (tags "Logo Symbol OSHW")
    (attr virtual)
    (fp_text reference REF*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value OSHW-Logo2_9.8x8mm_SilkScreen (at 0.75 0) (layer F.Fab) hide)
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 541A9B8D)
    (at 106.4895 100.33 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C13 (at 3.937 0 450) (layer F.SilkS))
    (fp_text value 0.1u (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 76 /RST))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 68 /DTR))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23_Handsoldering (layer F.Cu) (tedit 583F3954)
    (at 113.284 116.9035 270)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (attr smd)
    (fp_text reference D3 (at 2.0955 2.9845 360) (layer F.SilkS))
    (fp_text value D_TVS_x2_AAC (at 0 2.5 270) (layer F.Fab))
    (pad 1 smd rect (at -1.5 -0.95 270) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 8 /B))
    (pad 2 smd rect (at -1.5 0.95 270) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 7 /A))
    (pad 3 smd rect (at 1.5 0 270) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58307B90)
    (at 118.364 100.33 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R18 (at 0 -2.032 450) (layer F.SilkS))
    (fp_text value 10k (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 5 /RTS))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module satnogs:SOT-23-5_HandSoldering (layer F.Cu) (tedit 589C8D4B)
    (at 108.077 56.134 90)
    (descr "5-pin SOT23 package Hand Soldering")
    (tags "SOT-23-5 HandSoldering")
    (attr smd)
    (fp_text reference U8 (at 0 -2.9 270) (layer F.SilkS))
    (fp_text value TC74 (at 0 -2.54 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 -0.95 90) (size 1.5 0.65) (layers F.Cu F.Paste F.Mask)
      (net 75 "Net-(U8-Pad1)"))
    (pad 2 smd rect (at -1.35 0 90) (size 1.5 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -1.35 0.95 90) (size 1.5 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 4 smd rect (at 1.35 0.95 90) (size 1.5 0.65) (layers F.Cu F.Paste F.Mask)
      (net 20 /SCL1))
    (pad 5 smd rect (at 1.35 -0.95 90) (size 1.5 0.65) (layers F.Cu F.Paste F.Mask)
      (net 21 /SDA1))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module satnogs:SOIC-8_3.9x4.9mm_Pitch1.27mm_HandSoldering (layer F.Cu) (tedit 589C9480)
    (at 113.284 100.33 270)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U2 (at -3.556 -3.937 360) (layer F.SilkS))
    (fp_text value SN65HVD485EDR (at 0 3.5 270) (layer F.Fab))
    (pad 1 smd rect (at -2.95 -1.905 270) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 6 /RX))
    (pad 2 smd rect (at -2.95 -0.635 270) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 /RTS))
    (pad 3 smd rect (at -2.95 0.635 270) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 /RTS))
    (pad 4 smd rect (at -2.95 1.905 270) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 /TX))
    (pad 5 smd rect (at 2.95 1.905 270) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 smd rect (at 2.95 0.635 270) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 72 "Net-(R9-Pad2)"))
    (pad 7 smd rect (at 2.95 -0.635 270) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 71 "Net-(R8-Pad1)"))
    (pad 8 smd rect (at 2.95 -1.905 270) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (model Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1210_HandSoldering (layer F.Cu) (tedit 541A9C39)
    (at 152.527 112.649 270)
    (descr "Capacitor SMD 1210, hand soldering")
    (tags "capacitor 1210")
    (attr smd)
    (fp_text reference C2 (at 4.318 0 450) (layer F.SilkS))
    (fp_text value 2.2u (at 5.461 0 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 57 /SW_VIN))
    (pad 2 smd rect (at 2 0 270) (size 2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1210.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1210_HandSoldering (layer F.Cu) (tedit 541A9C39)
    (at 161.544 96.298 270)
    (descr "Capacitor SMD 1210, hand soldering")
    (tags "capacitor 1210")
    (attr smd)
    (fp_text reference C9 (at -0.032 -2.413 450) (layer F.SilkS))
    (fp_text value 47u (at 0 2.7 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 35 +12V))
    (pad 2 smd rect (at 2 0 270) (size 2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1210.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module satnogs:Inductor_Bourns-SRR1210_HandSoldering (layer F.Cu) (tedit 589C8C11)
    (at 173.482 99.834 90)
    (descr "Inductor, Bourns-SRR1210, HandSoldering")
    (tags "inductor HandSoldering")
    (attr smd)
    (fp_text reference L1 (at 0.012 -7.62 90) (layer F.SilkS))
    (fp_text value 27u (at 0 7.62 90) (layer F.Fab))
    (pad 1 smd rect (at -5.6 0 90) (size 3.9 5.3) (layers F.Cu F.Paste F.Mask)
      (net 59 /SW))
    (pad 2 smd rect (at 5.6 0 90) (size 3.9 5.3) (layers F.Cu F.Paste F.Mask)
      (net 35 +12V))
    (model /home/azisi/Documents/SatNOGS/satnogs-rotator-controller/library/satnogs.3dshapes/Inductor_Bourns-SRR1210.wrl
      (at (xyz 0 0 0.21))
      (scale (xyz 2.54 2.54 2.54))
      (rotate (xyz 90 180 90))
    )
  )
  (module satnogs:HSOP-8 (layer F.Cu) (tedit 589C943C)
    (at 164.338 112.776 270)
    (descr HSOP-8)
    (tags ThermalPad)
    (attr smd)
    (fp_text reference U5 (at 3.81 0 360) (layer F.SilkS))
    (fp_text value TPS54360DDA (at 3.81 0 360) (layer F.Fab))
    (pad 1 smd rect (at -1.905 2.875 270) (size 0.45 2.15) (layers F.Cu F.Paste F.Mask)
      (net 58 /BOOT))
    (pad 2 smd rect (at -0.635 2.875 270) (size 0.45 2.15) (layers F.Cu F.Paste F.Mask)
      (net 57 /SW_VIN))
    (pad 3 smd rect (at 0.635 2.875 270) (size 0.45 2.15) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(U5-Pad3)"))
    (pad 4 smd rect (at 1.905 2.875 270) (size 0.45 2.15) (layers F.Cu F.Paste F.Mask)
      (net 61 /RT/CLK))
    (pad 5 smd rect (at 1.905 -2.875 270) (size 0.45 2.15) (layers F.Cu F.Paste F.Mask)
      (net 55 /FB))
    (pad 6 smd rect (at 0.635 -2.875 270) (size 0.45 2.15) (layers F.Cu F.Paste F.Mask)
      (net 60 /COMP))
    (pad 7 smd rect (at -0.635 -2.875 270) (size 0.45 2.15) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 8 smd rect (at -1.905 -2.875 270) (size 0.45 2.15) (layers F.Cu F.Paste F.Mask)
      (net 59 /SW))
    (pad 9 smd rect (at 0 0 270) (size 3.1 2.4) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 9 thru_hole circle (at 1.3 -0.65 270) (size 0.4 0.4) (drill 0.33) (layers *.Cu F.SilkS)
      (net 2 GND))
    (pad 9 thru_hole circle (at 0 -0.65 270) (size 0.4 0.4) (drill 0.33) (layers *.Cu F.SilkS)
      (net 2 GND))
    (pad 9 thru_hole circle (at 1.3 0.65 270) (size 0.4 0.4) (drill 0.33) (layers *.Cu F.SilkS)
      (net 2 GND))
    (pad 9 thru_hole circle (at 0 0.65 270) (size 0.4 0.4) (drill 0.33) (layers *.Cu F.SilkS)
      (net 2 GND))
    (pad 9 thru_hole circle (at -1.3 -0.65 270) (size 0.4 0.4) (drill 0.33) (layers *.Cu F.SilkS)
      (net 2 GND))
    (pad 9 thru_hole circle (at -1.3 0.65 270) (size 0.4 0.4) (drill 0.33) (layers *.Cu F.SilkS)
      (net 2 GND))
    (model ../../../../../home/azisi/Documents/SatNOGS/satnogs-rotator-controller/library/satnogs.3dshapes/HSOP-8.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2_DIN965_Pad (layer F.Cu) (tedit 5A0C4FF3)
    (at 136.144 117.094)
    (descr "Mounting Hole 2.2mm, M2, DIN965")
    (tags "mounting hole 2.2mm m2 din965")
    (fp_text reference P5 (at 0 -2.9) (layer F.SilkS) hide)
    (fp_text value GND-PAD (at 0.381 2.921) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 3.8 3.8) (drill 2.2) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module satnogs:TSSOP-8_3x3mm_Pitch0.65mm_HandSoldering (layer F.Cu) (tedit 589CCEE2)
    (at 117.856 56.782 90)
    (descr "TSSOP8: plastic thin shrink small outline package; 8 leads; body width 3 mm; (see NXP SSOP-TSSOP-VSO-REFLOW.pdf and sot505-1_po.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U7 (at 0.013 2.667 270) (layer F.SilkS))
    (fp_text value PCA9540B (at 0 2.55 90) (layer F.Fab))
    (pad 1 smd rect (at -2.4 -0.975 90) (size 1.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 65 /SCL))
    (pad 2 smd rect (at -2.4 -0.325 90) (size 1.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 64 /SDA))
    (pad 3 smd rect (at -2.4 0.325 90) (size 1.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 4 smd rect (at -2.4 0.975 90) (size 1.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 62 /SDA0))
    (pad 5 smd rect (at 2.4 0.975 90) (size 1.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 63 /SCL0))
    (pad 6 smd rect (at 2.4 0.325 90) (size 1.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 7 smd rect (at 2.4 -0.325 90) (size 1.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 21 /SDA1))
    (pad 8 smd rect (at 2.4 -0.975 90) (size 1.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 20 /SCL1))
    (model Housings_SSOP.3dshapes/TSSOP-8_3x3mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 541A9B8D)
    (at 111.379 56.134 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C14 (at -3.048 0 360) (layer F.SilkS))
    (fp_text value 0.1u (at 4.064 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module satnogs:MKDS_1.5-4 (layer F.Cu) (tedit 589DCDC1)
    (at 145.288 48.514 180)
    (descr "4-way 5mm pitch terminal block, Phoenix MKDS series")
    (fp_text reference P8 (at 9.398 -6.35 180) (layer F.SilkS))
    (fp_text value Motor2 (at 0 5.588 180) (layer F.SilkS))
    (pad 4 thru_hole circle (at 7.5 0 180) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 28 /2BM2))
    (pad 3 thru_hole circle (at 2.5 0 180) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 26 /2AM2))
    (pad 1 thru_hole circle (at -7.5 0 180) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 29 /1BM2))
    (pad 2 thru_hole circle (at -2.5 0 180) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 27 /1AM2))
    (model /home/azisi/Documents/SatNOGS/satnogs-rotator-controller/library/satnogs.3dshapes/MKDS_1.5-4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module satnogs:MKDS_1.5-4 (layer F.Cu) (tedit 589DCDC7)
    (at 168.148 48.514 180)
    (descr "4-way 5mm pitch terminal block, Phoenix MKDS series")
    (fp_text reference P7 (at 9.525 -6.35 180) (layer F.SilkS))
    (fp_text value Motor1 (at 0 5.588 180) (layer F.SilkS))
    (pad 4 thru_hole circle (at 7.5 0 180) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 24 /2BM1))
    (pad 3 thru_hole circle (at 2.5 0 180) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 22 /2AM1))
    (pad 1 thru_hole circle (at -7.5 0 180) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 25 /1BM1))
    (pad 2 thru_hole circle (at -2.5 0 180) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 23 /1AM1))
    (model /home/azisi/Documents/SatNOGS/satnogs-rotator-controller/library/satnogs.3dshapes/MKDS_1.5-4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module satnogs:CP_Radial_D10.0mm_P5.00mm (layer F.Cu) (tedit 58A4529C)
    (at 152.527 103.171 90)
    (descr "CP, Radial series, Radial, pin pitch=5.00mm, , diameter=10mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 5.00mm  diameter 10mm Electrolytic Capacitor")
    (fp_text reference C15 (at 6.905 -5.334 90) (layer F.SilkS))
    (fp_text value 100u (at 2.5 6.06 90) (layer F.Fab))
    (fp_text user + (at -2.159 -4.318 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 57 /SW_VIN))
    (pad 2 thru_hole circle (at 5 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model /home/azisi/Documents/SatNOGS/satnogs-rotator-controller/PCB/library/satnogs.3dshapes/CP_Radial_D10.0mm_P5.00mm.wrl
      (at (xyz 0.098 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Fuse_Holders_and_Fuses:Fuse_SMD1206_HandSoldering (layer F.Cu) (tedit 0)
    (at 142.748 104.267 270)
    (descr "Fuse, Sicherung, SMD1206, Littlefuse-Wickmann 433 Series, Hand Soldering,")
    (tags "Fuse Sicherung SMD1206 Littlefuse-Wickmann 433 Series Hand Soldering ")
    (attr smd)
    (fp_text reference F1 (at -4.699 0 270) (layer F.SilkS))
    (fp_text value FUSE (at -0.15 2.5 270) (layer F.Fab))
    (pad 1 smd rect (at -2.09 0) (size 2.03 2.65) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(F1-Pad1)"))
    (pad 2 smd rect (at 2.09 0) (size 2.03 2.65) (layers F.Cu F.Paste F.Mask)
      (net 57 /SW_VIN))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x03_Pitch2.54mm (layer F.Cu) (tedit 5A0C068F)
    (at 93.98 55.88)
    (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.54mm double row")
    (fp_text reference P6 (at 1.27 -2.33) (layer F.SilkS) hide)
    (fp_text value ISP (at 1.27 7.41) (layer F.Fab))
    (fp_text user %R (at 1.27 2.54 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 66 /PB4))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 /PB5))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /M2IN1))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 76 /RST))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x05_Pitch2.54mm (layer F.Cu) (tedit 5A0C36EC)
    (at 128.27 115.824 270)
    (descr "Through hole straight pin header, 2x05, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x05 2.54mm double row")
    (fp_text reference P3 (at 1.27 -2.33 270) (layer F.SilkS) hide)
    (fp_text value ISP (at 1.27 12.49 270) (layer F.Fab))
    (fp_text user %R (at 1.27 5.08 360) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /VIN))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /VIN))
    (pad 3 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole oval (at 2.54 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 5 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 6 thru_hole oval (at 2.54 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 7 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /B))
    (pad 8 thru_hole oval (at 2.54 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /A))
    (pad 9 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 68 /DTR))
    (pad 10 thru_hole oval (at 2.54 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x05_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module satnogs:DO-214AB_Handsoldering (layer F.Cu) (tedit 5A0F2E40)
    (at 133.731 106.553 270)
    (descr "Jedec DO-214AB diode package. Designed according to Fairchild SS32 datasheet.")
    (tags "DO-214AB diode Handsoldering")
    (attr smd)
    (fp_text reference D4 (at 0 -4.2 270) (layer F.Fab))
    (fp_text value D_TVS (at 0 4.6 270) (layer F.Fab))
    (pad 2 smd rect (at 4.1 0 270) (size 3.6 3.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -4.1 0 270) (size 3.6 3.2) (layers F.Cu F.Paste F.Mask)
      (net 3 /VIN))
    (model /home/azisi/Documents/SatNOGS/satnogs-rotator-controller/library/satnogs.3dshapes/DO-214AB.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 180))
    )
  )
  (module satnogs:DO-214AB_Handsoldering (layer F.Cu) (tedit 5A0F2E40)
    (at 147.193 113.919 270)
    (descr "Jedec DO-214AB diode package. Designed according to Fairchild SS32 datasheet.")
    (tags "DO-214AB diode Handsoldering")
    (attr smd)
    (fp_text reference D2 (at 0 -4.2 270) (layer F.Fab))
    (fp_text value D_Schottky (at 0 4.6 270) (layer F.Fab))
    (pad 2 smd rect (at 4.1 0 270) (size 3.6 3.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -4.1 0 270) (size 3.6 3.2) (layers F.Cu F.Paste F.Mask)
      (net 57 /SW_VIN))
    (model /home/azisi/Documents/SatNOGS/satnogs-rotator-controller/library/satnogs.3dshapes/DO-214AB.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 180))
    )
  )
  (module satnogs:DO-214AB_Handsoldering (layer F.Cu) (tedit 5A0F2E40)
    (at 184.912 101.346 90)
    (descr "Jedec DO-214AB diode package. Designed according to Fairchild SS32 datasheet.")
    (tags "DO-214AB diode Handsoldering")
    (attr smd)
    (fp_text reference D1 (at 0 -4.2 90) (layer F.Fab))
    (fp_text value D_Schottky (at 0 4.6 90) (layer F.Fab))
    (pad 2 smd rect (at 4.1 0 90) (size 3.6 3.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -4.1 0 90) (size 3.6 3.2) (layers F.Cu F.Paste F.Mask)
      (net 59 /SW))
    (model /home/azisi/Documents/SatNOGS/satnogs-rotator-controller/library/satnogs.3dshapes/DO-214AB.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 180))
    )
  )
  (gr_text GND (at 125.857 111.76 90) (layer F.SilkS))
  (gr_text ISP (at 95.25 53.721) (layer F.SilkS))
  (gr_text GND (at 128.524 51.816 90) (layer F.SilkS))
  (gr_text +5V (at 130.175 51.943 90) (layer F.SilkS))
  (gr_text GND (at 115.951 51.181) (layer F.SilkS))
  (gr_text SDA0 (at 122.301 52.578) (layer F.SilkS))
  (gr_text GND (at 122.428 51.181) (layer F.SilkS))
  (gr_text +5V (at 112.522 51.181) (layer F.SilkS))
  (gr_text SCL1 (at 112.649 52.578) (layer F.SilkS))
  (gr_text SDA1 (at 115.951 52.578) (layer F.SilkS))
  (gr_text +5V (at 119.126 51.181) (layer F.SilkS))
  (gr_text SCL0 (at 119.126 52.578) (layer F.SilkS))
  (gr_text A3 (at 101.219 52.578) (layer F.SilkS))
  (gr_text +5V (at 101.092 51.181) (layer F.SilkS))
  (gr_text A2 (at 103.886 52.578) (layer F.SilkS))
  (gr_text +5V (at 106.426 51.181) (layer F.SilkS))
  (gr_text GND (at 109.22 52.578) (layer F.SilkS))
  (gr_text GND (at 103.886 51.181) (layer F.SilkS))
  (gr_text PB4 (at 109.22 51.181) (layer F.SilkS))
  (gr_text PB5 (at 106.553 52.578) (layer F.SilkS))
  (gr_text SW2 (at 126.111 51.181) (layer F.SilkS))
  (gr_text SW1 (at 126.111 52.578) (layer F.SilkS))
  (gr_text A (at 120.777 112.8395) (layer F.SilkS))
  (gr_text CTS (at 118.11 112.8395) (layer F.SilkS))
  (gr_text VIN (at 128.397 111.76 90) (layer F.SilkS))
  (gr_text MOTORS (at 183.769 50.8) (layer F.SilkS))
  (gr_text 1B (at 186.944 52.959) (layer F.SilkS))
  (gr_text 1A (at 184.912 52.959) (layer F.SilkS))
  (gr_text 2A (at 182.753 52.959) (layer F.SilkS))
  (gr_text 2B (at 180.594 52.959) (layer F.SilkS))
  (gr_text GND (at 123.19 111.76 90) (layer F.SilkS))
  (gr_text B (at 120.777 110.8075) (layer F.SilkS))
  (gr_text DTR (at 118.11 110.8075) (layer F.SilkS))
  (gr_text "SatNOGS Rotator Controller v2" (at 152.019 90.932) (layer F.SilkS))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.6))
    (min_thickness 0.5)
    (fill yes (arc_segments 32) (thermal_gap 0.4) (thermal_bridge_width 0.6) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 91.44 121.92) (xy 91.44 41.91) (xy 191.389 41.91) (xy 191.389 121.92)
      )
    )
  )
  (zone (net 59) (net_name /SW) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.6))
    (min_thickness 0.5)
    (fill yes (arc_segments 32) (thermal_gap 0.4) (thermal_bridge_width 0.6) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 166.116 111.252) (xy 169.545 111.252) (xy 169.545 110.363) (xy 188.087 110.363) (xy 188.087 102.362)
        (xy 166.116 102.362)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (priority 3)
    (connect_pads (clearance 0.6))
    (min_thickness 0.5)
    (fill yes (arc_segments 32) (thermal_gap 0.4) (thermal_bridge_width 0.6) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 191.389 101.854) (xy 165.608 101.854) (xy 165.608 113.157) (xy 191.389 113.157) (xy 191.389 121.92)
        (xy 91.44 121.92) (xy 91.44 41.91) (xy 191.389 41.91)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.5))
    (min_thickness 0.5)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 32) (thermal_gap 0.4) (thermal_bridge_width 0.6))
    (polygon
      (pts
        (xy 132.969 41.91) (xy 133.731 41.91) (xy 133.731 82.55) (xy 175.768 82.55) (xy 175.768 84.582)
        (xy 132.969 84.582)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.6))
    (min_thickness 0.5)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill yes (arc_segments 32) (thermal_gap 0.4) (thermal_bridge_width 0.6))
    (polygon
      (pts
        (xy 159.639 95.504) (xy 163.576 95.504) (xy 163.576 97.155) (xy 159.639 97.155)
      )
    )
  )
)
