(kicad_pcb (version 4) (host pcbnew 4.0.2+dfsg1-stable)
  (general
    (links 16)
    (no_connects 0)
    (area 141.415699 103.048999 163.409701 114.629001)
    (thickness 1.6)
    (drawings 7)
    (tracks 31)
    (zones 0)
    (modules 7)
    (nets 9)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.4)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (grid_origin 151.6507 109.474)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 "Net-(C1-Pad2)")
  (net 3 "Net-(C2-Pad1)")
  (net 4 "Net-(C2-Pad2)")
  (net 5 "Net-(P1-Pad2)")
  (net 6 "Net-(P1-Pad3)")
  (net 7 "Net-(P2-Pad2)")
  (net 8 "Net-(P2-Pad3)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.4)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C2-Pad2)")
    (add_net "Net-(P1-Pad2)")
    (add_net "Net-(P1-Pad3)")
    (add_net "Net-(P2-Pad2)")
    (add_net "Net-(P2-Pad3)")
  )
  (module uart:uart (layer B.Cu) (tedit 592B3B30)
    (at 143.1544 112.5347 90)
    (fp_text reference P2 (at 0 0 90) (layer Eco1.User) hide)
    (fp_text value uart (at 1.27 -1.27 90) (layer Eco1.User) hide)
    (fp_text user GND (at 7.6 1.9 90) (layer B.SilkS))
    (fp_text user RX (at 2.54 1.905 90) (layer B.SilkS))
    (fp_text user TX (at 5.08 1.905 90) (layer B.SilkS))
    (fp_text user VCC (at -0.1 1.9 90) (layer B.SilkS))
    (pad 1 thru_hole oval (at 0 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 7 "Net-(P2-Pad2)"))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 8 "Net-(P2-Pad3)"))
    (pad 4 thru_hole oval (at 7.62 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad2)"))
  )
  (module Housings_DIP:DIP-8_W7.62mm (layer F.Cu) (tedit 592EDA54)
    (at 148.5011 105.0036)
    (descr "8-lead dip package, row spacing 7.62 mm (300 mils)")
    (tags "dil dip 2.54 300")
    (fp_text reference U1 (at 2.4638 -1.3716) (layer F.SilkS))
    (fp_text value CPC5001 (at 3.7211 1.778) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(P2-Pad2)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(C1-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(P2-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(C1-Pad1)"))
    (pad 5 thru_hole oval (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(P1-Pad3)"))
    (pad 6 thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(C2-Pad2)"))
    (pad 7 thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(P1-Pad2)"))
    (pad 8 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(C2-Pad1)"))
    (model Housings_DIP.3dshapes/DIP-8_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module uart:uart_host (layer B.Cu) (tedit 592B3B78)
    (at 161.6837 105.1306 270)
    (fp_text reference P1 (at 0 0 270) (layer Eco1.User) hide)
    (fp_text value uart_host (at 1.27 -1.27 270) (layer Eco1.User) hide)
    (fp_text user GND (at 7.6 1.9 270) (layer B.SilkS))
    (fp_text user RX (at 5.08 1.905 270) (layer B.SilkS))
    (fp_text user TX (at 2.54 1.905 270) (layer B.SilkS))
    (fp_text user VCC (at -0.1 1.9 270) (layer B.SilkS))
    (pad 1 thru_hole oval (at 0 0 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 5 "Net-(P1-Pad2)"))
    (pad 3 thru_hole oval (at 5.08 0 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 6 "Net-(P1-Pad3)"))
    (pad 4 thru_hole oval (at 7.62 0 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 4 "Net-(C2-Pad2)"))
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 592EDA43)
    (at 146.2405 110.8583 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 3.6957 0.0889 90) (layer B.SilkS))
    (fp_text value C (at 0 -2.1 90) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 592EDA4E)
    (at 158.3563 107.6706 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at 2.8067 -0.0381 270) (layer B.SilkS))
    (fp_text value C (at 0 -2.1 270) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(C2-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 592EDA40)
    (at 146.2532 111.2774 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 4.2164 0.1143 90) (layer F.SilkS))
    (fp_text value R (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(P2-Pad3)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 592EDA48)
    (at 158.6992 106.3371 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at 4.0767 0.254 270) (layer F.SilkS))
    (fp_text value R (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(P1-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "uart isolator\nversion 0.1" (at 152.6667 108.712 270) (layer B.SilkS))
  (gr_text "GND RX  TX VCC" (at 160.2867 108.966 90) (layer F.SilkS))
  (gr_text "GND TX  RX VCC" (at 144.5387 108.712 270) (layer F.SilkS))
  (gr_line (start 141.4907 114.554) (end 141.4907 103.124) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 163.3347 114.554) (end 141.4907 114.554) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 163.3347 103.124) (end 163.3347 114.554) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 141.4907 103.124) (end 163.3347 103.124) (angle 90) (layer Edge.Cuts) (width 0.15))
)
