(kicad_pcb (version 20171130) (host pcbnew "(5.1.6-0-10_14)")
  (general
    (thickness 1.6)
    (drawings 35)
    (tracks 764)
    (zones 0)
    (modules 103)
    (nets 94)
  )
  (page USLedger)
  (title_block
    (date 2019-12-29)
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.2032)
    (trace_clearance 0.1778)
    (zone_clearance 0.2032)
    (zone_45_only no)
    (trace_min 0.1778)
    (via_size 0.6604)
    (via_drill 0.4064)
    (via_min_size 0.4064)
    (via_min_drill 0.3556)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 0.5 0.5)
    (mod_text_width 0.07)
    (pad_size 5.842 5.842)
    (pad_drill 3.200001)
    (pad_to_mask_clearance 0.0254)
    (solder_mask_min_width 0.0254)
    (aux_axis_origin 0 0)
    (visible_elements FEFDBF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 4)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 +3V3)
  (net 3 ~RESET~)
  (net 4 +3.3VP)
  (net 5 GNDA)
  (net 6 "Net-(CN22-Pad2)")
  (net 7 "Net-(CNQ1-Pad1)")
  (net 8 "Net-(CNQ2-Pad1)")
  (net 9 "Net-(CNRD1-Pad1)")
  (net 10 GNDPWR)
  (net 11 "Net-(CNRX+1-Pad1)")
  (net 12 "Net-(CNRX+1-Pad2)")
  (net 13 "Net-(CNRX-1-Pad1)")
  (net 14 "Net-(CNRX-1-Pad2)")
  (net 15 "Net-(CNTCT1-Pad2)")
  (net 16 "Net-(CPCC1-Pad2)")
  (net 17 "Net-(CPCC1-Pad1)")
  (net 18 /PV3)
  (net 19 "Net-(CPFIL1-Pad1)")
  (net 20 GNDREF)
  (net 21 /VPORTP)
  (net 22 /VPORTN)
  (net 23 /PVCC)
  (net 24 /RUN)
  (net 25 /NN)
  (net 26 /PP)
  (net 27 /PLUS)
  (net 28 /NGATE)
  (net 29 /RCLASS)
  (net 30 /SENSE)
  (net 31 "Net-(RN1-Pad1)")
  (net 32 "Net-(RN2-Pad1)")
  (net 33 "Net-(RN3-Pad1)")
  (net 34 "Net-(RN4-Pad1)")
  (net 35 "Net-(RN5-Pad1)")
  (net 36 "Net-(RNEXR1-Pad2)")
  (net 37 "Net-(RNLACT1-Pad2)")
  (net 38 "Net-(RNLDUP1-Pad2)")
  (net 39 "Net-(RNLNK1-Pad2)")
  (net 40 "Net-(RNLSPEED1-Pad2)")
  (net 41 "Net-(RNSPD1-Pad1)")
  (net 42 /SEN)
  (net 43 "Net-(RNDMPR-1-Pad2)")
  (net 44 "Net-(RNDMPT-1-Pad2)")
  (net 45 "Net-(PA1133-coil1-Pad4)")
  (net 46 "Net-(PA1133-coil1-Pad2)")
  (net 47 "Net-(PA1133-coil1-Pad1)")
  (net 48 "Net-(PS2911-Pad1)")
  (net 49 "Net-(RNAUTO1-Pad1)")
  (net 50 "Net-(RNDUP1-Pad1)")
  (net 51 "Net-(RNINT1-Pad1)")
  (net 52 "Net-(J_RJ45-Pad14)")
  (net 53 "Net-(J_RJ45-Pad5)")
  (net 54 "Net-(J_RJ45-Pad6)")
  (net 55 "Net-(J_RJ45-Pad12)")
  (net 56 "Net-(U_W5500-Pad47)")
  (net 57 "Net-(U_W5500-Pad46)")
  (net 58 "Net-(U_W5500-Pad18)")
  (net 59 "Net-(U_W5500-Pad13)")
  (net 60 "Net-(U_W5500-Pad12)")
  (net 61 "Net-(U_W5500-Pad7)")
  (net 62 "Net-(CN20-Pad2)")
  (net 63 "Net-(RN6-Pad2)")
  (net 64 "Net-(RNDMPR+1-Pad2)")
  (net 65 "Net-(RNDMPT+1-Pad2)")
  (net 66 "Net-(L_NDUP1-Pad1)")
  (net 67 "Net-(L_NSPD1-Pad1)")
  (net 68 "Net-(L_PLED1-Pad2)")
  (net 69 "Net-(D_PBAS1-Pad1)")
  (net 70 "Net-(D_PDS1040-Pad2)")
  (net 71 "Net-(L_PLED1-Pad1)")
  (net 72 +3V0)
  (net 73 "Net-(MPOE1-Pad1)")
  (net 74 "Net-(MPOE2-Pad1)")
  (net 75 "Net-(SP_N_HARDRESET_1-Pad2)")
  (net 76 "Net-(SP_N_SOFTRESET_1-Pad2)")
  (net 77 "Net-(MPOE3-Pad1)")
  (net 78 "Net-(MPOE4-Pad1)")
  (net 79 /NETRST)
  (net 80 /NET-MISO)
  (net 81 "Net-(U_LTC4267-Pad11)")
  (net 82 "Net-(U_LTC4267-Pad6)")
  (net 83 /SDA)
  (net 84 /SCL)
  (net 85 /PA04-D17)
  (net 86 PA12-MOSI)
  (net 87 PA14-MISO)
  (net 88 PA13-SCK)
  (net 89 PB13-D4-NET_RES)
  (net 90 PB14-D5-NET_CS)
  (net 91 /PA22-D1)
  (net 92 /PA23-D0)
  (net 93 PB15-D6-NET_INT)
  (net_class Default "This is the default net class."
    (clearance 0.1778)
    (trace_width 0.2032)
    (via_dia 0.6604)
    (via_drill 0.4064)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (diff_pair_width 0.2032)
    (diff_pair_gap 0.25)
    (add_net +3.3VP)
    (add_net +3V0)
    (add_net +3V3)
    (add_net /NET-MISO)
    (add_net /NETRST)
    (add_net /NGATE)
    (add_net /NN)
    (add_net /PA04-D17)
    (add_net /PA22-D1)
    (add_net /PA23-D0)
    (add_net /PLUS)
    (add_net /PP)
    (add_net /PV3)
    (add_net /PVCC)
    (add_net /RCLASS)
    (add_net /RUN)
    (add_net /SCL)
    (add_net /SDA)
    (add_net /SEN)
    (add_net /SENSE)
    (add_net /VPORTN)
    (add_net /VPORTP)
    (add_net GND)
    (add_net GNDA)
    (add_net GNDPWR)
    (add_net GNDREF)
    (add_net "Net-(CN20-Pad2)")
    (add_net "Net-(CN22-Pad2)")
    (add_net "Net-(CNQ1-Pad1)")
    (add_net "Net-(CNQ2-Pad1)")
    (add_net "Net-(CNRD1-Pad1)")
    (add_net "Net-(CNRX+1-Pad1)")
    (add_net "Net-(CNRX+1-Pad2)")
    (add_net "Net-(CNRX-1-Pad1)")
    (add_net "Net-(CNRX-1-Pad2)")
    (add_net "Net-(CNTCT1-Pad2)")
    (add_net "Net-(CPCC1-Pad1)")
    (add_net "Net-(CPCC1-Pad2)")
    (add_net "Net-(CPFIL1-Pad1)")
    (add_net "Net-(D_PBAS1-Pad1)")
    (add_net "Net-(D_PDS1040-Pad2)")
    (add_net "Net-(J_RJ45-Pad12)")
    (add_net "Net-(J_RJ45-Pad14)")
    (add_net "Net-(J_RJ45-Pad5)")
    (add_net "Net-(J_RJ45-Pad6)")
    (add_net "Net-(L_NDUP1-Pad1)")
    (add_net "Net-(L_NSPD1-Pad1)")
    (add_net "Net-(L_PLED1-Pad1)")
    (add_net "Net-(L_PLED1-Pad2)")
    (add_net "Net-(MPOE1-Pad1)")
    (add_net "Net-(MPOE2-Pad1)")
    (add_net "Net-(MPOE3-Pad1)")
    (add_net "Net-(MPOE4-Pad1)")
    (add_net "Net-(PA1133-coil1-Pad1)")
    (add_net "Net-(PA1133-coil1-Pad2)")
    (add_net "Net-(PA1133-coil1-Pad4)")
    (add_net "Net-(PS2911-Pad1)")
    (add_net "Net-(RN1-Pad1)")
    (add_net "Net-(RN2-Pad1)")
    (add_net "Net-(RN3-Pad1)")
    (add_net "Net-(RN4-Pad1)")
    (add_net "Net-(RN5-Pad1)")
    (add_net "Net-(RN6-Pad2)")
    (add_net "Net-(RNAUTO1-Pad1)")
    (add_net "Net-(RNDMPR+1-Pad2)")
    (add_net "Net-(RNDMPR-1-Pad2)")
    (add_net "Net-(RNDMPT+1-Pad2)")
    (add_net "Net-(RNDMPT-1-Pad2)")
    (add_net "Net-(RNDUP1-Pad1)")
    (add_net "Net-(RNEXR1-Pad2)")
    (add_net "Net-(RNINT1-Pad1)")
    (add_net "Net-(RNLACT1-Pad2)")
    (add_net "Net-(RNLDUP1-Pad2)")
    (add_net "Net-(RNLNK1-Pad2)")
    (add_net "Net-(RNLSPEED1-Pad2)")
    (add_net "Net-(RNSPD1-Pad1)")
    (add_net "Net-(SP_N_HARDRESET_1-Pad2)")
    (add_net "Net-(SP_N_SOFTRESET_1-Pad2)")
    (add_net "Net-(U_LTC4267-Pad11)")
    (add_net "Net-(U_LTC4267-Pad6)")
    (add_net "Net-(U_W5500-Pad12)")
    (add_net "Net-(U_W5500-Pad13)")
    (add_net "Net-(U_W5500-Pad18)")
    (add_net "Net-(U_W5500-Pad46)")
    (add_net "Net-(U_W5500-Pad47)")
    (add_net "Net-(U_W5500-Pad7)")
    (add_net PA12-MOSI)
    (add_net PA13-SCK)
    (add_net PA14-MISO)
    (add_net PB13-D4-NET_RES)
    (add_net PB14-D5-NET_CS)
    (add_net PB15-D6-NET_INT)
    (add_net ~RESET~)
  )
  (module min51j:PDS1040 (layer F.Cu) (tedit 5F42F808)
    (at 55.03672 75.65644 90)
    (descr "Microsemi Powermite 2 SMD power package (https://www.microsemi.com/packaging-information/partpackage/details?pid=5341)")
    (tags PowerMite2)
    (attr smd)
    (fp_text reference D_PDS1040 (at -0.68834 2.67462 90) (layer F.SilkS))
    (fp_text value PDS1040-13 (at -0.24384 -2.7432 90) (layer F.Fab) hide)
    (fp_text user %R (at -0.3 -1 90) (layer F.Fab))
    (pad 1 smd rect (at -0.6985 0 90) (size 5.33 4.2) (layers F.Cu F.Paste F.Mask)
      (net 18 /PV3))
    (pad 2 smd rect (at 3 0 90) (size 0.762 2.8) (layers F.Cu F.Paste F.Mask)
      (net 70 "Net-(D_PDS1040-Pad2)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_Powermite2_AK.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module min51j:LTC4267 (layer F.Cu) (tedit 5F41757B)
    (at 46.80204 45.6819 90)
    (descr "TSSOP, 16 Pin (JEDEC MO-153 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "TSSOP SO")
    (attr smd)
    (fp_text reference U_LTC4267 (at 0 -3.45 90) (layer F.SilkS))
    (fp_text value LTC4267IGN-1#PBF (at 0 3.45 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 1 smd roundrect (at -2.8625 -2.2225 90) (size 1.475 0.38) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 GNDREF))
    (pad 2 smd roundrect (at -2.8625 -1.5875 90) (size 1.475 0.38) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 /RUN))
    (pad 3 smd roundrect (at -2.8625 -0.9525 90) (size 1.475 0.38) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 28 /NGATE))
    (pad 4 smd roundrect (at -2.8625 -0.3175 90) (size 1.475 0.38) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 23 /PVCC))
    (pad 5 smd roundrect (at -2.8625 0.3175 90) (size 1.475 0.38) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 29 /RCLASS))
    (pad 6 smd roundrect (at -2.8625 0.9525 90) (size 1.475 0.38) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 82 "Net-(U_LTC4267-Pad6)"))
    (pad 7 smd roundrect (at -2.8625 1.5875 90) (size 1.475 0.38) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 /VPORTN))
    (pad 8 smd roundrect (at -2.8625 2.2225 90) (size 1.475 0.38) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 GNDREF))
    (pad 9 smd roundrect (at 2.8625 2.2225 90) (size 1.475 0.38) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 GNDREF))
    (pad 10 smd roundrect (at 2.8625 1.5875 90) (size 1.475 0.38) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 GNDREF))
    (pad 11 smd roundrect (at 2.8625 0.9525 90) (size 1.475 0.38) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 81 "Net-(U_LTC4267-Pad11)"))
    (pad 12 smd roundrect (at 2.8625 0.3175 90) (size 1.475 0.38) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 /VPORTN))
    (pad 13 smd roundrect (at 2.8625 -0.3175 90) (size 1.475 0.38) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 /VPORTP))
    (pad 14 smd roundrect (at 2.8625 -0.9525 90) (size 1.475 0.38) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 30 /SENSE))
    (pad 15 smd roundrect (at 2.8625 -1.5875 90) (size 1.475 0.38) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 GNDREF))
    (pad 16 smd roundrect (at 2.8625 -2.2225 90) (size 1.475 0.38) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 GNDREF))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/TSSOP-16_4.4x5mm_P0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module min51j:Si3440 (layer F.Cu) (tedit 5F416CAD)
    (at 48.39208 53.6448 180)
    (descr "TSOP-6 package (comparable to TSOT-23), https://www.vishay.com/docs/71200/71200.pdf")
    (tags "Jedec MO-193C TSOP-6L")
    (attr smd)
    (fp_text reference U_Si3440 (at -0.1524 2.3368) (layer F.SilkS))
    (fp_text value Si3440 (at 0 2.5) (layer F.Fab) hide)
    (fp_text user %R (at 0 -0.127 90) (layer F.Fab) hide)
    (pad 6 smd rect (at 1.16 -0.95 180) (size 1 0.51) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(PA1133-coil1-Pad4)"))
    (pad 5 smd rect (at 1.16 0 180) (size 1 0.51) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(PA1133-coil1-Pad4)"))
    (pad 4 smd rect (at 1.16 0.95 180) (size 1 0.51) (layers F.Cu F.Paste F.Mask)
      (net 42 /SEN))
    (pad 3 smd rect (at -1.16 0.95 180) (size 1 0.51) (layers F.Cu F.Paste F.Mask)
      (net 28 /NGATE))
    (pad 2 smd rect (at -1.16 0 180) (size 1 0.51) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(PA1133-coil1-Pad4)"))
    (pad 1 smd rect (at -1.16 -0.95 180) (size 1 0.51) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(PA1133-coil1-Pad4)"))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/TSOP-6_1.65x3.05mm_P0.95mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystal:Crystal_SMD_EuroQuartz_MJ-4Pin_5.0x3.2mm (layer F.Cu) (tedit 5EFAE664)
    (at 24.3459 62.14364)
    (descr "SMD Crystal EuroQuartz MJ series http://cdn-reichelt.de/documents/datenblatt/B400/MJ.pdf, 5.0x3.2mm^2 package")
    (tags "SMD SMT crystal")
    (attr smd)
    (fp_text reference QN1 (at 0.4699 -2.65684) (layer F.SilkS))
    (fp_text value "25.00 MHz 18pf" (at 0 2.8) (layer F.Fab) hide)
    (fp_text user %R (at 0.1016 3.9116) (layer F.Fab) hide)
    (pad 4 smd rect (at -1.85 -1.15) (size 1.9 1.1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 1.85 -1.15) (size 1.9 1.1) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(CNQ2-Pad1)"))
    (pad 2 smd rect (at 1.85 1.15) (size 1.9 1.1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.85 1.15) (size 1.9 1.1) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(CNQ1-Pad1)"))
    (model ${KISYS3DMOD}/Crystal.3dshapes/Crystal_SMD_EuroQuartz_MJ-4Pin_5.0x3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SMA (layer F.Cu) (tedit 5EFAE201)
    (at 45.56252 34.8234 180)
    (descr "Diode SMA (DO-214AC)")
    (tags "Diode SMA (DO-214AC)")
    (attr smd)
    (fp_text reference D_SMAJ58 (at -6.68528 0.127) (layer F.SilkS))
    (fp_text value SMAJ58A-13-F (at 0 2.6) (layer F.Fab) hide)
    (fp_text user %R (at -1.2192 2.6162) (layer F.Fab) hide)
    (pad 2 smd rect (at 2 0 180) (size 2.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 22 /VPORTN))
    (pad 1 smd rect (at -2 0 180) (size 2.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 27 /PLUS))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SMA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23_Handsoldering (layer F.Cu) (tedit 5EFAE14D)
    (at 41.97858 68.0339 270)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (attr smd)
    (fp_text reference U_TLV431 (at 0.0127 2.25298 90) (layer F.SilkS))
    (fp_text value TLV431 (at 0 2.5 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 3 smd rect (at 1.5 0 270) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -1.5 0.95 270) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(CPCC1-Pad1)"))
    (pad 1 smd rect (at -1.5 -0.95 270) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(CPCC1-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23-6_Handsoldering (layer F.Cu) (tedit 5EFBB84A)
    (at 30.099 70.739)
    (descr "6-pin SOT-23 package, Handsoldering")
    (tags "SOT-23-6 Handsoldering")
    (attr smd)
    (fp_text reference U_2G7RES1 (at -3.1496 0 90) (layer F.SilkS))
    (fp_text value SN74LVC2G07DBVR (at 0.0254 2.2098) (layer F.Fab) hide)
    (fp_text user %R (at 0.3302 2.9972 180) (layer F.Fab) hide)
    (pad 5 smd rect (at 1.35 0) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 6 smd rect (at 1.35 -0.95) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 76 "Net-(SP_N_SOFTRESET_1-Pad2)"))
    (pad 4 smd rect (at 1.35 0.95) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 75 "Net-(SP_N_HARDRESET_1-Pad2)"))
    (pad 3 smd rect (at -1.35 0.95) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 3 ~RESET~))
    (pad 2 smd rect (at -1.35 0) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.35 -0.95) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 89 PB13-D4-NET_RES))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_3.2mm_M3_Pad locked (layer F.Cu) (tedit 5EFA97D2)
    (at 62.23 77.47)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (attr virtual)
    (fp_text reference MPOE1 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MPOE1 (at 0 4.2) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask)
      (net 73 "Net-(MPOE1-Pad1)"))
  )
  (module MountingHole:MountingHole_3.2mm_M3_Pad locked (layer F.Cu) (tedit 5EFA97D2)
    (at 62.23 29.21)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (attr virtual)
    (fp_text reference MPOE2 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MPOE2 (at 0 4.2) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask)
      (net 74 "Net-(MPOE2-Pad1)"))
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5EFB79D2)
    (at 45.6438 72.644 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference RPOE1 (at 0.0508 -1.4224) (layer F.SilkS))
    (fp_text value "60.4K 1%" (at 0 1.65) (layer F.Fab) hide)
    (fp_text user %R (at -0.0762 2.3876) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 16 "Net-(CPCC1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5EFB79E5)
    (at 25.09774 44.58208 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference CN4 (at -0.0508 -1.397 90) (layer F.SilkS))
    (fp_text value 0.1uf (at 0 1.65 90) (layer F.Fab) hide)
    (fp_text user %R (at 0.0508 2.3876 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 4 +3.3VP))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 5 GNDA))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5EFB79E5)
    (at 21.10486 44.46016 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference CN8 (at -0.08636 -1.32334 90) (layer F.SilkS))
    (fp_text value 0.1uf (at 0 1.65 90) (layer F.Fab) hide)
    (fp_text user %R (at 0.0508 2.3876 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 4 +3.3VP))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 5 GNDA))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5EFB79E5)
    (at 18.77822 44.63288 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference CN11 (at 2.94132 -0.09398 90) (layer F.SilkS))
    (fp_text value 0.1uf (at 0 1.65 90) (layer F.Fab) hide)
    (fp_text user %R (at 0.0508 2.3876 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 4 +3.3VP))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 5 GNDA))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5EFB79E5)
    (at 14.20876 47.81296)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference CN15 (at -3.26136 0.11684) (layer F.SilkS))
    (fp_text value 0.1uf (at 0 1.65) (layer F.Fab) hide)
    (fp_text user %R (at 0.0508 2.3876) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 4 +3.3VP))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 5 GNDA))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5EFB79E5)
    (at 14.18844 49.93132)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference CN17 (at -3.29184 0.05588) (layer F.SilkS))
    (fp_text value 0.1uf (at 0 1.65) (layer F.Fab) hide)
    (fp_text user %R (at 0.0508 2.3876) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 4 +3.3VP))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 5 GNDA))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5EFB79E5)
    (at 14.20876 52.06746)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference CN20 (at -3.26136 0.02794) (layer F.SilkS))
    (fp_text value 10uf (at 0 1.65) (layer F.Fab) hide)
    (fp_text user %R (at 0.0508 2.3876) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 62 "Net-(CN20-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 5 GNDA))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5EFB79E5)
    (at 14.20114 54.08168)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference CN21 (at -3.17754 0.02032) (layer F.SilkS))
    (fp_text value 0.1uf (at 0 1.65) (layer F.Fab) hide)
    (fp_text user %R (at 0.0508 2.3876) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 4 +3.3VP))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 5 GNDA))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5EFB79E5)
    (at 14.21384 56.09844)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference CN22 (at -3.21564 -0.09144) (layer F.SilkS))
    (fp_text value 22nf (at 0 1.65) (layer F.Fab) hide)
    (fp_text user %R (at 0.0508 2.3876) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 6 "Net-(CN22-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 5 GNDA))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5EFB79E5)
    (at 36.068 69.8754 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference CNOR1 (at -0.0508 -1.397 90) (layer F.SilkS))
    (fp_text value 0.1uf (at 0 1.65 90) (layer F.Fab) hide)
    (fp_text user %R (at 0.0508 2.3876 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5EFB79E5)
    (at 19.71548 62.15634 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference CNQ1 (at -0.0508 -1.397 90) (layer F.SilkS))
    (fp_text value 27pf (at 0 1.65 90) (layer F.Fab) hide)
    (fp_text user %R (at 0.0508 2.3876 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 7 "Net-(CNQ1-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5EFB79E5)
    (at 28.76296 62.03442 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference CNQ2 (at -0.0508 -1.397 90) (layer F.SilkS))
    (fp_text value 27pf (at 0 1.65 90) (layer F.Fab) hide)
    (fp_text user %R (at 0.0508 2.3876 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 8 "Net-(CNQ2-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5EFB79E5)
    (at 17.1069 30.1244 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference CNRD1 (at -0.0508 -1.397) (layer F.SilkS))
    (fp_text value "10nf 100V" (at 0 1.65) (layer F.Fab) hide)
    (fp_text user %R (at 0.0508 2.3876) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 9 "Net-(CNRD1-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1806_4516Metric_Pad1.57x1.80mm_HandSolder (layer F.Cu) (tedit 5EFAE060)
    (at 29.33954 25.0698 270)
    (descr "Capacitor SMD 1806 (4516 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://www.modelithics.com/models/Vendor/MuRata/BLM41P.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference CNRJ1 (at 0.0508 -1.6764 90) (layer F.SilkS))
    (fp_text value "1nf 2KV" (at 0 1.85 90) (layer F.Fab) hide)
    (fp_text user %R (at 0.0254 2.921 90) (layer F.Fab))
    (pad 2 smd roundrect (at 2.0875 0 270) (size 1.575 1.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.15873)
      (net 1 GND))
    (pad 1 smd roundrect (at -2.0875 0 270) (size 1.575 1.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.15873)
      (net 10 GNDPWR))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1806_4516Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5EFB79E5)
    (at 20.50034 26.7208 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference CNRX+1 (at -0.0508 -1.397 90) (layer F.SilkS))
    (fp_text value "6.8nf 100V" (at 0 1.65 90) (layer F.Fab) hide)
    (fp_text user %R (at 0.0508 2.3876 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 12 "Net-(CNRX+1-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 11 "Net-(CNRX+1-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5EFB79E5)
    (at 22.68474 26.8478 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference CNRX-1 (at -0.0508 -1.397 90) (layer F.SilkS))
    (fp_text value "6.8nf 100V" (at 0 1.65 90) (layer F.Fab) hide)
    (fp_text user %R (at 0.0508 2.3876 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 14 "Net-(CNRX-1-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 13 "Net-(CNRX-1-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5EFB79E5)
    (at 16.13408 27.11958)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference CNTCT1 (at -0.0508 -1.397) (layer F.SilkS))
    (fp_text value "22nf 100V" (at 0 1.65) (layer F.Fab) hide)
    (fp_text user %R (at 0.0508 2.3876) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 15 "Net-(CNTCT1-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5EFB79E5)
    (at 15.33398 62.9666 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C28B1 (at -0.0508 -1.397 90) (layer F.SilkS))
    (fp_text value 0.1uf (at 0 1.65 90) (layer F.Fab) hide)
    (fp_text user %R (at 0.0508 2.3876 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5EFB79E5)
    (at 41.94302 63.70066)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference CPCC1 (at -2.31902 0.15494 90) (layer F.SilkS))
    (fp_text value 22nf (at 0 1.65) (layer F.Fab) hide)
    (fp_text user %R (at 0.0508 2.3876) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 16 "Net-(CPCC1-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 17 "Net-(CPCC1-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:CP_Elec_6.3x7.7 (layer F.Cu) (tedit 5EFAE089)
    (at 34.4678 76.8858 90)
    (descr "SMD capacitor, aluminum electrolytic, Nichicon, 6.3x7.7mm")
    (tags "capacitor electrolytic")
    (attr smd)
    (fp_text reference CPCOS-CON1 (at 0.127 -4.0894 90) (layer F.SilkS))
    (fp_text value "330uf 6.3V" (at 0 4.35 90) (layer F.Fab) hide)
    (fp_text user %R (at 0.2286 1.8796 90) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 2.7 0 90) (size 3.5 1.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.15625)
      (net 1 GND))
    (pad 1 smd roundrect (at -2.7 0 90) (size 3.5 1.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.15625)
      (net 18 /PV3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/CP_Elec_6.3x7.7.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5EFB79E5)
    (at 61.83122 69.7738)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference CPFIL1 (at 0.19558 1.4732) (layer F.SilkS))
    (fp_text value "470pf 50V" (at 0 1.65) (layer F.Fab) hide)
    (fp_text user %R (at 0.0508 2.3876) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 18 /PV3))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 19 "Net-(CPFIL1-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1812_4532Metric_Pad1.30x3.40mm_HandSolder (layer F.Cu) (tedit 5EFAE292)
    (at 62.17412 53.3781 180)
    (descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://www.nikhef.nl/pub/departments/mt/projects/detectorR_D/dtddice/ERJ2G.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference CPISO1 (at -0.08128 2.4511) (layer F.SilkS))
    (fp_text value "22nf 250V" (at 0 2.65) (layer F.Fab) hide)
    (fp_text user %R (at 0.0508 3.429) (layer F.Fab))
    (pad 2 smd roundrect (at 2.225 0 180) (size 1.3 3.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.192308)
      (net 20 GNDREF))
    (pad 1 smd roundrect (at -2.225 0 180) (size 1.3 3.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.192308)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1812_4532Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1210_3225Metric_Pad1.42x2.65mm_HandSolder (layer F.Cu) (tedit 5EFBB8EA)
    (at 53.50764 53.60924)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference CPLDA1 (at 0 -2.0066) (layer F.SilkS))
    (fp_text value "1uf 100V" (at 0 2.28) (layer F.Fab) hide)
    (fp_text user %R (at -0.0254 3.2766) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1.4875 0) (size 1.425 2.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 21 /VPORTP))
    (pad 1 smd roundrect (at -1.4875 0) (size 1.425 2.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 20 GNDREF))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:CP_Elec_8x10 (layer F.Cu) (tedit 5EFAE226)
    (at 61.3664 42.5196 90)
    (descr "SMD capacitor, aluminum electrolytic, Nichicon, 8.0x10mm")
    (tags "capacitor electrolytic")
    (attr smd)
    (fp_text reference CPLDB1 (at -0.0254 -4.9276 90) (layer F.SilkS))
    (fp_text value "4.7uf 100V" (at 0 5.2 90) (layer F.Fab) hide)
    (fp_text user %R (at 0.254 2.413 90) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 3.25 0 90) (size 3.5 2.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.1)
      (net 20 GNDREF))
    (pad 1 smd roundrect (at -3.25 0 90) (size 3.5 2.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.1)
      (net 21 /VPORTP))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/CP_Elec_8x10.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5EFBB95E)
    (at 44.577 39.80688)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference CPOE1 (at 0 -1.5748) (layer F.SilkS))
    (fp_text value "0.1uf 100V" (at 0 1.82) (layer F.Fab) hide)
    (fp_text user %R (at 0.0508 2.6924) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1.4875 0) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 21 /VPORTP))
    (pad 1 smd roundrect (at -1.4875 0) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 22 /VPORTN))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1210_3225Metric_Pad1.42x2.65mm_HandSolder (layer F.Cu) (tedit 5EFBB8EA)
    (at 49.784 77.47 90)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference CPOUT1 (at -3.0988 0.254 180) (layer F.SilkS))
    (fp_text value "100uf 10V " (at 0 2.28 90) (layer F.Fab) hide)
    (fp_text user %R (at -0.0254 3.2766 90) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1.4875 0 90) (size 1.425 2.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.4875 0 90) (size 1.425 2.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 18 /PV3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1210_3225Metric_Pad1.42x2.65mm_HandSolder (layer F.Cu) (tedit 5EFBB8EA)
    (at 45.72 77.47 90)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference CPOUT2 (at -3.0734 0.127 180) (layer F.SilkS))
    (fp_text value "100uf 10V " (at 0 2.28 90) (layer F.Fab) hide)
    (fp_text user %R (at -0.0254 3.2766 90) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1.4875 0 90) (size 1.425 2.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.4875 0 90) (size 1.425 2.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 18 /PV3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1210_3225Metric_Pad1.42x2.65mm_HandSolder (layer F.Cu) (tedit 5EFBB8EA)
    (at 41.656 77.47 90)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference CPOUT3 (at -3.0226 -0.2286 180) (layer F.SilkS))
    (fp_text value "100uf 10V " (at 0 2.28 90) (layer F.Fab) hide)
    (fp_text user %R (at -0.0254 3.2766 90) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1.4875 0 90) (size 1.425 2.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.4875 0 90) (size 1.425 2.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 18 /PV3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_Tantalum_SMD:CP_EIA-6032-15_Kemet-U_Pad2.25x2.35mm_HandSolder (layer F.Cu) (tedit 5EFAE307)
    (at 52.02174 45.9359 90)
    (descr "Tantalum Capacitor SMD Kemet-U (6032-15 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator")
    (tags "capacitor tantalum")
    (attr smd)
    (fp_text reference CPVCC1 (at 0.9271 2.51206 90) (layer F.SilkS))
    (fp_text value "4.7uf 50V TANT" (at 0 2.55 90) (layer F.Fab) hide)
    (fp_text user %R (at 0.0508 3.2766 90) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 2.55 0 90) (size 2.25 2.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.111111)
      (net 20 GNDREF))
    (pad 1 smd roundrect (at -2.55 0 90) (size 2.25 2.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.111111)
      (net 23 /PVCC))
    (model ${KISYS3DMOD}/Capacitor_Tantalum_SMD.3dshapes/CP_EIA-6032-15_Kemet-U.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-523 (layer F.Cu) (tedit 5EFAE1D1)
    (at 41.44772 48.49622 90)
    (descr "http://www.diodes.com/datasheets/ap02001.pdf p.144")
    (tags "Diode SOD523")
    (attr smd)
    (fp_text reference D_PBAS1 (at 0.0762 -1.397 90) (layer F.SilkS))
    (fp_text value BAS516.135 (at 0 1.4 90) (layer F.Fab) hide)
    (fp_text user %R (at 0.1016 2.6924 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.7 0 270) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 69 "Net-(D_PBAS1-Pad1)"))
    (pad 2 smd rect (at 0.7 0 270) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 24 /RUN))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-523.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5EFB79D2)
    (at 14.08684 35.94724 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference F_NBG1 (at 0.0508 -1.4224 90) (layer F.SilkS))
    (fp_text value "42 ohm Ferrite" (at 0 1.65 90) (layer F.Fab) hide)
    (fp_text user %R (at -0.0762 2.3876 90) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 5 GNDA))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5EFB79D2)
    (at 16.92148 37.33292 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference F_NBV1 (at 0.0508 -1.4224 90) (layer F.SilkS))
    (fp_text value "120 ohm Ferrite" (at 0 1.65 90) (layer F.Fab) hide)
    (fp_text user %R (at -0.0762 2.3876 90) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 +3V3))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 4 +3.3VP))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5EFB79D2)
    (at 12.8778 75.5904 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference F_PB1 (at 0.1778 1.651) (layer F.SilkS))
    (fp_text value "120 ohm Ferrite" (at 0 1.65) (layer F.Fab) hide)
    (fp_text user %R (at -0.0762 2.3876) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 72 +3V0))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 18 /PV3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5EFBBA39)
    (at 29.972 4.1656)
    (descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (attr smd)
    (fp_text reference L_NDUP1 (at -4.4704 0.0508) (layer F.SilkS))
    (fp_text value Red (at 0.3302 1.5494) (layer F.Fab) hide)
    (fp_text user %R (at 0.0254 2.2098) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 +3V3))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 66 "Net-(L_NDUP1-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5EFBBA39)
    (at 29.9212 1.8796)
    (descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (attr smd)
    (fp_text reference L_NSPD1 (at -4.4196 -0.0254) (layer F.SilkS))
    (fp_text value Green (at 0.3302 1.5494) (layer F.Fab) hide)
    (fp_text user %R (at 0.0254 2.2098) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 +3V3))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 67 "Net-(L_NSPD1-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5EFBBA39)
    (at 18.0848 79.0194 180)
    (descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (attr smd)
    (fp_text reference L_PLED1 (at -0.4064 -1.6002) (layer F.SilkS))
    (fp_text value Green (at 0.3302 1.5494) (layer F.Fab) hide)
    (fp_text user %R (at 0.0254 2.2098) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 68 "Net-(L_PLED1-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 71 "Net-(L_PLED1-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5EFB79D2)
    (at 34.74974 50.09388)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference RN1 (at -2.79654 0.09652) (layer F.SilkS))
    (fp_text value 10K (at 0 1.65) (layer F.Fab) hide)
    (fp_text user %R (at -0.0762 2.3876) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 31 "Net-(RN1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5EFB79D2)
    (at 34.74974 52.19954)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference RN2 (at -2.84734 -0.00254) (layer F.SilkS))
    (fp_text value 10K (at 0 1.65) (layer F.Fab) hide)
    (fp_text user %R (at -0.0762 2.3876) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 32 "Net-(RN2-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5EFB79D2)
    (at 34.77514 54.25948)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference RN3 (at -3.07594 0.04572) (layer F.SilkS))
    (fp_text value 10K (at 0 1.65) (layer F.Fab) hide)
    (fp_text user %R (at -0.0762 2.3876) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 33 "Net-(RN3-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5EFB79D2)
    (at 34.77514 56.33974)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference RN4 (at -2.87274 -0.00254) (layer F.SilkS))
    (fp_text value 10K (at 0 1.65) (layer F.Fab) hide)
    (fp_text user %R (at -0.0762 2.3876) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 34 "Net-(RN4-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5EFB79D2)
    (at 34.79292 58.41238)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference RN5 (at -2.89052 -0.01778) (layer F.SilkS))
    (fp_text value 10K (at 0 1.65) (layer F.Fab) hide)
    (fp_text user %R (at -0.0762 2.3876) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 35 "Net-(RN5-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5EFB79D2)
    (at 14.224 58.3438)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference RN6 (at -2.89052 -0.06096) (layer F.SilkS))
    (fp_text value 10K (at 0 1.65) (layer F.Fab) hide)
    (fp_text user %R (at -0.0762 2.3876) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 63 "Net-(RN6-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5EFB79D2)
    (at 34.60242 47.50054)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference RNAUTO1 (at 0.0508 -1.4224) (layer F.SilkS))
    (fp_text value 10K (at 0 1.65) (layer F.Fab) hide)
    (fp_text user %R (at -0.0762 2.3876) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 +3V3))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 49 "Net-(RNAUTO1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5EFB79D2)
    (at 22.16658 39.7764 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference RNDMPR+1 (at -0.4318 1.46558 90) (layer F.SilkS))
    (fp_text value "33 1%" (at 0 1.65 90) (layer F.Fab) hide)
    (fp_text user %R (at -0.0762 2.3876 90) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 64 "Net-(RNDMPR+1-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 11 "Net-(CNRX+1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5EFB79D2)
    (at 24.3078 39.751 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference RNDMPR-1 (at -0.254 -1.397 90) (layer F.SilkS))
    (fp_text value "33 1%" (at 0 1.65 90) (layer F.Fab) hide)
    (fp_text user %R (at -0.0762 2.3876 90) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 43 "Net-(RNDMPR-1-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 14 "Net-(CNRX-1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5EFB79D2)
    (at 27.44216 41.21912 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference RNDMPT+1 (at -4.74472 -0.06604 90) (layer F.SilkS))
    (fp_text value "33 1%" (at 0 1.65 90) (layer F.Fab) hide)
    (fp_text user %R (at -0.0762 2.3876 90) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 65 "Net-(RNDMPT+1-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 53 "Net-(J_RJ45-Pad5)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5EFB79D2)
    (at 29.56052 41.23436 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference RNDMPT-1 (at -4.65836 -0.00508 90) (layer F.SilkS))
    (fp_text value "33 1%" (at 0 1.65 90) (layer F.Fab) hide)
    (fp_text user %R (at -0.0762 2.3876 90) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 44 "Net-(RNDMPT-1-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 54 "Net-(J_RJ45-Pad6)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5EFB79D2)
    (at 34.54654 41.8592)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference RNDUP1 (at 0.0508 -1.4224) (layer F.SilkS))
    (fp_text value 10K (at 0 1.65) (layer F.Fab) hide)
    (fp_text user %R (at -0.0762 2.3876) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 +3V3))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 50 "Net-(RNDUP1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5EFB79D2)
    (at 14.18082 45.20184)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference RNEXR1 (at -3.86842 -0.01524) (layer F.SilkS))
    (fp_text value "12.4K 1%" (at 0 1.65) (layer F.Fab) hide)
    (fp_text user %R (at -0.0762 2.3876) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 36 "Net-(RNEXR1-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 5 GNDA))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5EFB79D2)
    (at 35.01644 64.23152)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference RNINT1 (at 0.0508 1.50368) (layer F.SilkS))
    (fp_text value 10K (at 0 1.65) (layer F.Fab) hide)
    (fp_text user %R (at -0.0762 2.3876) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 +3V3))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 51 "Net-(RNINT1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5EFB79D2)
    (at 33.91154 34.23412 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference RNLACT1 (at -0.09652 1.67894 90) (layer F.SilkS))
    (fp_text value 820 (at 0 1.65 90) (layer F.Fab) hide)
    (fp_text user %R (at -0.0762 2.3876 90) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 37 "Net-(RNLACT1-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 55 "Net-(J_RJ45-Pad12)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5EFB79D2)
    (at 12.6873 21.57222 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference RNLDUP1 (at 0.0508 -1.4224 90) (layer F.SilkS))
    (fp_text value 820 (at 0 1.65 90) (layer F.Fab) hide)
    (fp_text user %R (at -0.0762 2.3876 90) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 38 "Net-(RNLDUP1-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 66 "Net-(L_NDUP1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5EFB79D2)
    (at 36.17468 34.2519 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference RNLNK1 (at 0.0508 -1.4224 90) (layer F.SilkS))
    (fp_text value 820 (at 0 1.65 90) (layer F.Fab) hide)
    (fp_text user %R (at -0.0762 2.3876 90) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 39 "Net-(RNLNK1-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 52 "Net-(J_RJ45-Pad14)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5EFB79D2)
    (at 10.38606 21.57222 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference RNLSPEED1 (at -0.00762 1.44526 90) (layer F.SilkS))
    (fp_text value 820 (at 0 1.65 90) (layer F.Fab) hide)
    (fp_text user %R (at -0.0762 2.3876 90) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 40 "Net-(RNLSPEED1-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 67 "Net-(L_NSPD1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5EFB79D2)
    (at 24.64308 65.4431 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference RNQ1 (at 0.0508 -1.4224) (layer F.SilkS))
    (fp_text value 1Meg (at 0 1.65) (layer F.Fab) hide)
    (fp_text user %R (at -0.0762 2.3876) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 7 "Net-(CNQ1-Pad1)"))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 8 "Net-(CNQ2-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5EFB79D2)
    (at 24.257 35.19932)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference RNRDN1 (at 0.1778 -1.51892) (layer F.SilkS))
    (fp_text value "49.9 1%" (at 0 1.65) (layer F.Fab) hide)
    (fp_text user %R (at -0.0762 2.3876) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 9 "Net-(CNRD1-Pad1)"))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 14 "Net-(CNRX-1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5EFB79D2)
    (at 20.32762 35.07486)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference RNRDP1 (at -0.26162 -1.47066) (layer F.SilkS))
    (fp_text value "49.9 1%" (at 0 1.65) (layer F.Fab) hide)
    (fp_text user %R (at -0.0762 2.3876) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 11 "Net-(CNRX+1-Pad1)"))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 9 "Net-(CNRD1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5EFB79D2)
    (at 24.3332 70.7898 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference RNRES1 (at -0.0762 1.3208 90) (layer F.SilkS))
    (fp_text value 10K (at 0 1.65 90) (layer F.Fab) hide)
    (fp_text user %R (at -0.0762 2.3876 90) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 89 PB13-D4-NET_RES))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5EFB79D2)
    (at 34.94278 61.99886)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference RNRESET1 (at 0.0508 -1.4224) (layer F.SilkS))
    (fp_text value 10K (at 0 1.65) (layer F.Fab) hide)
    (fp_text user %R (at -0.0762 2.3876) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 +3V3))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 79 /NETRST))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5EFB79D2)
    (at 34.56686 44.67098)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference RNSPD1 (at 0.0508 -1.4224) (layer F.SilkS))
    (fp_text value 10K (at 0 1.65) (layer F.Fab) hide)
    (fp_text user %R (at -0.0762 2.3876) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 +3V3))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 41 "Net-(RNSPD1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5EFB79D2)
    (at 16.20012 23.53056)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference RNTCT1 (at 0.36068 -1.40716) (layer F.SilkS))
    (fp_text value "10 1%" (at 0 1.65) (layer F.Fab) hide)
    (fp_text user %R (at -0.0762 2.3876) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 15 "Net-(CNTCT1-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5EFB79D2)
    (at 29.84246 31.55442)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference RNTXN1 (at 0.12954 -1.48082) (layer F.SilkS))
    (fp_text value "49.9 1%" (at 0 1.65) (layer F.Fab) hide)
    (fp_text user %R (at -0.0762 2.3876) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 +3V3))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 54 "Net-(J_RJ45-Pad6)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5EFB79D2)
    (at 25.9334 31.60268)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference RNTXP1 (at -0.3556 -1.50368) (layer F.SilkS))
    (fp_text value "49.9 1%" (at 0 1.65) (layer F.Fab) hide)
    (fp_text user %R (at -0.0762 2.3876) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 53 "Net-(J_RJ45-Pad5)"))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5EFB79D2)
    (at 45.43298 66.77406 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference RPOE2 (at 0.0508 -1.4224 90) (layer F.SilkS))
    (fp_text value "100K 1%" (at 0 1.65 90) (layer F.Fab) hide)
    (fp_text user %R (at -0.0762 2.3876 90) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 16 "Net-(CPCC1-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 18 /PV3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5EFB79D2)
    (at 49.16424 40.31234)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference RPCLA1 (at 0.0508 -1.4224) (layer F.SilkS))
    (fp_text value "124 0.1%" (at 0 1.65) (layer F.Fab) hide)
    (fp_text user %R (at -0.0762 2.3876) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 29 /RCLASS))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 22 /VPORTN))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5EFB79D2)
    (at 57.9374 69.7738)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference RPFIL1 (at 0.3556 1.5494) (layer F.SilkS))
    (fp_text value "10 OHM" (at 0 1.65) (layer F.Fab) hide)
    (fp_text user %R (at -0.0762 2.3876) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 19 "Net-(CPFIL1-Pad1)"))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 70 "Net-(D_PDS1040-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5EFB79D2)
    (at 45.43298 62.43574 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference RPLIM1 (at 0.0508 -1.4224 90) (layer F.SilkS))
    (fp_text value "470 0.1%" (at 0 1.65 90) (layer F.Fab) hide)
    (fp_text user %R (at -0.0762 2.3876 90) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 18 /PV3))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 48 "Net-(PS2911-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5EFAE2BE)
    (at 54.02834 38.99154 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference RPOE4 (at -0.55626 1.57734) (layer F.SilkS))
    (fp_text value "10 OHM 1%" (at 0 1.82) (layer F.Fab) hide)
    (fp_text user %R (at -0.127 2.4892) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0 180) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 21 /VPORTP))
    (pad 1 smd roundrect (at -1.4875 0 180) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 27 /PLUS))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5EFB79D2)
    (at 55.68188 48.90008 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference RPOR1 (at 0.0508 -1.4224 90) (layer F.SilkS))
    (fp_text value "10K 1%" (at 0 1.65 90) (layer F.Fab) hide)
    (fp_text user %R (at -0.0762 2.3876 90) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 23 /PVCC))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 21 /VPORTP))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5EFB79D2)
    (at 25.3746 77.6732 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference RPLED1 (at 0 1.524) (layer F.SilkS))
    (fp_text value 330 (at 0 1.65) (layer F.Fab) hide)
    (fp_text user %R (at -0.0762 2.3876) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 68 "Net-(L_PLED1-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 18 /PV3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5EFB79D2)
    (at 41.90492 52.92344 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference RPPVC1 (at 0.01016 1.77292 90) (layer F.SilkS))
    (fp_text value "6.8K 1%" (at 0 1.65 90) (layer F.Fab) hide)
    (fp_text user %R (at -0.0762 2.3876 90) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 69 "Net-(D_PBAS1-Pad1)"))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 23 /PVCC))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5EFB79D2)
    (at 41.783 44.3865 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference RPRSL1 (at 0.3683 -1.4732 90) (layer F.SilkS))
    (fp_text value "10K 1%" (at 0 1.65 90) (layer F.Fab) hide)
    (fp_text user %R (at -0.0762 2.3876 90) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 30 /SENSE))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 42 /SEN))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5EFAE2BE)
    (at 44.72432 53.86324 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference RPSEN1 (at 0.90424 -1.41732 90) (layer F.SilkS))
    (fp_text value "0.1 OHM 1%" (at 0 1.82 90) (layer F.Fab) hide)
    (fp_text user %R (at -0.127 2.4892 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0 90) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 42 /SEN))
    (pad 1 smd roundrect (at -1.4875 0 90) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 20 GNDREF))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_QFP:TQFP-48_7x7mm_P0.5mm (layer F.Cu) (tedit 5EFBB90C)
    (at 23.5077 52.92852 270)
    (descr "48 LEAD TQFP 7x7mm (see MICREL TQFP7x7-48LD-PL-1.pdf)")
    (tags "QFP 0.5")
    (attr smd)
    (fp_text reference U_W5500 (at 0.0254 -5.715 90) (layer F.SilkS))
    (fp_text value W5500 (at 0 6 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 48 smd rect (at -2.75 -4.35) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 5 GNDA))
    (pad 47 smd rect (at -2.25 -4.35) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(U_W5500-Pad47)"))
    (pad 46 smd rect (at -1.75 -4.35) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 57 "Net-(U_W5500-Pad46)"))
    (pad 45 smd rect (at -1.25 -4.35) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(RNDUP1-Pad1)"))
    (pad 44 smd rect (at -0.75 -4.35) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(RNSPD1-Pad1)"))
    (pad 43 smd rect (at -0.25 -4.35) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(RNAUTO1-Pad1)"))
    (pad 42 smd rect (at 0.25 -4.35) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(RN1-Pad1)"))
    (pad 41 smd rect (at 0.75 -4.35) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(RN2-Pad1)"))
    (pad 40 smd rect (at 1.25 -4.35) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(RN3-Pad1)"))
    (pad 39 smd rect (at 1.75 -4.35) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(RN4-Pad1)"))
    (pad 38 smd rect (at 2.25 -4.35) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(RN5-Pad1)"))
    (pad 37 smd rect (at 2.75 -4.35) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 79 /NETRST))
    (pad 36 smd rect (at 4.35 -2.75 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(RNINT1-Pad1)"))
    (pad 35 smd rect (at 4.35 -2.25 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 86 PA12-MOSI))
    (pad 34 smd rect (at 4.35 -1.75 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 80 /NET-MISO))
    (pad 33 smd rect (at 4.35 -1.25 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 88 PA13-SCK))
    (pad 32 smd rect (at 4.35 -0.75 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 90 PB14-D5-NET_CS))
    (pad 31 smd rect (at 4.35 -0.25 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(CNQ2-Pad1)"))
    (pad 30 smd rect (at 4.35 0.25 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(CNQ1-Pad1)"))
    (pad 29 smd rect (at 4.35 0.75 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 28 smd rect (at 4.35 1.25 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 27 smd rect (at 4.35 1.75 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(RNLACT1-Pad2)"))
    (pad 26 smd rect (at 4.35 2.25 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(RNLDUP1-Pad2)"))
    (pad 25 smd rect (at 4.35 2.75 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(RNLNK1-Pad2)"))
    (pad 24 smd rect (at 2.75 4.35) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(RNLSPEED1-Pad2)"))
    (pad 23 smd rect (at 2.25 4.35) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(RN6-Pad2)"))
    (pad 22 smd rect (at 1.75 4.35) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(CN22-Pad2)"))
    (pad 21 smd rect (at 1.25 4.35) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3.3VP))
    (pad 20 smd rect (at 0.75 4.35) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 62 "Net-(CN20-Pad2)"))
    (pad 19 smd rect (at 0.25 4.35) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 5 GNDA))
    (pad 18 smd rect (at -0.25 4.35) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 58 "Net-(U_W5500-Pad18)"))
    (pad 17 smd rect (at -0.75 4.35) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3.3VP))
    (pad 16 smd rect (at -1.25 4.35) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 5 GNDA))
    (pad 15 smd rect (at -1.75 4.35) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3.3VP))
    (pad 14 smd rect (at -2.25 4.35) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 5 GNDA))
    (pad 13 smd rect (at -2.75 4.35) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 59 "Net-(U_W5500-Pad13)"))
    (pad 12 smd rect (at -4.35 2.75 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 60 "Net-(U_W5500-Pad12)"))
    (pad 11 smd rect (at -4.35 2.25 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3.3VP))
    (pad 10 smd rect (at -4.35 1.75 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(RNEXR1-Pad2)"))
    (pad 9 smd rect (at -4.35 1.25 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 5 GNDA))
    (pad 8 smd rect (at -4.35 0.75 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3.3VP))
    (pad 7 smd rect (at -4.35 0.25 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 61 "Net-(U_W5500-Pad7)"))
    (pad 6 smd rect (at -4.35 -0.25 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(RNDMPR+1-Pad2)"))
    (pad 5 smd rect (at -4.35 -0.75 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(RNDMPR-1-Pad2)"))
    (pad 4 smd rect (at -4.35 -1.25 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3.3VP))
    (pad 3 smd rect (at -4.35 -1.75 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 5 GNDA))
    (pad 2 smd rect (at -4.35 -2.25 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 65 "Net-(RNDMPT+1-Pad2)"))
    (pad 1 smd rect (at -4.35 -2.75 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(RNDMPT-1-Pad2)"))
    (model ${KISYS3DMOD}/Package_QFP.3dshapes/TQFP-48_7x7mm_P0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Jumper:SolderJumper-2_P1.3mm_Open_Pad1.0x1.5mm (layer B.Cu) (tedit 5EFBBB13)
    (at 35.702 47.31258)
    (descr "SMD Solder Jumper, 1x1.5mm Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference SP_AUTO1 (at -0.72644 1.73482) (layer B.SilkS))
    (fp_text value S_AUTO (at 0 -1.9) (layer B.Fab) hide)
    (pad 1 smd rect (at -0.65 0) (size 1 1.5) (layers B.Cu B.Mask)
      (net 49 "Net-(RNAUTO1-Pad1)"))
    (pad 2 smd rect (at 0.65 0) (size 1 1.5) (layers B.Cu B.Mask)
      (net 1 GND))
  )
  (module Jumper:SolderJumper-2_P1.3mm_Open_Pad1.0x1.5mm (layer B.Cu) (tedit 5EFBBB13)
    (at 36.04514 40.19296)
    (descr "SMD Solder Jumper, 1x1.5mm Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference SP_DUPLEX1 (at -0.73914 1.71704) (layer B.SilkS))
    (fp_text value S_DUPLEX (at 0 -1.9) (layer B.Fab) hide)
    (pad 1 smd rect (at -0.65 0) (size 1 1.5) (layers B.Cu B.Mask)
      (net 50 "Net-(RNDUP1-Pad1)"))
    (pad 2 smd rect (at 0.65 0) (size 1 1.5) (layers B.Cu B.Mask)
      (net 1 GND))
  )
  (module Jumper:SolderJumper-2_P1.3mm_Open_Pad1.0x1.5mm (layer B.Cu) (tedit 5EFBBB13)
    (at 21.082 5.4102 180)
    (descr "SMD Solder Jumper, 1x1.5mm Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference SP_POEN1 (at -1.143 1.7272) (layer B.SilkS))
    (fp_text value S_POEN (at 0 -1.9) (layer B.Fab) hide)
    (pad 1 smd rect (at -0.65 0 180) (size 1 1.5) (layers B.Cu B.Mask)
      (net 25 /NN))
    (pad 2 smd rect (at 0.65 0 180) (size 1 1.5) (layers B.Cu B.Mask)
      (net 22 /VPORTN))
  )
  (module Jumper:SolderJumper-2_P1.3mm_Open_Pad1.0x1.5mm (layer B.Cu) (tedit 5EFBBB13)
    (at 15.7226 5.334)
    (descr "SMD Solder Jumper, 1x1.5mm Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference SP_POEP1 (at -1.1938 -1.7018) (layer B.SilkS))
    (fp_text value S_POEP (at 0 -1.9) (layer B.Fab) hide)
    (pad 1 smd rect (at -0.65 0) (size 1 1.5) (layers B.Cu B.Mask)
      (net 26 /PP))
    (pad 2 smd rect (at 0.65 0) (size 1 1.5) (layers B.Cu B.Mask)
      (net 27 /PLUS))
  )
  (module Jumper:SolderJumper-2_P1.3mm_Open_Pad1.0x1.5mm (layer B.Cu) (tedit 5EFBBB13)
    (at 36.02736 43.77944)
    (descr "SMD Solder Jumper, 1x1.5mm Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference SP_SPEED1 (at -0.41656 1.71196) (layer B.SilkS))
    (fp_text value S_SPEED (at 0 -1.9) (layer B.Fab) hide)
    (pad 1 smd rect (at -0.65 0) (size 1 1.5) (layers B.Cu B.Mask)
      (net 41 "Net-(RNSPD1-Pad1)"))
    (pad 2 smd rect (at 0.65 0) (size 1 1.5) (layers B.Cu B.Mask)
      (net 1 GND))
  )
  (module Capacitor_Tantalum_SMD:CP_EIA-3216-18_Kemet-A_Pad1.58x1.35mm_HandSolder (layer F.Cu) (tedit 5EFA9D23)
    (at 13.208 63.27394 270)
    (descr "Tantalum Capacitor SMD Kemet-A (3216-18 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator")
    (tags "capacitor tantalum")
    (attr smd)
    (fp_text reference C28A1 (at -0.45974 1.6256 90) (layer F.SilkS))
    (fp_text value "10uf TANT" (at -0.0254 1.4732 90) (layer F.Fab) hide)
    (fp_text user %R (at -0.0254 2.4384 90) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1.4375 0 270) (size 1.575 1.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.185185)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.4375 0 270) (size 1.575 1.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.185185)
      (net 2 +3V3))
    (model ${KISYS3DMOD}/Capacitor_Tantalum_SMD.3dshapes/CP_EIA-3216-18_Kemet-A.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_Tantalum_SMD:CP_EIA-3216-18_Kemet-A_Pad1.58x1.35mm_HandSolder (layer F.Cu) (tedit 5EFA9D23)
    (at 14.97584 41.0972 180)
    (descr "Tantalum Capacitor SMD Kemet-A (3216-18 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator")
    (tags "capacitor tantalum")
    (attr smd)
    (fp_text reference CNW6 (at 4.02844 0.0508) (layer F.SilkS))
    (fp_text value "10uf TANT" (at -0.0254 1.4732) (layer F.Fab) hide)
    (fp_text user %R (at -0.0254 2.4384) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1.4375 0 180) (size 1.575 1.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.185185)
      (net 5 GNDA))
    (pad 1 smd roundrect (at -1.4375 0 180) (size 1.575 1.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.185185)
      (net 4 +3.3VP))
    (model ${KISYS3DMOD}/Capacitor_Tantalum_SMD.3dshapes/CP_EIA-3216-18_Kemet-A.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Jumper:SolderJumper-2_P1.3mm_Open_Pad1.0x1.5mm (layer B.Cu) (tedit 5EFBBB13)
    (at 20.3708 76.5556 180)
    (descr "SMD Solder Jumper, 1x1.5mm Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference SP_POELED1 (at 0 1.8) (layer B.SilkS))
    (fp_text value S_ENBUZ (at 0 -1.9) (layer B.Fab) hide)
    (pad 1 smd rect (at -0.65 0 180) (size 1 1.5) (layers B.Cu B.Mask)
      (net 71 "Net-(L_PLED1-Pad1)"))
    (pad 2 smd rect (at 0.65 0 180) (size 1 1.5) (layers B.Cu B.Mask)
      (net 1 GND))
  )
  (module Jumper:SolderJumper-2_P1.3mm_Open_Pad1.0x1.5mm (layer B.Cu) (tedit 5EFBBB13)
    (at 18.2372 67.9704 180)
    (descr "SMD Solder Jumper, 1x1.5mm Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference SP_NET_INT9 (at 0 1.8) (layer B.SilkS))
    (fp_text value S_NETINT (at 0 -1.9) (layer B.Fab) hide)
    (pad 1 smd rect (at -0.65 0 180) (size 1 1.5) (layers B.Cu B.Mask)
      (net 51 "Net-(RNINT1-Pad1)"))
    (pad 2 smd rect (at 0.65 0 180) (size 1 1.5) (layers B.Cu B.Mask)
      (net 93 PB15-D6-NET_INT))
  )
  (module Jumper:SolderJumper-2_P1.3mm_Open_Pad1.0x1.5mm (layer B.Cu) (tedit 5EFBBB13)
    (at 34.544 66.548 270)
    (descr "SMD Solder Jumper, 1x1.5mm Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference SP_N_HARDRESET_1 (at 0.4572 -2.4384 90) (layer B.SilkS))
    (fp_text value S_N_HARDRESET (at 0 -1.9 90) (layer B.Fab) hide)
    (pad 1 smd rect (at -0.65 0 270) (size 1 1.5) (layers B.Cu B.Mask)
      (net 79 /NETRST))
    (pad 2 smd rect (at 0.65 0 270) (size 1 1.5) (layers B.Cu B.Mask)
      (net 75 "Net-(SP_N_HARDRESET_1-Pad2)"))
  )
  (module Jumper:SolderJumper-2_P1.3mm_Open_Pad1.0x1.5mm (layer B.Cu) (tedit 5EFBBB13)
    (at 32.004 66.548 270)
    (descr "SMD Solder Jumper, 1x1.5mm Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference SP_N_SOFTRESET_1 (at 0.4826 1.9304 90) (layer B.SilkS))
    (fp_text value S_N_SOFTRESET (at 0 -1.9 90) (layer B.Fab) hide)
    (pad 1 smd rect (at -0.65 0 270) (size 1 1.5) (layers B.Cu B.Mask)
      (net 79 /NETRST))
    (pad 2 smd rect (at 0.65 0 270) (size 1 1.5) (layers B.Cu B.Mask)
      (net 76 "Net-(SP_N_SOFTRESET_1-Pad2)"))
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5EFB79E5)
    (at 17.9578 71.0946)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference CNMISO1 (at -0.0254 1.6256) (layer F.SilkS))
    (fp_text value 0.1uf (at 0 1.65) (layer F.Fab) hide)
    (fp_text user %R (at 0.0508 2.3876) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5EFB79D2)
    (at 17.9324 68.9864)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference RNCS1 (at 0.0254 -1.397) (layer F.SilkS))
    (fp_text value 10K (at 0 1.65) (layer F.Fab) hide)
    (fp_text user %R (at -0.0762 2.3876) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 +3V3))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 90 PB14-D5-NET_CS))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23-5_HandSoldering (layer F.Cu) (tedit 5EFBBE5C)
    (at 12.446 70.0532)
    (descr "5-pin SOT23 package")
    (tags "SOT-23-5 hand-soldering")
    (attr smd)
    (fp_text reference U_74G1NCS1 (at -0.1778 -2.5908) (layer F.SilkS))
    (fp_text value SN74LVC1G125DBVR (at 0.0254 2.3622) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 5 smd rect (at 1.35 -0.95) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 4 smd rect (at 1.35 0.95) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 87 PA14-MISO))
    (pad 3 smd rect (at -1.35 0.95) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -1.35 0) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 80 /NET-MISO))
    (pad 1 smd rect (at -1.35 -0.95) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 90 PB14-D5-NET_CS))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x10_P2.54mm_Vertical (layer F.Cu) (tedit 5EFBBED5)
    (at 2.54 40.64)
    (descr "Through hole straight pin header, 2x10, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x10 2.54mm double row")
    (fp_text reference JTO_CPU1 (at 1.2954 25.527) (layer F.SilkS))
    (fp_text value Conn_02x10_Odd_Even (at 5.0546 11.7856 90) (layer F.Fab) hide)
    (fp_text user %R (at -2.667 11.0998 90) (layer F.Fab) hide)
    (pad 20 thru_hole oval (at 2.54 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 72 +3V0))
    (pad 19 thru_hole oval (at 0 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 72 +3V0))
    (pad 18 thru_hole oval (at 2.54 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 17 thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 16 thru_hole oval (at 2.54 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 83 /SDA))
    (pad 15 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 85 /PA04-D17))
    (pad 14 thru_hole oval (at 2.54 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 ~RESET~))
    (pad 13 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 84 /SCL))
    (pad 12 thru_hole oval (at 2.54 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 86 PA12-MOSI))
    (pad 11 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 93 PB15-D6-NET_INT))
    (pad 10 thru_hole oval (at 2.54 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 87 PA14-MISO))
    (pad 9 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 88 PA13-SCK))
    (pad 8 thru_hole oval (at 2.54 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 89 PB13-D4-NET_RES))
    (pad 7 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 90 PB14-D5-NET_CS))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 91 /PA22-D1))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 92 /PA23-D0))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 +3V3))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 +3V3))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x10_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_3.2mm_M3_Pad (layer F.Cu) (tedit 5EFA97D2)
    (at 5.08 77.47 90)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (attr virtual)
    (fp_text reference MPOE3 (at 0 -4.2 90) (layer F.SilkS) hide)
    (fp_text value MPOE3 (at 0 4.2 90) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask)
      (net 77 "Net-(MPOE3-Pad1)"))
  )
  (module MountingHole:MountingHole_3.2mm_M3_Pad (layer F.Cu) (tedit 5EFA97D2)
    (at 5.08 5.08 90)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (attr virtual)
    (fp_text reference MPOE4 (at 0 -4.2 90) (layer F.SilkS) hide)
    (fp_text value MPOE4 (at 0 4.2 90) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask)
      (net 78 "Net-(MPOE4-Pad1)"))
  )
  (module min51j:RJ45_Wuerth_7499211121A_Horizontal (layer F.Cu) (tedit 5DC67AA1)
    (at 28.448 13.716 270)
    (descr "10/100Base-TX RJ45 ethernet magnetic transformer connector horizontal https://katalog.we-online.de/pbs/datasheet/7499010121A.pdf")
    (tags "RJ45 ethernet magnetic")
    (fp_text reference J_RJ45 (at -8.9 8.6) (layer F.SilkS))
    (fp_text value Wuerth_7499211121A (at 9.8 4.65) (layer F.Fab) hide)
    (fp_text user %R (at 0.05 0.05 180) (layer F.Fab) hide)
    (pad 12 thru_hole circle (at 4.09 -4.08 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 55 "Net-(J_RJ45-Pad12)"))
    (pad 9 thru_hole circle (at -4.445 8.89 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 26 /PP))
    (pad 11 thru_hole circle (at 6.661 -4.08 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 +3V3))
    (pad 10 thru_hole circle (at -5.715 6.35 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 25 /NN))
    (pad 16 thru_hole circle (at 7.745 3.05 90) (size 2.4 2.4) (drill 1.6) (layers *.Cu *.Mask)
      (net 10 GNDPWR))
    (pad 15 thru_hole circle (at -7.745 3.05 90) (size 2.4 2.4) (drill 1.6) (layers *.Cu *.Mask)
      (net 10 GNDPWR))
    (pad "" np_thru_hole circle (at 5.715 0 90) (size 3.250001 3.250001) (drill 3.250001) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -5.715 0 90) (size 3.250001 3.250001) (drill 3.250001) (layers *.Cu *.Mask))
    (pad 8 thru_hole circle (at -3.175 6.35 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask))
    (pad 7 thru_hole circle (at -1.905 8.89 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask))
    (pad 6 thru_hole circle (at -0.635 6.35 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 54 "Net-(J_RJ45-Pad6)"))
    (pad 5 thru_hole circle (at 0.635 8.89 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 53 "Net-(J_RJ45-Pad5)"))
    (pad 4 thru_hole circle (at 1.905 6.35 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 15 "Net-(CNTCT1-Pad2)"))
    (pad 3 thru_hole circle (at 3.175 8.89 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 9 "Net-(CNRD1-Pad1)"))
    (pad 2 thru_hole circle (at 4.445 6.35 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 13 "Net-(CNRX-1-Pad1)"))
    (pad 1 thru_hole roundrect (at 5.715 8.89 90) (size 1.2 1.6) (drill 0.7) (layers *.Cu *.Mask) (roundrect_rratio 0.155)
      (net 12 "Net-(CNRX+1-Pad2)"))
    (pad 13 thru_hole circle (at -4.09 -4.08) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 +3V3))
    (pad 14 thru_hole circle (at -6.661 -4.08) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 52 "Net-(J_RJ45-Pad14)"))
    (model ${KISYS3DMOD}/Connector_RJ.3dshapes/RJ45_Wuerth_7499010121A_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module min51j:PA1133 (layer F.Cu) (tedit 5EFAE107)
    (at 56.261 61.341 270)
    (fp_text reference PA1133-coil1 (at 5.46608 0.42418) (layer F.SilkS))
    (fp_text value PA1133NLT (at -5.461 -0.6858) (layer F.Fab))
    (pad 1 smd rect (at 3.75 6.6 270) (size 1.27 2.54) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(PA1133-coil1-Pad1)"))
    (pad 2 smd rect (at 1.25 6.6 270) (size 1.27 2.54) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(PA1133-coil1-Pad2)"))
    (pad 3 smd rect (at -1.25 6.6 270) (size 1.27 2.54) (layers F.Cu F.Paste F.Mask)
      (net 21 /VPORTP))
    (pad 4 smd rect (at -3.75 6.6 270) (size 1.27 2.54) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(PA1133-coil1-Pad4)"))
    (pad 8 smd rect (at 3.75 -6.6 270) (size 1.27 2.54) (layers F.Cu F.Paste F.Mask)
      (net 70 "Net-(D_PDS1040-Pad2)"))
    (pad 7 smd rect (at 1.25 -6.6 270) (size 1.27 2.54) (layers F.Cu F.Paste F.Mask)
      (net 70 "Net-(D_PDS1040-Pad2)"))
    (pad 6 smd rect (at -1.25 -6.6 270) (size 1.27 2.54) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at -3.75 -6.6 270) (size 1.27 2.54) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module min51j:PS2911 (layer F.Cu) (tedit 5EFAE12E)
    (at 41.656 59.309)
    (fp_text reference PS2911 (at 0.2286 -3.5306) (layer F.SilkS))
    (fp_text value PS2911-1-F3-AX (at 0.6096 3.6068) (layer F.Fab) hide)
    (pad 4 smd rect (at -0.64 -2.35) (size 0.8 1) (layers F.Cu F.Paste F.Mask)
      (net 69 "Net-(D_PBAS1-Pad1)"))
    (pad 3 smd rect (at 0.64 -2.35) (size 0.8 1) (layers F.Cu F.Paste F.Mask)
      (net 20 GNDREF))
    (pad 1 smd rect (at -0.64 2.35) (size 0.8 1) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(PS2911-Pad1)"))
    (pad 2 smd rect (at 0.54 2.35) (size 0.8 1) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(CPCC1-Pad1)"))
  )
  (gr_text ~RST (at 7.28726 48.2727) (layer F.SilkS))
  (gr_text ~CS (at 0.7112 48.34382) (layer F.SilkS))
  (gr_text "W5500 is 3.3 volts only.\nDo not use 5 volts." (at 4.0132 18.2626 90) (layer B.SilkS))
  (gr_text "|- SAMD51J Pin ID’s -|" (at 7.1882 33.02 90) (layer F.SilkS))
  (gr_text "3V3 3V3\nGND GND\nPA23 PA22\nPB14 PB13\nSCK MISO\nPB15 MOSI\n SCL ~RESET~\nPA04 SDA\nGND GND\n3POE 3POE" (at 3.67538 33.14446) (layer F.SilkS))
  (gr_text "W5500 is 3.3 volts only.\nDo not use 5 volts." (at 3.7592 17.907 90) (layer F.SilkS))
  (gr_text "Network ~CS~\nPB14 D5" (at 33.147 56.769) (layer B.SilkS))
  (gr_text "PoE diodes are\nin the RJ45 Socket" (at 48.387 27.2542) (layer F.SilkS))
  (gr_text "Network Hardware reset\nvia Hardware reset button" (at 40.22598 67.28714 90) (layer B.SilkS))
  (gr_text "Network Hardware\nreset via software" (at 26.162 66.675 90) (layer B.SilkS))
  (gr_text "Network Reset" (at 33.4518 60.6806) (layer B.SilkS))
  (gr_text "PA09\nD3" (at 18.2372 70.3072) (layer B.SilkS))
  (gr_text "24 Aug 2020" (at 24.13 39.51224) (layer B.SilkS))
  (gr_text "Mini51jNet Ver 01a" (at 24.86152 34.86404) (layer B.SilkS))
  (gr_line (start 37.592 0) (end 37.592 25.4) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 37.592 25.4) (end 66.04 25.4) (layer Edge.Cuts) (width 0.05))
  (gr_text "RJ45 10/100 Socket\nwith PoE Diodes" (at 35.9664 13.7668 90) (layer F.SilkS))
  (gr_text "Input: Active PoE ~~48V\nOutput: 3.3V at Appr 600ma" (at 49.5808 31.2166) (layer F.SilkS))
  (gr_text RJ45 (at 28.44292 12.62634) (layer B.SilkS))
  (gr_text ~RESET (at 34.62274 70.23862 90) (layer B.SilkS))
  (gr_text "PB13\nD4" (at 32.00146 69.65696 90) (layer B.SilkS))
  (gr_text DUPLEX (at 34.5186 4.1656) (layer F.SilkS))
  (gr_text SPEED (at 33.9852 1.905) (layer F.SilkS))
  (gr_text "3V PoE\nPower" (at 18.2372 76.4032) (layer F.SilkS))
  (gr_line (start 0 82.55) (end 0 0) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 66.04 82.55) (end 0 82.55) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 66.04 25.4) (end 66.04 82.55) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 0 0) (end 37.592 0) (layer Edge.Cuts) (width 0.05))
  (zone (net 20) (net_name GNDREF) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2032))
    (min_thickness 0.2286)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.254))
    (polygon
      (pts
        (xy 66.559827 33.133824) (xy 66.866728 59.001646) (xy 39.864072 58.854354) (xy 39.5732 32.9438)
      )
    )
  )
  (zone (net 20) (net_name GNDREF) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2032))
    (min_thickness 0.2286)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.254))
    (polygon
      (pts
        (xy 66.671508 33.15716) (xy 66.898044 58.95848) (xy 39.832756 58.89752) (xy 39.564945 33.14446)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2032))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.381) (thermal_bridge_width 0.381))
    (polygon
      (pts
        (xy 39.056112 -1.039079) (xy 39.188172 82.865962) (xy -0.173772 82.894438) (xy -0.120412 -0.922973)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2032))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.381) (thermal_bridge_width 0.381))
    (polygon
      (pts
        (xy 38.959512 -0.428876) (xy 39.096692 83.107107) (xy -0.183892 82.856493) (xy -0.085487 -0.750927)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.2032))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 88.824027 32.810977) (xy 91.395777 32.799547) (xy 91.401175 37.17057) (xy 88.81863 37.162315)
      )
    )
  )
  (zone (net 0) (net_name "") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2032))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 23.521353 10.204292) (xy 14.068108 10.186829) (xy 14.070013 -0.224949) (xy 38.1 -0.254) (xy 38.1 25.146)
        (xy 39.878 25.146) (xy 39.878 32.004) (xy 34.626233 27.8638) (xy 34.629408 4.141788) (xy 23.524528 4.111149)
      )
    )
  )
  (zone (net 0) (net_name "") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2032))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 67.31 59.436) (xy 67.183 51.054) (xy 60.833 51.054) (xy 60.96 59.436)
      )
    )
  )
)
