(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 120)
    (no_connects 0)
    (area 20.879999 20.977 120.620001 109.631)
    (thickness 1.6)
    (drawings 8)
    (tracks 477)
    (zones 0)
    (modules 47)
    (nets 35)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 1)
    (trace_clearance 0.6)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 0.000001 0.000001)
    (mod_text_width 0.15)
    (pad_size 1.75 1.75)
    (pad_drill 0.8)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin true)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory K:/YOU_TUBE/DC_Voltage_Calibrator_Part3/DC_Cal_main_PCB_Gerber_Files/))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(C2-Pad1)")
  (net 3 "Net-(C2-Pad2)")
  (net 4 "Net-(C3-Pad1)")
  (net 5 "Net-(C7-Pad2)")
  (net 6 "Net-(C14-Pad1)")
  (net 7 +5V)
  (net 8 +4.096V)
  (net 9 "Net-(D1-Pad2)")
  (net 10 "Net-(J1-Pad3)")
  (net 11 "Net-(J3-Pad1)")
  (net 12 "Net-(J4-Pad2)")
  (net 13 "Net-(J5-Pad1)")
  (net 14 "Net-(RV1-Pad2)")
  (net 15 "Net-(U1-Pad5)")
  (net 16 A4)
  (net 17 "Net-(U2-Pad3)")
  (net 18 A2)
  (net 19 A3)
  (net 20 A1)
  (net 21 A0)
  (net 22 -15V)
  (net 23 +15V)
  (net 24 Vref)
  (net 25 "Net-(J7-Pad6)")
  (net 26 "Net-(J7-Pad7)")
  (net 27 "Net-(J7-Pad8)")
  (net 28 +1.024V)
  (net 29 "Net-(U1-Pad1)")
  (net 30 "Net-(U5-Pad2)")
  (net 31 "Net-(D2-Pad2)")
  (net 32 "Net-(JP1-Pad1)")
  (net 33 "Net-(JP1-Pad2)")
  (net 34 "Net-(D1-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.6)
    (trace_width 1)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +1.024V)
    (add_net +15V)
    (add_net +4.096V)
    (add_net +5V)
    (add_net -15V)
    (add_net A0)
    (add_net A1)
    (add_net A2)
    (add_net A3)
    (add_net A4)
    (add_net GND)
    (add_net "Net-(C14-Pad1)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C2-Pad2)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C7-Pad2)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J3-Pad1)")
    (add_net "Net-(J4-Pad2)")
    (add_net "Net-(J5-Pad1)")
    (add_net "Net-(J7-Pad6)")
    (add_net "Net-(J7-Pad7)")
    (add_net "Net-(J7-Pad8)")
    (add_net "Net-(JP1-Pad1)")
    (add_net "Net-(JP1-Pad2)")
    (add_net "Net-(RV1-Pad2)")
    (add_net "Net-(U1-Pad1)")
    (add_net "Net-(U1-Pad5)")
    (add_net "Net-(U2-Pad3)")
    (add_net "Net-(U5-Pad2)")
    (add_net Vref)
  )
  (module Wire_Connections_Bridges:WireConnection_0.80mmDrill (layer F.Cu) (tedit 5A440525)
    (at 113.284 43.1165 180)
    (descr "WireConnection with 0.8mm drill")
    (fp_text reference -----JP1----- (at 4.8514 0.2032 180) (layer F.SilkS))
    (fp_text value Jumper (at 5.715 0.4445 180) (layer F.Fab))
    (pad 1 thru_hole circle (at -2.54 0 180) (size 2 2) (drill 0.8001) (layers *.Cu *.Mask)
      (net 32 "Net-(JP1-Pad1)"))
    (pad 2 thru_hole circle (at 12.7 0 180) (size 2 2) (drill 0.8001) (layers *.Cu *.Mask)
      (net 33 "Net-(JP1-Pad2)"))
  )
  (module Capacitors_THT:CP_Radial_D5.0mm_P2.00mm (layer F.Cu) (tedit 5A44077D)
    (at 51.435 71.247 180)
    (descr "CP, Radial series, Radial, pin pitch=2.00mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.00mm  diameter 5mm Electrolytic Capacitor")
    (fp_text reference C2 (at -3.302 0.0635 180) (layer F.SilkS))
    (fp_text value 22uF (at 1 3.81 180) (layer F.Fab))
    (fp_text user %R (at 1 0 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 2.4) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(C2-Pad1)"))
    (pad 2 thru_hole oval (at 2 0 180) (size 1.6 2.4) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C2-Pad2)"))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D5.0mm_P2.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:CP_Radial_D8.0mm_P5.00mm (layer F.Cu) (tedit 5A353D55)
    (at 38.9255 78.0415 90)
    (descr "CP, Radial series, Radial, pin pitch=5.00mm, , diameter=8mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 5.00mm  diameter 8mm Electrolytic Capacitor")
    (fp_text reference C3 (at 2.5 -5.31 90) (layer F.SilkS))
    (fp_text value 220uF (at 2.7305 3.3655 90) (layer F.Fab))
    (fp_text user %R (at 2.5 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (pad 2 thru_hole circle (at 5 0 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D8.0mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Rect_L7.0mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 5A353D7D)
    (at 83.312 75.438 180)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7*2.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7mm width 2.5mm Capacitor")
    (fp_text reference C4 (at 2.5 -2.56 180) (layer F.SilkS))
    (fp_text value 100nF (at 2.413 -2.7305 180) (layer F.Fab))
    (fp_text user %R (at 2.5 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 -15V))
    (pad 2 thru_hole circle (at 5 0 180) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Rect_L7.0mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Rect_L7.0mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 5A43FFEF)
    (at 36.6395 82.423)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7*2.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7mm width 2.5mm Capacitor")
    (fp_text reference C5 (at -2.413 0.0635) (layer F.SilkS))
    (fp_text value 100nF (at 2.5 2.56) (layer F.Fab))
    (fp_text user %R (at 2.5 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (pad 2 thru_hole circle (at 5 0) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Rect_L7.0mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Rect_L7.0mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 5A43FF64)
    (at 71.374 84.709 270)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7*2.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7mm width 2.5mm Capacitor")
    (fp_text reference C6 (at -2.794 0 270) (layer F.SilkS))
    (fp_text value 100nF (at 2.5 2.56 270) (layer F.Fab))
    (fp_text user %R (at 2.5 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 +15V))
    (pad 2 thru_hole circle (at 5 0 270) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Rect_L7.0mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Rect_L7.0mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 5A44001F)
    (at 36.2585 58.2295)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7*2.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7mm width 2.5mm Capacitor")
    (fp_text reference C8 (at 4.3815 -2.286) (layer F.SilkS))
    (fp_text value 100nF (at 2.5 2.56) (layer F.Fab))
    (fp_text user %R (at 2.5 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 +15V))
    (pad 2 thru_hole circle (at 5 0) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Rect_L7.0mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Rect_L7.0mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 5A43FF27)
    (at 62.9285 97.5995)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7*2.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7mm width 2.5mm Capacitor")
    (fp_text reference C9 (at 7.493 1.143) (layer F.SilkS))
    (fp_text value 100nF (at 2.5 2.56) (layer F.Fab))
    (fp_text user %R (at 2.5 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(C7-Pad2)"))
    (pad 2 thru_hole circle (at 5 0) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Rect_L7.0mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:CP_Radial_D5.0mm_P2.00mm (layer F.Cu) (tedit 5A357382)
    (at 51.8795 63.6905)
    (descr "CP, Radial series, Radial, pin pitch=2.00mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.00mm  diameter 5mm Electrolytic Capacitor")
    (fp_text reference C14 (at 5.5245 -0.3175) (layer F.SilkS))
    (fp_text value 1uF (at 1 3.81) (layer F.Fab))
    (fp_text user %R (at 1 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 2.4) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(C14-Pad1)"))
    (pad 2 thru_hole oval (at 2 0) (size 1.6 2.4) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D5.0mm_P2.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Rect_L7.0mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 5A440017)
    (at 41.2115 52.197 180)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7*2.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7mm width 2.5mm Capacitor")
    (fp_text reference C15 (at 5.207 -2.286 180) (layer F.SilkS))
    (fp_text value 100nF (at 2.5 2.56 180) (layer F.Fab))
    (fp_text user %R (at 2.5 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 +5V))
    (pad 2 thru_hole circle (at 5 0 180) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Rect_L7.0mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:CP_Radial_D5.0mm_P2.00mm (layer F.Cu) (tedit 5A357424)
    (at 65.7225 53.594 270)
    (descr "CP, Radial series, Radial, pin pitch=2.00mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.00mm  diameter 5mm Electrolytic Capacitor")
    (fp_text reference C18 (at 4.826 -1.7145 270) (layer F.SilkS))
    (fp_text value 22uF (at 3.3655 2.413 270) (layer F.Fab))
    (fp_text user %R (at 1 0 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 +4.096V))
    (pad 2 thru_hole circle (at 2 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D5.0mm_P2.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_THT:D_T-1_P10.16mm_Horizontal (layer F.Cu) (tedit 5A440299)
    (at 32.5755 86.4235 270)
    (descr "D, T-1 series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=3.2*2.6mm^2, , http://www.diodes.com/_files/packages/T-1.pdf")
    (tags "D T-1 series Axial Horizontal pin pitch 10.16mm  length 3.2mm diameter 2.6mm")
    (fp_text reference D1 (at 6.223 -2.413 270) (layer F.SilkS))
    (fp_text value 1N4007 (at 5.08 2.36 270) (layer F.Fab))
    (fp_text user %R (at 5.08 0 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.5 2.5) (drill 1) (layers *.Cu *.Mask)
      (net 34 "Net-(D1-Pad1)"))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 2.5 2) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/Diodes_THT.3dshapes/D_T-1_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors:BARREL_JACK (layer F.Cu) (tedit 5A4402A8)
    (at 40.132 94.742 90)
    (descr "DC Barrel Jack")
    (tags "Power Jack")
    (fp_text reference J1 (at 0.508 6.35 270) (layer F.SilkS))
    (fp_text value "18 Volt DC In" (at -9.9695 2.54 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 3.5 3.5) (drill oval 1 3) (layers *.Cu *.Mask)
      (net 9 "Net-(D1-Pad2)"))
    (pad 2 thru_hole rect (at -6 0 90) (size 3.5 3.5) (drill oval 1 3) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole rect (at -3 4.7 90) (size 3.5 3.5) (drill oval 3 1) (layers *.Cu *.Mask)
      (net 10 "Net-(J1-Pad3)"))
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 5A43FE8B)
    (at 94.8055 42.6085 180)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J3 (at -2.921 0.6985 180) (layer F.SilkS))
    (fp_text value "B Vref." (at -0.3175 5.334 180) (layer F.Fab))
    (fp_text user %R (at 0 1.27 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.4 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(J3-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.4 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 Vref))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-8_W7.62mm_Socket_LongPads (layer F.Cu) (tedit 59C78D6B)
    (at 75.7555 70.6755 90)
    (descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket, LongPads")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket LongPads")
    (fp_text reference U1 (at 3.81 -2.33 90) (layer F.SilkS))
    (fp_text value INA105 (at 3.81 9.95 90) (layer F.Fab))
    (fp_text user %R (at 3.81 3.81 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "Net-(U1-Pad1)"))
    (pad 5 thru_hole oval (at 7.62 7.62 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(U1-Pad5)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6 thru_hole oval (at 7.62 5.08 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(U1-Pad5)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "Net-(U1-Pad1)"))
    (pad 7 thru_hole oval (at 7.62 2.54 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 +15V))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 -15V))
    (pad 8 thru_hole oval (at 7.62 0 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-8_W7.62mm_Socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-14_W7.62mm_Socket_LongPads (layer F.Cu) (tedit 59C78D6B)
    (at 91.5035 70.6755 90)
    (descr "14-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket, LongPads")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket LongPads")
    (fp_text reference U2 (at 3.81 -2.33 90) (layer F.SilkS))
    (fp_text value DG303B (at 3.81 17.57 90) (layer F.Fab))
    (fp_text user %R (at 3.81 7.62 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 7.62 15.24 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 -15V))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "Net-(U1-Pad1)"))
    (pad 9 thru_hole oval (at 7.62 12.7 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 A4))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(U2-Pad3)"))
    (pad 10 thru_hole oval (at 7.62 10.16 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 +4.096V))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(U2-Pad3)"))
    (pad 11 thru_hole oval (at 7.62 7.62 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 Vref))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(U1-Pad5)"))
    (pad 12 thru_hole oval (at 7.62 5.08 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 Vref))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 A3))
    (pad 13 thru_hole oval (at 7.62 2.54 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 +1.024V))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 14 thru_hole oval (at 7.62 0 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 +15V))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-14_W7.62mm_Socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-8_W7.62mm_Socket_LongPads (layer F.Cu) (tedit 59C78D6B)
    (at 56.134 77.089 270)
    (descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket, LongPads")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket LongPads")
    (fp_text reference U3 (at 3.81 -2.33 270) (layer F.SilkS))
    (fp_text value TC962 (at 3.81 9.95 270) (layer F.Fab))
    (fp_text user %R (at 3.81 3.81 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 7.62 7.62 270) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(C7-Pad2)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(C2-Pad1)"))
    (pad 6 thru_hole oval (at 7.62 5.08 270) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 7 thru_hole oval (at 7.62 2.54 270) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C2-Pad2)"))
    (pad 8 thru_hole oval (at 7.62 0 270) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 +15V))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-8_W7.62mm_Socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-8_W7.62mm_Socket_LongPads (layer F.Cu) (tedit 59C78D6B)
    (at 75.692 91.059 90)
    (descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket, LongPads")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket LongPads")
    (fp_text reference U5 (at 3.81 -2.33 90) (layer F.SilkS))
    (fp_text value INA105 (at 3.81 9.95 90) (layer F.Fab))
    (fp_text user %R (at 3.81 3.81 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 "Net-(JP1-Pad1)"))
    (pad 5 thru_hole oval (at 7.62 7.62 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "Net-(U1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 "Net-(U5-Pad2)"))
    (pad 6 thru_hole oval (at 7.62 5.08 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "Net-(U1-Pad1)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 "Net-(JP1-Pad1)"))
    (pad 7 thru_hole oval (at 7.62 2.54 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 +15V))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 -15V))
    (pad 8 thru_hole oval (at 7.62 0 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-8_W7.62mm_Socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-14_W7.62mm_Socket_LongPads (layer F.Cu) (tedit 59C78D6B)
    (at 91.44 90.932 90)
    (descr "14-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket, LongPads")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket LongPads")
    (fp_text reference U6 (at 3.81 -2.33 90) (layer F.SilkS))
    (fp_text value DG303B (at 3.81 17.57 90) (layer F.Fab))
    (fp_text user %R (at 3.81 7.62 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 7.62 15.24 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 -15V))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "Net-(U1-Pad1)"))
    (pad 9 thru_hole oval (at 7.62 12.7 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 A2))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 "Net-(U5-Pad2)"))
    (pad 10 thru_hole oval (at 7.62 10.16 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(U2-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 "Net-(U5-Pad2)"))
    (pad 11 thru_hole oval (at 7.62 7.62 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(J5-Pad1)"))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 12 thru_hole oval (at 7.62 5.08 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(J5-Pad1)"))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 A1))
    (pad 13 thru_hole oval (at 7.62 2.54 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 14 thru_hole oval (at 7.62 0 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 +15V))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-14_W7.62mm_Socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-14_W7.62mm_Socket_LongPads (layer F.Cu) (tedit 59C78D6B)
    (at 81.28 38.989)
    (descr "14-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket, LongPads")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket LongPads")
    (fp_text reference U9 (at 3.81 -2.33) (layer F.SilkS))
    (fp_text value MCP4922EP (at 3.81 17.57) (layer F.Fab))
    (fp_text user %R (at 3.81 7.62) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 +5V))
    (pad 8 thru_hole oval (at 7.62 15.24) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 A0))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 9 thru_hole oval (at 7.62 12.7) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 "Net-(J7-Pad6)"))
    (pad 10 thru_hole oval (at 7.62 10.16) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(J4-Pad2)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 "Net-(J7-Pad7)"))
    (pad 11 thru_hole oval (at 7.62 7.62) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(J3-Pad1)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 "Net-(J7-Pad8)"))
    (pad 12 thru_hole oval (at 7.62 5.08) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6 thru_hole oval (at 0 12.7) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 13 thru_hole oval (at 7.62 2.54) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 Vref))
    (pad 7 thru_hole oval (at 0 15.24) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 14 thru_hole oval (at 7.62 0) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 "Net-(JP1-Pad2)"))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-14_W7.62mm_Socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-8_W7.62mm_Socket_LongPads (layer F.Cu) (tedit 59C78D6B)
    (at 46.4185 57.658 90)
    (descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket, LongPads")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket LongPads")
    (fp_text reference U10 (at 3.81 -2.33 90) (layer F.SilkS))
    (fp_text value MAX6341 (at 3.81 9.95 90) (layer F.Fab))
    (fp_text user %R (at 3.81 3.81 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 7.62 7.62 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(RV1-Pad2)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 +15V))
    (pad 6 thru_hole oval (at 7.62 5.08 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 +4.096V))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(C14-Pad1)"))
    (pad 7 thru_hole oval (at 7.62 2.54 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 8 thru_hole oval (at 7.62 0 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-8_W7.62mm_Socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Power_Integrations:TO-220 (layer F.Cu) (tedit 0)
    (at 27.051 77.851 90)
    (descr "Non Isolated JEDEC TO-220 Package")
    (tags "Power Integration YN Package")
    (fp_text reference U4 (at 0 -4.318 90) (layer F.SilkS))
    (fp_text value LM7815_TO220 (at 0 -4.318 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 0 90) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole oval (at 2.54 0 90) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask)
      (net 23 +15V))
    (pad 1 thru_hole oval (at -2.54 0 90) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask)
      (net 4 "Net-(C3-Pad1)"))
  )
  (module Power_Integrations:TO-220 (layer F.Cu) (tedit 0)
    (at 60.8965 102.6795 180)
    (descr "Non Isolated JEDEC TO-220 Package")
    (tags "Power Integration YN Package")
    (fp_text reference U7 (at 0 -4.318 180) (layer F.SilkS))
    (fp_text value LM7915_TO220 (at 0 -4.318 180) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 0 180) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask)
      (net 5 "Net-(C7-Pad2)"))
    (pad 3 thru_hole oval (at 2.54 0 180) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask)
      (net 22 -15V))
    (pad 1 thru_hole oval (at -2.54 0 180) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Power_Integrations:TO-220 (layer F.Cu) (tedit 0)
    (at 26.924 44.958 90)
    (descr "Non Isolated JEDEC TO-220 Package")
    (tags "Power Integration YN Package")
    (fp_text reference U8 (at 0 -4.318 90) (layer F.SilkS))
    (fp_text value LM7805_TO220 (at 0 -4.318 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 0 90) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole oval (at 2.54 0 90) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask)
      (net 7 +5V))
    (pad 1 thru_hole oval (at -2.54 0 90) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask)
      (net 31 "Net-(D2-Pad2)"))
  )
  (module Capacitors_THT:CP_Radial_D8.0mm_P2.50mm (layer F.Cu) (tedit 5A3573A5)
    (at 54.6735 91.059 270)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=8mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 8mm Electrolytic Capacitor")
    (fp_text reference C7 (at 6.7945 1.143 270) (layer F.SilkS))
    (fp_text value 100uF (at 1.25 5.31 270) (layer F.Fab))
    (fp_text user %R (at 3.3655 2.921 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 2.4) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 2.5 0 270) (size 1.6 2.4) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(C7-Pad2)"))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D8.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Rect_L7.0mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 5A35369A)
    (at 83.312 102.743 180)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7*2.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7mm width 2.5mm Capacitor")
    (fp_text reference C11 (at 2.5 -2.56 180) (layer F.SilkS))
    (fp_text value 100nF (at 2.5 2.56 180) (layer F.Fab))
    (fp_text user %R (at 2.5 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 -15V))
    (pad 2 thru_hole circle (at 5 0 180) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Rect_L7.0mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Rect_L7.0mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 5A193DD9)
    (at 75.184 34.29 270)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7*2.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7mm width 2.5mm Capacitor")
    (fp_text reference C17 (at 2.5 -2.56 270) (layer F.SilkS))
    (fp_text value 100nF (at 2.5 2.56 270) (layer F.Fab))
    (fp_text user %R (at 2.5 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 5 0 270) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 +5V))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Rect_L7.0mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:CP_Radial_D8.0mm_P2.50mm (layer F.Cu) (tedit 5A353D3B)
    (at 38.9255 64.516 270)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=8mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 8mm Electrolytic Capacitor")
    (fp_text reference C10 (at 1.25 -5.31 270) (layer F.SilkS))
    (fp_text value 100uF (at 1.27 -2.667 270) (layer F.Fab))
    (fp_text user %R (at 1.25 0 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 2.4) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 +15V))
    (pad 2 thru_hole oval (at 2.5 0 270) (size 1.6 2.4) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D8.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:CP_Radial_D8.0mm_P2.50mm (layer F.Cu) (tedit 5A43FF49)
    (at 65.532 90.678 180)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=8mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 8mm Electrolytic Capacitor")
    (fp_text reference C13 (at 1.2065 5.2705 180) (layer F.SilkS))
    (fp_text value 100uF (at -0.635 -3.429 180) (layer F.Fab))
    (fp_text user %R (at 3.6195 2.6035 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 2.4) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 2.5 0 180) (size 1.6 2.4) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 -15V))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D8.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:CP_Radial_D8.0mm_P2.50mm (layer F.Cu) (tedit 5A1940A4)
    (at 38.4175 43.815 270)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=8mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 8mm Electrolytic Capacitor")
    (fp_text reference C16 (at 1.25 -5.31 270) (layer F.SilkS))
    (fp_text value 100uF (at 1.25 5.31 270) (layer F.Fab))
    (fp_text user %R (at 1.25 0 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 2.4) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 +5V))
    (pad 2 thru_hole oval (at 2.5 0 270) (size 1.6 2.4) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D8.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Rect_L7.0mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 5A43FF7B)
    (at 71.247 62.738 270)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7*2.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7mm width 2.5mm Capacitor")
    (fp_text reference C1 (at -2.7305 0 270) (layer F.SilkS))
    (fp_text value 100nF (at 2.5 2.56 270) (layer F.Fab))
    (fp_text user %R (at 2.5 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 +15V))
    (pad 2 thru_hole circle (at 5 0 270) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Rect_L7.0mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Rect_L7.0mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 5A353686)
    (at 61.849 81.153)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7*2.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7mm width 2.5mm Capacitor")
    (fp_text reference C12 (at 2.5 -2.56) (layer F.SilkS))
    (fp_text value 100nF (at 2.5 2.56) (layer F.Fab))
    (fp_text user %R (at 2.5 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 -15V))
    (pad 2 thru_hole circle (at 5 0) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Rect_L7.0mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Rect_L7.0mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 5A44061A)
    (at 61.722 34.9885)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7*2.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7mm width 2.5mm Capacitor")
    (fp_text reference C19 (at 2.5 -2.56) (layer F.SilkS))
    (fp_text value 2.2uF (at 2.5 2.56) (layer F.Fab))
    (fp_text user %R (at 2.5 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 3.5 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 +5V))
    (pad 2 thru_hole rect (at 5 0) (size 3.5 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Rect_L7.0mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_JST:JST_XH_B02B-XH-A_02x2.50mm_Straight (layer F.Cu) (tedit 5A440746)
    (at 96.774 47.879 270)
    (descr "JST XH series connector, B02B-XH-A, top entry type, through hole")
    (tags "connector jst xh tht top vertical 2.50mm")
    (fp_text reference J4 (at 1.27 -3.937 270) (layer F.SilkS))
    (fp_text value "DAC B Out" (at 1.524 -4.318 270) (layer F.Fab))
    (fp_text user %R (at 1.25 2.5 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.75 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.75 1.75) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(J4-Pad2)"))
    (model Connectors_JST.3dshapes/JST_XH_B02B-XH-A_02x2.50mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_JST:JST_XH_B02B-XH-A_02x2.50mm_Straight (layer F.Cu) (tedit 5A4400CB)
    (at 96.393 77.216 180)
    (descr "JST XH series connector, B02B-XH-A, top entry type, through hole")
    (tags "connector jst xh tht top vertical 2.50mm")
    (fp_text reference J5 (at -4.2545 0.127 180) (layer F.SilkS))
    (fp_text value "DC Reference Output" (at 0.889 -3.4925 180) (layer F.Fab))
    (fp_text user %R (at 1.25 2.5 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.75 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(J5-Pad1)"))
    (pad 2 thru_hole oval (at 2.5 0 180) (size 1.75 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model Connectors_JST.3dshapes/JST_XH_B02B-XH-A_02x2.50mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_JST:JST_XH_B10B-XH-A_10x2.50mm_Straight (layer F.Cu) (tedit 5A440061)
    (at 103.886 30.099 180)
    (descr "JST XH series connector, B10B-XH-A, top entry type, through hole")
    (tags "connector jst xh tht top vertical 2.50mm")
    (fp_text reference J7 (at 10.9855 -4.0005 180) (layer F.SilkS))
    (fp_text value "To Display/Nano" (at 11.303 5.08 180) (layer F.Fab))
    (fp_text user %R (at -4.191 0.9525 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.75 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 A0))
    (pad 2 thru_hole oval (at 2.5 0 180) (size 1.75 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 A1))
    (pad 3 thru_hole oval (at 5 0 180) (size 1.75 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 A2))
    (pad 4 thru_hole oval (at 7.5 0 180) (size 1.75 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 A3))
    (pad 5 thru_hole oval (at 10 0 180) (size 1.75 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 A4))
    (pad 6 thru_hole oval (at 12.5 0 180) (size 1.75 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 "Net-(J7-Pad6)"))
    (pad 7 thru_hole oval (at 15 0 180) (size 1.75 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 "Net-(J7-Pad7)"))
    (pad 8 thru_hole oval (at 17.5 0 180) (size 1.75 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 "Net-(J7-Pad8)"))
    (pad 9 thru_hole oval (at 20 0 180) (size 1.75 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 10 thru_hole oval (at 22.5 0 180) (size 1.75 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 +5V))
    (model Connectors_JST.3dshapes/JST_XH_B10B-XH-A_10x2.50mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_JST:JST_XH_B04B-XH-A_04x2.50mm_Straight (layer F.Cu) (tedit 5A44004A)
    (at 37.4015 29.083)
    (descr "JST XH series connector, B04B-XH-A, top entry type, through hole")
    (tags "connector jst xh tht top vertical 2.50mm")
    (fp_text reference J8 (at 3.3655 -4.191) (layer F.SilkS))
    (fp_text value "Option Power" (at 3.75 4.5) (layer F.Fab))
    (fp_text user %R (at 3.75 2.5) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.75 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 -15V))
    (pad 2 thru_hole oval (at 2.5 0) (size 1.75 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 +5V))
    (pad 3 thru_hole oval (at 5 0) (size 1.75 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 +15V))
    (pad 4 thru_hole oval (at 7.5 0) (size 1.75 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model Connectors_JST.3dshapes/JST_XH_B04B-XH-A_04x2.50mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 5A353DC4)
    (at 64.389 41.7195)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U11 (at 0 -3.5) (layer F.SilkS))
    (fp_text value MCP1501_10 (at -0.0635 4.1275) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 +5V))
    (pad 2 smd rect (at -2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 +5V))
    (pad 4 smd rect (at -2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 7 smd rect (at 2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 28 +1.024V))
    (pad 8 smd rect (at 2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 28 +1.024V))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_THT:D_DO-201AD_P15.24mm_Horizontal (layer F.Cu) (tedit 5A353D21)
    (at 30.734 68.834 90)
    (descr "D, DO-201AD series, Axial, Horizontal, pin pitch=15.24mm, , length*diameter=9.5*5.2mm^2, , http://www.diodes.com/_files/packages/DO-201AD.pdf")
    (tags "D DO-201AD series Axial Horizontal pin pitch 15.24mm  length 9.5mm diameter 5.2mm")
    (fp_text reference D2 (at 7.62 -3.66 90) (layer F.SilkS))
    (fp_text value 1N5338B (at 8.255 0.9525 90) (layer F.Fab))
    (fp_text user %R (at 8.0645 -1.4605 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 3.2 3.2) (drill 1.6) (layers *.Cu *.Mask)
      (net 23 +15V))
    (pad 2 thru_hole oval (at 15.24 0 90) (size 3.2 3.2) (drill 1.6) (layers *.Cu *.Mask)
      (net 31 "Net-(D2-Pad2)"))
    (model ${KISYS3DMOD}/Diodes_THT.3dshapes/D_DO-201AD_P15.24mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Potentiometers:Potentiometer_Trimmer_Bourns_3296W (layer F.Cu) (tedit 5A357436)
    (at 58.9915 50.165 90)
    (descr "Spindle Trimmer Potentiometer, Bourns 3296W, https://www.bourns.com/pdfs/3296.pdf")
    (tags "Spindle Trimmer Potentiometer   Bourns 3296W")
    (fp_text reference RV1 (at -8.3185 0.1905 180) (layer F.SilkS))
    (fp_text value 10K (at -2.54 3.67 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.7 1.7) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at -2.54 0 90) (size 1.7 1.7) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(RV1-Pad2)"))
    (pad 3 thru_hole circle (at -5.08 0 90) (size 1.7 1.7) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 +4.096V))
    (model Potentiometers.3dshapes/Potentiometer_Trimmer_Bourns_3296W.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Capacitors_THT:C_Rect_L4.6mm_W2.0mm_P2.50mm_MKS02_FKP02 (layer F.Cu) (tedit 5A4406A6)
    (at 69.596 46.863 180)
    (descr "C, Rect series, Radial, pin pitch=2.50mm, , length*width=4.6*2mm^2, Capacitor, http://www.wima.de/DE/WIMA_MKS_02.pdf")
    (tags "C Rect series Radial pin pitch 2.50mm  length 4.6mm width 2mm Capacitor")
    (fp_text reference C20 (at 1.25 -2.31 180) (layer F.SilkS))
    (fp_text value 220pF (at 1.25 2.31 180) (layer F.Fab))
    (fp_text user %R (at 1.25 0 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 28 +1.024V))
    (pad 2 thru_hole rect (at 2.5 0 180) (size 1.8 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Rect_L4.6mm_W2.0mm_P2.50mm_MKS02_FKP02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_JST:JST_XH_B03B-XH-A_03x2.50mm_Straight (layer F.Cu) (tedit 5A43FDA3)
    (at 26.797 91.44 270)
    (descr "JST XH series connector, B03B-XH-A, top entry type, through hole")
    (tags "connector jst xh tht top vertical 2.50mm")
    (fp_text reference J2 (at 2.5 -3.5 270) (layer F.SilkS))
    (fp_text value Battery (at 2.5 4.5 270) (layer F.Fab))
    (fp_text user %R (at 2.5 2.5 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.75 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 "Net-(D1-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.75 1.75) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(J1-Pad3)"))
    (pad 3 thru_hole circle (at 5 0 270) (size 1.75 1.75) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model Connectors_JST.3dshapes/JST_XH_B03B-XH-A_03x2.50mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_JST:JST_XH_B02B-XH-A_02x2.50mm_Straight (layer F.Cu) (tedit 5A440283)
    (at 40.7035 88.9 180)
    (descr "JST XH series connector, B02B-XH-A, top entry type, through hole")
    (tags "connector jst xh tht top vertical 2.50mm")
    (fp_text reference J6 (at -4.064 -0.508 180) (layer F.SilkS))
    (fp_text value "On/Off Switch" (at 1.25 4.5 180) (layer F.Fab))
    (fp_text user %R (at 1.25 2.5 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.75 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.75 1.75) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 "Net-(D1-Pad1)"))
    (model Connectors_JST.3dshapes/JST_XH_B02B-XH-A_02x2.50mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors:1pin (layer F.Cu) (tedit 5A440493)
    (at 116.967 25.4)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference "" (at 0 -3.048) (layer F.SilkS))
    (fp_text value 1pin (at 0 3) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask))
  )
  (module Connectors:1pin (layer F.Cu) (tedit 5A44049C)
    (at 116.967 105.156)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference "" (at 0 -3.048) (layer F.SilkS))
    (fp_text value 1pin (at 0 3) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask))
  )
  (module Connectors:1pin (layer F.Cu) (tedit 5A44047A)
    (at 24.511 105.156)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference "" (at 0 -3.048) (layer F.SilkS))
    (fp_text value 1pin (at 0 3) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask))
  )
  (module Connectors:1pin (layer F.Cu) (tedit 5A440488)
    (at 24.511 25.4)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference "" (at 0 -3.048) (layer F.SilkS))
    (fp_text value 1pin (at 0 3) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask))
  )
  (gr_text • (at 59.69 38.4175) (layer F.Cu))
  (gr_line (start 120.545 108.585) (end 20.955 108.585) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text "Ver 2.2" (at 65.2145 71.5645) (layer B.Cu))
  (gr_line (start 20.955 108.585) (end 20.955 21.59) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 120.545 21.59) (end 120.545 108.585) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 20.955 21.59) (end 120.545 21.59) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text "Programmable\nD.C. Reference" (at 95.123 103.251) (layer B.Cu))
  (gr_text "SCULLCOM HOBBY ELECTRONICS" (at 60.5155 23.368) (layer B.Cu))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 77.851 102.87) (xy 63.373 102.87) (xy 63.3095 107.823) (xy 119.888 107.8865) (xy 119.761 22.4155)
        (xy 80.264 22.4155) (xy 80.264 26.0985) (xy 108.6485 26.0985) (xy 108.6485 36.5125) (xy 117.9195 36.5125)
        (xy 117.983 91.567) (xy 106.553 102.997) (xy 106.553 105.41) (xy 104.521 107.061) (xy 81.407 107.061)
        (xy 78.232 104.14) (xy 77.851 103.0605)
      )
    )
  )
)
