(kicad_pcb (version 4) (host pcbnew 4.0.0-rc1-stable)
  (general
    (links 51)
    (no_connects 25)
    (area 121.424999 79.924999 146.075001 152.075001)
    (thickness 1.6)
    (drawings 17)
    (tracks 57)
    (zones 0)
    (modules 31)
    (nets 10)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu power)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (47 F.CrtYd user hide)
  )
  (setup
    (last_trace_width 1.5)
    (user_trace_width 0.75)
    (user_trace_width 1)
    (user_trace_width 1.25)
    (user_trace_width 1.5)
    (trace_clearance 0.1)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.5)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.6 1.6)
    (pad_drill 0.8)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFEFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 "Net-(C1-Pad2)")
  (net 3 "Net-(C2-Pad2)")
  (net 4 "Net-(C3-Pad2)")
  (net 5 "Net-(C4-Pad2)")
  (net 6 "Net-(D1-Pad1)")
  (net 7 "Net-(D1-Pad2)")
  (net 8 "Net-(K1-Pad2)")
  (net 9 "Net-(K1-Pad3)")
  (net_class Default "This is the default net class."
    (clearance 0.1)
    (trace_width 1)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(C2-Pad2)")
    (add_net "Net-(C3-Pad2)")
    (add_net "Net-(C4-Pad2)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(K1-Pad3)")
  )
  (net_class COM ""
    (clearance 0.1)
    (trace_width 1.5)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(K1-Pad2)")
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 59706DA2)
    (at 137.5 140.5 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (solder_mask_margin 0.1)
    (attr smd)
    (fp_text reference C4 (at 0 1.75 180) (layer B.SilkS))
    (fp_text value C (at 0 -1.75 180) (layer B.Fab))
    (fp_text user %R (at 0 1.75 180) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(C4-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module GNUCOMP:SPST_SMD_2P (layer F.Cu) (tedit 597017B5)
    (at 137.25 108.5)
    (fp_text reference SW10 (at 0 3) (layer F.SilkS) hide)
    (fp_text value SW_PUSH (at 0 -3) (layer F.Fab))
    (pad 2 smd rect (at 2.7 0) (size 3.2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 1 smd rect (at -2.7 0) (size 3.2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad2)"))
  )
  (module Buttons_Switches_ThroughHole:SW_PUSH_6mm_h5mm (layer F.Cu) (tedit 59700A53)
    (at 135 113.5 90)
    (descr "tactile push button, 6x6mm e.g. PHAP33xx series, height=5mm")
    (tags "tact sw push 6mm")
    (fp_text reference SW3 (at 3.25 -2 90) (layer F.SilkS) hide)
    (fp_text value SW_PUSH (at 3.75 6.7 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 4.5 180) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(C2-Pad2)"))
    (pad 2 thru_hole circle (at 6.5 4.5 180) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 1 thru_hole circle (at 6.5 0 180) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(C2-Pad2)"))
    (model ${KISYS3DMOD}/Buttons_Switches_THT.3dshapes/SW_PUSH_6mm_h5mm.wrl
      (at (xyz 0.005 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 58AA84A8)
    (at 137.5 110.5 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (solder_mask_margin 0.1)
    (attr smd)
    (fp_text reference C2 (at 0 1.75 180) (layer B.SilkS))
    (fp_text value C (at 0 -1.75 180) (layer B.Fab))
    (fp_text user %R (at 0 1.75 180) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(C2-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module GNUCOMP:SPST_SMD_2P (layer F.Cu) (tedit 597017BC)
    (at 137.25 123.5)
    (fp_text reference SW11 (at 0 3) (layer F.SilkS) hide)
    (fp_text value SW_PUSH (at 0 -3) (layer F.Fab))
    (pad 2 smd rect (at 2.7 0) (size 3.2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 1 smd rect (at -2.7 0) (size 3.2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C3-Pad2)"))
  )
  (module Buttons_Switches_ThroughHole:SW_PUSH_6mm_h5mm (layer F.Cu) (tedit 596D791B)
    (at 135 128.5 90)
    (descr "tactile push button, 6x6mm e.g. PHAP33xx series, height=5mm")
    (tags "tact sw push 6mm")
    (fp_text reference SW5 (at 3.25 -2 90) (layer F.SilkS) hide)
    (fp_text value SW_PUSH (at 3.75 6.7 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 4.5 180) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(C3-Pad2)"))
    (pad 2 thru_hole circle (at 6.5 4.5 180) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 1 thru_hole circle (at 6.5 0 180) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(C3-Pad2)"))
    (model ${KISYS3DMOD}/Buttons_Switches_THT.3dshapes/SW_PUSH_6mm_h5mm.wrl
      (at (xyz 0.005 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module GNUCOMP:Tactile_push_6x6_SMD (layer F.Cu) (tedit 597064B6)
    (at 136 109.2)
    (fp_text reference REF** (at 0 5.5) (layer F.SilkS) hide)
    (fp_text value Tactile_push_6x6_SMD (at 0 -5.5) (layer F.Fab))
    (pad 2 smd rect (at 2.25 3.5) (size 1.4 2.1) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at 2.25 -3.5) (size 1.4 2.1) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at -2.25 -3.5) (size 1.4 2.1) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at -2.25 3.5) (size 1.4 2.1) (layers F.Cu F.Paste F.Mask))
  )
  (module GNUCOMP:Tactile_push_6x6_SMD (layer F.Cu) (tedit 5970649F)
    (at 136 124.2)
    (fp_text reference REF** (at 0 5.5) (layer F.SilkS) hide)
    (fp_text value Tactile_push_6x6_SMD (at 0 -5.5) (layer F.Fab))
    (pad 2 smd rect (at 2.25 3.5) (size 1.4 2.1) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at 2.25 -3.5) (size 1.4 2.1) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at -2.25 -3.5) (size 1.4 2.1) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at -2.25 3.5) (size 1.4 2.1) (layers F.Cu F.Paste F.Mask))
  )
  (module GNUCOMP:SPST_SMD_2P (layer F.Cu) (tedit 597017C3)
    (at 137.25 138.5)
    (fp_text reference SW12 (at 0 3) (layer F.SilkS) hide)
    (fp_text value SW_PUSH (at 0 -3) (layer F.Fab))
    (pad 2 smd rect (at 2.7 0) (size 3.2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 1 smd rect (at -2.7 0) (size 3.2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C4-Pad2)"))
  )
  (module GNUCOMP:Tactile_push_6x6_SMD (layer F.Cu) (tedit 59706498)
    (at 136 139.2)
    (fp_text reference REF** (at 0 5.5) (layer F.SilkS) hide)
    (fp_text value Tactile_push_6x6_SMD (at 0 -5.5) (layer F.Fab))
    (pad 2 smd rect (at 2.25 3.5) (size 1.4 2.1) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at 2.25 -3.5) (size 1.4 2.1) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at -2.25 -3.5) (size 1.4 2.1) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at -2.25 3.5) (size 1.4 2.1) (layers F.Cu F.Paste F.Mask))
  )
  (module Buttons_Switches_ThroughHole:SW_PUSH_6mm_h5mm (layer F.Cu) (tedit 59706A5A)
    (at 135 143.5 90)
    (descr "tactile push button, 6x6mm e.g. PHAP33xx series, height=5mm")
    (tags "tact sw push 6mm")
    (fp_text reference SW7 (at 3.25 -2 90) (layer F.SilkS) hide)
    (fp_text value SW_PUSH (at 3.75 6.7 90) (layer F.Fab))
    (fp_text user %R (at 3.25 2.25 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 4.5 180) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(C4-Pad2)"))
    (pad 2 thru_hole circle (at 6.5 4.5 180) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 1 thru_hole circle (at 6.5 0 180) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(C4-Pad2)"))
    (model ${KISYS3DMOD}/Buttons_Switches_THT.3dshapes/SW_PUSH_6mm_h5mm.wrl
      (at (xyz 0.005 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D3.0mm (layer F.Cu) (tedit 597069D3)
    (at 126 142.5 90)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference LED (at 1.25 0 180) (layer F.SilkS))
    (fp_text value LED (at 1.27 2.96 90) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0 90) (size 1.8 1.8) (drill 0.9) (layers B.Cu B.Mask)
      (net 6 "Net-(D1-Pad1)"))
    (pad "" np_thru_hole circle (at 2.54 0 90) (size 1.8 1.8) (drill 0.9) (layers B.Cu B.Mask))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module GNUCOMP:Push_Keyboard_Switch (layer F.Cu) (tedit 597067C4)
    (at 135 135.5)
    (descr "E-Switch KS01Q01 http://spec_sheets.e-switch.com/specs/29-KS01Q01.pdf")
    (tags "Push Button")
    (fp_text reference SW8 (at 2.5 -4.5) (layer F.SilkS) hide)
    (fp_text value SW_PUSH (at 2.5 9.5) (layer F.Fab))
    (fp_text user %R (at 2.5 2.5) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 2 2) (drill 1.1) (layers B.Cu B.Mask))
    (pad 2 np_thru_hole circle (at 5 0) (size 2 2) (drill 1.1) (layers B.Cu B.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 np_thru_hole circle (at 5 5) (size 2 2) (drill 1.1) (layers B.Cu B.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 1 np_thru_hole circle (at 0 5) (size 2 2) (drill 1.1) (layers B.Cu B.Mask)
      (net 5 "Net-(C4-Pad2)"))
    (model ${KISYS3DMOD}/Buttons_Switches_THT.3dshapes/Push_E-Switch_KS01Q01.wrl
      (at (xyz 0.1 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module GNUCOMP:Push_Keyboard_Switch (layer F.Cu) (tedit 597067AE)
    (at 135 120.5)
    (descr "E-Switch KS01Q01 http://spec_sheets.e-switch.com/specs/29-KS01Q01.pdf")
    (tags "Push Button")
    (fp_text reference SW6 (at 2.5 -4.5) (layer F.SilkS) hide)
    (fp_text value SW_PUSH (at 2.5 9.5) (layer F.Fab))
    (fp_text user %R (at 2.5 2.5) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 2 2) (drill 1.1) (layers B.Cu B.Mask))
    (pad 2 np_thru_hole circle (at 5 0) (size 2 2) (drill 1.1) (layers B.Cu B.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 np_thru_hole circle (at 5 5) (size 2 2) (drill 1.1) (layers B.Cu B.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 1 np_thru_hole circle (at 0 5) (size 2 2) (drill 1.1) (layers B.Cu B.Mask)
      (net 4 "Net-(C3-Pad2)"))
    (model ${KISYS3DMOD}/Buttons_Switches_THT.3dshapes/Push_E-Switch_KS01Q01.wrl
      (at (xyz 0.1 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module GNUCOMP:Push_Keyboard_Switch (layer F.Cu) (tedit 59706788)
    (at 135 105.5)
    (descr "E-Switch KS01Q01 http://spec_sheets.e-switch.com/specs/29-KS01Q01.pdf")
    (tags "Push Button")
    (fp_text reference SW4 (at 2.5 -4.5) (layer F.SilkS) hide)
    (fp_text value SW_PUSH (at 2.5 9.5) (layer F.Fab))
    (fp_text user %R (at 2.5 2.5) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2 2) (drill 1.1) (layers B.Cu B.Mask)
      (net 3 "Net-(C2-Pad2)"))
    (pad 2 np_thru_hole circle (at 5 0) (size 2 2) (drill 1.1) (layers B.Cu B.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 np_thru_hole circle (at 5 5) (size 2 2) (drill 1.1) (layers B.Cu B.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 1 np_thru_hole circle (at 0 5) (size 2 2) (drill 1.1) (layers B.Cu B.Mask)
      (net 3 "Net-(C2-Pad2)"))
    (model ${KISYS3DMOD}/Buttons_Switches_THT.3dshapes/Push_E-Switch_KS01Q01.wrl
      (at (xyz 0.1 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module GNUCOMP:Push_Keyboard_Switch (layer F.Cu) (tedit 5970670F)
    (at 135 90.5)
    (descr "E-Switch KS01Q01 http://spec_sheets.e-switch.com/specs/29-KS01Q01.pdf")
    (tags "Push Button")
    (fp_text reference SW2 (at 2.5 -4.5) (layer F.SilkS) hide)
    (fp_text value SW_PUSH (at 2.5 9.5) (layer F.Fab))
    (fp_text user %R (at 2.5 2.5) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2 2) (drill 1.1) (layers B.Cu B.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (pad 2 np_thru_hole circle (at 5 0) (size 2 2) (drill 1.1) (layers B.Cu B.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 np_thru_hole circle (at 5 5) (size 2 2) (drill 1.1) (layers B.Cu B.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 1 np_thru_hole circle (at 0 5) (size 2 2) (drill 1.1) (layers B.Cu B.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (model ${KISYS3DMOD}/Buttons_Switches_THT.3dshapes/Push_E-Switch_KS01Q01.wrl
      (at (xyz 0.1 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_ThroughHole:SW_PUSH_6mm_h5mm (layer F.Cu) (tedit 59706579)
    (at 135 98.5 90)
    (descr "tactile push button, 6x6mm e.g. PHAP33xx series, height=5mm")
    (tags "tact sw push 6mm")
    (fp_text reference SW1 (at 3.25 -2 90) (layer F.SilkS) hide)
    (fp_text value SW_PUSH (at 3.75 6.7 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 4.5 180) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (pad 2 thru_hole circle (at 6.5 4.5 180) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 1 thru_hole circle (at 6.5 0 180) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (model ${KISYS3DMOD}/Buttons_Switches_THT.3dshapes/SW_PUSH_6mm_h5mm.wrl
      (at (xyz 0.005 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module GNUCOMP:Tactile_push_6x6_SMD (layer F.Cu) (tedit 59706640)
    (at 136 94.2)
    (fp_text reference REF** (at 0 5.5) (layer F.SilkS) hide)
    (fp_text value Tactile_push_6x6_SMD (at 0 -5.5) (layer F.Fab))
    (pad 2 smd rect (at 2.25 3.5) (size 1.4 2.1) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at 2.25 -3.5) (size 1.4 2.1) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at -2.25 -3.5) (size 1.4 2.1) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at -2.25 3.5) (size 1.4 2.1) (layers F.Cu F.Paste F.Mask))
  )
  (module GNUCOMP:SPST_SMD_2P (layer F.Cu) (tedit 597065F1)
    (at 137.25 93.5)
    (fp_text reference SW9 (at 0 3) (layer F.SilkS) hide)
    (fp_text value SW_PUSH (at 0 -3) (layer F.Fab))
    (pad 2 smd rect (at 2.7 0) (size 3.2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 1 smd rect (at -2.7 0) (size 3.2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad2)"))
  )
  (module Socket_Strips:Socket_Strip_Straight_1x06_Pitch2.54mm (layer F.Cu) (tedit 59703F21)
    (at 126 107)
    (descr "Through hole straight socket strip, 1x06, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x06 2.54mm single row")
    (fp_text reference P1 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value CONN_6 (at 0 15.03) (layer F.Fab))
    (fp_text user %R (at 0 -2.33) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 1.7 1.7) (drill 1) (layers B.Cu B.Mask))
    (pad 2 np_thru_hole circle (at 0 2.54) (size 1.7 1.7) (drill 1) (layers B.Cu B.Mask)
      (net 9 "Net-(K1-Pad3)"))
    (pad 3 np_thru_hole circle (at 0 5.08) (size 1.7 1.7) (drill 1) (layers B.Cu B.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (pad 4 np_thru_hole circle (at 0 7.62) (size 1.7 1.7) (drill 1) (layers B.Cu B.Mask)
      (net 3 "Net-(C2-Pad2)"))
    (pad 5 np_thru_hole circle (at 0 10.16) (size 1.7 1.7) (drill 1) (layers B.Cu B.Mask)
      (net 4 "Net-(C3-Pad2)"))
    (pad 6 np_thru_hole circle (at 0 12.7) (size 1.7 1.7) (drill 1) (layers B.Cu B.Mask)
      (net 5 "Net-(C4-Pad2)"))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x06_Pitch2.54mm.wrl
      (at (xyz 0 -0.25 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Connect:GS3 (layer F.Cu) (tedit 59702FD9)
    (at 126 102.5 90)
    (descr "3-pin solder bridge")
    (tags "solder bridge")
    (solder_mask_margin 0.25)
    (clearance 0.15)
    (attr virtual)
    (fp_text reference K1 (at -1.7 0 360) (layer B.SilkS) hide)
    (fp_text value CONN_3 (at 1.8 0 180) (layer F.Fab))
    (pad 1 smd rect (at 0 -2 90) (size 2.54 1.65) (layers B.Cu B.Mask)
      (net 6 "Net-(D1-Pad1)") (solder_mask_margin 0.2))
    (pad 2 smd rect (at 0 0 90) (size 2.54 1.65) (layers B.Cu B.Mask)
      (net 8 "Net-(K1-Pad2)") (solder_mask_margin 0.2))
    (pad 3 smd rect (at 0 2 90) (size 2.54 1.65) (layers B.Cu B.Mask)
      (net 9 "Net-(K1-Pad3)") (solder_mask_margin 0.2))
  )
  (module GNUCOMP:M3_mounting (layer F.Cu) (tedit 592E1C28)
    (at 142 148)
    (fp_text reference REF** (at 0 5) (layer F.SilkS) hide)
    (fp_text value M3_mounting (at 0 -5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu)
      (solder_mask_margin 0.1) (clearance 2.15) (zone_connect 0))
  )
  (module GNUCOMP:M3_mounting (layer F.Cu) (tedit 592E1C28)
    (at 125.5 148)
    (fp_text reference REF** (at 0 5) (layer F.SilkS) hide)
    (fp_text value M3_mounting (at 0 -5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu)
      (solder_mask_margin 0.1) (clearance 2.15) (zone_connect 0))
  )
  (module GNUCOMP:M3_mounting (layer F.Cu) (tedit 59703066)
    (at 142 84)
    (fp_text reference REF** (at 0 5) (layer F.SilkS) hide)
    (fp_text value M3_mounting (at 0 -5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu)
      (solder_mask_margin 0.1) (clearance 2) (zone_connect 0))
  )
  (module Measurement_Points:Measurement_Point_Square-SMD-Pad_Small (layer F.Cu) (tedit 59701AD0)
    (at 126 95.2)
    (descr "Mesurement Point, Square, SMD Pad,  1.5mm x 1.5mm,")
    (tags "Mesurement Point Square SMD Pad 1.5x1.5mm")
    (attr virtual)
    (fp_text reference P2 (at 0 -2) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 0 2) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 1.5 2) (layers B.Cu B.Mask)
      (net 8 "Net-(K1-Pad2)") (solder_mask_margin 0.25))
  )
  (module Measurement_Points:Measurement_Point_Square-SMD-Pad_Small (layer F.Cu) (tedit 59701AC7)
    (at 126 92.9)
    (descr "Mesurement Point, Square, SMD Pad,  1.5mm x 1.5mm,")
    (tags "Mesurement Point Square SMD Pad 1.5x1.5mm")
    (attr virtual)
    (fp_text reference P3 (at 0 -2) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 0 2) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 1.5 2) (layers B.Cu B.Mask)
      (net 1 "Net-(C1-Pad1)") (solder_mask_margin 0.25))
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 58AA84A8)
    (at 137.5 95.5 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (solder_mask_margin 0.1)
    (attr smd)
    (fp_text reference C1 (at 0 1.75 180) (layer B.SilkS))
    (fp_text value C (at 0 -1.75 180) (layer B.Fab))
    (fp_text user %R (at 0 1.75 180) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 58AA84A8)
    (at 137.5 125.5 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (solder_mask_margin 0.1)
    (attr smd)
    (fp_text reference C3 (at 0 1.75 180) (layer B.SilkS))
    (fp_text value C (at 0 -1.75 180) (layer B.Fab))
    (fp_text user %R (at 0 1.75 180) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(C3-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 597072B8)
    (at 126 89 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R2 (at 5 0 360) (layer F.SilkS) hide)
    (fp_text value 1k0 (at 5 0 270) (layer F.SilkS))
    (pad "" np_thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers B.Cu B.Mask))
    (pad 2 np_thru_hole circle (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers B.Cu B.Mask)
      (net 8 "Net-(K1-Pad2)"))
    (model Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 59703E70)
    (at 126 126 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R1 (at 5 0 360) (layer F.SilkS) hide)
    (fp_text value 330R (at 5 0 270) (layer F.SilkS))
    (pad "" np_thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers B.Cu B.Mask))
    (pad 2 np_thru_hole circle (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers B.Cu B.Mask)
      (net 7 "Net-(D1-Pad2)"))
    (model Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module GNUCOMP:M3_mounting (layer F.Cu) (tedit 59703077)
    (at 125.5 84)
    (fp_text reference REF** (at 0 5) (layer F.SilkS) hide)
    (fp_text value M3_mounting (at 0 -5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu)
      (solder_mask_margin 0.1) (clearance 2) (zone_connect 0))
  )
  (gr_text "GNUcomp 2017" (at 142.4 115.8 90) (layer F.Cu))
  (gr_text "(\n(" (at 125.75 100.5 90) (layer B.SilkS))
  (gr_text "High\n\nLow" (at 125.8 99.8 90) (layer B.SilkS))
  (gr_arc (start 122.5 151) (end 122.5 152) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 145 151) (end 146 151) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 145 81) (end 145 80) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 122.5 81) (end 121.5 81) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 121.5 151) (end 121.5 81) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text "4 x switch board for Arduino" (at 130 113.25 90) (layer F.SilkS))
  (gr_line (start 145 152) (end 122.5 152) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 146 81) (end 146 151) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 122.5 80) (end 145 80) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text "5V\n\nGND\n\n1\n\n2\n\n3\n\n4" (at 123.2 113.4) (layer F.SilkS))
  (gr_text SW4 (at 137.5 140.5) (layer F.SilkS))
  (gr_text SW3 (at 137.5 125.5) (layer F.SilkS))
  (gr_text SW2 (at 137.5 110.5) (layer F.SilkS))
  (gr_text SW1 (at 137.5 95.5) (layer F.SilkS))
)
