(kicad_pcb (version 20171130) (host pcbnew "(5.1.0)-1")
  (general
    (thickness 1.6)
    (drawings 26)
    (tracks 279)
    (zones 0)
    (modules 44)
    (nets 54)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user hide)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.381)
    (user_trace_width 0.1778)
    (user_trace_width 0.254)
    (user_trace_width 0.3048)
    (user_trace_width 0.381)
    (user_trace_width 0.508)
    (user_trace_width 0.635)
    (user_trace_width 0.762)
    (user_trace_width 1.016)
    (trace_clearance 0.1778)
    (zone_clearance 0.3556)
    (zone_45_only yes)
    (trace_min 0.1778)
    (via_size 0.69)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.32766)
    (user_via 0.6858 0.3302)
    (user_via 0.8636 0.508)
    (user_via 1.1176 0.762)
    (user_via 1.3716 1.016)
    (uvia_size 0.508)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (edge_width 0.15)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 0.508 0.508)
    (mod_text_width 0.127)
    (pad_size 1.7272 1.7272)
    (pad_drill 1.016)
    (pad_to_mask_clearance 0.1016)
    (aux_axis_origin 139.065 111.125)
    (visible_elements 7FFDDF7F)
    (pcbplotparams
      (layerselection 0x010fc_80000001)
      (usegerberextensions true)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue false)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "Gerber/"))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad10)")
  (net 2 "Net-(J1-Pad12)")
  (net 3 "Net-(J1-Pad6)")
  (net 4 "Net-(J1-Pad8)")
  (net 5 "Net-(J1-Pad3)")
  (net 6 "Net-(J1-Pad1)")
  (net 7 "Net-(J1-Pad5)")
  (net 8 "Net-(J1-Pad7)")
  (net 9 "Net-(J1-Pad9)")
  (net 10 "Net-(J1-Pad11)")
  (net 11 "Net-(J2-Pad8)")
  (net 12 "Net-(J2-Pad10)")
  (net 13 "Net-(J2-Pad11)")
  (net 14 "Net-(J2-Pad12)")
  (net 15 "Net-(J2-Pad13)")
  (net 16 "Net-(J2-Pad15)")
  (net 17 "Net-(J2-Pad16)")
  (net 18 "Net-(J2-Pad18)")
  (net 19 "Net-(J2-Pad19)")
  (net 20 "Net-(J2-Pad21)")
  (net 21 "Net-(J2-Pad22)")
  (net 22 "Net-(J2-Pad23)")
  (net 23 "Net-(J2-Pad24)")
  (net 24 "Net-(J2-Pad26)")
  (net 25 "Net-(J2-Pad27)")
  (net 26 "Net-(J2-Pad28)")
  (net 27 "Net-(J2-Pad29)")
  (net 28 "Net-(J2-Pad31)")
  (net 29 "Net-(J2-Pad32)")
  (net 30 "Net-(J2-Pad33)")
  (net 31 "Net-(J2-Pad35)")
  (net 32 "Net-(J2-Pad36)")
  (net 33 "Net-(J2-Pad37)")
  (net 34 "Net-(J2-Pad38)")
  (net 35 "Net-(J2-Pad40)")
  (net 36 GND)
  (net 37 "Net-(C1-Pad1)")
  (net 38 "Net-(C2-Pad1)")
  (net 39 "Net-(C3-Pad1)")
  (net 40 "Net-(C4-Pad1)")
  (net 41 "Net-(C5-Pad1)")
  (net 42 "Net-(C6-Pad1)")
  (net 43 "Net-(C7-Pad1)")
  (net 44 "Net-(C8-Pad1)")
  (net 45 "Net-(C9-Pad2)")
  (net 46 "Net-(C9-Pad1)")
  (net 47 "Net-(C10-Pad1)")
  (net 48 +3V3)
  (net 49 +5V)
  (net 50 SDA)
  (net 51 SCL)
  (net 52 Alert)
  (net 53 "Net-(R17-Pad3)")
  (net_class Default "This is the default net class."
    (clearance 0.1778)
    (trace_width 0.1778)
    (via_dia 0.69)
    (via_drill 0.3302)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net +3V3)
    (add_net +5V)
    (add_net Alert)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C10-Pad1)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(C6-Pad1)")
    (add_net "Net-(C7-Pad1)")
    (add_net "Net-(C8-Pad1)")
    (add_net "Net-(C9-Pad1)")
    (add_net "Net-(C9-Pad2)")
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad10)")
    (add_net "Net-(J1-Pad11)")
    (add_net "Net-(J1-Pad12)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J1-Pad7)")
    (add_net "Net-(J1-Pad8)")
    (add_net "Net-(J1-Pad9)")
    (add_net "Net-(J2-Pad10)")
    (add_net "Net-(J2-Pad11)")
    (add_net "Net-(J2-Pad12)")
    (add_net "Net-(J2-Pad13)")
    (add_net "Net-(J2-Pad15)")
    (add_net "Net-(J2-Pad16)")
    (add_net "Net-(J2-Pad18)")
    (add_net "Net-(J2-Pad19)")
    (add_net "Net-(J2-Pad21)")
    (add_net "Net-(J2-Pad22)")
    (add_net "Net-(J2-Pad23)")
    (add_net "Net-(J2-Pad24)")
    (add_net "Net-(J2-Pad26)")
    (add_net "Net-(J2-Pad27)")
    (add_net "Net-(J2-Pad28)")
    (add_net "Net-(J2-Pad29)")
    (add_net "Net-(J2-Pad31)")
    (add_net "Net-(J2-Pad32)")
    (add_net "Net-(J2-Pad33)")
    (add_net "Net-(J2-Pad35)")
    (add_net "Net-(J2-Pad36)")
    (add_net "Net-(J2-Pad37)")
    (add_net "Net-(J2-Pad38)")
    (add_net "Net-(J2-Pad40)")
    (add_net "Net-(J2-Pad8)")
    (add_net "Net-(R17-Pad3)")
    (add_net SCL)
    (add_net SDA)
  )
  (module Housings_SSOP:TSSOP-16_4.4x5mm_Pitch0.65mm (layer F.Cu) (tedit 54130A77)
    (at 145.415 79.375 90)
    (descr "16-Lead Plastic Thin Shrink Small Outline (ST)-4.4 mm Body [TSSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U2 (at -3.175 -3.55 90) (layer F.SilkS))
    (fp_text value NCD9830 (at 0 3.55 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -2.95 -2.275 90) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at -2.95 -1.625 90) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(C2-Pad1)"))
    (pad 3 smd rect (at -2.95 -0.975 90) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(C3-Pad1)"))
    (pad 4 smd rect (at -2.95 -0.325 90) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(C4-Pad1)"))
    (pad 5 smd rect (at -2.95 0.325 90) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(C5-Pad1)"))
    (pad 6 smd rect (at -2.95 0.975 90) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(C6-Pad1)"))
    (pad 7 smd rect (at -2.95 1.625 90) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(C7-Pad1)"))
    (pad 8 smd rect (at -2.95 2.275 90) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(C8-Pad1)"))
    (pad 9 smd rect (at 2.95 2.275 90) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 36 GND))
    (pad 10 smd rect (at 2.95 1.625 90) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(C10-Pad1)"))
    (pad 11 smd rect (at 2.95 0.975 90) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 36 GND))
    (pad 12 smd rect (at 2.95 0.325 90) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 36 GND))
    (pad 13 smd rect (at 2.95 -0.325 90) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 36 GND))
    (pad 14 smd rect (at 2.95 -0.975 90) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 51 SCL))
    (pad 15 smd rect (at 2.95 -1.625 90) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 50 SDA))
    (pad 16 smd rect (at 2.95 -2.275 90) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 48 +3V3))
    (model ${KISYS3DMOD}/Housings_SSOP.3dshapes/TSSOP-16_4.4x5mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module digikey-footprints:MSOP-10_W3mm (layer F.Cu) (tedit 596E4A9E)
    (at 121.92 80.645 180)
    (fp_text reference U1 (at -1.905 2.54 270) (layer F.SilkS))
    (fp_text value INA233 (at 0 4.8 180) (layer F.Fab))
    (fp_text user REF** (at 0 0 180) (layer F.Fab))
    (pad 10 smd rect (at -1 -2.2 180) (size 0.3 1.45) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(C9-Pad1)") (solder_mask_margin 0.05))
    (pad 9 smd rect (at -0.5 -2.2 180) (size 0.3 1.45) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(C9-Pad2)") (solder_mask_margin 0.05))
    (pad 8 smd rect (at 0 -2.2 180) (size 0.3 1.45) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(J1-Pad3)") (solder_mask_margin 0.05))
    (pad 7 smd rect (at 0.5 -2.2 180) (size 0.3 1.45) (layers F.Cu F.Paste F.Mask)
      (net 36 GND) (solder_mask_margin 0.05))
    (pad 5 smd rect (at 1 2.2 180) (size 0.3 1.45) (layers F.Cu F.Paste F.Mask)
      (net 51 SCL) (solder_mask_margin 0.05))
    (pad 4 smd rect (at 0.5 2.2 180) (size 0.3 1.45) (layers F.Cu F.Paste F.Mask)
      (net 50 SDA) (solder_mask_margin 0.05))
    (pad 3 smd rect (at 0 2.2 180) (size 0.3 1.45) (layers F.Cu F.Paste F.Mask)
      (net 52 Alert) (solder_mask_margin 0.05))
    (pad 2 smd rect (at -0.5 2.2 180) (size 0.3 1.45) (layers F.Cu F.Paste F.Mask)
      (net 36 GND) (solder_mask_margin 0.05))
    (pad 6 smd rect (at 1 -2.2 180) (size 0.3 1.45) (layers F.Cu F.Paste F.Mask)
      (net 48 +3V3) (solder_mask_margin 0.05))
    (pad 1 smd rect (at -1 2.2 180) (size 0.3 1.45) (layers F.Cu F.Paste F.Mask)
      (net 36 GND) (solder_mask_margin 0.05))
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 128.905 77.47)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R21 (at 0 -1.45) (layer F.SilkS))
    (fp_text value 10k (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 48 +3V3))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 50 SDA))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 128.905 80.645)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R20 (at 0 1.27) (layer F.SilkS))
    (fp_text value 10k (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 48 +3V3))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 51 SCL))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 124.46 75.565 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R19 (at 0 -1.27 180) (layer F.SilkS))
    (fp_text value 10k (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 48 +3V3))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 52 Alert))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 123.19 85.725 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R18 (at 0 -1.45 270) (layer F.SilkS))
    (fp_text value 5 (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(C9-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(R17-Pad3)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module PJS_smt_parts:LVK12 (layer F.Cu) (tedit 5D6D8CAB)
    (at 121.92 88.9)
    (fp_text reference R17 (at 0 2.032) (layer F.SilkS))
    (fp_text value LVK12R010DER (at 0 -2.159) (layer F.Fab))
    (pad 4 smd rect (at 1.375 0.7) (size 1.75 1.1) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(J1-Pad3)"))
    (pad 3 smd rect (at 1.375 -0.7) (size 1.75 1.1) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(R17-Pad3)"))
    (pad 2 smd rect (at -1.375 -0.7) (size 1.75 1.1) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(C9-Pad2)"))
    (pad 1 smd rect (at -1.375 0.7) (size 1.75 1.1) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(J1-Pad1)"))
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 157.48 87.63 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R16 (at 3.175 0 180) (layer F.SilkS))
    (fp_text value 100k (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(C8-Pad1)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 36 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 153.67 87.63 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R15 (at 3.175 0 180) (layer F.SilkS))
    (fp_text value 100k (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(C7-Pad1)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 36 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 149.86 87.63 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R14 (at 3.175 0 180) (layer F.SilkS))
    (fp_text value 100k (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(C6-Pad1)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 36 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 146.05 87.63 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R13 (at 3.175 0 180) (layer F.SilkS))
    (fp_text value 100k (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(C5-Pad1)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 36 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 142.24 87.63 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R12 (at 3.175 0 180) (layer F.SilkS))
    (fp_text value 100k (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(C4-Pad1)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 36 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 138.43 87.63 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R11 (at 3.175 0 180) (layer F.SilkS))
    (fp_text value 100k (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 36 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 134.62 87.63 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R10 (at 3.175 0 180) (layer F.SilkS))
    (fp_text value 100k (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 36 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 130.81 87.63 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R9 (at 3.175 0 180) (layer F.SilkS))
    (fp_text value 100k (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 36 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 158.115 90.17)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R8 (at -1.905 0 90) (layer F.SilkS))
    (fp_text value 500k (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J1-Pad12)"))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(C8-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 154.305 90.17)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R7 (at -1.905 0 90) (layer F.SilkS))
    (fp_text value 500k (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(J1-Pad11)"))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(C7-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 150.495 90.17)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R6 (at -1.905 0 90) (layer F.SilkS))
    (fp_text value 140k (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(J1-Pad10)"))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(C6-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 146.685 90.17)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at -1.905 0 90) (layer F.SilkS))
    (fp_text value 140k (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(C5-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(J1-Pad9)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 142.875 90.17)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at -1.905 0 90) (layer F.SilkS))
    (fp_text value 140k (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(C4-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J1-Pad8)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 139.065 90.17)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at -1.905 0 90) (layer F.SilkS))
    (fp_text value 60k (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(J1-Pad7)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 135.255 90.17)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at -1.905 0 90) (layer F.SilkS))
    (fp_text value 60k (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J1-Pad6)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 131.445 90.17)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at -1.905 0 90) (layer F.SilkS))
    (fp_text value 60k (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(J1-Pad5)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TerminalBlocks_Phoenix:TerminalBlock_Phoenix_PT-3.5mm_12pol (layer F.Cu) (tedit 59FF0755)
    (at 118.73 94.615)
    (descr "12-way 3.5mm pitch terminal block, Phoenix PT series")
    (fp_text reference J1 (at -1.89 -3.81) (layer F.SilkS))
    (fp_text value OSTTE120104 (at 19.25 6) (layer F.Fab))
    (fp_text user %R (at 19.25 0) (layer F.Fab))
    (pad 3 thru_hole circle (at 7 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad3)"))
    (pad 2 thru_hole circle (at 3.5 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 36 GND))
    (pad 4 thru_hole circle (at 10.5 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 36 GND))
    (pad 5 thru_hole circle (at 14 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-Pad5)"))
    (pad 6 thru_hole circle (at 17.5 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad6)"))
    (pad 7 thru_hole circle (at 21 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 8 "Net-(J1-Pad7)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad1)"))
    (pad 8 thru_hole circle (at 24.5 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad8)"))
    (pad 9 thru_hole circle (at 28 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 9 "Net-(J1-Pad9)"))
    (pad 10 thru_hole circle (at 31.5 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad10)"))
    (pad 11 thru_hole circle (at 35 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 10 "Net-(J1-Pad11)"))
    (pad 12 thru_hole circle (at 38.5 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad12)"))
    (model ${KISYS3DMOD}/TerminalBlock_Phoenix.3dshapes/TerminalBlock_Phoenix_PT-3.5mm_12pol.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module PJS-icons:metroid (layer F.Cu) (tedit 5A0106A6)
    (at 114.3 94.615)
    (fp_text reference icon1 (at 0 2.54) (layer F.Fab) hide)
    (fp_text value Metroid (at 0 -2.54) (layer F.SilkS) hide)
    (pad "" smd circle (at 0 -0.635) (size 0.635 0.635) (layers F.Cu F.Paste F.Mask))
    (pad "" smd circle (at 0.635 0) (size 0.635 0.635) (layers F.Cu F.Paste F.Mask))
    (pad "" smd circle (at -0.635 0) (size 0.635 0.635) (layers F.Cu F.Paste F.Mask))
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58AA8463)
    (at 113.665 76.835 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C14 (at 0 -1.5 270) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 48 +3V3))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 36 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58AA8463)
    (at 132.715 75.565 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C13 (at 0 -1.5 180) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 180) (layer F.Fab))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 48 +3V3))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 36 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 140.335 76.2 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C12 (at 0 1.27 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 36 GND))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 48 +3V3))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 118.745 81.915 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C11 (at 0 -1.5 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 36 GND))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 48 +3V3))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 149.86 78.105 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C10 (at 0 1.27 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 36 GND))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(C10-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 120.65 86.36 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C9 (at 0 1.27 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(C9-Pad2)"))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(C9-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 159.385 87.63 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C8 (at 3.175 0 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 36 GND))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(C8-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 155.575 87.63 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C7 (at 3.175 0 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 36 GND))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(C7-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 151.765 87.63 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C6 (at 3.175 0 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 36 GND))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(C6-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 147.955 87.63 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C5 (at 3.175 0 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 36 GND))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(C5-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 144.145 87.63 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C4 (at 3.175 0 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 36 GND))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(C4-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 140.335 87.63 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C3 (at 3.175 0 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 36 GND))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(C3-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 136.525 87.63 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at 3.175 0 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 36 GND))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(C2-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 132.715 87.63 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at 3.175 0 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 36 GND))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(C1-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RPi_Hat:RPi_Hat_Mounting_Hole locked (layer F.Cu) (tedit 55217CCB)
    (at 108.71 94.18)
    (descr "Mounting hole, Befestigungsbohrung, 2,7mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,7mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -4.0005) (layer F.SilkS) hide)
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 2.75 2.75) (drill 2.75) (layers *.Cu *.Mask)
      (solder_mask_margin 1.725) (clearance 1.725))
  )
  (module RPi_Hat:RPi_Hat_Mounting_Hole locked (layer F.Cu) (tedit 55217C7B)
    (at 166.71 71.18)
    (descr "Mounting hole, Befestigungsbohrung, 2,7mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,7mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -4.0005) (layer F.SilkS) hide)
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 2.75 2.75) (drill 2.75) (layers *.Cu *.Mask)
      (solder_mask_margin 1.725) (clearance 1.725))
  )
  (module RPi_Hat:RPi_Hat_Mounting_Hole locked (layer F.Cu) (tedit 55217CCB)
    (at 166.71 94.18)
    (descr "Mounting hole, Befestigungsbohrung, 2,7mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,7mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -4.0005) (layer F.SilkS) hide)
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 2.75 2.75) (drill 2.75) (layers *.Cu *.Mask)
      (solder_mask_margin 1.725) (clearance 1.725))
  )
  (module RPi_Hat:RPi_Hat_Mounting_Hole locked (layer F.Cu) (tedit 55217CA2)
    (at 108.71 71.18)
    (descr "Mounting hole, Befestigungsbohrung, 2,7mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,7mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -4.0005) (layer F.SilkS) hide)
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 2.75 2.75) (drill 2.75) (layers *.Cu *.Mask)
      (solder_mask_margin 1.725) (clearance 1.725))
  )
  (module Pin_Headers:Pin_Header_Straight_2x20_Pitch2.54mm (layer F.Cu) (tedit 59650533)
    (at 113.58 72.45 90)
    (descr "Through hole straight pin header, 2x20, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x20 2.54mm double row")
    (fp_text reference J2 (at -1.845 -1.82 180) (layer F.SilkS))
    (fp_text value Raspberry_Pi_2_3 (at 1.27 50.59 90) (layer F.Fab))
    (fp_text user %R (at 1.27 24.13 180) (layer F.Fab))
    (pad 40 thru_hole oval (at 2.54 48.26 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 "Net-(J2-Pad40)"))
    (pad 39 thru_hole oval (at 0 48.26 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 GND))
    (pad 38 thru_hole oval (at 2.54 45.72 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 "Net-(J2-Pad38)"))
    (pad 37 thru_hole oval (at 0 45.72 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 "Net-(J2-Pad37)"))
    (pad 36 thru_hole oval (at 2.54 43.18 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 "Net-(J2-Pad36)"))
    (pad 35 thru_hole oval (at 0 43.18 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 "Net-(J2-Pad35)"))
    (pad 34 thru_hole oval (at 2.54 40.64 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 GND))
    (pad 33 thru_hole oval (at 0 40.64 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 "Net-(J2-Pad33)"))
    (pad 32 thru_hole oval (at 2.54 38.1 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 "Net-(J2-Pad32)"))
    (pad 31 thru_hole oval (at 0 38.1 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 "Net-(J2-Pad31)"))
    (pad 30 thru_hole oval (at 2.54 35.56 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 GND))
    (pad 29 thru_hole oval (at 0 35.56 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 "Net-(J2-Pad29)"))
    (pad 28 thru_hole oval (at 2.54 33.02 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "Net-(J2-Pad28)"))
    (pad 27 thru_hole oval (at 0 33.02 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 "Net-(J2-Pad27)"))
    (pad 26 thru_hole oval (at 2.54 30.48 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(J2-Pad26)"))
    (pad 25 thru_hole oval (at 0 30.48 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 GND))
    (pad 24 thru_hole oval (at 2.54 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(J2-Pad24)"))
    (pad 23 thru_hole oval (at 0 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(J2-Pad23)"))
    (pad 22 thru_hole oval (at 2.54 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(J2-Pad22)"))
    (pad 21 thru_hole oval (at 0 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(J2-Pad21)"))
    (pad 20 thru_hole oval (at 2.54 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 GND))
    (pad 19 thru_hole oval (at 0 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(J2-Pad19)"))
    (pad 18 thru_hole oval (at 2.54 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(J2-Pad18)"))
    (pad 17 thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 48 +3V3))
    (pad 16 thru_hole oval (at 2.54 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(J2-Pad16)"))
    (pad 15 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(J2-Pad15)"))
    (pad 14 thru_hole oval (at 2.54 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 GND))
    (pad 13 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(J2-Pad13)"))
    (pad 12 thru_hole oval (at 2.54 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(J2-Pad12)"))
    (pad 11 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(J2-Pad11)"))
    (pad 10 thru_hole oval (at 2.54 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(J2-Pad10)"))
    (pad 9 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 GND))
    (pad 8 thru_hole oval (at 2.54 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(J2-Pad8)"))
    (pad 7 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 52 Alert))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 GND))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 51 SCL))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 49 +5V))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 50 SDA))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 49 +5V))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 48 +3V3))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x20_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "Copyright (c) 2019 Peter Shabino\n\nPermission is hereby granted, free of charge, to any person obtaining a copy of this hardware, software, and associated documentation files \n(the \"Product\"), to deal in the Product without restriction, including without limitation the rights to use, copy, modify, merge, publish, \ndistribute, sublicense, and/or sell copies of the Product, and to permit persons to whom the Product is furnished to do so, subject to the \nfollowing conditions:\n\nThe above copyright notice and this permission notice shall be included in all copies or substantial portions of the Product.\n\nTHE PRODUCT IS PROVIDED \"AS IS\", WITHOUT WARRANTY OF ANY KIND, EXPRESS OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES OF \nMERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE AND NONINFRINGEMENT. IN NO EVENT SHALL THE AUTHORS OR COPYRIGHT HOLDERS BE LIABLE \nFOR ANY CLAIM, DAMAGES OR OTHER LIABILITY, WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE, ARISING FROM, OUT OF OR IN CONNECTION \nWITH THE PRODUCT OR THE USE OR OTHER DEALINGS IN THE PRODUCT." (at 178.435 173.99) (layer B.SilkS))
  (gr_text "Copyright (c) 2019 Peter Shabino\n\nPermission is hereby granted, free of charge, to any person obtaining a copy of this hardware, software, and associated documentation files \n(the \"Product\"), to deal in the Product without restriction, including without limitation the rights to use, copy, modify, merge, publish, \ndistribute, sublicense, and/or sell copies of the Product, and to permit persons to whom the Product is furnished to do so, subject to the \nfollowing conditions:\n\nThe above copyright notice and this permission notice shall be included in all copies or substantial portions of the Product.\n\nTHE PRODUCT IS PROVIDED \"AS IS\", WITHOUT WARRANTY OF ANY KIND, EXPRESS OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES OF \nMERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE AND NONINFRINGEMENT. IN NO EVENT SHALL THE AUTHORS OR COPYRIGHT HOLDERS BE LIABLE \nFOR ANY CLAIM, DAMAGES OR OTHER LIABILITY, WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE, ARISING FROM, OUT OF OR IN CONNECTION \nWITH THE PRODUCT OR THE USE OR OTHER DEALINGS IN THE PRODUCT." (at 178.435 173.99) (layer F.SilkS))
  (gr_text "Copyright (c) 2019 Peter Shabino\n\nPermission is hereby granted, free of charge, to any person obtaining a copy of this hardware, software, and associated documentation files \n(the \"Product\"), to deal in the Product without restriction, including without limitation the rights to use, copy, modify, merge, publish, \ndistribute, sublicense, and/or sell copies of the Product, and to permit persons to whom the Product is furnished to do so, subject to the \nfollowing conditions:\n\nThe above copyright notice and this permission notice shall be included in all copies or substantial portions of the Product.\n\nTHE PRODUCT IS PROVIDED \"AS IS\", WITHOUT WARRANTY OF ANY KIND, EXPRESS OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES OF \nMERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE AND NONINFRINGEMENT. IN NO EVENT SHALL THE AUTHORS OR COPYRIGHT HOLDERS BE LIABLE \nFOR ANY CLAIM, DAMAGES OR OTHER LIABILITY, WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE, ARISING FROM, OUT OF OR IN CONNECTION \nWITH THE PRODUCT OR THE USE OR OTHER DEALINGS IN THE PRODUCT." (at 178.435 173.99) (layer B.Cu))
  (gr_text "Copyright (c) 2019 Peter Shabino\n\nPermission is hereby granted, free of charge, to any person obtaining a copy of this hardware, software, and associated documentation files \n(the \"Product\"), to deal in the Product without restriction, including without limitation the rights to use, copy, modify, merge, publish, \ndistribute, sublicense, and/or sell copies of the Product, and to permit persons to whom the Product is furnished to do so, subject to the \nfollowing conditions:\n\nThe above copyright notice and this permission notice shall be included in all copies or substantial portions of the Product.\n\nTHE PRODUCT IS PROVIDED \"AS IS\", WITHOUT WARRANTY OF ANY KIND, EXPRESS OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES OF \nMERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE AND NONINFRINGEMENT. IN NO EVENT SHALL THE AUTHORS OR COPYRIGHT HOLDERS BE LIABLE \nFOR ANY CLAIM, DAMAGES OR OTHER LIABILITY, WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE, ARISING FROM, OUT OF OR IN CONNECTION \nWITH THE PRODUCT OR THE USE OR OTHER DEALINGS IN THE PRODUCT." (at 178.435 173.99) (layer F.Cu))
  (gr_text "PJS 07Sep2019 MIT license \nRPi battery power logger\nwww.wire2wire.org" (at 167.005 82.55 90) (layer F.SilkS))
  (gr_text "PJS 07Sep2019 MIT license \nRPi battery power logger\nwww.wire2wire.org" (at 143.51 81.28) (layer B.SilkS))
  (gr_text "Vreg 8 in\n(15V max)" (at 157.226 90.17 270) (layer B.SilkS))
  (gr_text "Vreg 7 in\n(15V max)" (at 153.67 90.17 270) (layer B.SilkS))
  (gr_text "Vreg 6 in\n(6V max)" (at 150.241 90.17 270) (layer B.SilkS))
  (gr_text "Vreg 5 in\n(6V max)" (at 146.685 90.17 270) (layer B.SilkS))
  (gr_text "Vreg 4 in\n(6V max)" (at 143.256 90.17 270) (layer B.SilkS))
  (gr_text "Vreg 3 in\n(4V max)" (at 139.7 90.17 270) (layer B.SilkS))
  (gr_text "Vreg 2 in\n(4V max)" (at 136.271 90.17 270) (layer B.SilkS))
  (gr_text "Vreg 1 in\n(4V max)" (at 132.715 90.17 270) (layer B.SilkS))
  (gr_text Gnd (at 129.159 91.44 270) (layer B.SilkS))
  (gr_text Gnd (at 122.174 91.44 270) (layer B.SilkS))
  (gr_text "Vbat in (36V max)" (at 125.73 87.63 270) (layer B.SilkS))
  (gr_text "Vbat out (36V max)" (at 118.745 87.63 270) (layer B.SilkS))
  (gr_arc (start 108.21 70.68) (end 105.21 70.68) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 108.21 67.68) (end 167.21 67.68) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 167.21 70.68) (end 167.21 67.68) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 167.21 94.68) (end 170.21 94.68) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 108.21 94.68) (end 108.21 97.68) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 105.21 70.68) (end 105.21 94.68) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 108.21 97.68) (end 167.21 97.68) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 170.21 70.68) (end 170.21 94.68) (angle 90) (layer Edge.Cuts) (width 0.1))
  (zone (net 36) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3556))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 104.775 67.31) (xy 170.815 67.31) (xy 170.815 98.425) (xy 104.775 98.425)
      )
    )
  )
  (zone (net 36) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3556))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 104.775 67.31) (xy 170.815 67.31) (xy 170.815 98.425) (xy 104.775 98.425)
      )
    )
  )
)
