(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 23)
    (no_connects 2)
    (area 49.708999 63.932999 64.591001 79.323001)
    (thickness 1.6)
    (drawings 22)
    (tracks 136)
    (zones 0)
    (modules 8)
    (nets 10)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.1778)
    (zone_45_only no)
    (trace_min 0.1778)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF5F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(C35-Pad2)")
  (net 3 /sheet5A330123/I_IN)
  (net 4 "Net-(U6-Pad5)")
  (net 5 /sheet5A330123/GUARD)
  (net 6 "Net-(R108-Pad2)")
  (net 7 "Net-(C36-Pad1)")
  (net 8 "Net-(C36-Pad2)")
  (net 9 "Net-(R57-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /sheet5A330123/GUARD)
    (add_net /sheet5A330123/I_IN)
    (add_net GND)
    (add_net "Net-(C35-Pad2)")
    (add_net "Net-(C36-Pad1)")
    (add_net "Net-(C36-Pad2)")
    (add_net "Net-(R108-Pad2)")
    (add_net "Net-(R57-Pad2)")
    (add_net "Net-(U6-Pad5)")
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5A398F9C)
    (at 53.975 66.5226)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C35 (at 3.3782 0) (layer F.SilkS))
    (fp_text value 0.1u (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.5) (layer F.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C35-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5A387F15)
    (at 55.9054 76.2 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C36 (at -0.0254 1.6002 180) (layer F.SilkS) hide)
    (fp_text value 10pF (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 180) (layer F.Fab))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C36-Pad1)"))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C36-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:SMS-201 locked (layer F.Cu) (tedit 5A1DF9B5)
    (at 50.419 64.2874)
    (fp_text reference J17 (at 12 -1) (layer F.SilkS) hide)
    (fp_text value RF_Shield_One_Piece (at 3 -1) (layer F.Fab) hide)
    (pad 1 smd rect (at 6.7945 14.0208 90) (size 0.9906 3.7846) (layers F.Cu F.Paste F.Mask)
      (net 5 /sheet5A330123/GUARD))
    (pad 1 smd rect (at 6.7945 0.508 90) (size 0.9906 3.7846) (layers F.Cu F.Paste F.Mask)
      (net 5 /sheet5A330123/GUARD))
    (pad 1 smd rect (at 0.508 12.9413 180) (size 0.9906 3.175) (layers F.Cu F.Paste F.Mask)
      (net 5 /sheet5A330123/GUARD))
    (pad 1 smd rect (at 1.3716 14.0208) (size 2.7432 0.9906) (layers F.Cu F.Paste F.Mask)
      (net 5 /sheet5A330123/GUARD))
    (pad 1 smd rect (at 12.0396 14.0208 270) (size 0.9906 3.0988) (layers F.Cu F.Paste F.Mask)
      (net 5 /sheet5A330123/GUARD))
    (pad 1 smd rect (at 13.1064 2 180) (size 0.9906 3.175) (layers F.Cu F.Paste F.Mask)
      (net 5 /sheet5A330123/GUARD))
    (pad 1 smd rect (at 12.0396 0.508 270) (size 0.9906 3.0988) (layers F.Cu F.Paste F.Mask)
      (net 5 /sheet5A330123/GUARD))
    (pad 1 smd rect (at 13.1064 12.9413) (size 0.9906 3.175) (layers F.Cu F.Paste F.Mask)
      (net 5 /sheet5A330123/GUARD))
    (pad 1 smd rect (at 1.3716 0.508 90) (size 0.9906 2.7432) (layers F.Cu F.Paste F.Mask)
      (net 5 /sheet5A330123/GUARD))
    (pad 1 smd rect (at 13.1064 7.2517) (size 0.9906 3.7846) (layers F.Cu F.Paste F.Mask)
      (net 5 /sheet5A330123/GUARD))
    (pad 1 smd rect (at 0.508 7.2517) (size 0.762 3.7846) (layers F.Cu F.Paste F.Mask)
      (net 5 /sheet5A330123/GUARD))
    (pad 1 smd rect (at 0.508 1.7145) (size 0.9906 3.175) (layers F.Cu F.Paste F.Mask)
      (net 5 /sheet5A330123/GUARD))
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5A387F2C)
    (at 55.88 74.2696 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R55 (at 0 -1.65 180) (layer F.SilkS) hide)
    (fp_text value 100M (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C36-Pad1)"))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C36-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5A398F8B)
    (at 59.7154 76.2508 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R57 (at -2.3876 0.2032 270) (layer F.SilkS))
    (fp_text value 0 (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(R57-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5A398F80)
    (at 59.7408 74.2188 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R60 (at -2.3368 0.9652 270) (layer F.SilkS))
    (fp_text value 10K (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(R108-Pad2)"))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(R57-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 5A398F5D)
    (at 55.5752 70.2818 180)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U6 (at 0.127 1.2446 180) (layer F.SilkS))
    (fp_text value lmp7721 (at 0 3.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -1.905 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(R57-Pad2)"))
    (pad 2 smd rect (at -2.7 -0.635 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 /sheet5A330123/GUARD))
    (pad 3 smd rect (at -2.7 0.635 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at -2.7 1.905 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C36-Pad1)"))
    (pad 5 smd rect (at 2.7 1.905 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(U6-Pad5)"))
    (pad 6 smd rect (at 2.7 0.635 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C35-Pad2)"))
    (pad 7 smd rect (at 2.7 -0.635 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 /sheet5A330123/GUARD))
    (pad 8 smd rect (at 2.7 -1.905 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C36-Pad2)"))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5A397FD2)
    (at 52.9082 75.1586 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R64 (at 0 -1.65 270) (layer F.SilkS) hide)
    (fp_text value 100 (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C36-Pad2)"))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 /sheet5A330123/I_IN))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 64.516 64.008) (end 49.784 64.008) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 64.516 79.248) (end 64.516 64.008) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 49.784 79.248) (end 64.516 79.248) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 49.784 64.008) (end 49.784 79.248) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text "ground plane or separate guard plane for tia?" (at 72.136 55.372) (layer Cmts.User))
  (gr_text "INST AMP" (at 72.7456 87.7824) (layer Cmts.User))
  (gr_text TIA (at 76.6064 69.4944) (layer Cmts.User))
  (gr_text "PRECISION MIDPOINT" (at 119.2784 103.4288) (layer Cmts.User))
  (gr_text "GUARD BUFFER" (at 122.3264 54.864) (layer Cmts.User))
  (gr_text "LNA FRONTEND" (at 101.8032 49.784) (layer Cmts.User))
  (gr_text PWR (at 141.6304 56.0832) (layer Cmts.User))
  (zone (net 0) (net_name "") (layer B.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.1778))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 49.0982 80.5434) (xy 49.0982 81.0514) (xy 49.5554 81.4832) (xy 54.1528 81.4832) (xy 55.626 79.9846)
        (xy 55.6006 79.2988) (xy 55.9308 78.8924) (xy 59.3598 78.9178) (xy 60.325 77.9018) (xy 60.2996 71.12)
        (xy 59.7662 70.6628) (xy 51.9938 70.6374) (xy 51.6636 70.7136) (xy 50.9016 71.374) (xy 47.3202 71.4756)
        (xy 46.355 72.263) (xy 46.3804 75.3364) (xy 48.4886 77.4446) (xy 51.054 77.47) (xy 52.2478 78.6384)
        (xy 52.8828 78.6384) (xy 53.4924 79.248) (xy 53.4924 79.502) (xy 53.0352 79.9084) (xy 49.7078 79.9084)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.1778))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 59.7662 70.6628) (xy 60.2996 71.12) (xy 60.325 77.9018) (xy 59.3598 78.9178) (xy 55.9308 78.8924)
        (xy 55.6006 79.2988) (xy 55.626 79.9846) (xy 54.1528 81.4832) (xy 52.013585 81.4832) (xy 52.0446 82.2198)
        (xy 52.0954 82.6008) (xy 57.15 82.6516) (xy 57.1246 83.2358) (xy 56.5404 83.8454) (xy 56.515 85.344)
        (xy 56.515 93.8276) (xy 51.7906 93.8276) (xy 50.7238 95.2754) (xy 44.3484 95.2754) (xy 43.688 94.5896)
        (xy 42.6212 94.5896) (xy 42.6212 94.2086) (xy 42.2148 94.2086) (xy 41.8084 93.7768) (xy 39.4716 93.7768)
        (xy 38.0746 92.4052) (xy 38.1 85.2678) (xy 40.0558 83.312) (xy 41.5036 83.312) (xy 43.18 81.6356)
        (xy 44.5008 81.661) (xy 45.7708 80.3402) (xy 45.7708 77.6986) (xy 46.228 77.3176) (xy 47.8536 77.3176)
        (xy 48.7426 78.1558) (xy 48.7426 79.8068) (xy 51.943 79.8068) (xy 51.947278 79.9084) (xy 53.0352 79.9084)
        (xy 53.4924 79.502) (xy 53.4924 79.248) (xy 52.8828 78.6384) (xy 52.2478 78.6384) (xy 51.054 77.47)
        (xy 48.4886 77.4446) (xy 46.3804 75.3364) (xy 46.355 72.263) (xy 47.3202 71.4756) (xy 50.9016 71.374)
        (xy 51.6636 70.7136) (xy 51.9938 70.6374)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1778))
    (min_thickness 0.1778)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 69.088 81.788) (xy 48.26 81.534) (xy 48.768 63.754) (xy 66.802 60.198)
      )
    )
  )
)
