(kicad_pcb (version 20170123) (host pcbnew "(2017-03-07 revision cf373e543)-makepkg")
  (general
    (links 57)
    (no_connects 0)
    (area 134.337667 66.08375 159.794334 112.9865)
    (thickness 1.6)
    (drawings 23)
    (tracks 195)
    (zones 0)
    (modules 33)
    (nets 49)
  )
  (page A4)
  (title_block
    (date "jeu. 02 avril 2015")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.15)
    (edge_width 0.1)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 0.5 0.5)
    (mod_text_width 0.125)
    (pad_size 1.5 1.5)
    (pad_drill 0.6)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 138.176 110.617)
    (grid_origin 143.159411 81.749783)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010f0_ffffffff)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "/1(Tx)")
  (net 2 "/0(Rx)")
  (net 3 /Reset)
  (net 4 GND)
  (net 5 /2)
  (net 6 "/3(**)")
  (net 7 /4)
  (net 8 "/5(**)")
  (net 9 "/6(**)")
  (net 10 /7)
  (net 11 /8)
  (net 12 "/9(**)")
  (net 13 "/10(**/SS)")
  (net 14 "/11(**/MISO)")
  (net 15 "/12(MOSI)")
  (net 16 /Vin)
  (net 17 +5V)
  (net 18 /A7)
  (net 19 /A6)
  (net 20 /A5)
  (net 21 /A4)
  (net 22 /A3)
  (net 23 /A2)
  (net 24 /A0)
  (net 25 /AREF)
  (net 26 "/13(SCK)")
  (net 27 "Net-(P3-Pad1)")
  (net 28 "Net-(P4-Pad1)")
  (net 29 "Net-(P5-Pad1)")
  (net 30 "Net-(P6-Pad1)")
  (net 31 +3V3)
  (net 32 "Net-(R1-Pad2)")
  (net 33 "Net-(C1-Pad2)")
  (net 34 /A1)
  (net 35 "Net-(R6-Pad1)")
  (net 36 +BATT)
  (net 37 "Net-(R5-Pad1)")
  (net 38 "Net-(D1-Pad1)")
  (net 39 "Net-(R7-Pad2)")
  (net 40 "Net-(J4-Pad2)")
  (net 41 "Net-(D3-Pad4)")
  (net 42 "Net-(D3-Pad6)")
  (net 43 "Net-(D3-Pad5)")
  (net 44 "Net-(LEDS1-Pad2)")
  (net 45 "Net-(LEDS1-Pad4)")
  (net 46 "Net-(LEDS1-Pad3)")
  (net 47 "Net-(PZO1-Pad1)")
  (net 48 "Net-(D2-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net +5V)
    (add_net +BATT)
    (add_net "/0(Rx)")
    (add_net "/1(Tx)")
    (add_net "/10(**/SS)")
    (add_net "/11(**/MISO)")
    (add_net "/12(MOSI)")
    (add_net "/13(SCK)")
    (add_net /2)
    (add_net "/3(**)")
    (add_net /4)
    (add_net "/5(**)")
    (add_net "/6(**)")
    (add_net /7)
    (add_net /8)
    (add_net "/9(**)")
    (add_net /A0)
    (add_net /A1)
    (add_net /A2)
    (add_net /A3)
    (add_net /A4)
    (add_net /A5)
    (add_net /A6)
    (add_net /A7)
    (add_net /AREF)
    (add_net /Reset)
    (add_net /Vin)
    (add_net GND)
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D3-Pad4)")
    (add_net "Net-(D3-Pad5)")
    (add_net "Net-(D3-Pad6)")
    (add_net "Net-(J4-Pad2)")
    (add_net "Net-(LEDS1-Pad2)")
    (add_net "Net-(LEDS1-Pad3)")
    (add_net "Net-(LEDS1-Pad4)")
    (add_net "Net-(P3-Pad1)")
    (add_net "Net-(P4-Pad1)")
    (add_net "Net-(P5-Pad1)")
    (add_net "Net-(P6-Pad1)")
    (add_net "Net-(PZO1-Pad1)")
    (add_net "Net-(R1-Pad2)")
    (add_net "Net-(R5-Pad1)")
    (add_net "Net-(R6-Pad1)")
    (add_net "Net-(R7-Pad2)")
  )
  (module Potentiometers:Potentiometer_Bourns_3339P_Angular_ScrewUp (layer B.Cu) (tedit 5899D346)
    (at 143.002 88.646)
    (descr "5/16, Round, Trimming, Potentiometer, Bourns, 3339")
    (tags "5/16, Round, Trimming, Potentiometer, Bourns, 3339")
    (fp_text reference RV1 (at -1.016 3.048) (layer B.SilkS))
    (fp_text value "10K POT" (at 8.128 -1.778 180) (layer B.Fab))
    (pad 3 thru_hole circle (at 5.08 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 17 +5V))
    (pad 2 thru_hole circle (at 2.54 2.54) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 39 "Net-(R7-Pad2)"))
    (model Potentiometers.3dshapes/Potentiometer_Bourns_3339P_Angular_ScrewUp.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module NMOS_SOT23:SOT-23 (layer F.Cu) (tedit 58C38456)
    (at 143.526 81.296 90)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q1 (at 1.254 1.27 -180) (layer F.SilkS))
    (fp_text value Q_NMOS_DGS (at -3.048 -0.508 -180) (layer F.Fab))
    (pad 1 smd rect (at 1 0 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(LEDS1-Pad2)"))
    (pad 3 smd rect (at -1 0.95 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 2 smd rect (at -1 -0.95 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 6 "/3(**)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module NMOS_SOT23:SOT-23 (layer F.Cu) (tedit 58C38456)
    (at 147.386 81.28 90)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q2 (at 1.254 1.27 -180) (layer F.SilkS))
    (fp_text value Q_NMOS_DGS (at -3.048 -0.508 -180) (layer F.Fab))
    (pad 1 smd rect (at 1 0 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(LEDS1-Pad3)"))
    (pad 3 smd rect (at -1 0.95 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 2 smd rect (at -1 -0.95 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 8 "/5(**)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module NMOS_SOT23:SOT-23 (layer F.Cu) (tedit 58C38456)
    (at 151.196 81.296 90)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q3 (at 1.254 1.27 -180) (layer F.SilkS))
    (fp_text value Q_NMOS_DGS (at -3.048 -0.508 -180) (layer F.Fab))
    (pad 2 smd rect (at -1 -0.95 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 9 "/6(**)"))
    (pad 3 smd rect (at -1 0.95 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 1 smd rect (at 1 0 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(LEDS1-Pad4)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Buttons_Switches_SMD:SW_DIP_x1_W7.62mm_Slide_Copal_CHS-B (layer B.Cu) (tedit 586545EC)
    (at 147.828 83.312 180)
    (descr "1x-dip-switch, Slide, row spacing 7.62 mm (300 mils), Copal_CHS-B")
    (tags "DIP Switch Slide 7.62mm 300mil Copal_CHS-B")
    (attr smd)
    (fp_text reference SW1 (at -3.302 -2.032 180) (layer B.SilkS))
    (fp_text value SW_SPST (at 0 -2.39 180) (layer B.Fab))
    (pad 2 smd rect (at 3.81 0 180) (size 1.6 0.76) (layers B.Cu B.Mask)
      (net 16 /Vin))
    (pad 1 smd rect (at -3.81 0 180) (size 1.6 0.76) (layers B.Cu B.Mask)
      (net 48 "Net-(D2-Pad1)"))
    (model ${KIPRJMOD}/Drumlights.3dshapes/SW_DIP_x1_W7.62mm_Slide_Copal_CHS-B.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 -90))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58307A47)
    (at 143.002 99.822 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R6 (at 1.778 0.127 270) (layer F.SilkS))
    (fp_text value 10K (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(R6-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58307A47)
    (at 143.002 94.234)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at 0 -1.143) (layer F.SilkS))
    (fp_text value 470 (at 0 1.9) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(D1-Pad1)"))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(R5-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_JST:JST_PH_S2B-PH-K_02x2.00mm_Angled (layer F.Cu) (tedit 56B07786)
    (at 149.352 104.394)
    (descr http://www.jst-mfg.com/product/pdf/eng/ePH.pdf)
    (tags "connector jst ph")
    (fp_text reference PZO1 (at 2.286 -1.778) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 1 7.5) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.2 1.7) (drill 0.7) (layers *.Cu *.Mask)
      (net 47 "Net-(PZO1-Pad1)"))
    (pad 2 thru_hole oval (at 2 0) (size 1.2 1.7) (drill 0.7) (layers *.Cu *.Mask)
      (net 4 GND))
    (model ${KIPRJMOD}/Drumlights.3dshapes/JST_PH_S2B-PH-K_02x2.00mm_Angled.STEP
      (at (xyz 0.3405511811023622 0.1062992125984252 0.2362204724409449))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module Connectors_JST:JST_PH_S2B-PH-K_02x2.00mm_Angled (layer F.Cu) (tedit 56B07786)
    (at 142.748 104.394)
    (descr http://www.jst-mfg.com/product/pdf/eng/ePH.pdf)
    (tags "connector jst ph")
    (fp_text reference BAT1 (at 1.524 -1.524) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 1 7.5) (layer F.Fab))
    (pad 2 thru_hole oval (at 2 0) (size 1.2 1.7) (drill 0.7) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 1 thru_hole rect (at 0 0) (size 1.2 1.7) (drill 0.7) (layers *.Cu *.Mask)
      (net 36 +BATT))
    (model ${KIPRJMOD}/Drumlights.3dshapes/JST_PH_S2B-PH-K_02x2.00mm_Angled.STEP
      (at (xyz 0.3405511811023622 0.1062992125984252 0.2362204724409449))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module Connectors_Molex:Molex_NanoFit_1x04x2.50mm_Angled (layer F.Cu) (tedit 5757C4B3)
    (at 143.256 78.3)
    (descr "Molex Nano Fit, single row, side entry, through hole, Datasheet:http://www.molex.com/pdm_docs/sd/1053131208_sd.pdf")
    (tags "connector molex nano-fit 105313-xx08")
    (fp_text reference LEDS1 (at 9.144 -0.068 90) (layer F.SilkS))
    (fp_text value CONN_01X04 (at 3.75 3.5) (layer F.Fab))
    (pad "" np_thru_hole circle (at 7.5 -7.18) (size 1.6 1.6) (drill 1.6) (layers *.Cu))
    (pad "" np_thru_hole circle (at 0 -7.18) (size 1.6 1.6) (drill 1.6) (layers *.Cu))
    (pad 4 thru_hole circle (at 7.5 0) (size 1.9 1.9) (drill 1.2) (layers *.Cu *.Mask)
      (net 45 "Net-(LEDS1-Pad4)"))
    (pad 3 thru_hole circle (at 5 0) (size 1.9 1.9) (drill 1.2) (layers *.Cu *.Mask)
      (net 46 "Net-(LEDS1-Pad3)"))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.9 1.9) (drill 1.2) (layers *.Cu *.Mask)
      (net 44 "Net-(LEDS1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.9 1.9) (drill 1.2) (layers *.Cu *.Mask)
      (net 36 +BATT))
    (model ${KIPRJMOD}/Drumlights.3dshapes/Connectors_Molex.3dshapesMolex_NanoFit_1x04x2.50mm_Angled.stp
      (at (xyz 0.1476377952755906 0.2362204724409449 0.07480314960629922))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 180))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58307A47)
    (at 142.506 86.868)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R8 (at -1.409 0 90) (layer F.SilkS))
    (fp_text value 100 (at 0 1.9) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(D3-Pad6)"))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 9 "/6(**)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58307A47)
    (at 142.506 83.82)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R10 (at -1.409 0 90) (layer F.SilkS))
    (fp_text value 150 (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 "/3(**)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(D3-Pad4)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58307A47)
    (at 142.506 85.344)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R9 (at -1.409 0 90) (layer F.SilkS))
    (fp_text value 100 (at 0 1.9) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(D3-Pad5)"))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 "/5(**)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_RGB_PLCC-6 (layer F.Cu) (tedit 587A6CD4)
    (at 146.558 85.344 180)
    (descr "RGB LED PLCC-6")
    (tags "RGB LED PLCC-6")
    (attr smd)
    (fp_text reference D3 (at 0 -2.55) (layer F.SilkS))
    (fp_text value LED_RGB (at 0 2.8 180) (layer F.Fab))
    (pad 6 smd rect (at 1.55 -1.1 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(D3-Pad6)"))
    (pad 5 smd rect (at 1.55 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(D3-Pad5)"))
    (pad 4 smd rect (at 1.55 1.1 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(D3-Pad4)"))
    (pad 3 smd rect (at -1.55 1.1 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 2 smd rect (at -1.55 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 1 smd rect (at -1.55 -1.1 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model ${KIPRJMOD}/Drumlights.3dshapes/LED_RGB_PLCC-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.2 0.2 0.2))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SOD-123 (layer F.Cu) (tedit 58645DC7)
    (at 151.638 88.9 270)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D2 (at -3.048 0) (layer F.SilkS))
    (fp_text value D_Schottky (at 0 2.1 270) (layer F.Fab))
    (pad 2 smd rect (at 1.65 0 270) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 36 +BATT))
    (pad 1 smd rect (at -1.65 0 270) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(D2-Pad1)"))
    (model ${KIPRJMOD}/Drumlights.3dshapes/SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connect:GS3 (layer B.Cu) (tedit 58613494)
    (at 151.638 90.678)
    (descr "3-pin solder bridge")
    (tags "solder bridge")
    (attr smd)
    (fp_text reference J4 (at -1.7 0 -90) (layer B.SilkS))
    (fp_text value GS3 (at 1.8 0 -90) (layer B.Fab))
    (pad 3 smd rect (at 0 -1.27) (size 1.27 0.97) (layers B.Cu B.Paste B.Mask)
      (net 24 /A0))
    (pad 2 smd rect (at 0 0) (size 1.27 0.97) (layers B.Cu B.Paste B.Mask)
      (net 40 "Net-(J4-Pad2)"))
    (pad 1 smd rect (at 0 1.27) (size 1.27 0.97) (layers B.Cu B.Paste B.Mask)
      (net 25 /AREF))
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58307A47)
    (at 148.59 91.44 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R7 (at 0 -1.27 180) (layer F.SilkS))
    (fp_text value 5K (at 0 1.9 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(R7-Pad2)"))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(J4-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23-5 (layer F.Cu) (tedit 583F3A3F)
    (at 150.876 96.774 180)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U1 (at 0.127 2.159 180) (layer F.SilkS))
    (fp_text value TLV2771 (at 0 2.9 180) (layer F.Fab))
    (pad 5 smd rect (at 1.1 -0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 17 +5V))
    (pad 4 smd rect (at 1.1 0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(C1-Pad2)"))
    (pad 3 smd rect (at -1.1 0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(R1-Pad2)"))
    (pad 2 smd rect (at -1.1 0 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 1 smd rect (at -1.1 -0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 34 /A1))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 145.288 100.584 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at 0 -1.27 270) (layer F.SilkS))
    (fp_text value 4.7uF (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 17 +5V))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 143.002 101.346 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C3 (at 1.778 0 270) (layer F.SilkS))
    (fp_text value 4.7uF (at 0 1.9 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 36 +BATT))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 57FE93A5)
    (at 146.304 97.244 270)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D1 (at -1.867 0) (layer F.SilkS))
    (fp_text value LED (at 0 1.35 270) (layer F.Fab))
    (pad 1 smd rect (at -0.8 0 90) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at 0.8 0 90) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 17 +5V))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23-5 (layer F.Cu) (tedit 5883B1A6)
    (at 143.51 97.028)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U2 (at 1.397 -2.286) (layer F.SilkS))
    (fp_text value MCP73831 (at 0 2.9) (layer F.Fab))
    (pad 5 smd rect (at 1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(R6-Pad1)"))
    (pad 4 smd rect (at 1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 17 +5V))
    (pad 3 smd rect (at -1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 36 +BATT))
    (pad 2 smd rect (at -1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 1 smd rect (at -1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(R5-Pad1)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 151.396 101.346 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at 1.79 0.254 270) (layer F.SilkS))
    (fp_text value 10pF (at 0 1.9 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(C1-Pad2)"))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 34 /A1))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58307A47)
    (at 151.384 99.568 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at -1.524 0 270) (layer F.SilkS))
    (fp_text value 100K (at 0 1.9 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(C1-Pad2)"))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 34 /A1))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58307A47)
    (at 148.602 99.568 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at 0 -1.27 180) (layer F.SilkS))
    (fp_text value 100 (at 0 1.9 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(PZO1-Pad1)"))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(C1-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58307A47)
    (at 148.082 94.5 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at 0.012 -1.27 90) (layer F.SilkS))
    (fp_text value 10K (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(R1-Pad2)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58307A47)
    (at 148.082 97.282 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at -1.905 -1.27 90) (layer F.SilkS))
    (fp_text value 10K (at 0 1.9 90) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(R1-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 17 +5V))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x15 locked (layer F.Cu) (tedit 0)
    (at 154.686 71.247 270)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P2 (at 22.479 2.286 270) (layer F.SilkS))
    (fp_text value Analog (at 0 -3.1 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 16 /Vin))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 3 thru_hole oval (at 5.08 0 270) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 /Reset))
    (pad 4 thru_hole oval (at 7.62 0 270) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 17 +5V))
    (pad 5 thru_hole oval (at 10.16 0 270) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 18 /A7))
    (pad 6 thru_hole oval (at 12.7 0 270) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 19 /A6))
    (pad 7 thru_hole oval (at 15.24 0 270) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 20 /A5))
    (pad 8 thru_hole oval (at 17.78 0 270) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 21 /A4))
    (pad 9 thru_hole oval (at 20.32 0 270) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 22 /A3))
    (pad 10 thru_hole oval (at 22.86 0 270) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 23 /A2))
    (pad 11 thru_hole oval (at 25.4 0 270) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 34 /A1))
    (pad 12 thru_hole oval (at 27.94 0 270) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 24 /A0))
    (pad 13 thru_hole oval (at 30.48 0 270) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 25 /AREF))
    (pad 14 thru_hole oval (at 33.02 0 270) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 31 +3V3))
    (pad 15 thru_hole oval (at 35.56 0 270) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 26 "/13(SCK)"))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x15.wrl
      (at (xyz 0.7 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x15 locked (layer F.Cu) (tedit 0)
    (at 139.446 71.247 270)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P1 (at 21.463 -2.286 270) (layer F.SilkS))
    (fp_text value Digital (at 0 -3.1 270) (layer F.Fab))
    (pad 15 thru_hole oval (at 35.56 0 270) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 15 "/12(MOSI)"))
    (pad 14 thru_hole oval (at 33.02 0 270) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 14 "/11(**/MISO)"))
    (pad 13 thru_hole oval (at 30.48 0 270) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 13 "/10(**/SS)"))
    (pad 12 thru_hole oval (at 27.94 0 270) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 12 "/9(**)"))
    (pad 11 thru_hole oval (at 25.4 0 270) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 11 /8))
    (pad 10 thru_hole oval (at 22.86 0 270) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 10 /7))
    (pad 9 thru_hole oval (at 20.32 0 270) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 9 "/6(**)"))
    (pad 8 thru_hole oval (at 17.78 0 270) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 8 "/5(**)"))
    (pad 7 thru_hole oval (at 15.24 0 270) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 7 /4))
    (pad 6 thru_hole oval (at 12.7 0 270) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 6 "/3(**)"))
    (pad 5 thru_hole oval (at 10.16 0 270) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 5 /2))
    (pad 4 thru_hole oval (at 7.62 0 270) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 3 thru_hole oval (at 5.08 0 270) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 /Reset))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 "/0(Rx)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 "/1(Tx)"))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x15.wrl
      (at (xyz 0.7 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Socket_Arduino_Nano:1pin_Nano locked (layer F.Cu) (tedit 5521156E)
    (at 139.446 68.707)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference P3 (at 0 -2.032) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 2.032) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 2.54 2.54) (drill 1.778) (layers *.Cu *.Mask F.SilkS)
      (net 27 "Net-(P3-Pad1)"))
  )
  (module Socket_Arduino_Nano:1pin_Nano locked (layer F.Cu) (tedit 55211594)
    (at 139.446 109.347)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference P4 (at 0 -2.032) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 2.032) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 2.54 2.54) (drill 1.778) (layers *.Cu *.Mask F.SilkS)
      (net 28 "Net-(P4-Pad1)"))
  )
  (module Socket_Arduino_Nano:1pin_Nano locked (layer F.Cu) (tedit 552115A5)
    (at 154.686 109.347)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference P5 (at 0 -2.032) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 2.032) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 2.54 2.54) (drill 1.778) (layers *.Cu *.Mask F.SilkS)
      (net 29 "Net-(P5-Pad1)"))
  )
  (module Socket_Arduino_Nano:1pin_Nano locked (layer F.Cu) (tedit 552115BD)
    (at 154.686 68.707)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference P6 (at 0 -2.032) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 2.032) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 2.54 2.54) (drill 1.778) (layers *.Cu *.Mask F.SilkS)
      (net 30 "Net-(P6-Pad1)"))
  )
  (gr_text 12/03/2017 (at 147.066 80.01) (layer B.SilkS))
  (gr_text http://whatnick.com (at 146.812 75.692) (layer B.SilkS))
  (gr_text "Arduino Nano \nDrumlights v1.1" (at 146.812 73.914) (layer B.SilkS))
  (gr_text 1 (at 141.732 71.247) (layer F.SilkS))
  (gr_line (start 138.176 67.437) (end 138.176 110.617) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 155.956 67.437) (end 138.176 67.437) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 155.956 110.617) (end 155.956 67.437) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 138.176 110.617) (end 155.956 110.617) (angle 90) (layer Edge.Cuts) (width 0.1))
  (zone (net 4) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 138.176 67.564) (xy 155.956 67.564) (xy 155.956 110.744) (xy 138.176 110.744)
      )
    )
  )
  (zone (net 36) (net_name +BATT) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 138.176 67.056) (xy 155.956 67.056) (xy 155.956 110.744) (xy 138.176 110.744)
      )
    )
  )
)
