<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="30.15" y2="0" width="0" layer="20"/>
<wire x1="30.15" y1="0" x2="30.15" y2="38.09" width="0" layer="20"/>
<wire x1="30.15" y1="38.09" x2="0" y2="38.09" width="0" layer="20"/>
<wire x1="0" y1="38.09" x2="0" y2="0" width="0" layer="20"/>
</plain>
<libraries>
<library name="capacitor-wima">
<description>&lt;b&gt;WIMA Capacitors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="C7.5B4">
<description>&lt;B&gt;MKS3&lt;/B&gt;, 10 x 4 mm, grid 7.62 mm</description>
</package>
<package name="C7.5B3">
<description>&lt;B&gt;MKS3&lt;/B&gt;, 10 x 3 mm, grid 7.62 mm</description>
</package>
</packages>
</library>
<library name="burr-brown">
<description>&lt;b&gt;Burr-Brown Components&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOT223">
<description>&lt;b&gt;Smal Outline Transistor&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X08">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X06">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X02">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Electromechanical">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find anything that moves- switches, relays, buttons, potentiometers. Also, anything that goes on a board but isn't electrical in nature- screws, standoffs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SWITCH-SPDT">
</package>
</packages>
</library>
<library name="esp8266modules">
<packages>
<package name="ESP12E-SMD">
<description>ESP8266 Module 12E</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="100UF" library="capacitor-wima" package="C7.5B4" value=""/>
<element name="100UF2" library="capacitor-wima" package="C7.5B4" value=""/>
<element name="10UF" library="capacitor-wima" package="C7.5B3" value=""/>
<element name="470+UF" library="capacitor-wima" package="C7.5B4" value=""/>
<element name="IC1" library="burr-brown" package="SOT223" value="REG1117">
<attribute name="MPN" value="REG1117"/>
<attribute name="OC_NEWARK" value="14P6981"/>
<attribute name="OC_FARNELL" value="1097566"/>
<attribute name="MF" value=""/>
</element>
<element name="JP1" library="pinhead" package="1X08" value=""/>
<element name="JP2" library="pinhead" package="1X08" value=""/>
<element name="JP3" library="pinhead" package="1X06" value=""/>
<element name="S1" library="SparkFun-Electromechanical" package="SWITCH-SPDT" value="">
<attribute name="PROD_ID" value="SWCH-08261"/>
</element>
<element name="TR" library="pinhead" package="1X02" value=""/>
<element name="U1" library="esp8266modules" package="ESP12E-SMD" value=""/>
<element name="VG" library="pinhead" package="1X02" value=""/>
</elements>
<signals>
<signal name="TX">
<contactref element="TR" pad="1"/>
<contactref element="U1" pad="TXD0"/>
<contactref element="JP2" pad="1"/>
</signal>
<signal name="RX">
<contactref element="TR" pad="2"/>
<contactref element="U1" pad="RXD0"/>
<contactref element="JP2" pad="2"/>
</signal>
<signal name="VCC">
<contactref element="VG" pad="1"/>
<contactref element="470+UF" pad="1"/>
<contactref element="IC1" pad="3"/>
<contactref element="100UF" pad="1"/>
</signal>
<signal name="GND">
<contactref element="VG" pad="2"/>
<contactref element="470+UF" pad="2"/>
<contactref element="S1" pad="3"/>
<contactref element="IC1" pad="1"/>
<contactref element="100UF" pad="2"/>
<contactref element="100UF2" pad="2"/>
<contactref element="10UF" pad="2"/>
<contactref element="U1" pad="GND"/>
<contactref element="JP2" pad="8"/>
</signal>
<signal name="3.3">
<contactref element="S1" pad="1"/>
<contactref element="IC1" pad="2"/>
<contactref element="100UF2" pad="1"/>
<contactref element="10UF" pad="1"/>
<contactref element="U1" pad="VCC"/>
<contactref element="JP1" pad="8"/>
</signal>
<signal name="GPIO0">
<contactref element="S1" pad="2"/>
<contactref element="U1" pad="GPIO0"/>
<contactref element="JP2" pad="5"/>
</signal>
<signal name="RESET">
<contactref element="U1" pad="RESET"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="ADC">
<contactref element="U1" pad="ADC"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="CH_PD">
<contactref element="U1" pad="CH_PD"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="GPIO16">
<contactref element="U1" pad="GPIO16"/>
<contactref element="JP1" pad="4"/>
</signal>
<signal name="GPIO14">
<contactref element="U1" pad="GPIO14"/>
<contactref element="JP1" pad="5"/>
</signal>
<signal name="GPIO12">
<contactref element="U1" pad="GPIO12"/>
<contactref element="JP1" pad="6"/>
</signal>
<signal name="GPIO13">
<contactref element="U1" pad="GPIO13"/>
<contactref element="JP1" pad="7"/>
</signal>
<signal name="GPIO15">
<contactref element="U1" pad="GPIO15"/>
<contactref element="JP2" pad="7"/>
</signal>
<signal name="GPIO2">
<contactref element="U1" pad="GPIO2"/>
<contactref element="JP2" pad="6"/>
</signal>
<signal name="GPIO4">
<contactref element="U1" pad="GPIO4"/>
<contactref element="JP2" pad="4"/>
</signal>
<signal name="GPIO5">
<contactref element="U1" pad="GPIO5"/>
<contactref element="JP2" pad="3"/>
</signal>
<signal name="SCLK">
<contactref element="U1" pad="SCLK"/>
<contactref element="JP3" pad="6"/>
</signal>
<signal name="MOSI">
<contactref element="U1" pad="MOSI"/>
<contactref element="JP3" pad="5"/>
</signal>
<signal name="GPIO10">
<contactref element="U1" pad="GPIO10"/>
<contactref element="JP3" pad="4"/>
</signal>
<signal name="GPIO9">
<contactref element="U1" pad="GPIO9"/>
<contactref element="JP3" pad="3"/>
</signal>
<signal name="CSO">
<contactref element="U1" pad="CS0"/>
<contactref element="JP3" pad="1"/>
</signal>
<signal name="MISO">
<contactref element="U1" pad="MISO"/>
<contactref element="JP3" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
