<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.4.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="74.93" y2="0" width="0" layer="20"/>
<wire x1="74.93" y1="0" x2="74.93" y2="25.4" width="0" layer="20"/>
<wire x1="74.93" y1="25.4" x2="0" y2="25.4" width="0" layer="20"/>
<wire x1="0" y1="25.4" x2="0" y2="0" width="0" layer="20"/>
<text>RST</text>
<text>BOOT</text>
<text>SWDIO</text>
<text>SWCLK</text>
<text>SWCLK</text>
<text>STM32F10RCT6</text>
<text>DEVIATIONTX.COM</text>
</plain>
<libraries>
<library name="stm32f4stamp">
<packages>
<package name="LQFP64">
</package>
<package name="USB-MICROB-SMD">
<description>Micro USB Package</description>
</package>
<package name="0603-RES">
</package>
<package name="1X02_2MM_TH">
</package>
<package name="EIA3216-KIT">
<description>&lt;h3&gt;EIA3216-KIT&lt;/h3&gt;
&lt;b&gt;Warning:&lt;/b&gt; This is the KIT version of this package. This package has longer pads to make hand soldering easier.&lt;br&gt;</description>
</package>
<package name="0603-CAP">
</package>
<package name="SOT23-5">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
<package name="1X1-HEADER-HOLE">
</package>
<package name="SWITCH-TACT-B3U-1100P-B">
</package>
<package name="CRYSTAL-SMD-5X3">
</package>
<package name="LED-0603">
</package>
<package name="SJ_2S">
<description>Small solder jumper with big paste layer so it will short during reflow.</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U1" library="stm32f4stamp" package="LQFP64" value="STM32F405RGT">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="USB" library="stm32f4stamp" package="USB-MICROB-SMD" value="USB-MICROB-SMD">
<attribute name="NAME"/>
</element>
<element name="R1" library="stm32f4stamp" package="0603-RES" value="22R">
<attribute name="NAME"/>
</element>
<element name="R2" library="stm32f4stamp" package="0603-RES" value="22R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JMP-USB" library="stm32f4stamp" package="1X02_2MM_TH" value=""/>
<element name="C1" library="stm32f4stamp" package="EIA3216-KIT" value="4u7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="stm32f4stamp" package="0603-CAP" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="stm32f4stamp" package="0603-CAP" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="stm32f4stamp" package="0603-CAP" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="stm32f4stamp" package="0603-CAP" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="stm32f4stamp" package="0603-CAP" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="stm32f4stamp" package="0603-CAP" value="2u2">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="stm32f4stamp" package="0603-CAP" value="2u2">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C9" library="stm32f4stamp" package="EIA3216-KIT" value="4u7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C10" library="stm32f4stamp" package="EIA3216-KIT" value="4u7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC1" library="stm32f4stamp" package="SOT23-5" value="VREG-3V3">
<attribute name="NAME"/>
</element>
<element name="C11" library="stm32f4stamp" package="0603-CAP" value="470p">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP2" library="stm32f4stamp" package="1X1-HEADER-HOLE" value="5V">
<attribute name="VALUE"/>
<attribute name="VALUE"/>
</element>
<element name="JP3" library="stm32f4stamp" package="1X1-HEADER-HOLE" value="GND">
<attribute name="VALUE"/>
<attribute name="VALUE"/>
</element>
<element name="JP4" library="stm32f4stamp" package="1X1-HEADER-HOLE" value="3V3">
<attribute name="VALUE"/>
<attribute name="VALUE"/>
</element>
<element name="JP5" library="stm32f4stamp" package="1X1-HEADER-HOLE" value="GND">
<attribute name="VALUE"/>
<attribute name="VALUE"/>
</element>
<element name="JP6" library="stm32f4stamp" package="1X1-HEADER-HOLE" value="GND">
<attribute name="VALUE"/>
<attribute name="VALUE"/>
</element>
<element name="JP7" library="stm32f4stamp" package="1X1-HEADER-HOLE" value="GND">
<attribute name="VALUE"/>
<attribute name="VALUE"/>
</element>
<element name="JP8" library="stm32f4stamp" package="1X1-HEADER-HOLE" value="PB8">
<attribute name="VALUE"/>
<attribute name="VALUE"/>
</element>
<element name="JP9" library="stm32f4stamp" package="1X1-HEADER-HOLE" value="PA10">
<attribute name="VALUE"/>
<attribute name="VALUE"/>
</element>
<element name="JP10" library="stm32f4stamp" package="1X1-HEADER-HOLE" value="PA8">
<attribute name="VALUE"/>
<attribute name="VALUE"/>
</element>
<element name="JP11" library="stm32f4stamp" package="1X1-HEADER-HOLE" value="PA13">
<attribute name="VALUE"/>
<attribute name="VALUE"/>
</element>
<element name="JP12" library="stm32f4stamp" package="1X1-HEADER-HOLE" value="PC9">
<attribute name="VALUE"/>
<attribute name="VALUE"/>
</element>
<element name="SW1" library="stm32f4stamp" package="SWITCH-TACT-B3U-1100P-B" value="!RST"/>
<element name="Y1" library="stm32f4stamp" package="CRYSTAL-SMD-5X3" value="8MHz">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C12" library="stm32f4stamp" package="0603-CAP" value="22p">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C13" library="stm32f4stamp" package="0603-CAP" value="22p">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP13" library="stm32f4stamp" package="1X1-HEADER-HOLE" value="PC15">
<attribute name="VALUE"/>
<attribute name="VALUE"/>
</element>
<element name="JP14" library="stm32f4stamp" package="1X1-HEADER-HOLE" value="PC14">
<attribute name="VALUE"/>
<attribute name="VALUE"/>
</element>
<element name="JP15" library="stm32f4stamp" package="1X1-HEADER-HOLE" value="PC13">
<attribute name="VALUE"/>
<attribute name="VALUE"/>
</element>
<element name="JP16" library="stm32f4stamp" package="1X1-HEADER-HOLE" value="PC12">
<attribute name="VALUE"/>
<attribute name="VALUE"/>
</element>
<element name="JP17" library="stm32f4stamp" package="1X1-HEADER-HOLE" value="PC11">
<attribute name="VALUE"/>
<attribute name="VALUE"/>
</element>
<element name="JP18" library="stm32f4stamp" package="1X1-HEADER-HOLE" value="PC10">
<attribute name="VALUE"/>
<attribute name="VALUE"/>
</element>
<element name="JP19" library="stm32f4stamp" package="1X1-HEADER-HOLE" value="PC8">
<attribute name="VALUE"/>
<attribute name="VALUE"/>
</element>
<element name="JP20" library="stm32f4stamp" package="1X1-HEADER-HOLE" value="PC7">
<attribute name="VALUE"/>
<attribute name="VALUE"/>
</element>
<element name="JP21" library="stm32f4stamp" package="1X1-HEADER-HOLE" value="PC6">
<attribute name="VALUE"/>
<attribute name="VALUE"/>
</element>
<element name="JP22" library="stm32f4stamp" package="1X1-HEADER-HOLE" value="PC5">
<attribute name="VALUE"/>
<attribute name="VALUE"/>
</element>
<element name="JP23" library="stm32f4stamp" package="1X1-HEADER-HOLE" value="PC4">
<attribute name="VALUE"/>
<attribute name="VALUE"/>
</element>
<element name="JP24" library="stm32f4stamp" package="1X1-HEADER-HOLE" value="PC3">
<attribute name="VALUE"/>
<attribute name="VALUE"/>
</element>
<element name="JP25" library="stm32f4stamp" package="1X1-HEADER-HOLE" value="PC2">
<attribute name="VALUE"/>
<attribute name="VALUE"/>
</element>
<element name="JP26" library="stm32f4stamp" package="1X1-HEADER-HOLE" value="PC1">
<attribute name="VALUE"/>
<attribute name="VALUE"/>
</element>
<element name="JP27" library="stm32f4stamp" package="1X1-HEADER-HOLE" value="PC0">
<attribute name="VALUE"/>
<attribute name="VALUE"/>
</element>
<element name="JP28" library="stm32f4stamp" package="1X1-HEADER-HOLE" value="PD2">
<attribute name="VALUE"/>
<attribute name="VALUE"/>
</element>
<element name="JP29" library="stm32f4stamp" package="1X1-HEADER-HOLE" value="PA0">
<attribute name="VALUE"/>
<attribute name="VALUE"/>
</element>
<element name="JP30" library="stm32f4stamp" package="1X1-HEADER-HOLE" value="PA1">
<attribute name="VALUE"/>
<attribute name="VALUE"/>
</element>
<element name="JP31" library="stm32f4stamp" package="1X1-HEADER-HOLE" value="PA2">
<attribute name="VALUE"/>
<attribute name="VALUE"/>
</element>
<element name="JP32" library="stm32f4stamp" package="1X1-HEADER-HOLE" value="PA3">
<attribute name="VALUE"/>
<attribute name="VALUE"/>
</element>
<element name="JP33" library="stm32f4stamp" package="1X1-HEADER-HOLE" value="PA4">
<attribute name="VALUE"/>
<attribute name="VALUE"/>
</element>
<element name="JP34" library="stm32f4stamp" package="1X1-HEADER-HOLE" value="PA5">
<attribute name="VALUE"/>
<attribute name="VALUE"/>
</element>
<element name="JP35" library="stm32f4stamp" package="1X1-HEADER-HOLE" value="PA6">
<attribute name="VALUE"/>
<attribute name="VALUE"/>
</element>
<element name="JP36" library="stm32f4stamp" package="1X1-HEADER-HOLE" value="PA7">
<attribute name="VALUE"/>
<attribute name="VALUE"/>
</element>
<element name="JP37" library="stm32f4stamp" package="1X1-HEADER-HOLE" value="PA14">
<attribute name="VALUE"/>
<attribute name="VALUE"/>
</element>
<element name="JP38" library="stm32f4stamp" package="1X1-HEADER-HOLE" value="PA15">
<attribute name="VALUE"/>
<attribute name="VALUE"/>
</element>
<element name="JP39" library="stm32f4stamp" package="1X1-HEADER-HOLE" value="PB0">
<attribute name="VALUE"/>
<attribute name="VALUE"/>
</element>
<element name="JP40" library="stm32f4stamp" package="1X1-HEADER-HOLE" value="PB1">
<attribute name="VALUE"/>
<attribute name="VALUE"/>
</element>
<element name="JP41" library="stm32f4stamp" package="1X1-HEADER-HOLE" value="PB3">
<attribute name="VALUE"/>
<attribute name="VALUE"/>
</element>
<element name="JP42" library="stm32f4stamp" package="1X1-HEADER-HOLE" value="PB4">
<attribute name="VALUE"/>
<attribute name="VALUE"/>
</element>
<element name="JP43" library="stm32f4stamp" package="1X1-HEADER-HOLE" value="PB5">
<attribute name="VALUE"/>
<attribute name="VALUE"/>
</element>
<element name="JP44" library="stm32f4stamp" package="1X1-HEADER-HOLE" value="PB6">
<attribute name="VALUE"/>
<attribute name="VALUE"/>
</element>
<element name="JP45" library="stm32f4stamp" package="1X1-HEADER-HOLE" value="PB7">
<attribute name="VALUE"/>
<attribute name="VALUE"/>
</element>
<element name="JP46" library="stm32f4stamp" package="1X1-HEADER-HOLE" value="PB9">
<attribute name="VALUE"/>
<attribute name="VALUE"/>
</element>
<element name="JP47" library="stm32f4stamp" package="1X1-HEADER-HOLE" value="PB10">
<attribute name="VALUE"/>
<attribute name="VALUE"/>
</element>
<element name="JP48" library="stm32f4stamp" package="1X1-HEADER-HOLE" value="PB11">
<attribute name="VALUE"/>
<attribute name="VALUE"/>
</element>
<element name="JP49" library="stm32f4stamp" package="1X1-HEADER-HOLE" value="PB12">
<attribute name="VALUE"/>
<attribute name="VALUE"/>
</element>
<element name="JP50" library="stm32f4stamp" package="1X1-HEADER-HOLE" value="PB13">
<attribute name="VALUE"/>
<attribute name="VALUE"/>
</element>
<element name="JP51" library="stm32f4stamp" package="1X1-HEADER-HOLE" value="PB14">
<attribute name="VALUE"/>
<attribute name="VALUE"/>
</element>
<element name="JP52" library="stm32f4stamp" package="1X1-HEADER-HOLE" value="PB15">
<attribute name="VALUE"/>
<attribute name="VALUE"/>
</element>
<element name="JP53" library="stm32f4stamp" package="1X1-HEADER-HOLE" value="VBAT">
<attribute name="VALUE"/>
<attribute name="VALUE"/>
</element>
<element name="JP54" library="stm32f4stamp" package="1X1-HEADER-HOLE" value="!RST">
<attribute name="VALUE"/>
<attribute name="VALUE"/>
</element>
<element name="JP55" library="stm32f4stamp" package="1X1-HEADER-HOLE" value="BOOT0">
<attribute name="VALUE"/>
<attribute name="VALUE"/>
</element>
<element name="JMP-HOLDER" library="stm32f4stamp" package="1X02_2MM_TH" value=""/>
<element name="LED1" library="stm32f4stamp" package="LED-0603" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="stm32f4stamp" package="0603-RES" value="470R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="stm32f4stamp" package="0603-RES" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SW2" library="stm32f4stamp" package="SWITCH-TACT-B3U-1100P-B" value="BOOT"/>
<element name="R5" library="stm32f4stamp" package="0603-RES" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP56" library="stm32f4stamp" package="1X1-HEADER-HOLE" value="USB-ID">
<attribute name="VALUE"/>
<attribute name="VALUE"/>
</element>
<element name="JMP-UID" library="stm32f4stamp" package="SJ_2S" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="U1" pad="45"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="U1" pad="44"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="GND">
<contactref element="C1" pad="C"/>
<contactref element="USB" pad="GND"/>
<contactref element="USB" pad="MT1"/>
<contactref element="USB" pad="MT2"/>
<contactref element="USB" pad="MT3"/>
<contactref element="USB" pad="MT4"/>
<contactref element="U1" pad="18"/>
<contactref element="U1" pad="63"/>
<contactref element="U1" pad="12"/>
<contactref element="C6" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="C11" pad="1"/>
<contactref element="C10" pad="C"/>
<contactref element="C9" pad="C"/>
<contactref element="IC1" pad="2"/>
<contactref element="JP5" pad="1"/>
<contactref element="JP3" pad="1"/>
<contactref element="JP6" pad="1"/>
<contactref element="JP7" pad="1"/>
<contactref element="C13" pad="2"/>
<contactref element="C12" pad="2"/>
<contactref element="U1" pad="28"/>
<contactref element="R3" pad="1"/>
<contactref element="SW2" pad="BOSS"/>
<contactref element="SW1" pad="BOSS"/>
<contactref element="R5" pad="2"/>
<contactref element="SW1" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="USB" pad="VBUS"/>
<contactref element="JMP-USB" pad="1"/>
<contactref element="U1" pad="42"/>
<contactref element="C1" pad="A"/>
</signal>
<signal name="5V">
<contactref element="JMP-USB" pad="2"/>
<contactref element="IC1" pad="1"/>
<contactref element="IC1" pad="3"/>
<contactref element="C9" pad="A"/>
<contactref element="JP2" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="USB" pad="D+"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="USB" pad="D-"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="3.3V">
<contactref element="U1" pad="19"/>
<contactref element="C2" pad="1"/>
<contactref element="U1" pad="64"/>
<contactref element="C5" pad="1"/>
<contactref element="U1" pad="48"/>
<contactref element="C4" pad="1"/>
<contactref element="U1" pad="32"/>
<contactref element="C3" pad="1"/>
<contactref element="U1" pad="13"/>
<contactref element="C6" pad="1"/>
<contactref element="C10" pad="A"/>
<contactref element="IC1" pad="5"/>
<contactref element="JP4" pad="1"/>
<contactref element="R4" pad="2"/>
<contactref element="LED1" pad="A"/>
<contactref element="SW2" pad="1"/>
</signal>
<signal name="N$13">
<contactref element="U1" pad="31"/>
<contactref element="C7" pad="1"/>
</signal>
<signal name="N$14">
<contactref element="U1" pad="47"/>
<contactref element="C8" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="IC1" pad="4"/>
<contactref element="C11" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="U1" pad="61"/>
<contactref element="JP8" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="U1" pad="41"/>
<contactref element="JP10" pad="1"/>
</signal>
<signal name="N$11">
<contactref element="U1" pad="46"/>
<contactref element="JP11" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="U1" pad="40"/>
<contactref element="JP12" pad="1"/>
</signal>
<signal name="N$12">
<contactref element="U1" pad="6"/>
<contactref element="Y1" pad="1"/>
<contactref element="C13" pad="1"/>
</signal>
<signal name="N$15">
<contactref element="U1" pad="5"/>
<contactref element="Y1" pad="3"/>
<contactref element="C12" pad="1"/>
</signal>
<signal name="N$16">
<contactref element="U1" pad="60"/>
<contactref element="JP55" pad="1"/>
<contactref element="R5" pad="1"/>
<contactref element="SW2" pad="2"/>
</signal>
<signal name="N$17">
<contactref element="U1" pad="7"/>
<contactref element="JP54" pad="1"/>
<contactref element="R4" pad="1"/>
<contactref element="SW1" pad="1"/>
</signal>
<signal name="N$23">
<contactref element="U1" pad="4"/>
<contactref element="JP13" pad="1"/>
</signal>
<signal name="N$24">
<contactref element="U1" pad="3"/>
<contactref element="JP14" pad="1"/>
</signal>
<signal name="N$25">
<contactref element="U1" pad="2"/>
<contactref element="JP15" pad="1"/>
</signal>
<signal name="N$26">
<contactref element="U1" pad="53"/>
<contactref element="JP16" pad="1"/>
</signal>
<signal name="N$27">
<contactref element="U1" pad="52"/>
<contactref element="JP17" pad="1"/>
</signal>
<signal name="N$28">
<contactref element="U1" pad="51"/>
<contactref element="JP18" pad="1"/>
</signal>
<signal name="N$29">
<contactref element="U1" pad="39"/>
<contactref element="JP19" pad="1"/>
</signal>
<signal name="N$30">
<contactref element="U1" pad="38"/>
<contactref element="JP20" pad="1"/>
</signal>
<signal name="N$31">
<contactref element="U1" pad="37"/>
<contactref element="JP21" pad="1"/>
</signal>
<signal name="N$32">
<contactref element="U1" pad="25"/>
<contactref element="JP22" pad="1"/>
</signal>
<signal name="N$33">
<contactref element="U1" pad="24"/>
<contactref element="JP23" pad="1"/>
</signal>
<signal name="N$34">
<contactref element="U1" pad="11"/>
<contactref element="JP24" pad="1"/>
</signal>
<signal name="N$35">
<contactref element="U1" pad="10"/>
<contactref element="JP25" pad="1"/>
</signal>
<signal name="N$36">
<contactref element="U1" pad="9"/>
<contactref element="JP26" pad="1"/>
</signal>
<signal name="N$37">
<contactref element="U1" pad="8"/>
<contactref element="JP27" pad="1"/>
</signal>
<signal name="N$38">
<contactref element="U1" pad="54"/>
<contactref element="JP28" pad="1"/>
</signal>
<signal name="N$39">
<contactref element="U1" pad="14"/>
<contactref element="JP29" pad="1"/>
</signal>
<signal name="N$40">
<contactref element="U1" pad="15"/>
<contactref element="JP30" pad="1"/>
</signal>
<signal name="N$41">
<contactref element="U1" pad="16"/>
<contactref element="JP31" pad="1"/>
</signal>
<signal name="N$42">
<contactref element="U1" pad="17"/>
<contactref element="JP32" pad="1"/>
</signal>
<signal name="N$43">
<contactref element="U1" pad="20"/>
<contactref element="JP33" pad="1"/>
</signal>
<signal name="N$44">
<contactref element="U1" pad="21"/>
<contactref element="JP34" pad="1"/>
</signal>
<signal name="N$45">
<contactref element="U1" pad="22"/>
<contactref element="JP35" pad="1"/>
</signal>
<signal name="N$46">
<contactref element="U1" pad="23"/>
<contactref element="JP36" pad="1"/>
</signal>
<signal name="N$47">
<contactref element="U1" pad="49"/>
<contactref element="JP37" pad="1"/>
</signal>
<signal name="N$48">
<contactref element="U1" pad="50"/>
<contactref element="JP38" pad="1"/>
</signal>
<signal name="N$49">
<contactref element="U1" pad="26"/>
<contactref element="JP39" pad="1"/>
</signal>
<signal name="N$50">
<contactref element="U1" pad="27"/>
<contactref element="JP40" pad="1"/>
</signal>
<signal name="N$51">
<contactref element="U1" pad="55"/>
<contactref element="JP41" pad="1"/>
</signal>
<signal name="N$52">
<contactref element="U1" pad="56"/>
<contactref element="JP42" pad="1"/>
</signal>
<signal name="N$53">
<contactref element="U1" pad="57"/>
<contactref element="JP43" pad="1"/>
</signal>
<signal name="N$54">
<contactref element="U1" pad="58"/>
<contactref element="JP44" pad="1"/>
</signal>
<signal name="N$55">
<contactref element="U1" pad="59"/>
<contactref element="JP45" pad="1"/>
</signal>
<signal name="N$56">
<contactref element="U1" pad="62"/>
<contactref element="JP46" pad="1"/>
</signal>
<signal name="N$57">
<contactref element="U1" pad="29"/>
<contactref element="JP47" pad="1"/>
</signal>
<signal name="N$58">
<contactref element="U1" pad="30"/>
<contactref element="JP48" pad="1"/>
</signal>
<signal name="N$59">
<contactref element="U1" pad="33"/>
<contactref element="JP49" pad="1"/>
</signal>
<signal name="N$60">
<contactref element="U1" pad="34"/>
<contactref element="JP50" pad="1"/>
</signal>
<signal name="N$61">
<contactref element="U1" pad="35"/>
<contactref element="JP51" pad="1"/>
</signal>
<signal name="N$62">
<contactref element="U1" pad="36"/>
<contactref element="JP52" pad="1"/>
</signal>
<signal name="N$63">
<contactref element="U1" pad="1"/>
<contactref element="JP53" pad="1"/>
</signal>
<signal name="N$18">
<contactref element="LED1" pad="C"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="N$20">
<contactref element="USB" pad="ID"/>
<contactref element="JP56" pad="1"/>
<contactref element="JMP-UID" pad="2"/>
</signal>
<signal name="N$22">
<contactref element="JMP-UID" pad="1"/>
<contactref element="U1" pad="43"/>
<contactref element="JP9" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
