(kicad_pcb (version 4) (host pcbnew 4.0.5)
  (general
    (links 78)
    (no_connects 0)
    (area 118.629981 103.3626 177.676209 154.405401)
    (thickness 1.6002)
    (drawings 61)
    (tracks 313)
    (zones 0)
    (modules 40)
    (nets 31)
  )
  (page A4)
  (layers
    (0 Top signal)
    (31 Bottom signal)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (42 Eco1.User user)
    (44 Edge.Cuts user)
  )
  (setup
    (last_trace_width 0.3)
    (user_trace_width 0.3)
    (user_trace_width 0.5)
    (user_trace_width 0.8)
    (user_trace_width 1)
    (user_trace_width 1.3)
    (user_trace_width 1.5)
    (user_trace_width 1.8)
    (user_trace_width 2)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.762)
    (uvia_drill 0.508)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 0.6 0.6)
    (pad_drill 0.3)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 VIN)
  (net 2 GNDPWR)
  (net 3 VCC)
  (net 4 XTAL1)
  (net 5 XTAL2)
  (net 6 "Net-(C7-Pad1)")
  (net 7 DTR)
  (net 8 RESET)
  (net 9 "Net-(D1-Pad1)")
  (net 10 "Net-(D2-Pad1)")
  (net 11 D9)
  (net 12 D0)
  (net 13 D10)
  (net 14 D1)
  (net 15 MOSI)
  (net 16 D2)
  (net 17 MISO)
  (net 18 D3)
  (net 19 SCK)
  (net 20 D4)
  (net 21 A0)
  (net 22 A1)
  (net 23 D5)
  (net 24 A2)
  (net 25 D6)
  (net 26 A3)
  (net 27 D7)
  (net 28 A4)
  (net 29 D8)
  (net 30 A5)
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
    (add_net A0)
    (add_net A1)
    (add_net A2)
    (add_net A3)
    (add_net A4)
    (add_net A5)
    (add_net D0)
    (add_net D1)
    (add_net D10)
    (add_net D2)
    (add_net D3)
    (add_net D4)
    (add_net D5)
    (add_net D6)
    (add_net D7)
    (add_net D8)
    (add_net D9)
    (add_net DTR)
    (add_net GNDPWR)
    (add_net MISO)
    (add_net MOSI)
    (add_net "Net-(C7-Pad1)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D2-Pad1)")
    (add_net RESET)
    (add_net SCK)
    (add_net VCC)
    (add_net VIN)
    (add_net XTAL1)
    (add_net XTAL2)
  )
  (module Capacitors_THT:CP_Radial_D7.5mm_P2.50mm (layer Top) (tedit 5884A904)
    (at 140.335 144.78)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=7.5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 7.5mm Electrolytic Capacitor")
    (fp_text reference C1 (at 4.6228 -3.8354) (layer F.SilkS))
    (fp_text value 100u (at 1.25 4.81) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 VIN))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GNDPWR))
    (model Capacitors_ThroughHole.3dshapes/CP_Radial_D7.5mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:CP_Radial_D7.5mm_P2.50mm (layer Top) (tedit 58849643)
    (at 133.35 139.7)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=7.5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 7.5mm Electrolytic Capacitor")
    (fp_text reference C2 (at -2.54 -3.175) (layer F.SilkS))
    (fp_text value 100u (at 1.25 4.81) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GNDPWR))
    (model Capacitors_ThroughHole.3dshapes/CP_Radial_D7.5mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Disc_D5.0mm_W2.5mm_P2.50mm (layer Top) (tedit 5884BCBD)
    (at 143.51 127.635 180)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 5mm width 2.5mm Capacitor")
    (fp_text reference C3 (at 4.445 0 270) (layer F.SilkS))
    (fp_text value 22pf (at 1.25 2.31 180) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GNDPWR))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 XTAL1))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D5.0mm_W2.5mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Disc_D5.0mm_W2.5mm_P2.50mm (layer Top) (tedit 5884BCD0)
    (at 140.97 137.795)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 5mm width 2.5mm Capacitor")
    (fp_text reference C4 (at 1.27 2.159 180) (layer F.SilkS))
    (fp_text value 22pf (at 1.25 2.31) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GNDPWR))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 XTAL2))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D5.0mm_W2.5mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:CP_Radial_D7.5mm_P2.50mm (layer Top) (tedit 5884A944)
    (at 163.83 109.22)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=7.5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 7.5mm Electrolytic Capacitor")
    (fp_text reference C5 (at 4.699 -3.4544) (layer F.SilkS))
    (fp_text value 10u (at 1.25 4.81) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GNDPWR))
    (model Capacitors_ThroughHole.3dshapes/CP_Radial_D7.5mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Disc_D5.0mm_W2.5mm_P2.50mm (layer Top) (tedit 5884A93A)
    (at 143.51 106.68 270)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 5mm width 2.5mm Capacitor")
    (fp_text reference C6 (at 4.8514 0.0508 360) (layer F.SilkS))
    (fp_text value 100n (at 1.25 2.31 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GNDPWR))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 VCC))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D5.0mm_W2.5mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Disc_D5.0mm_W2.5mm_P2.50mm (layer Top) (tedit 5884A952)
    (at 163.83 127 90)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 5mm width 2.5mm Capacitor")
    (fp_text reference C7 (at -2.3114 0.0762 180) (layer F.SilkS))
    (fp_text value 100n (at 1.25 2.31 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(C7-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GNDPWR))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D5.0mm_W2.5mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Disc_D5.0mm_W2.5mm_P2.50mm (layer Top) (tedit 5884A94D)
    (at 163.83 119.38 90)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 5mm width 2.5mm Capacitor")
    (fp_text reference C8 (at -2.4384 0 180) (layer F.SilkS))
    (fp_text value 10n (at 1.25 2.31 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GNDPWR))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 VCC))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D5.0mm_W2.5mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Disc_D5.0mm_W2.5mm_P2.50mm (layer Top) (tedit 5884A933)
    (at 143.51 119.38 90)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 5mm width 2.5mm Capacitor")
    (fp_text reference C9 (at -2.2098 0.0254 180) (layer F.SilkS))
    (fp_text value 100n (at 1.27 -1.905 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 DTR))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 RESET))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D5.0mm_W2.5mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D3.0mm (layer Top) (tedit 5884987F)
    (at 165.1 149.86 180)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D1 (at 1.27 2.794 180) (layer F.SilkS))
    (fp_text value PWR (at 1.27 2.96 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 9 "Net-(D1-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 GNDPWR))
    (model LEDs.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D3.0mm (layer Top) (tedit 58849895)
    (at 165.1 135.89 180)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D2 (at 1.27 3.048 180) (layer F.SilkS))
    (fp_text value "LED 2" (at 1.27 2.96 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 10 "Net-(D2-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 GNDPWR))
    (model LEDs.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-28_W7.62mm_LongPads (layer Top) (tedit 58849A2D)
    (at 149.86 114.3)
    (descr "28-lead dip package, row spacing 7.62 mm (300 mils), LongPads")
    (tags "DIL DIP PDIP 2.54mm 7.62mm 300mil LongPads")
    (fp_text reference IC1 (at 3.81 35.56) (layer F.SilkS))
    (fp_text value ATMEGA328P-P (at 3.81 35.41) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 RESET))
    (pad 15 thru_hole oval (at 7.62 33.02) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 D9))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 D0))
    (pad 16 thru_hole oval (at 7.62 30.48) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 D10))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 D1))
    (pad 17 thru_hole oval (at 7.62 27.94) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 MOSI))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 D2))
    (pad 18 thru_hole oval (at 7.62 25.4) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 MISO))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 D3))
    (pad 19 thru_hole oval (at 7.62 22.86) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 SCK))
    (pad 6 thru_hole oval (at 0 12.7) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 D4))
    (pad 20 thru_hole oval (at 7.62 20.32) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 7 thru_hole oval (at 0 15.24) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 21 thru_hole oval (at 7.62 17.78) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(C7-Pad1)"))
    (pad 8 thru_hole oval (at 0 17.78) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GNDPWR))
    (pad 22 thru_hole oval (at 7.62 15.24) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GNDPWR))
    (pad 9 thru_hole oval (at 0 20.32) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 XTAL1))
    (pad 23 thru_hole oval (at 7.62 12.7) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 A0))
    (pad 10 thru_hole oval (at 0 22.86) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 XTAL2))
    (pad 24 thru_hole oval (at 7.62 10.16) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 A1))
    (pad 11 thru_hole oval (at 0 25.4) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 D5))
    (pad 25 thru_hole oval (at 7.62 7.62) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 A2))
    (pad 12 thru_hole oval (at 0 27.94) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 D6))
    (pad 26 thru_hole oval (at 7.62 5.08) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 A3))
    (pad 13 thru_hole oval (at 0 30.48) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 D7))
    (pad 27 thru_hole oval (at 7.62 2.54) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 A4))
    (pad 14 thru_hole oval (at 0 33.02) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 D8))
    (pad 28 thru_hole oval (at 7.62 0) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 A5))
    (model Housings_DIP.3dshapes/DIP-28_W7.62mm_LongPads.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer Top) (tedit 58849659)
    (at 128.905 144.78 180)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference P1 (at 0 5.08 180) (layer F.SilkS) hide)
    (fp_text value CONN_2 (at 0 4.93 180) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 VIN))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GNDPWR))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x10_Pitch2.54mm (layer Top) (tedit 588497EF)
    (at 169.545 115.57)
    (descr "Through hole straight pin header, 2x10, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x10 2.54mm double row")
    (fp_text reference P2 (at 1.27 -2.39) (layer F.SilkS))
    (fp_text value CONN_10X2 (at 1.27 25.25) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 D0))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GNDPWR))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 D1))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 RESET))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 D2))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 A0))
    (pad 7 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 D3))
    (pad 8 thru_hole oval (at 2.54 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 A1))
    (pad 9 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 D4))
    (pad 10 thru_hole oval (at 2.54 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 A2))
    (pad 11 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 D5))
    (pad 12 thru_hole oval (at 2.54 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 A3))
    (pad 13 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 D6))
    (pad 14 thru_hole oval (at 2.54 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 A4))
    (pad 15 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 D7))
    (pad 16 thru_hole oval (at 2.54 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 A5))
    (pad 17 thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 D8))
    (pad 18 thru_hole oval (at 2.54 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 19 thru_hole oval (at 0 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 D9))
    (pad 20 thru_hole oval (at 2.54 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 VCC))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x10_Pitch2.54mm.wrl
      (at (xyz 0.05 -0.45 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Discret:R1 (layer Top) (tedit 5884A967)
    (at 163.83 144.78)
    (descr "Resistance verticale")
    (tags R)
    (fp_text reference R1 (at 3.175 -0.1016 90) (layer F.SilkS))
    (fp_text value 330R (at -1.143 2.54) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at -1.27 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 9 "Net-(D1-Pad1)"))
    (pad 2 thru_hole circle (at 1.27 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 3 VCC))
    (model Discret.3dshapes/R1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Discret:R1 (layer Top) (tedit 5884A962)
    (at 163.83 140.97 180)
    (descr "Resistance verticale")
    (tags R)
    (fp_text reference R2 (at -3.556 0.0254 270) (layer F.SilkS))
    (fp_text value 330r (at -1.143 2.54 180) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at -1.27 0 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 10 "Net-(D2-Pad1)"))
    (pad 2 thru_hole circle (at 1.27 0 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 13 D10))
    (model Discret.3dshapes/R1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Discret:R1 (layer Top) (tedit 0)
    (at 130.81 132.08)
    (descr "Resistance verticale")
    (tags R)
    (fp_text reference R3 (at -1.016 2.54) (layer F.SilkS))
    (fp_text value 10K (at -1.143 2.54) (layer F.Fab))
    (pad 1 thru_hole circle (at -1.27 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 2 thru_hole circle (at 1.27 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 8 RESET))
    (model Discret.3dshapes/R1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_THT:SW_PUSH_6mm (layer Top) (tedit 5884A9C8)
    (at 129.54 123.19)
    (descr https://www.omron.com/ecb/products/pdf/en-b3f.pdf)
    (tags "tact sw push 6mm")
    (fp_text reference SW1 (at 3.3782 2.2098 180) (layer F.SilkS))
    (fp_text value SW_PUSH (at 3.75 6.7) (layer F.Fab) hide)
    (pad 2 thru_hole circle (at 0 4.5 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 8 RESET))
    (pad 1 thru_hole circle (at 0 0 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 GNDPWR))
    (pad 2 thru_hole circle (at 6.5 4.5 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 8 RESET))
    (pad 1 thru_hole circle (at 6.5 0 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 GNDPWR))
    (model Buttons_Switches_ThroughHole.3dshapes/SW_PUSH_6mm.wrl
      (at (xyz 0.005 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module G0TDJ:78XX (layer Top) (tedit 588496CE)
    (at 139.7 151.13 180)
    (descr "Non Isolated JEDEC TO-220 Package")
    (tags "Power Integration YN Package")
    (fp_text reference U1 (at 3.81 2.54 180) (layer F.SilkS))
    (fp_text value LM7805 (at -6.985 -0.635 180) (layer F.Fab))
    (pad GND thru_hole oval (at 0 0 180) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask)
      (net 2 GNDPWR))
    (pad VO thru_hole oval (at 2.54 0 180) (size 2.032 2.54) (drill oval 1.143) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad VI thru_hole oval (at -2.54 0 180) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask)
      (net 1 VIN))
  )
  (module G0TDJ:XTAL-RES_HC49-4H_Vertical (layer Top) (tedit 5884A913)
    (at 137.16 132.715)
    (descr "Crystal THT HC-49-4H http://5hertz.com/pdfs/04404_D.pdf")
    (tags "THT crystalHC-49-4H")
    (fp_text reference X1 (at 6.5278 -0.0508 90) (layer F.SilkS))
    (fp_text value "XTAL/RES 16MHz" (at 2.44 3.525) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 XTAL1))
    (pad 2 thru_hole circle (at 4.88 0) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 XTAL2))
    (pad 3 thru_hole circle (at 2.44 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GNDPWR))
    (model Crystals.3dshapes/Crystal_HC49-4H_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x06_Pitch2.54mm (layer Top) (tedit 58849544)
    (at 138.43 119.38 180)
    (descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x06 2.54mm single row")
    (fp_text reference P3 (at 0 -2.39 180) (layer F.SilkS) hide)
    (fp_text value CONN_6 (at 0 15.09 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 DTR))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 D1))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 D0))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GNDPWR))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GNDPWR))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x06_Pitch2.54mm.wrl
      (at (xyz 0 -0.25 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x03_Pitch2.54mm (layer Top) (tedit 588497F6)
    (at 169.545 144.78)
    (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.54mm double row")
    (fp_text reference P4 (at 1.27 -2.39) (layer F.SilkS))
    (fp_text value CONN_3X2 (at 1.27 7.47) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 MISO))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 SCK))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 MOSI))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 RESET))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GNDPWR))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x03_Pitch2.54mm.wrl
      (at (xyz 0.05 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module G0TDJ:minDUINO_v1p6_logo (layer Top) (tedit 58848F2B)
    (at 153.3652 131.3688 90)
    (fp_text reference G*** (at -0.13 -2.88 90) (layer F.SilkS) hide)
    (fp_text value LOGO (at -0.03 3.91 90) (layer F.SilkS) hide)
  )
  (module G0TDJ:minDUINO_v1p6_logo (layer Bottom) (tedit 5884D930)
    (at 153.3652 131.5212 270)
    (fp_text reference G7 (at -0.13 2.88 270) (layer B.SilkS) hide)
    (fp_text value LOGO (at 3.81 3.175 270) (layer B.SilkS) hide)
  )
  (module G0TDJ:minDUINO_worm_logo (layer Top) (tedit 5884BF51)
    (at 153.67 108.585)
    (fp_text reference G2 (at -0.01 -2.93) (layer F.SilkS) hide)
    (fp_text value LOGO (at -0.01 4) (layer F.SilkS) hide)
  )
  (module Connectors:1pin (layer Top) (tedit 5884BF6A)
    (at 172.72 107.95)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF1 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 3) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 5 5) (drill 3.5) (layers *.Cu *.Mask))
  )
  (module Connectors:1pin (layer Top) (tedit 5884BF70)
    (at 130.81 107.95)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF2 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 3) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5 5) (drill 3.5) (layers *.Cu *.Mask))
  )
  (module Connectors:1pin (layer Top) (tedit 5884BF76)
    (at 130.81 149.86)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF3 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 3) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5 5) (drill 3.5) (layers *.Cu *.Mask))
  )
  (module G0TDJ:VIA_0.6mm (layer Top) (tedit 5884D10C)
    (at 160.02 130.175)
    (fp_text reference REF** (at 0 1) (layer F.SilkS) hide)
    (fp_text value .6mm_VIA (at 0 -1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GNDPWR) (zone_connect 2))
  )
  (module G0TDJ:VIA_0.6mm (layer Top) (tedit 5884D162)
    (at 154.94 125.73)
    (fp_text reference REF** (at 0 1) (layer F.SilkS) hide)
    (fp_text value .6mm_VIA (at 0 -1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GNDPWR) (zone_connect 2))
  )
  (module G0TDJ:VIA_0.6mm (layer Top) (tedit 5884D1C4)
    (at 152.4 133.35)
    (fp_text reference REF** (at 0 1) (layer F.SilkS) hide)
    (fp_text value .6mm_VIA (at 0 -1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GNDPWR) (zone_connect 2))
  )
  (module G0TDJ:VIA_0.6mm (layer Top) (tedit 5884D5AC)
    (at 174 113)
    (fp_text reference REF** (at 0 1) (layer F.SilkS) hide)
    (fp_text value .6mm_VIA (at 0 -1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GNDPWR) (zone_connect 2))
  )
  (module G0TDJ:VIA_0.6mm (layer Top) (tedit 5884D65B)
    (at 165 116)
    (fp_text reference REF** (at 0 1) (layer F.SilkS) hide)
    (fp_text value .6mm_VIA (at 0 -1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GNDPWR) (zone_connect 2))
  )
  (module G0TDJ:VIA_0.6mm (layer Top) (tedit 5884D7C2)
    (at 152.4 151.13)
    (fp_text reference REF** (at 0 1) (layer F.SilkS) hide)
    (fp_text value .6mm_VIA (at 0 -1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GNDPWR) (zone_connect 2))
  )
  (module G0TDJ:VIA_0.6mm (layer Top) (tedit 5884D826)
    (at 172.085 151.765)
    (fp_text reference REF** (at 0 1) (layer F.SilkS) hide)
    (fp_text value .6mm_VIA (at 0 -1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GNDPWR) (zone_connect 2))
  )
  (module G0TDJ:VIA_0.6mm (layer Top) (tedit 5884D888)
    (at 131.445 142.24)
    (fp_text reference REF** (at 0 1) (layer F.SilkS) hide)
    (fp_text value .6mm_VIA (at 0 -1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GNDPWR) (zone_connect 2))
  )
  (module G0TDJ:minDUINO_16_F.Cu (layer Top) (tedit 5884E563)
    (at 128.80848 116.41328 90)
    (fp_text reference G*** (at 0 -2 90) (layer Top) hide)
    (fp_text value LOGO (at 0 2 90) (layer Top) hide)
  )
  (module G0TDJ:minDUINO_16_F.Mask (layer Top) (tedit 5884E587)
    (at 128.80848 116.41328 90)
    (fp_text reference G*** (at 0 -2 90) (layer F.Mask) hide)
    (fp_text value LOGO (at 0 2 90) (layer F.Mask) hide)
  )
  (module Symbols:KiCad-Logo2_6mm_SilkScreen (layer Bottom) (tedit 0)
    (at 153.67 108.585 180)
    (descr "KiCad Logo")
    (tags "Logo KiCad")
    (attr virtual)
    (fp_text reference REF*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value KiCad-Logo2_6mm_SilkScreen (at 0.75 0 180) (layer B.Fab) hide)
  )
  (module Symbols:OSHW-Logo_7.5x8mm_SilkScreen (layer Bottom) (tedit 0)
    (at 132.08 116.205 180)
    (descr "Open Source Hardware Logo")
    (tags "Logo OSHW")
    (attr virtual)
    (fp_text reference REF*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value OSHW-Logo_7.5x8mm_SilkScreen (at 0.75 0 180) (layer B.Fab) hide)
  )
  (gr_text ICSP (at 173.99 147.32 90) (layer B.SilkS))
  (gr_text FTDI/Serial (at 140.335 113.03 90) (layer B.SilkS))
  (gr_text VCC (at 174.625 138.43) (layer B.SilkS))
  (gr_text VCC (at 174.625 135.89) (layer B.SilkS))
  (gr_text A5 (at 174.625 133.35) (layer B.SilkS))
  (gr_text A4 (at 174.625 130.81) (layer B.SilkS))
  (gr_text A3 (at 174.625 128.27) (layer B.SilkS))
  (gr_text A2 (at 174.625 125.73) (layer B.SilkS))
  (gr_text A1 (at 174.625 123.19) (layer B.SilkS))
  (gr_text A0 (at 174.625 120.65) (layer B.SilkS))
  (gr_text RES (at 174.625 118.11) (layer B.SilkS))
  (gr_text D9 (at 167.005 138.43) (layer B.SilkS))
  (gr_text D7 (at 167.005 133.35) (layer B.SilkS))
  (gr_text D8 (at 167.005 135.89) (layer B.SilkS))
  (gr_text D6 (at 167.005 130.81) (layer B.SilkS))
  (gr_text D5 (at 167.005 128.27) (layer B.SilkS))
  (gr_text D4 (at 167.005 125.73) (layer B.SilkS))
  (gr_text D3 (at 167.005 123.19) (layer B.SilkS))
  (gr_text D2 (at 167.005 120.65) (layer B.SilkS))
  (gr_text D1 (at 167.005 118.11) (layer B.SilkS))
  (gr_text D0 (at 174.625 115.57) (layer B.SilkS))
  (gr_text D0 (at 167.005 115.57) (layer B.SilkS))
  (gr_text ICSP (at 174.625 147.32 90) (layer F.SilkS))
  (gr_text VCC (at 174.625 138.43) (layer F.SilkS))
  (gr_text VCC (at 174.625 135.89) (layer F.SilkS))
  (gr_text A5 (at 174.625 133.35) (layer F.SilkS))
  (gr_text A4 (at 174.625 130.81) (layer F.SilkS))
  (gr_text A3 (at 174.625 128.27) (layer F.SilkS))
  (gr_text A2 (at 174.625 125.73) (layer F.SilkS))
  (gr_text A1 (at 174.625 123.19) (layer F.SilkS))
  (gr_text A0 (at 174.625 120.65) (layer F.SilkS))
  (gr_text D9 (at 167.005 138.43) (layer F.SilkS))
  (gr_text D8 (at 167.005 135.89) (layer F.SilkS))
  (gr_text D7 (at 167.005 133.35) (layer F.SilkS))
  (gr_text D6 (at 167.005 130.81) (layer F.SilkS))
  (gr_text D5 (at 167.005 128.27) (layer F.SilkS))
  (gr_text D4 (at 167.005 125.73) (layer F.SilkS))
  (gr_text D3 (at 167.005 123.19) (layer F.SilkS))
  (gr_text D2 (at 167.005 120.65) (layer F.SilkS))
  (gr_text D1 (at 167.005 118.11) (layer F.SilkS))
  (gr_text +VIN (at 132.08 144.78) (layer F.SilkS))
  (gr_text GND (at 128.905 139.065 90) (layer F.SilkS))
  (gr_text "Designed by\nSteve Smith\nG0TDJ" (at 131.699 120.65 90) (layer F.SilkS))
  (gr_text D0 (at 167.005 115.57) (layer F.SilkS))
  (gr_text RES (at 174.625 118.11) (layer F.SilkS))
  (gr_text GND (at 174.625 115.57) (layer F.SilkS))
  (gr_text DTR (at 135.255 119.38) (layer F.SilkS))
  (gr_text RXD (at 135.255 116.84) (layer F.SilkS))
  (gr_text TXD (at 135.255 114.3) (layer F.SilkS))
  (gr_text VCC (at 135.255 111.76) (layer F.SilkS))
  (gr_text CTS (at 135.255 109.22) (layer F.SilkS))
  (gr_text GND (at 135.255 106.68) (layer F.SilkS))
  (gr_text FTDI/Serial (at 140.97 113.03 90) (layer F.SilkS))
  (gr_arc (start 129.54 106.68) (end 127 106.68) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 129.54 151.13) (end 129.54 153.67) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 173.99 153.67) (end 129.54 153.67) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 173.99 104.14) (end 129.54 104.14) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 127 151.13) (end 127 106.68) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 176.53 106.68) (end 176.53 151.13) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 173.99 151.13) (end 176.53 151.13) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 173.99 106.68) (end 173.99 104.14) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GNDPWR) (layer Top) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 176.53 153.67) (xy 127 153.67) (xy 127 104.14) (xy 176.53 104.14)
      )
    )
  )
  (zone (net 2) (net_name GNDPWR) (layer Bottom) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 176.53 153.67) (xy 127 153.67) (xy 127 104.14) (xy 176.53 104.14)
      )
    )
  )
)
