(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "Net-(Cc22-Pad2)")
  (net 2 "Net-(Cf720-Pad1)")
  (net 3 "Net-(Cf720-Pad2)")
  (net 4 "Net-(Cc12-Pad2)")
  (net 5 "Net-(Cf619-Pad1)")
  (net 6 "Net-(Cf619-Pad2)")
  (net 7 "Net-(Cf2221-Pad2)")
  (net 8 "/6")
  (net 9 "Net-(Cf1718-Pad2)")
  (net 10 "Net-(Cf2221-Pad1)")
  (net 11 "Net-(Cf1718-Pad1)")
  (net 12 "Net-(Cf821-Pad2)")
  (net 13 "Net-(Cf518-Pad2)")
  (net 14 "Net-(Cf1023-Pad1)")
  (net 15 "Net-(Cc22-Pad1)")
  (net 16 "Net-(Cf316-Pad1)")
  (net 17 "Net-(Cc12-Pad1)")
  (net 18 "/14")
  (net 19 "Net-(Cf1225-Pad2)")
  (net 20 "/15")
  (net 21 "Net-(J24-Pad1)")
  (net 22 "/16")
  (net 23 "/17")
  (net 24 "/18")
  (net 25 "Net-(J2-Pad1)")
  (net 26 "Net-(D4K2-Pad2)")
  (net 27 "Net-(J11-Pad1)")
  (net 28 "Net-(D4K2-Pad11)")
  (net 29 "Net-(J15-Pad1)")
  (net 30 "Net-(D4K2-Pad15)")
  (net 31 "Net-(D4K2-Pad24)")
  (net 32 "/19")
  (net 33 "/5")
  (net 34 "/1")
  (net 35 "Net-(Cf114-Pad1)")
  (net 36 "/2")
  (net 37 "/3")
  (net 38 "Net-(Cf316-Pad2)")
  (net 39 "/4")
  (net 40 "Net-(Cf416-Pad1)")
  (net 41 "Net-(Cf923-Pad1)")
  (net 42 "Net-(Cf1023-Pad2)")
  (net 43 "Net-(Cf1225-Pad1)")
  (net 44 "Net-(Cf114-Pad2)")
  (net 45 "unconnected-(D4K1-Pad13)")
  (net 46 "unconnected-(D4K2-Pad5)")
  (net 47 "unconnected-(D4K2-Pad6)")
  (net 48 "unconnected-(D4K2-Pad7)")
  (net 49 "unconnected-(D4K2-Pad8)")
  (net 50 "unconnected-(D4K2-Pad13)")
  (net 51 "unconnected-(D4K2-Pad17)")
  (net 52 "unconnected-(D4K2-Pad18)")
  (net 53 "unconnected-(D4K2-Pad19)")
  (net 54 "unconnected-(D4K2-Pad20)")
  (net 55 "unconnected-(D4K2-Pad21)")
  (net 56 "unconnected-(D4K2-Pad22)")
  (net 57 "/12")
  (net 58 "/25")
  (net 59 "/24")
  (net 60 "/23")
  (net 61 "/22")
  (net 62 "/21")
  (net 63 "/20")
  (net 64 "/7")
  (net 65 "/8")
  (net 66 "/9")
  (net 67 "/10")
  (net 68 "/11")
  (footprint "MountingHole:MountingHole_4.3mm_M4_Pad_Via" (layer "F.Cu")
    (tedit 56DDBFD7)
    (at 203.962 58.166)
    (descr "Mounting Hole 4.3mm, M4")
    (tags "mounting hole 4.3mm m4")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -5.3) (layer "F.SilkS"))
    (fp_text value "MountingHole_4.3mm_M4_Pad_Via" (at 0 5.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at -3.225 0) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle (at 0 3.225) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle (at 2.280419 -2.280419) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle (at 3.225 0) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle (at -2.280419 -2.280419) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle (at 2.280419 2.280419) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle (at 0 0) (size 8.6 8.6) (drill 4.3) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle (at 0 -3.225) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle (at -2.280419 2.280419) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask))
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 135.65964 71.421159 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "SplitStage-4K-V2.0.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Rf6" (at 0 -1.82 90) (layer "F.SilkS"))
    (fp_text value "R=" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 8 "/6") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 5 "Net-(Cf619-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 140.640248 71.421159 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "SplitStage-4K-V2.0.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Rf19" (at 0 -1.82 90) (layer "F.SilkS"))
    (fp_text value "R=" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 32 "/19") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 6 "Net-(Cf619-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_4.3mm_M4_Pad_Via" (layer "F.Cu")
    (tedit 56DDBFD7)
    (at 83.312 58.166)
    (descr "Mounting Hole 4.3mm, M4")
    (tags "mounting hole 4.3mm m4")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -5.3) (layer "F.SilkS"))
    (fp_text value "MountingHole_4.3mm_M4_Pad_Via" (at 0 5.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at -3.225 0) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle (at 0 -3.225) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle (at 2.280419 2.280419) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle (at 0 0) (size 8.6 8.6) (drill 4.3) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle (at -2.280419 2.280419) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle (at -2.280419 -2.280419) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle (at 3.225 0) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle (at 0 3.225) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle (at 2.280419 -2.280419) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask))
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 185.46572 71.421159 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "SplitStage-4K-V2.0.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Rf11" (at 0 -1.82 90) (layer "F.SilkS"))
    (fp_text value "R=" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 68 "/11") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 27 "Net-(J11-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1812_4532Metric_Pad1.57x3.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 199.26456 79.081492)
    (descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "SplitStage-4K-V2.0.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Cf1225" (at 0 -2.65) (layer "F.SilkS"))
    (fp_text value "C=" (at 0 2.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.1375 0) (size 1.575 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15873)
      (net 43 "Net-(Cf1225-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 2.1375 0) (size 1.575 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15873)
      (net 19 "Net-(Cf1225-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1812_4532Metric_Pad1.57x3.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 132.990224 87.471825 -90)
    (descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "SplitStage-4K-V2.0.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Csc1" (at 0 -2.65 90) (layer "F.SilkS"))
    (fp_text value "C=  " (at 0 2.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.1375 0 270) (size 1.575 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15873)
      (net 9 "Net-(Cf1718-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 2.1375 0 270) (size 1.575 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15873)
      (net 6 "Net-(Cf619-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1812_4532Metric_Pad1.57x3.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 173.17176 79.081492)
    (descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "SplitStage-4K-V2.0.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Cf923" (at 0 -2.65) (layer "F.SilkS"))
    (fp_text value "C=" (at 0 2.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.1375 0) (size 1.575 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15873)
      (net 41 "Net-(Cf923-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 2.1375 0) (size 1.575 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15873)
      (net 14 "Net-(Cf1023-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 146.234 87.471825 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "SplitStage-4K-V2.0.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Rsc2" (at 0 -1.82 90) (layer "F.SilkS"))
    (fp_text value "R=  " (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 7 "Net-(Cf2221-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 3 "Net-(Cf720-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 155.582072 71.421159 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "SplitStage-4K-V2.0.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Rf8" (at 0 -1.82 90) (layer "F.SilkS"))
    (fp_text value "R=" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 65 "/8") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 12 "Net-(Cf821-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 170.523896 71.421159 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "SplitStage-4K-V2.0.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Rf9" (at 0 -1.82 90) (layer "F.SilkS"))
    (fp_text value "R=" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 66 "/9") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 41 "Net-(Cf923-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 100.795384 71.421159 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "SplitStage-4K-V2.0.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Rf15" (at 0 -1.82 90) (layer "F.SilkS"))
    (fp_text value "R=" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 20 "/15") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 29 "Net-(J15-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 175.504504 71.421159 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "SplitStage-4K-V2.0.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Rf23" (at 0 -1.82 90) (layer "F.SilkS"))
    (fp_text value "R=" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 60 "/23") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 14 "Net-(Cf1023-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 90.834168 71.421159 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "SplitStage-4K-V2.0.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Rf14" (at 0 -1.82 90) (layer "F.SilkS"))
    (fp_text value "R=" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 18 "/14") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 44 "Net-(Cf114-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 115.737208 71.421159 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "SplitStage-4K-V2.0.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Rf4" (at 0 -1.82 90) (layer "F.SilkS"))
    (fp_text value "R=" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 39 "/4") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 40 "Net-(Cf416-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1812_4532Metric_Pad1.57x3.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 86.99656 79.081492)
    (descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "SplitStage-4K-V2.0.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Cf114" (at 0 -2.65) (layer "F.SilkS"))
    (fp_text value "C=" (at 0 2.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.1375 0) (size 1.575 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15873)
      (net 35 "Net-(Cf114-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 2.1375 0) (size 1.575 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15873)
      (net 44 "Net-(Cf114-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 160.307776 87.471825 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "SplitStage-4K-V2.0.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Rgn2" (at 0 -1.82 90) (layer "F.SilkS"))
    (fp_text value "R=" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 12 "Net-(Cf821-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 2 "Net-(Cf720-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1812_4532Metric_Pad1.57x3.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 104.50616 79.081492 180)
    (descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "SplitStage-4K-V2.0.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Cf316" (at 0 -2.65) (layer "F.SilkS"))
    (fp_text value "C=" (at 0 2.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.1375 0 180) (size 1.575 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15873)
      (net 16 "Net-(Cf316-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 2.1375 0 180) (size 1.575 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15873)
      (net 38 "Net-(Cf316-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1812_4532Metric_Pad1.57x3.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 153.270888 87.471825 -90)
    (descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "SplitStage-4K-V2.0.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Csc2" (at 0 -2.65 90) (layer "F.SilkS"))
    (fp_text value "C=  " (at 0 2.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.1375 0 270) (size 1.575 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15873)
      (net 7 "Net-(Cf2221-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 2.1375 0 270) (size 1.575 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15873)
      (net 3 "Net-(Cf720-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 97.98296 79.081492 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "SplitStage-4K-V2.0.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "J15" (at 0 -1.82 90) (layer "F.SilkS"))
    (fp_text value "R=" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 29 "Net-(J15-Pad1)") (pinfunction "A") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 30 "Net-(D4K2-Pad15)") (pinfunction "B") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1812_4532Metric_Pad1.57x3.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 113.08936 79.081492 180)
    (descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "SplitStage-4K-V2.0.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Cf416" (at 0 -2.65) (layer "F.SilkS"))
    (fp_text value "C=" (at 0 2.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.1375 0 180) (size 1.575 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15873)
      (net 40 "Net-(Cf416-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 2.1375 0 180) (size 1.575 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15873)
      (net 16 "Net-(Cf316-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 120.717816 71.421159 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "SplitStage-4K-V2.0.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Rf17" (at 0 -1.82 90) (layer "F.SilkS"))
    (fp_text value "R=" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 23 "/17") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 11 "Net-(Cf1718-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1812_4532Metric_Pad1.57x3.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 163.24231 96.702158 180)
    (descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "SplitStage-4K-V2.0.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Cc22" (at 0 -2.65) (layer "F.SilkS"))
    (fp_text value "C=" (at 0 2.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.1375 0 180) (size 1.575 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15873)
      (net 15 "Net-(Cc22-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 2.1375 0 180) (size 1.575 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15873)
      (net 1 "Net-(Cc22-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 110.7566 71.421159 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "SplitStage-4K-V2.0.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Rf16" (at 0 -1.82 90) (layer "F.SilkS"))
    (fp_text value "R=" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 22 "/16") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 16 "Net-(Cf316-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 165.543288 71.421159 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "SplitStage-4K-V2.0.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Rf22" (at 0 -1.82 90) (layer "F.SilkS"))
    (fp_text value "R=" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 61 "/22") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 10 "Net-(Cf2221-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 190.446328 71.421159 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "SplitStage-4K-V2.0.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Rf24" (at 0 -1.82 90) (layer "F.SilkS"))
    (fp_text value "R=" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 59 "/24") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 21 "Net-(J24-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 150.601464 71.421159 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "SplitStage-4K-V2.0.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Rf20" (at 0 -1.82 90) (layer "F.SilkS"))
    (fp_text value "R=" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 63 "/20") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 3 "Net-(Cf720-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Transistor_Power_Module:CryoHEMTTransistor" (layer "F.Cu")
    (tedit 0)
    (at 136.06331 95.752158)
    (property "Sheetfile" "SplitStage-4K-V2.0.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Q12" (at 0 -2.54 unlocked) (layer "F.SilkS"))
    (fp_text value "200pF" (at 0 5.08 unlocked) (layer "F.Fab"))
    (fp_text user "G" (at -2.475 -0.32) (layer "F.SilkS"))
    (fp_text user "D" (at -2.475 2.22) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0.7 0.95 90) (layer "F.Fab"))
    (pad "1" smd rect (at -0.65 0) (size 1.65 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "Net-(Cc12-Pad2)") (pinfunction "G") (pintype "input"))
    (pad "2" smd rect (at -0.65 1.9) (size 1.65 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "Net-(Cf619-Pad1)") (pinfunction "D") (pintype "passive"))
    (pad "3" smd rect (at 2.06 0.95) (size 1.65 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "Net-(Cf619-Pad2)") (pinfunction "S") (pintype "passive"))
  )
  (footprint "Capacitor_SMD:C_1812_4532Metric_Pad1.57x3.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 164.58856 79.081492 180)
    (descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "SplitStage-4K-V2.0.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Cf2221" (at 0 -2.65) (layer "F.SilkS"))
    (fp_text value "C=" (at 0 2.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.1375 0 180) (size 1.575 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15873)
      (net 10 "Net-(Cf2221-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 2.1375 0 180) (size 1.575 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15873)
      (net 7 "Net-(Cf2221-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 160.56268 71.421159 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "SplitStage-4K-V2.0.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Rf21" (at 0 -1.82 90) (layer "F.SilkS"))
    (fp_text value "R=" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 62 "/21") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 7 "Net-(Cf2221-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 125.698424 71.421159 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "SplitStage-4K-V2.0.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Rf18" (at 0 -1.82 90) (layer "F.SilkS"))
    (fp_text value "R=" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 24 "/18") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 9 "Net-(Cf1718-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 145.620856 71.421159 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "SplitStage-4K-V2.0.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Rf7" (at 0 -1.82 90) (layer "F.SilkS"))
    (fp_text value "R=" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 64 "/7") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 2 "Net-(Cf720-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1812_4532Metric_Pad1.57x3.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 138.83896 79.081492)
    (descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "SplitStage-4K-V2.0.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Cf619" (at 0 -2.65) (layer "F.SilkS"))
    (fp_text value "C=" (at 0 2.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.1375 0) (size 1.575 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15873)
      (net 5 "Net-(Cf619-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 2.1375 0) (size 1.575 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15873)
      (net 6 "Net-(Cf619-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1812_4532Metric_Pad1.57x3.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 123.01881 96.702158)
    (descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "SplitStage-4K-V2.0.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Cc12" (at 0 -2.65) (layer "F.SilkS"))
    (fp_text value "C=" (at 0 2.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.1375 0) (size 1.575 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15873)
      (net 17 "Net-(Cc12-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 2.1375 0) (size 1.575 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15873)
      (net 4 "Net-(Cc12-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 140.027112 87.471825 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "SplitStage-4K-V2.0.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Rsc1" (at 0 -1.82 90) (layer "F.SilkS"))
    (fp_text value "R=  " (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 9 "Net-(Cf1718-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 6 "Net-(Cf619-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1812_4532Metric_Pad1.57x3.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 130.25576 79.081492)
    (descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "SplitStage-4K-V2.0.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Cf518" (at 0 -2.65) (layer "F.SilkS"))
    (fp_text value "C=" (at 0 2.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.1375 0) (size 1.575 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15873)
      (net 9 "Net-(Cf1718-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 2.1375 0) (size 1.575 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15873)
      (net 13 "Net-(Cf518-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 195.426936 71.421159 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "SplitStage-4K-V2.0.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Rf12" (at 0 -1.82 90) (layer "F.SilkS"))
    (fp_text value "R=" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 57 "/12") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 43 "Net-(Cf1225-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 188.27816 79.081492 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "SplitStage-4K-V2.0.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "J11" (at 0 -1.82 90) (layer "F.SilkS"))
    (fp_text value "R=" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 27 "Net-(J11-Pad1)") (pinfunction "A") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 28 "Net-(D4K2-Pad11)") (pinfunction "B") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 105.775992 71.421159 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "SplitStage-4K-V2.0.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Rf3" (at 0 -1.82 90) (layer "F.SilkS"))
    (fp_text value "R=" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 37 "/3") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 38 "Net-(Cf316-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 85.85356 71.421159 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "SplitStage-4K-V2.0.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Rf1" (at 0 -1.82 90) (layer "F.SilkS"))
    (fp_text value "R=" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 34 "/1") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 35 "Net-(Cf114-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 93.51976 79.081492 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "SplitStage-4K-V2.0.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "J2" (at 0 -1.82 90) (layer "F.SilkS"))
    (fp_text value "R=" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 25 "Net-(J2-Pad1)") (pinfunction "A") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 26 "Net-(D4K2-Pad2)") (pinfunction "B") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Transistor_Power_Module:CryoHEMTTransistor" (layer "F.Cu")
    (tedit 0)
    (at 148.78781 95.752158)
    (property "Sheetfile" "SplitStage-4K-V2.0.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Q22" (at 0 -2.54 unlocked) (layer "F.SilkS"))
    (fp_text value "200pF" (at 0 5.08 unlocked) (layer "F.Fab"))
    (fp_text user "G" (at -2.475 -0.32) (layer "F.SilkS"))
    (fp_text user "D" (at -2.475 2.22) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0.7 0.95 90) (layer "F.Fab"))
    (pad "1" smd rect (at -0.65 0) (size 1.65 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "Net-(Cc22-Pad2)") (pinfunction "G") (pintype "input"))
    (pad "2" smd rect (at -0.65 1.9) (size 1.65 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "Net-(Cf720-Pad1)") (pinfunction "D") (pintype "passive"))
    (pad "3" smd rect (at 2.06 0.95) (size 1.65 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "Net-(Cf720-Pad2)") (pinfunction "S") (pintype "passive"))
  )
  (footprint "Capacitor_SMD:C_1812_4532Metric_Pad1.57x3.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 156.00536 79.081492 180)
    (descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "SplitStage-4K-V2.0.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Cf821" (at 0 -2.65) (layer "F.SilkS"))
    (fp_text value "C=" (at 0 2.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.1375 0 180) (size 1.575 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15873)
      (net 7 "Net-(Cf2221-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 2.1375 0 180) (size 1.575 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15873)
      (net 12 "Net-(Cf821-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 113.53956 87.471825 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "SplitStage-4K-V2.0.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Rfol1" (at 0 -1.82 90) (layer "F.SilkS"))
    (fp_text value "R=" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 16 "Net-(Cf316-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 17 "Net-(Cc12-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1812_4532Metric_Pad1.57x3.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 121.67256 79.081492)
    (descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "SplitStage-4K-V2.0.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Cf1718" (at 0 -2.65) (layer "F.SilkS"))
    (fp_text value "C=" (at 0 2.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.1375 0) (size 1.575 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15873)
      (net 11 "Net-(Cf1718-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 2.1375 0) (size 1.575 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15873)
      (net 9 "Net-(Cf1718-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 95.814776 71.421159 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "SplitStage-4K-V2.0.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Rf2" (at 0 -1.82 90) (layer "F.SilkS"))
    (fp_text value "R=" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 36 "/2") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 25 "Net-(J2-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_4.3mm_M4_Pad_Via" (layer "F.Cu")
    (tedit 56DDBFD7)
    (at 203.962 115.316)
    (descr "Mounting Hole 4.3mm, M4")
    (tags "mounting hole 4.3mm m4")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -5.3) (layer "F.SilkS"))
    (fp_text value "MountingHole_4.3mm_M4_Pad_Via" (at 0 5.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 3.225 0) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle (at 0 -3.225) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle (at 2.280419 -2.280419) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle (at -2.280419 2.280419) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle (at -2.280419 -2.280419) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle (at -3.225 0) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle (at 0 0) (size 8.6 8.6) (drill 4.3) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle (at 0 3.225) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle (at 2.280419 2.280419) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask))
  )
  (footprint "Connector_Dsub:mdm25-male-footprint" (layer "F.Cu")
    (tedit 0)
    (at 143.13056 108.760326)
    (descr "380-025-213L001-1")
    (tags "Connector")
    (property "Sheetfile" "SplitStage-4K-V2.0.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D4K2" (at 0.420856 2.383599) (layer "F.SilkS"))
    (fp_text value "MDM25_Male" (at 0.254 -2.54) (layer "F.SilkS"))
    (fp_text user "1" (at -10.16 -2.54) (layer "F.SilkS"))
    (fp_text user "25" (at 10.16 2.54) (layer "F.SilkS"))
    (fp_text user "14" (at -10.16 2.54) (layer "F.SilkS"))
    (fp_text user "13" (at 10.16 -2.54) (layer "F.SilkS"))
    (pad "1" thru_hole circle (at -7.62 -0.65) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask)
      (net 35 "Net-(Cf114-Pad1)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at -6.35 -0.65) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask)
      (net 26 "Net-(D4K2-Pad2)") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle (at -5.08 -0.65) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask)
      (net 38 "Net-(Cf316-Pad2)") (pinfunction "3") (pintype "passive"))
    (pad "4" thru_hole circle (at -3.81 -0.65) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask)
      (net 40 "Net-(Cf416-Pad1)") (pinfunction "4") (pintype "passive"))
    (pad "5" thru_hole circle (at -2.54 -0.65) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask)
      (net 46 "unconnected-(D4K2-Pad5)") (pinfunction "5") (pintype "passive"))
    (pad "6" thru_hole circle (at -1.27 -0.65) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask)
      (net 47 "unconnected-(D4K2-Pad6)") (pinfunction "6") (pintype "passive"))
    (pad "7" thru_hole circle (at 0 -0.65) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask)
      (net 48 "unconnected-(D4K2-Pad7)") (pinfunction "7") (pintype "passive"))
    (pad "8" thru_hole circle (at 1.27 -0.65) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask)
      (net 49 "unconnected-(D4K2-Pad8)") (pinfunction "8") (pintype "passive"))
    (pad "9" thru_hole circle (at 2.54 -0.65) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask)
      (net 41 "Net-(Cf923-Pad1)") (pinfunction "9") (pintype "passive"))
    (pad "10" thru_hole circle (at 3.81 -0.65) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask)
      (net 42 "Net-(Cf1023-Pad2)") (pinfunction "10") (pintype "passive"))
    (pad "11" thru_hole circle (at 5.08 -0.65) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask)
      (net 28 "Net-(D4K2-Pad11)") (pinfunction "11") (pintype "passive"))
    (pad "12" thru_hole circle (at 6.35 -0.65) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask)
      (net 43 "Net-(Cf1225-Pad1)") (pinfunction "12") (pintype "passive"))
    (pad "13" thru_hole circle (at 7.62 -0.65) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask)
      (net 50 "unconnected-(D4K2-Pad13)") (pinfunction "13") (pintype "passive"))
    (pad "14" thru_hole circle (at -6.99 0.45) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask)
      (net 44 "Net-(Cf114-Pad2)") (pinfunction "P14") (pintype "passive"))
    (pad "15" thru_hole circle (at -5.72 0.45) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask)
      (net 30 "Net-(D4K2-Pad15)") (pinfunction "P15") (pintype "passive"))
    (pad "16" thru_hole circle (at -4.45 0.45) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask)
      (net 17 "Net-(Cc12-Pad1)") (pinfunction "P16") (pintype "passive"))
    (pad "17" thru_hole circle (at -3.18 0.45) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask)
      (net 51 "unconnected-(D4K2-Pad17)") (pinfunction "P17") (pintype "passive"))
    (pad "18" thru_hole circle (at -1.91 0.45) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask)
      (net 52 "unconnected-(D4K2-Pad18)") (pinfunction "P18") (pintype "passive"))
    (pad "19" thru_hole circle (at -0.64 0.45) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask)
      (net 53 "unconnected-(D4K2-Pad19)") (pinfunction "P19") (pintype "passive"))
    (pad "20" thru_hole circle (at 0.64 0.45) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask)
      (net 54 "unconnected-(D4K2-Pad20)") (pinfunction "P20") (pintype "passive"))
    (pad "21" thru_hole circle (at 1.91 0.45) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask)
      (net 55 "unconnected-(D4K2-Pad21)") (pinfunction "P21") (pintype "passive"))
    (pad "22" thru_hole circle (at 3.18 0.45) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask)
      (net 56 "unconnected-(D4K2-Pad22)") (pinfunction "P22") (pintype "passive"))
    (pad "23" thru_hole circle (at 4.45 0.45) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask)
      (net 15 "Net-(Cc22-Pad1)") (pinfunction "P23") (pintype "passive"))
    (pad "24" thru_hole circle (at 5.72 0.45) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask)
      (net 31 "Net-(D4K2-Pad24)") (pinfunction "P24") (pintype "passive"))
    (pad "25" thru_hole circle (at 6.99 0.45) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask)
      (net 19 "Net-(Cf1225-Pad2)") (pinfunction "P25") (pintype "passive"))
    (pad "MH1" thru_hole circle (at -12.275 -0.1) (size 4.305 4.305) (drill 2.87) (layers *.Cu *.Mask))
    (pad "MH2" thru_hole circle (at 12.275 -0.1) (size 4.305 4.305) (drill 2.87) (layers *.Cu *.Mask))
    (model "380-025-213L001.stp"
      (offset (xyz 7.62 0.65 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1812_4532Metric_Pad1.57x3.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 181.75496 79.081492)
    (descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "SplitStage-4K-V2.0.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Cf1023" (at 0 -2.65) (layer "F.SilkS"))
    (fp_text value "C=" (at 0 2.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.1375 0) (size 1.575 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15873)
      (net 14 "Net-(Cf1023-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 2.1375 0) (size 1.575 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15873)
      (net 42 "Net-(Cf1023-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1812_4532Metric_Pad1.57x3.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 147.42216 79.081492)
    (descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "SplitStage-4K-V2.0.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Cf720" (at 0 -2.65) (layer "F.SilkS"))
    (fp_text value "C=" (at 0 2.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.1375 0) (size 1.575 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15873)
      (net 2 "Net-(Cf720-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 2.1375 0) (size 1.575 3.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15873)
      (net 3 "Net-(Cf720-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 192.74136 79.081492 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "SplitStage-4K-V2.0.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "J24" (at 0 -1.82 90) (layer "F.SilkS"))
    (fp_text value "R=" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 21 "Net-(J24-Pad1)") (pinfunction "A") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 31 "Net-(D4K2-Pad24)") (pinfunction "B") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 172.72156 87.471825 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "SplitStage-4K-V2.0.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Rfol2" (at 0 -1.82 90) (layer "F.SilkS"))
    (fp_text value "R=" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 14 "Net-(Cf1023-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 15 "Net-(Cc22-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 200.40756 71.421159 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "SplitStage-4K-V2.0.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Rf25" (at 0 -1.82 90) (layer "F.SilkS"))
    (fp_text value "R=" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 58 "/25") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 19 "Net-(Cf1225-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_4.3mm_M4_Pad_Via" (layer "F.Cu")
    (tedit 56DDBFD7)
    (at 83.312 115.316)
    (descr "Mounting Hole 4.3mm, M4")
    (tags "mounting hole 4.3mm m4")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -5.3) (layer "F.SilkS"))
    (fp_text value "MountingHole_4.3mm_M4_Pad_Via" (at 0 5.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at -2.280419 -2.280419) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle (at 2.280419 -2.280419) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle (at 2.280419 2.280419) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle (at 0 0) (size 8.6 8.6) (drill 4.3) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle (at 0 -3.225) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle (at -3.225 0) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle (at 3.225 0) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle (at -2.280419 2.280419) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle (at 0 3.225) (size 0.9 0.9) (drill 0.6) (layers *.Cu *.Mask))
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 166.514664 87.471825 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "SplitStage-4K-V2.0.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Rgt2" (at 0 -1.82 90) (layer "F.SilkS"))
    (fp_text value "R=" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 10 "Net-(Cf2221-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 1 "Net-(Cc22-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 180.485112 71.421159 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "SplitStage-4K-V2.0.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Rf10" (at 0 -1.82 90) (layer "F.SilkS"))
    (fp_text value "R=" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 67 "/10") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 42 "Net-(Cf1023-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 119.746448 87.471825 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "SplitStage-4K-V2.0.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Rgt1" (at 0 -1.82 90) (layer "F.SilkS"))
    (fp_text value "R=" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 11 "Net-(Cf1718-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 4 "Net-(Cc12-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 130.679032 71.421159 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "SplitStage-4K-V2.0.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Rf5" (at 0 -1.82 90) (layer "F.SilkS"))
    (fp_text value "R=" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 33 "/5") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 13 "Net-(Cf518-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 125.953336 87.471825 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "SplitStage-4K-V2.0.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Rgn1" (at 0 -1.82 90) (layer "F.SilkS"))
    (fp_text value "R=" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 13 "Net-(Cf518-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 5 "Net-(Cf619-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Dsub:mdm25_footprint" (layer "F.Cu")
    (tedit 0)
    (at 143.13056 62.278326 180)
    (descr "380-025-213L001-1")
    (tags "Connector")
    (property "Sheetfile" "SplitStage-4K-V2.0.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole board_only)
    (fp_text reference "D4K1" (at 0.420856 2.383599) (layer "F.SilkS"))
    (fp_text value "MDM25_Female" (at 0 -2.54) (layer "F.SilkS"))
    (fp_text user "13" (at -10.16 -2.54 unlocked) (layer "F.SilkS"))
    (fp_text user "1" (at 10.16 -2.54 unlocked) (layer "F.SilkS"))
    (fp_text user "14" (at 10.16 2.54 unlocked) (layer "F.SilkS"))
    (fp_text user "25" (at -10.16 2.54 unlocked) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 -0.338) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 7.62 -0.65 180) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask)
      (net 34 "/1") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 6.35 -0.65 180) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask)
      (net 36 "/2") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle (at 5.08 -0.65 180) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask)
      (net 37 "/3") (pinfunction "3") (pintype "passive"))
    (pad "4" thru_hole circle (at 3.81 -0.65 180) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask)
      (net 39 "/4") (pinfunction "4") (pintype "passive"))
    (pad "5" thru_hole circle (at 2.54 -0.65 180) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask)
      (net 33 "/5") (pinfunction "5") (pintype "passive"))
    (pad "6" thru_hole circle (at 1.27 -0.65 180) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask)
      (net 8 "/6") (pinfunction "6") (pintype "passive"))
    (pad "7" thru_hole circle (at 0 -0.65 180) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask)
      (net 64 "/7") (pinfunction "7") (pintype "passive"))
    (pad "8" thru_hole circle (at -1.27 -0.65 180) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask)
      (net 65 "/8") (pinfunction "8") (pintype "passive"))
    (pad "9" thru_hole circle (at -2.54 -0.65 180) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask)
      (net 66 "/9") (pinfunction "9") (pintype "passive"))
    (pad "10" thru_hole circle (at -3.81 -0.65 180) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask)
      (net 67 "/10") (pinfunction "10") (pintype "passive"))
    (pad "11" thru_hole circle (at -5.08 -0.65 180) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask)
      (net 68 "/11") (pinfunction "11") (pintype "passive"))
    (pad "12" thru_hole circle (at -6.35 -0.65 180) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask)
      (net 57 "/12") (pinfunction "12") (pintype "passive"))
    (pad "13" thru_hole circle (at -7.62 -0.65 180) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask)
      (net 45 "unconnected-(D4K1-Pad13)") (pinfunction "13") (pintype "passive"))
    (pad "14" thru_hole circle (at 6.99 0.45 180) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask)
      (net 18 "/14") (pinfunction "P14") (pintype "passive"))
    (pad "15" thru_hole circle (at 5.72 0.45 180) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask)
      (net 20 "/15") (pinfunction "P15") (pintype "passive"))
    (pad "16" thru_hole circle (at 4.45 0.45 180) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask)
      (net 22 "/16") (pinfunction "P16") (pintype "passive"))
    (pad "17" thru_hole circle (at 3.18 0.45 180) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask)
      (net 23 "/17") (pinfunction "P17") (pintype "passive"))
    (pad "18" thru_hole circle (at 1.91 0.45 180) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask)
      (net 24 "/18") (pinfunction "P18") (pintype "passive"))
    (pad "19" thru_hole circle (at 0.64 0.45 180) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask)
      (net 32 "/19") (pinfunction "P19") (pintype "passive"))
    (pad "20" thru_hole circle (at -0.64 0.45 180) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask)
      (net 63 "/20") (pinfunction "P20") (pintype "passive"))
    (pad "21" thru_hole circle (at -1.91 0.45 180) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask)
      (net 62 "/21") (pinfunction "P21") (pintype "passive"))
    (pad "22" thru_hole circle (at -3.18 0.45 180) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask)
      (net 61 "/22") (pinfunction "P22") (pintype "passive"))
    (pad "23" thru_hole circle (at -4.45 0.45 180) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask)
      (net 60 "/23") (pinfunction "P23") (pintype "passive"))
    (pad "24" thru_hole circle (at -5.72 0.45 180) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask)
      (net 59 "/24") (pinfunction "P24") (pintype "passive"))
    (pad "25" thru_hole circle (at -6.99 0.45 180) (size 1.05 1.05) (drill 0.61) (layers *.Cu *.Mask)
      (net 58 "/25") (pinfunction "P25") (pintype "passive"))
    (pad "MH1" thru_hole circle (at -12.275 -0.1 180) (size 4.305 4.305) (drill 2.87) (layers *.Cu *.Mask))
    (pad "MH2" thru_hole circle (at 12.275 -0.1 180) (size 4.305 4.305) (drill 2.87) (layers *.Cu *.Mask))
    (model "380-025-213L001.stp"
      (offset (xyz 7.62 0.65 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 0 0))
    )
  )
  (gr_rect (start 73.77 49.26) (end 212.55 123.43) (layer "Edge.Cuts") (width 0.05) (fill none))
  (gr_text "SPLENDOR\nSplit Stage Charge Amp \n4K board\nJadyn Anczarski\n20230419" (at 190.74 108.6) (layer "F.SilkS"))
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 211.074 121.92)
        (xy 76.2 121.92)
        (xy 76.2 50.546)
        (xy 211.074 50.546)
      )
    )
  )
)
