<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.2.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="15" x2="12" y2="27" width="0.2" layer="20"/>
<wire x1="12" y1="27" x2="33" y2="27" width="0.2" layer="20"/>
<wire x1="33" y1="27" x2="45" y2="15" width="0.2" layer="20"/>
<wire x1="45" y1="15" x2="45" y2="9" width="0.2" layer="20"/>
<wire x1="45" y1="9" x2="36" y2="0" width="0.2" layer="20"/>
<wire x1="36" y1="0" x2="9" y2="0" width="0.2" layer="20"/>
<wire x1="0" y1="15" x2="0" y2="9" width="0.2" layer="20"/>
<wire x1="0" y1="9" x2="9" y2="0" width="0.2" layer="20"/>
<text>Shoulder Angel Rev. A
Josiah Hester
09/2015
</text>
</plain>
<libraries>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
<package name="C0805">
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X04">
</package>
<package name="1X08-1.27MM">
</package>
</packages>
</library>
<library name="msp430">
<packages>
<package name="RGE24_2P1X2P1">
</package>
<package name="RHA40">
<description>*** TI: RHA *** JEDEC: S-PQFP-N40 *** 40 PINS *** 
---&gt; PIN TP (exposed thermal die pad) should be connected with GND</description>
</package>
</packages>
</library>
<library name="fdg6303n">
<description>&lt;b&gt;FDG6303N Dual N-Channel, Digital FET&lt;/b&gt;&lt;br&gt;
&lt;p&gt;These dual N-Channel logic level enhancement mode field effect transistors are produced using Fairchild's proprietary, high cell density, DMOS technology. This very high density process is especially tailored to minimize on-state resistance. This device has been designed especially for low voltage applications as a replacement for bipolar digital transistors and small signal MOSFETs.&lt;/p&gt;</description>
<packages>
<package name="SC70-6">
<description>&lt;b&gt;6-Lead Thin Shrink Small Outline Transistor Package SC70&lt;/b&gt;&lt;p&gt;
Source: http://www.analog.com/static/imported-files/data_sheets/ADA4853-1_4853-2_4853-3.pdf</description>
</package>
</packages>
</library>
<library name="fsusb42">
<description>&lt;b&gt;Low-Power, Two-Port, High-Speed, USB2.0 (480Mbps) UART Switch&lt;/b&gt;
&lt;br&gt;
&lt;p&gt;The FSUSB42 is a bi-directional, low-power, two-port, high-speed, USB2.0 switch. Configured as a double- pole, double-throw switch (DPDT) switch, it is optimized for switching between any combination of high-speed (480 Mbps) or Full-Speed (12 Mbps) sources.&lt;/p&gt;
&lt;p&gt;The FSUSB42 is compatible with the requirements of USB2.0 and features an extremely low on capacitance (CON) of 3.7 pF. The wide bandwidth of this device (720 MHz) exceeds the bandwidth needed to pass the third harmonic, resulting in signals with minimum edge and phase distortion. Superior channel-to-channel crosstalk also minimizes interference.&lt;/p&gt;
&lt;p&gt;The FSUSB42 contains special circuitry on the switch I/O pins for applications where the VCC supply is powered-off (VCC=0V), which allows the device to withstand an over-voltage condition. This device is designed to minimize current consumption even when the control voltage applied to the SEL pin is lower than the supply voltage (VCC). This feature is especially valuable to ultra-portable applications, such as cell phones, allowing for direct interface with the general- purpose I/Os of the baseband processor. Other applications include switching and connector sharing in portable cell phones, PDAs, digital cameras, printers, and notebook computers.&lt;/p&gt;</description>
<packages>
<package name="MSOP10">
<description>&lt;b&gt;10-Lead Mini Small Outline Package [MSOP]&lt;/b&gt; (RM-10)&lt;p&gt;
Source: http://www.analog.com/UploadedFiles/Data_Sheets/35641221898805SSM2167_b.pdf&lt;br&gt;
COMPLIANT TO JEDEC STANDARDS MO-187BA</description>
</package>
</packages>
</library>
<library name="max9938">
<description>&lt;b&gt;1ÃÂÃÂ¼A, 4-Bump UCSP/SOT23, Precision Current-Sense Amplifier&lt;/b&gt;&lt;br&gt;
&lt;p&gt;The MAX9938 high-side current-sense amplifier offers precision accuracy specifications of VOS less than 500ÃÂÃÂ¼V (max) and gain error less than 0.5% (max). Quiescent supply current is an ultra-low 1ÃÂÃÂ¼A. The MAX9938 fits in a tiny, 1mm x 1mm UCSPTM package size or a 5-pin SOT23 package, making the part ideal for applications in notebook computers, cell phones, PDAs, and all battery-operated portable devices where accura- cy, low quiescent current, and small size are critical.&lt;/p&gt;&lt;p&gt;
The MAX9938 features an input common-mode voltage range from 1.6V to 28V. These current-sense amplifiers have a voltage output and are offered in four gain versions: 25V/V (MAX9938T), 50V/V (MAX9938F), 100V/V (MAX9938H), and 200V/V (MAX9938W).&lt;/p&gt;&lt;p&gt;
The four gain selections offer flexibility in the choice of the external current-sense resistor. The very low 500ÃÂÃÂ¼V (max) input offset voltage allows small 25mV to 50mV full-scale VSENSE voltage for very low voltage drop at full-current measurement.&lt;/p&gt;&lt;p&gt;
The MAX9938 is offered in tiny 4-bump, UCSP (1mm x 1mm x 0.6mm footprint), 5-pin SOT23, and 6-pin ÃÂÃÂ¼DFN (2mm x 2mm x 0.8mm) packages specified for operation over the -40ÃÂÃÂ°C to +85ÃÂÃÂ°C extended temperature range.&lt;/p&gt;</description>
<packages>
<package name="SOT23-5">
<description>&lt;b&gt;5-Lead Small Outline Transistor&lt;/b&gt; Package SOT-23&lt;p&gt;
Source: http://www.analog.com/UploadedFiles/Data_Sheets/346131962AD8067_a.pdf</description>
</package>
</packages>
</library>
<library name="ncp583">
<packages>
<package name="SC82-AB_1PRIMARY">
<description>Original name &lt;b&gt;SC82-AB&lt;/b&gt;&lt;p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="R5" library="SparkFun-Passives" package="0805" value="10-150">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="0805" value="1M"/>
<element name="R3" library="SparkFun-Resistors" package="0805" value="1M"/>
<element name="C3" library="SparkFun-Capacitors" package="0805" value="470nF">
<attribute name="PROD_ID" value="CAP-08064"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="SparkFun-Capacitors" package="0805" value="10uF">
<attribute name="PROD_ID" value="CAP-08064"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="SparkFun-Capacitors" package="0805" value="2.2nF">
<attribute name="PROD_ID" value="CAP-08064"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="0805" value="47k">
<attribute name="PROD_ID" value="RES-09883"/>
</element>
<element name="JP2" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="VALUE"/>
</element>
<element name="JP3" library="SparkFun-Connectors" package="1X08-1.27MM" value="">
<attribute name="VALUE"/>
</element>
<element name="U1" library="msp430" package="RGE24_2P1X2P1" value="MSP430FR5728_RGE_24">
<attribute name="DATASHEETURL" value="http://www.ti.com/lit/gpn/MSP430FR5728"/>
<attribute name="PIN_COUNT" value="24"/>
<attribute name="GENERIC_PART_NUMBER" value="MSP430FR5728"/>
<attribute name="DESCRIPTION" value="MSP430FR573x,MSP430FR572x Mixed Signal Microcontroller"/>
<attribute name="FAMILY_NAME" value="FRAM Series"/>
<attribute name="MANUFACTURER" value="Texas Instruments"/>
<attribute name="INDUSTRY_STD_PKG_TYPE" value="VQFN"/>
<attribute name="VENDOR" value="Texas Instruments"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="msp430fr5728_rge_24"/>
<attribute name="PACKAGE_DESIGNATOR" value="RGE"/>
<attribute name="NAME"/>
</element>
<element name="JP1" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="VALUE"/>
</element>
<element name="U2" library="msp430" package="RHA40" value="MSP430FR5739-RHARHAPACKAGE"/>
<element name="C1" library="SparkFun-Capacitors" package="0805" value="0.1uF">
<attribute name="PROD_ID" value="CAP-08064"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$4" library="fdg6303n" package="SC70-6" value="FDG6303N"/>
<element name="U3" library="fsusb42" package="MSOP10" value="FSUSB42"/>
<element name="U4" library="max9938" package="SOT23-5" value="MAX9938"/>
<element name="U$1" library="fdg6303n" package="SC70-6" value="FDG6303N"/>
<element name="R4" library="SparkFun-Passives" package="0805" value="10">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="SparkFun-Passives" package="0805" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U5" library="ncp583" package="SC82-AB_1PRIMARY" value="NCP583"/>
<element name="C4" library="SparkFun-Capacitors" package="C0805" value="0.1uF"/>
<element name="C8" library="SparkFun-Capacitors" package="C0805" value="470nF"/>
<element name="C9" library="SparkFun-Capacitors" package="C0805" value="100uF"/>
<element name="R7" library="SparkFun-Resistors" package="0805" value="47k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C10" library="SparkFun-Capacitors" package="C0805" value="2.2nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="R3" pad="1"/>
<contactref element="C3" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="JP2" pad="1"/>
<contactref element="JP3" pad="8"/>
<contactref element="JP1" pad="1"/>
<contactref element="U2" pad="39"/>
<contactref element="U2" pad="31"/>
<contactref element="C1" pad="2"/>
<contactref element="U3" pad="5"/>
<contactref element="U3" pad="10"/>
<contactref element="U4" pad="2"/>
<contactref element="U4" pad="1"/>
<contactref element="U5" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="U1" pad="19"/>
<contactref element="C4" pad="2"/>
<contactref element="U1" pad="23"/>
<contactref element="C9" pad="1"/>
<contactref element="C10" pad="1"/>
<contactref element="U1" pad="25"/>
</signal>
<signal name="LOAD_V+">
<contactref element="R5" pad="2"/>
<contactref element="R2" pad="1"/>
<contactref element="U$4" pad="4"/>
<contactref element="U$4" pad="1"/>
<contactref element="U4" pad="4"/>
<contactref element="U$1" pad="3"/>
<contactref element="U$1" pad="6"/>
</signal>
<signal name="VS_ADC">
<contactref element="R3" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="U1" pad="2"/>
</signal>
<signal name="VBAT">
</signal>
<signal name="SCK">
<contactref element="JP3" pad="2"/>
<contactref element="U1" pad="15"/>
<contactref element="U2" pad="23"/>
</signal>
<signal name="MOSI">
<contactref element="JP3" pad="4"/>
<contactref element="U3" pad="7"/>
<contactref element="U3" pad="8"/>
</signal>
<signal name="VCC_TARGET">
<contactref element="C5" pad="1"/>
<contactref element="R1" pad="2"/>
<contactref element="JP2" pad="2"/>
<contactref element="JP3" pad="1"/>
<contactref element="U2" pad="40"/>
<contactref element="U2" pad="32"/>
<contactref element="C1" pad="1"/>
<contactref element="U$4" pad="6"/>
</signal>
<signal name="MISO">
<contactref element="JP3" pad="3"/>
<contactref element="U3" pad="6"/>
<contactref element="U3" pad="9"/>
</signal>
<signal name="N$1">
<contactref element="C3" pad="1"/>
<contactref element="U2" pad="30"/>
</signal>
<signal name="TEST_T">
<contactref element="JP2" pad="3"/>
<contactref element="U2" pad="19"/>
<contactref element="U1" pad="9"/>
</signal>
<signal name="GDO2">
<contactref element="JP3" pad="7"/>
<contactref element="U1" pad="6"/>
<contactref element="U2" pad="26"/>
</signal>
<signal name="GDO0">
<contactref element="JP3" pad="5"/>
<contactref element="U1" pad="7"/>
<contactref element="U2" pad="17"/>
</signal>
<signal name="!CS_RADIO">
<contactref element="JP3" pad="6"/>
<contactref element="U1" pad="8"/>
<contactref element="U2" pad="8"/>
</signal>
<signal name="CS_ADC">
<contactref element="U1" pad="1"/>
<contactref element="U4" pad="3"/>
</signal>
<signal name="TEST_SA">
<contactref element="U1" pad="11"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="SHUNT1">
<contactref element="U1" pad="22"/>
<contactref element="U$1" pad="5"/>
</signal>
<signal name="SHUNT2">
<contactref element="U1" pad="21"/>
<contactref element="U$1" pad="2"/>
</signal>
<signal name="VCC_RADIO">
<contactref element="U$4" pad="3"/>
</signal>
<signal name="VCC_GATE_TARGET">
<contactref element="U$4" pad="2"/>
<contactref element="U1" pad="4"/>
</signal>
<signal name="VCC_GATE_RADIO">
<contactref element="U$4" pad="5"/>
<contactref element="U1" pad="5"/>
</signal>
<signal name="!RST_T">
<contactref element="U1" pad="10"/>
<contactref element="U2" pad="20"/>
<contactref element="R1" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="JP2" pad="4"/>
</signal>
<signal name="!RST_SA">
<contactref element="JP1" pad="2"/>
<contactref element="U1" pad="12"/>
<contactref element="R7" pad="1"/>
<contactref element="C10" pad="2"/>
</signal>
<signal name="MISO_SA">
<contactref element="U1" pad="17"/>
<contactref element="U3" pad="4"/>
</signal>
<signal name="MOSI_SA">
<contactref element="U1" pad="16"/>
<contactref element="U3" pad="3"/>
</signal>
<signal name="MISO_T">
<contactref element="U2" pad="29"/>
</signal>
<signal name="MOSI_T">
<contactref element="U2" pad="28"/>
</signal>
<signal name="BUS_SEL">
<contactref element="U1" pad="3"/>
<contactref element="U3" pad="2"/>
</signal>
<signal name="BATT+">
<contactref element="JP1" pad="4"/>
<contactref element="U5" pad="1"/>
<contactref element="U5" pad="4"/>
</signal>
<signal name="N$5">
<contactref element="U$1" pad="4"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="U$1" pad="1"/>
<contactref element="R6" pad="2"/>
</signal>
<signal name="VCC">
<contactref element="R5" pad="1"/>
<contactref element="U5" pad="3"/>
<contactref element="U4" pad="5"/>
<contactref element="R6" pad="1"/>
<contactref element="R4" pad="1"/>
<contactref element="U3" pad="1"/>
<contactref element="C9" pad="2"/>
<contactref element="R7" pad="2"/>
<contactref element="C4" pad="1"/>
<contactref element="U1" pad="24"/>
<contactref element="U1" pad="20"/>
</signal>
<signal name="N$8">
<contactref element="U1" pad="18"/>
<contactref element="C8" pad="1"/>
</signal>
<signal name="BSL_TX">
<contactref element="U2" pad="21"/>
<contactref element="U1" pad="14"/>
</signal>
<signal name="BSL_RX">
<contactref element="U2" pad="22"/>
<contactref element="U1" pad="13"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
